(kicad_pcb (version 20171130) (host pcbnew "(5.1.5-0-10_14)")
  (general
    (thickness 1.6)
    (drawings 5)
    (tracks 145)
    (zones 0)
    (modules 25)
    (nets 16)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(H2-Pad1)")
  (net 2 "Net-(H2-Pad3)")
  (net 3 "Net-(H2-Pad5)")
  (net 4 "Net-(H2-Pad7)")
  (net 5 "Net-(H2-Pad10)")
  (net 6 "Net-(H2-Pad15)")
  (net 7 "Net-(J1-Pad1)")
  (net 8 "Net-(J2-Pad10)")
  (net 9 "Net-(J3-Pad1)")
  (net 10 "Net-(J4-Pad1)")
  (net 11 "Net-(J5-Pad1)")
  (net 12 "Net-(J7-Pad10)")
  (net 13 "Net-(J8-Pad10)")
  (net 14 "Net-(J10-Pad1)")
  (net 15 "Net-(J11-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(H2-Pad1)")
    (add_net "Net-(H2-Pad10)")
    (add_net "Net-(H2-Pad15)")
    (add_net "Net-(H2-Pad3)")
    (add_net "Net-(H2-Pad5)")
    (add_net "Net-(H2-Pad7)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J10-Pad1)")
    (add_net "Net-(J11-Pad1)")
    (add_net "Net-(J2-Pad10)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(J4-Pad1)")
    (add_net "Net-(J5-Pad1)")
    (add_net "Net-(J7-Pad10)")
    (add_net "Net-(J8-Pad10)")
  )
  (module "chillpizza:graphic button gang text" (layer F.Cu) (tedit 0)
    (at 135 180)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module "chillpizza:graphic pants rear" (layer B.Cu) (tedit 0)
    (at 135 123.75 180)
    (fp_text reference G*** (at 0 0) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer B.SilkS) hide)
  )
  (module "chillpizza:graphic button gang options" (layer F.Cu) (tedit 0)
    (at 134.25 149.5)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module "chillpizza:graphic button gang options" (layer F.Cu) (tedit 0)
    (at 134.25 108.5)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module "chillpizza:graphic button gang options" (layer F.Cu) (tedit 0)
    (at 134.25 69.5)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module "chillpizza:beat farm vertical only a" (layer F.Cu) (tedit 0)
    (at 140.5 62.5)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module "chillpizza:beat farm vertical no a" (layer F.Cu) (tedit 0)
    (at 140.5 62.5)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 132.5 62.5)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference H1 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 132.5 185)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference H3 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 127.35 71.5)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference J1 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value Conn_01x01_Female (at 0 2.33) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 142.75 77.25)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference J3 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value Conn_01x01_Female (at 0 2.33) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J3-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module keyswitches:Kailh_socket_MX (layer F.Cu) (tedit 5F2323EC)
    (at 135 88)
    (descr "MX-style keyswitch with Kailh socket mount")
    (tags MX,cherry,gateron,kailh,pg1511,socket)
    (attr smd)
    (fp_text reference SW1 (at 0 -8.255) (layer B.SilkS) hide)
    (fp_text value SW_SPST (at 0 8.255) (layer F.Fab))
    (fp_text user %R (at -0.635 -4.445) (layer B.Fab))
    (fp_text user %V (at -0.635 0.635) (layer B.Fab))
    (pad 1 smd rect (at 6.29 -5.08) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(J3-Pad1)"))
    (pad "" np_thru_hole circle (at 2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
    (pad 2 smd rect (at -7.56 -2.54) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(J2-Pad10)"))
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x08_P2.54mm_Vertical_SMD (layer B.Cu) (tedit 59FED5CC)
    (at 140 144 180)
    (descr "surface-mounted straight pin header, 2x08, 2.54mm pitch, double rows")
    (tags "Surface mounted pin header SMD 2x08 2.54mm double row")
    (attr smd)
    (fp_text reference H2 (at 0 11.22) (layer B.SilkS) hide)
    (fp_text value EURO_PWR_2x8 (at 0 -11.22) (layer B.Fab))
    (fp_text user %R (at 0 0 -90) (layer B.Fab))
    (pad 1 smd rect (at -2.525 8.89 180) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 1 "Net-(H2-Pad1)"))
    (pad 2 smd rect (at 2.525 8.89 180) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 1 "Net-(H2-Pad1)"))
    (pad 3 smd rect (at -2.525 6.35 180) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(H2-Pad3)"))
    (pad 4 smd rect (at 2.525 6.35 180) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(H2-Pad3)"))
    (pad 5 smd rect (at -2.525 3.81 180) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(H2-Pad5)"))
    (pad 6 smd rect (at 2.525 3.81 180) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(H2-Pad5)"))
    (pad 7 smd rect (at -2.525 1.27 180) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(H2-Pad7)"))
    (pad 8 smd rect (at 2.525 1.27 180) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(H2-Pad7)"))
    (pad 9 smd rect (at -2.525 -1.27 180) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(H2-Pad10)"))
    (pad 10 smd rect (at 2.525 -1.27 180) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(H2-Pad10)"))
    (pad 11 smd rect (at -2.525 -3.81 180) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(H2-Pad10)"))
    (pad 12 smd rect (at 2.525 -3.81 180) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(H2-Pad10)"))
    (pad 13 smd rect (at -2.525 -6.35 180) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(H2-Pad10)"))
    (pad 14 smd rect (at 2.525 -6.35 180) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(H2-Pad10)"))
    (pad 15 smd rect (at -2.525 -8.89 180) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(H2-Pad15)"))
    (pad 16 smd rect (at 2.525 -8.89 180) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(H2-Pad15)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x08_P2.54mm_Vertical_SMD.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 127.35 110.5)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference J4 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value Conn_01x01_Female (at 0 2.33) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J4-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 127.35 151.5)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference J5 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value Conn_01x01_Female (at 0 2.33) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J5-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x05_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 137.5 113.75 270)
    (descr "Through hole straight pin header, 2x05, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x05 2.54mm double row")
    (fp_text reference J7 (at 1.27 -2.33 90) (layer F.SilkS) hide)
    (fp_text value Conn_02x05_Odd_Even (at 1.27 12.49 90) (layer F.Fab))
    (fp_text user %R (at 1.27 5.08) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(H2-Pad7)"))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J7-Pad10)"))
    (pad 3 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(H2-Pad5)"))
    (pad 4 thru_hole oval (at 2.54 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J7-Pad10)"))
    (pad 5 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(H2-Pad10)"))
    (pad 6 thru_hole oval (at 2.54 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J7-Pad10)"))
    (pad 7 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(H2-Pad15)"))
    (pad 8 thru_hole oval (at 2.54 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J7-Pad10)"))
    (pad 9 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J4-Pad1)"))
    (pad 10 thru_hole oval (at 2.54 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J7-Pad10)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x05_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x05_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 137.5 154.75 270)
    (descr "Through hole straight pin header, 2x05, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x05 2.54mm double row")
    (fp_text reference J8 (at 1.27 -2.33 90) (layer F.SilkS) hide)
    (fp_text value Conn_02x05_Odd_Even (at 1.27 12.49 90) (layer F.Fab))
    (fp_text user %R (at 1.27 5.08) (layer F.Fab))
    (pad 10 thru_hole oval (at 2.54 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(J8-Pad10)"))
    (pad 9 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J5-Pad1)"))
    (pad 8 thru_hole oval (at 2.54 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(J8-Pad10)"))
    (pad 7 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(H2-Pad15)"))
    (pad 6 thru_hole oval (at 2.54 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(J8-Pad10)"))
    (pad 5 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(H2-Pad10)"))
    (pad 4 thru_hole oval (at 2.54 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(J8-Pad10)"))
    (pad 3 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(H2-Pad5)"))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(J8-Pad10)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(H2-Pad7)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x05_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 142.75 116.25)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference J10 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value Conn_01x01_Female (at 0 2.33) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(J10-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 142.75 157.25)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference J11 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value Conn_01x01_Female (at 0 2.33) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(J11-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module keyswitches:SW_PG1350 (layer F.Cu) (tedit 5DD50112)
    (at 135 88)
    (descr "Kailh \"Choc\" PG1350 keyswitch")
    (tags kailh,choc)
    (fp_text reference SW2 (at 0 -8.255) (layer F.SilkS) hide)
    (fp_text value SW_SPST (at 0 8.255) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 3.429 3.429) (drill 3.429) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at -5 3.8) (size 2.032 2.032) (drill 1.27) (layers *.Cu *.Mask)
      (net 8 "Net-(J2-Pad10)"))
    (pad 1 thru_hole circle (at 0 5.9) (size 2.032 2.032) (drill 1.27) (layers *.Cu *.Mask)
      (net 9 "Net-(J3-Pad1)"))
    (pad "" np_thru_hole circle (at 5.22 -4.2) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 5.5 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -5.5 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
  )
  (module keyswitches:Kailh_socket_MX (layer F.Cu) (tedit 5F2323EC)
    (at 135 127)
    (descr "MX-style keyswitch with Kailh socket mount")
    (tags MX,cherry,gateron,kailh,pg1511,socket)
    (attr smd)
    (fp_text reference SW3 (at 0 -8.255) (layer B.SilkS) hide)
    (fp_text value SW_SPST (at 0 8.255) (layer F.Fab))
    (fp_text user %R (at -0.635 -4.445) (layer B.Fab))
    (fp_text user %V (at -0.635 0.635) (layer B.Fab))
    (pad 1 smd rect (at 6.29 -5.08) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(J10-Pad1)"))
    (pad "" np_thru_hole circle (at 2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
    (pad 2 smd rect (at -7.56 -2.54) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(J7-Pad10)"))
  )
  (module keyswitches:SW_PG1350 (layer F.Cu) (tedit 5DD50112)
    (at 135 127)
    (descr "Kailh \"Choc\" PG1350 keyswitch")
    (tags kailh,choc)
    (fp_text reference SW4 (at 0 -8.255) (layer F.SilkS) hide)
    (fp_text value SW_SPST (at 0 8.255) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad "" np_thru_hole circle (at -5.5 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 5.5 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 5.22 -4.2) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 5.9) (size 2.032 2.032) (drill 1.27) (layers *.Cu *.Mask)
      (net 14 "Net-(J10-Pad1)"))
    (pad 2 thru_hole circle (at -5 3.8) (size 2.032 2.032) (drill 1.27) (layers *.Cu *.Mask)
      (net 12 "Net-(J7-Pad10)"))
    (pad "" np_thru_hole circle (at 0 0) (size 3.429 3.429) (drill 3.429) (layers *.Cu *.Mask))
  )
  (module keyswitches:Kailh_socket_MX (layer F.Cu) (tedit 5F2323EC)
    (at 135 168)
    (descr "MX-style keyswitch with Kailh socket mount")
    (tags MX,cherry,gateron,kailh,pg1511,socket)
    (attr smd)
    (fp_text reference SW5 (at 0 -8.255) (layer B.SilkS) hide)
    (fp_text value SW_SPST (at 0 8.255) (layer F.Fab))
    (fp_text user %V (at -0.635 0.635) (layer B.Fab))
    (fp_text user %R (at -0.635 -4.445) (layer B.Fab))
    (pad 2 smd rect (at -7.56 -2.54) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(J8-Pad10)"))
    (pad "" np_thru_hole circle (at -5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
    (pad 1 smd rect (at 6.29 -5.08) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask)
      (net 15 "Net-(J11-Pad1)"))
  )
  (module keyswitches:SW_PG1350 (layer F.Cu) (tedit 5DD50112)
    (at 135 168)
    (descr "Kailh \"Choc\" PG1350 keyswitch")
    (tags kailh,choc)
    (fp_text reference SW6 (at 0 -8.255) (layer F.SilkS) hide)
    (fp_text value SW_SPST (at 0 8.255) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 3.429 3.429) (drill 3.429) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at -5 3.8) (size 2.032 2.032) (drill 1.27) (layers *.Cu *.Mask)
      (net 13 "Net-(J8-Pad10)"))
    (pad 1 thru_hole circle (at 0 5.9) (size 2.032 2.032) (drill 1.27) (layers *.Cu *.Mask)
      (net 15 "Net-(J11-Pad1)"))
    (pad "" np_thru_hole circle (at 5.22 -4.2) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 5.5 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -5.5 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x05_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 137.5 74.75 270)
    (descr "Through hole straight pin header, 2x05, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x05 2.54mm double row")
    (fp_text reference J2 (at 1.27 -2.33 90) (layer F.SilkS) hide)
    (fp_text value Conn_02x05_Odd_Even (at 1.27 12.49 90) (layer F.Fab))
    (fp_text user %R (at 1.27 5.08) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(H2-Pad7)"))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J2-Pad10)"))
    (pad 3 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(H2-Pad5)"))
    (pad 4 thru_hole oval (at 2.54 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J2-Pad10)"))
    (pad 5 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(H2-Pad10)"))
    (pad 6 thru_hole oval (at 2.54 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J2-Pad10)"))
    (pad 7 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(H2-Pad15)"))
    (pad 8 thru_hole oval (at 2.54 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J2-Pad10)"))
    (pad 9 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad1)"))
    (pad 10 thru_hole oval (at 2.54 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J2-Pad10)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x05_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 145 59.5) (end 125 59.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 145 188) (end 145 59.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 125 188) (end 145 188) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 125 59.5) (end 125 188) (layer Edge.Cuts) (width 0.05))
)
