<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<board>
<plain>
<wire x1="-5.207" y1="0" x2="5.207" y2="0" width="0" layer="20"/>
<wire x1="5.207" y1="0" x2="5.207" y2="16.637" width="0" layer="20"/>
<wire x1="5.207" y1="16.637" x2="-5.207" y2="16.637" width="0" layer="20"/>
<wire x1="-5.207" y1="16.637" x2="-5.207" y2="0" width="0" layer="20"/>
<text>I</text>
<text>O</text>
<text>LT3042
 VREG</text>
</plain>
<libraries>
<library name="IRT2008CON">
<packages>
<package name="WIREPAD60-40">
</package>
</packages>
</library>
<library name="IRT2008Passive">
<packages>
<package name="BOURNS-3296Y">
</package>
<package name="603">
</package>
<package name="1206">
</package>
<package name="1206P">
</package>
</packages>
</library>
<library name="Dan_Con">
<description>Dan Contract Library.</description>
<packages>
<package name="MSOP-10">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="R1" library="IRT2008Passive" package="BOURNS-3296Y" value="OPEN (WAS 100K)">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="IRT2008Passive" package="1206" value="22uF">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="VIN" library="IRT2008CON" package="WIREPAD60-40" value="WIREPAD60-40"/>
<element name="C2" library="IRT2008Passive" package="1206" value="10uF">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="U1" library="Dan_Con" package="MSOP-10" value="LT3042MSE">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="R3" library="IRT2008Passive" package="603" value="000">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="R2" library="IRT2008Passive" package="603" value="100K">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="C4" library="IRT2008Passive" package="1206P" value="33uF Tant">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="GND" library="IRT2008CON" package="WIREPAD60-40" value="WIREPAD60-40"/>
<element name="VOUT" library="IRT2008CON" package="WIREPAD60-40" value="WIREPAD60-40"/>
<element name="C1" library="IRT2008Passive" package="1206P" value="22uF Tant">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="VBATT">
<contactref element="C2" pad="2"/>
<contactref element="U1" pad="2"/>
<contactref element="U1" pad="1"/>
<contactref element="U1" pad="6"/>
<contactref element="U1" pad="3"/>
<contactref element="VIN" pad="P$1"/>
<contactref element="C1" pad="+"/>
</signal>
<signal name="VOUT">
<contactref element="C3" pad="2"/>
<contactref element="U1" pad="10"/>
<contactref element="VOUT" pad="P$1"/>
<contactref element="U1" pad="9"/>
</signal>
<signal name="GND">
<contactref element="C3" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="U1" pad="PAD"/>
<contactref element="U1" pad="8"/>
<contactref element="R3" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="C4" pad="-"/>
<contactref element="GND" pad="P$1"/>
<contactref element="C1" pad="-"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="R3" pad="1"/>
<contactref element="U1" pad="5"/>
</signal>
<signal name="N$2">
<contactref element="R1" pad="2"/>
<contactref element="R1" pad="3"/>
<contactref element="C4" pad="+"/>
<contactref element="R2" pad="1"/>
<contactref element="U1" pad="7"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
