<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<text>apa102-wing
r1</text>
<text>(choco)lab</text>
</plain>
<libraries>
<library name="Ai_LED">
<description>&lt;h3&gt;Ai LED&lt;/h3&gt;
&lt;p&gt;
This library includes LEDs of all shapes and sizes.
&lt;/p&gt;</description>
<packages>
<package name="LED-APA102">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="FEATHERWING">
</package>
<package name="PUSHBUTTON_SMD_SJ">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="LED1" library="Ai_LED" package="LED-APA102" value="LED-APA102"/>
<element name="LED2" library="Ai_LED" package="LED-APA102" value="LED-APA102"/>
<element name="LED3" library="Ai_LED" package="LED-APA102" value="LED-APA102"/>
<element name="MS1" library="adafruit" package="FEATHERWING" value="FEATHERWING"/>
<element name="SW1" library="adafruit" package="PUSHBUTTON_SMD_SJ" value=""/>
</elements>
<signals>
<signal name="SCK">
<contactref element="MS1" pad="11"/>
<contactref element="LED1" pad="2"/>
</signal>
<signal name="MOSI">
<contactref element="LED1" pad="1"/>
<contactref element="MS1" pad="12"/>
</signal>
<signal name="N$5">
<contactref element="LED2" pad="1"/>
<contactref element="LED1" pad="6"/>
</signal>
<signal name="N$6">
<contactref element="LED2" pad="2"/>
<contactref element="LED1" pad="5"/>
</signal>
<signal name="N$8">
<contactref element="LED3" pad="1"/>
<contactref element="LED2" pad="6"/>
</signal>
<signal name="N$9">
<contactref element="LED3" pad="2"/>
<contactref element="LED2" pad="5"/>
</signal>
<signal name="MISO">
<contactref element="MS1" pad="13"/>
<contactref element="SW1" pad="P$1"/>
</signal>
<signal name="3V">
<contactref element="LED1" pad="4"/>
<contactref element="LED2" pad="4"/>
<contactref element="LED3" pad="4"/>
<contactref element="MS1" pad="2"/>
</signal>
<signal name="GND">
<contactref element="LED1" pad="3"/>
<contactref element="LED2" pad="3"/>
<contactref element="LED3" pad="3"/>
<contactref element="SW1" pad="P$2"/>
<contactref element="MS1" pad="4"/>
</signal>
<signal name="N$1">
</signal>
<signal name="N$2">
</signal>
<signal name="N$3">
</signal>
<signal name="N$4">
</signal>
<signal name="N$7">
</signal>
</signals>
</board>
</drawing>
</eagle>
