(kicad_pcb (version 20171130) (host pcbnew "(5.1.5-0-10_14)")
  (general
    (thickness 1.2)
    (drawings 16)
    (tracks 34)
    (zones 0)
    (modules 2)
    (nets 7)
  )
  (page A4)
  (title_block
    (title GB-BRK-LINK-B)
    (rev v1.0)
    (company https://gekkio.fi)
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.3)
    (user_trace_width 0.8)
    (trace_clearance 0.3)
    (zone_clearance 0.4)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.15)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (solder_mask_min_width 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile true)
      (excludeedgelayer false)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerber/"))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad1)")
  (net 2 "Net-(J1-Pad2)")
  (net 3 "Net-(J1-Pad3)")
  (net 4 "Net-(J1-Pad4)")
  (net 5 "Net-(J1-Pad5)")
  (net 6 /GND)
  (net_class Default "This is the default net class."
    (clearance 0.3)
    (trace_width 0.3)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /GND)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
  )
  (module Gekkio_Connector:GameBoy_LinkPort_MGB_Horizontal (layer F.Cu) (tedit 5C33E0BE)
    (at 150.965 95.68)
    (fp_text reference J2 (at 2.5 -4.6) (layer F.SilkS) hide)
    (fp_text value GameBoy_LinkPort (at 2.5 8.8) (layer F.Fab))
    (fp_text user %R (at 5.5 2 90) (layer F.Fab))
    (pad 6 thru_hole circle (at 2 4) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 6 /GND))
    (pad 5 thru_hole circle (at 0 4) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad5)"))
    (pad 4 thru_hole circle (at 2 2) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad4)"))
    (pad 3 thru_hole circle (at 0 2) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad3)"))
    (pad 2 thru_hole circle (at 2 0) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (pad SH thru_hole oval (at 1.6 6.5 90) (size 1.4 2.2) (drill oval 1 1.8) (layers *.Cu *.Mask)
      (net 6 /GND))
    (pad SH thru_hole oval (at 1.6 -2.5 90) (size 1.4 2.2) (drill oval 1 1.8) (layers *.Cu *.Mask)
      (net 6 /GND))
    (model ${KISYS3DMOD}/Gekkio_Connector.3dshapes/GameBoy_LinkPort_MGB_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Vertical (layer F.Cu) (tedit 5C33E0BC)
    (at 143.138 91.33)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (fp_text reference J1 (at -2.8 -0.7) (layer F.SilkS) hide)
    (fp_text value Conn_01x06 (at 0 15.03) (layer F.Fab))
    (fp_text user %R (at 0 6.35 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x06_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text 2020/04 (at 147.828 92.329) (layer B.SilkS))
  (gr_text Poldet (at 147.955 90.805) (layer B.SilkS))
  (gr_arc (start 142.589 104.426) (end 140.589 104.426) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 153.575 104.426) (end 153.575 106.426) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 153.67 90.9) (end 155.67 90.9) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 142.589 90.9) (end 142.589 88.9) (angle -90.91665426) (layer Edge.Cuts) (width 0.15))
  (gr_text GND (at 144.938 104.03) (layer F.SilkS))
  (gr_text SC (at 144.938 101.58) (layer F.SilkS))
  (gr_text SD (at 144.938 99.03) (layer F.SilkS))
  (gr_text SI (at 144.938 96.48) (layer F.SilkS))
  (gr_text SO (at 144.938 93.93) (layer F.SilkS))
  (gr_text VDD (at 144.938 91.38) (layer F.SilkS))
  (gr_line (start 142.589 106.426) (end 153.575 106.426) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 155.67 90.9) (end 155.575 104.426) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 142.589 88.9) (end 153.67 88.9) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 140.589 90.932) (end 140.589 104.426) (layer Edge.Cuts) (width 0.15))
  (zone (net 6) (net_name /GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.4))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 156.337 88.5825) (xy 140.335 88.5825) (xy 140.335 106.9975) (xy 156.337 106.9975)
      )
    )
  )
)
