(kicad_pcb (version 4) (host pcbnew 4.0.2+e4-6225~38~ubuntu14.04.1-stable)
  (general
    (links 141)
    (no_connects 0)
    (area 93.439999 32.294999 193.590001 112.365001)
    (thickness 1.6)
    (drawings 13)
    (tracks 794)
    (zones 0)
    (modules 21)
    (nets 86)
  )
  (page A4)
  (title_block
    (title "FlashROM 99 Cartridge")
    (date 2016-06-10)
    (rev 2)
    (company "Copyright (c) 2016 Ralph Benzinger")
    (comment 2 "Released as Open Source Hardware under CERN OHL 1.2 and GNU GPL 3 licenses")
    (comment 4 "A TI 99 cartridge that allows for running ROM images stored on an SD card")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.778 15)
    (pad_drill 0)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (grid_origin 92.075 31.75)
    (visible_elements FFFDFF7F)
    (pcbplotparams
      (layerselection 0x010e0_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference false)
      (plotvalue true)
      (plotinvisibletext true)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerber/))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 +5V)
  (net 3 "Net-(D1-Pad2)")
  (net 4 /D0)
  (net 5 /D1)
  (net 6 /D2)
  (net 7 /D3)
  (net 8 /D4)
  (net 9 /D5)
  (net 10 /D6)
  (net 11 /D7)
  (net 12 BUSE)
  (net 13 /A11)
  (net 14 /A12)
  (net 15 /A13)
  (net 16 /A14)
  (net 17 /A10)
  (net 18 /A9)
  (net 19 /A8)
  (net 20 /A7)
  (net 21 /A6)
  (net 22 /A5)
  (net 23 /A4)
  (net 24 /A3)
  (net 25 /A2)
  (net 26 /A1)
  (net 27 /A0)
  (net 28 "Net-(M1-Pad7)")
  (net 29 "Net-(P1-Pad33)")
  (net 30 "Net-(P1-Pad31)")
  (net 31 "Net-(P1-Pad1)")
  (net 32 "Net-(P1-Pad27)")
  (net 33 "Net-(P1-Pad25)")
  (net 34 "Net-(P1-Pad23)")
  (net 35 "Net-(P1-Pad21)")
  (net 36 "Net-(P1-Pad17)")
  (net 37 "Net-(P1-Pad15)")
  (net 38 "Net-(P1-Pad13)")
  (net 39 "Net-(P1-Pad11)")
  (net 40 "Net-(P1-Pad9)")
  (net 41 "Net-(P1-Pad7)")
  (net 42 "Net-(P1-Pad5)")
  (net 43 "Net-(P1-Pad3)")
  (net 44 "Net-(P1-Pad36)")
  (net 45 ROMS)
  (net 46 "Net-(P1-Pad30)")
  (net 47 "Net-(P1-Pad28)")
  (net 48 "Net-(P1-Pad26)")
  (net 49 "Net-(P1-Pad24)")
  (net 50 "Net-(P1-Pad22)")
  (net 51 "Net-(P1-Pad20)")
  (net 52 "Net-(P1-Pad18)")
  (net 53 "Net-(P1-Pad16)")
  (net 54 "Net-(P1-Pad14)")
  (net 55 "Net-(P1-Pad12)")
  (net 56 "Net-(P1-Pad10)")
  (net 57 "Net-(P1-Pad8)")
  (net 58 "Net-(P1-Pad6)")
  (net 59 "Net-(P1-Pad4)")
  (net 60 "Net-(U1-Pad3)")
  (net 61 "Net-(U1-Pad4)")
  (net 62 "Net-(U4-Pad2)")
  (net 63 "Net-(U4-Pad3)")
  (net 64 "Net-(U4-Pad4)")
  (net 65 "Net-(U4-Pad5)")
  (net 66 "Net-(U4-Pad6)")
  (net 67 "Net-(U4-Pad7)")
  (net 68 "Net-(U4-Pad8)")
  (net 69 "Net-(U4-Pad9)")
  (net 70 "Net-(C7-Pad1)")
  (net 71 "Net-(M1-Pad2)")
  (net 72 "Net-(M1-Pad3)")
  (net 73 "Net-(M1-Pad4)")
  (net 74 "Net-(M1-Pad5)")
  (net 75 "Net-(R2-Pad2)")
  (net 76 "Net-(R3-Pad2)")
  (net 77 "Net-(U1-Pad18)")
  (net 78 "Net-(U4-Pad12)")
  (net 79 "Net-(U4-Pad15)")
  (net 80 "Net-(U5-Pad20)")
  (net 81 "Net-(U5-Pad27)")
  (net 82 "Net-(U6-Pad5)")
  (net 83 "Net-(U6-Pad18)")
  (net 84 "Net-(U6-Pad19)")
  (net 85 "Net-(P1-Pad32)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /A0)
    (add_net /A1)
    (add_net /A10)
    (add_net /A11)
    (add_net /A12)
    (add_net /A13)
    (add_net /A14)
    (add_net /A2)
    (add_net /A3)
    (add_net /A4)
    (add_net /A5)
    (add_net /A6)
    (add_net /A7)
    (add_net /A8)
    (add_net /A9)
    (add_net /D0)
    (add_net /D1)
    (add_net /D2)
    (add_net /D3)
    (add_net /D4)
    (add_net /D5)
    (add_net /D6)
    (add_net /D7)
    (add_net BUSE)
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(M1-Pad2)")
    (add_net "Net-(M1-Pad3)")
    (add_net "Net-(M1-Pad4)")
    (add_net "Net-(M1-Pad5)")
    (add_net "Net-(M1-Pad7)")
    (add_net "Net-(P1-Pad1)")
    (add_net "Net-(P1-Pad10)")
    (add_net "Net-(P1-Pad11)")
    (add_net "Net-(P1-Pad12)")
    (add_net "Net-(P1-Pad13)")
    (add_net "Net-(P1-Pad14)")
    (add_net "Net-(P1-Pad15)")
    (add_net "Net-(P1-Pad16)")
    (add_net "Net-(P1-Pad17)")
    (add_net "Net-(P1-Pad18)")
    (add_net "Net-(P1-Pad20)")
    (add_net "Net-(P1-Pad21)")
    (add_net "Net-(P1-Pad22)")
    (add_net "Net-(P1-Pad23)")
    (add_net "Net-(P1-Pad24)")
    (add_net "Net-(P1-Pad25)")
    (add_net "Net-(P1-Pad26)")
    (add_net "Net-(P1-Pad27)")
    (add_net "Net-(P1-Pad28)")
    (add_net "Net-(P1-Pad3)")
    (add_net "Net-(P1-Pad30)")
    (add_net "Net-(P1-Pad31)")
    (add_net "Net-(P1-Pad32)")
    (add_net "Net-(P1-Pad33)")
    (add_net "Net-(P1-Pad36)")
    (add_net "Net-(P1-Pad4)")
    (add_net "Net-(P1-Pad5)")
    (add_net "Net-(P1-Pad6)")
    (add_net "Net-(P1-Pad7)")
    (add_net "Net-(P1-Pad8)")
    (add_net "Net-(P1-Pad9)")
    (add_net "Net-(R2-Pad2)")
    (add_net "Net-(R3-Pad2)")
    (add_net "Net-(U1-Pad18)")
    (add_net "Net-(U1-Pad3)")
    (add_net "Net-(U1-Pad4)")
    (add_net "Net-(U4-Pad12)")
    (add_net "Net-(U4-Pad15)")
    (add_net "Net-(U4-Pad2)")
    (add_net "Net-(U4-Pad3)")
    (add_net "Net-(U4-Pad4)")
    (add_net "Net-(U4-Pad5)")
    (add_net "Net-(U4-Pad6)")
    (add_net "Net-(U4-Pad7)")
    (add_net "Net-(U4-Pad8)")
    (add_net "Net-(U4-Pad9)")
    (add_net "Net-(U5-Pad20)")
    (add_net "Net-(U5-Pad27)")
    (add_net "Net-(U6-Pad18)")
    (add_net "Net-(U6-Pad19)")
    (add_net "Net-(U6-Pad5)")
    (add_net ROMS)
  )
  (net_class Power ""
    (clearance 0.3)
    (trace_width 0.5)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net GND)
  )
  (module flashcart-footprints:SD_MODULE (layer F.Cu) (tedit 575A60AC)
    (at 161.925 82.55)
    (fp_text reference M1 (at 27.94 2.54) (layer F.SilkS))
    (fp_text value SD (at 2.54 2.54) (layer F.SilkS))
    (pad 1 thru_hole circle (at 6.35 3.81) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole circle (at 8.89 3.81) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 71 "Net-(M1-Pad2)"))
    (pad 3 thru_hole circle (at 11.43 3.81) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 72 "Net-(M1-Pad3)"))
    (pad 4 thru_hole circle (at 13.97 3.81) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 73 "Net-(M1-Pad4)"))
    (pad 5 thru_hole circle (at 16.51 3.81) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 74 "Net-(M1-Pad5)"))
    (pad 6 thru_hole circle (at 19.05 3.81) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 +5V))
    (pad 7 thru_hole circle (at 21.59 3.81) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 28 "Net-(M1-Pad7)"))
    (pad 8 thru_hole circle (at 24.13 3.81) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 8 thru_hole circle (at 24.13 1.27) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 7 thru_hole circle (at 21.59 1.27) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 28 "Net-(M1-Pad7)"))
    (pad 6 thru_hole circle (at 19.05 1.27) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 +5V))
    (pad 5 thru_hole circle (at 16.51 1.27) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 74 "Net-(M1-Pad5)"))
    (pad 4 thru_hole circle (at 13.97 1.27) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 73 "Net-(M1-Pad4)"))
    (pad 3 thru_hole circle (at 11.43 1.27) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 72 "Net-(M1-Pad3)"))
    (pad 2 thru_hole circle (at 8.89 1.27) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 71 "Net-(M1-Pad2)"))
    (pad 1 thru_hole circle (at 6.35 1.27) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
  )
  (module Housings_DIP:DIP-40_W15.24mm (layer F.Cu) (tedit 575A6085)
    (at 99.06 107.95 90)
    (descr "40-lead dip package, row spacing 15.24 mm (600 mils)")
    (tags "dil dip 2.54 600")
    (fp_text reference U6 (at 17.78 -0.635 180) (layer F.SilkS))
    (fp_text value 8515 (at 5.08 0.635 180) (layer F.SilkS))
    (pad 1 thru_hole oval (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 74 "Net-(M1-Pad5)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 72 "Net-(M1-Pad3)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 73 "Net-(M1-Pad4)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 71 "Net-(M1-Pad2)"))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 82 "Net-(U6-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 79 "Net-(U4-Pad15)"))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 78 "Net-(U4-Pad12)"))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 75 "Net-(R2-Pad2)"))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 76 "Net-(R3-Pad2)"))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 4 /D0))
    (pad 11 thru_hole oval (at 0 25.4 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 5 /D1))
    (pad 12 thru_hole oval (at 0 27.94 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 6 /D2))
    (pad 13 thru_hole oval (at 0 30.48 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 7 /D3))
    (pad 14 thru_hole oval (at 0 33.02 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 8 /D4))
    (pad 15 thru_hole oval (at 0 35.56 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 9 /D5))
    (pad 16 thru_hole oval (at 0 38.1 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 10 /D6))
    (pad 17 thru_hole oval (at 0 40.64 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 11 /D7))
    (pad 18 thru_hole oval (at 0 43.18 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 83 "Net-(U6-Pad18)"))
    (pad 19 thru_hole oval (at 0 45.72 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 84 "Net-(U6-Pad19)"))
    (pad 20 thru_hole oval (at 0 48.26 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 21 thru_hole oval (at 15.24 48.26 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 80 "Net-(U5-Pad20)"))
    (pad 22 thru_hole oval (at 15.24 45.72 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 77 "Net-(U1-Pad18)"))
    (pad 23 thru_hole oval (at 15.24 43.18 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 81 "Net-(U5-Pad27)"))
    (pad 24 thru_hole oval (at 15.24 40.64 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 12 BUSE))
    (pad 25 thru_hole oval (at 15.24 38.1 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 13 /A11))
    (pad 26 thru_hole oval (at 15.24 35.56 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 14 /A12))
    (pad 27 thru_hole oval (at 15.24 33.02 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 15 /A13))
    (pad 28 thru_hole oval (at 15.24 30.48 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 16 /A14))
    (pad 29 thru_hole oval (at 15.24 27.94 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 17 /A10))
    (pad 30 thru_hole oval (at 15.24 25.4 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 18 /A9))
    (pad 31 thru_hole oval (at 15.24 22.86 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 19 /A8))
    (pad 32 thru_hole oval (at 15.24 20.32 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 20 /A7))
    (pad 33 thru_hole oval (at 15.24 17.78 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 21 /A6))
    (pad 34 thru_hole oval (at 15.24 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 22 /A5))
    (pad 35 thru_hole oval (at 15.24 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 23 /A4))
    (pad 36 thru_hole oval (at 15.24 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 24 /A3))
    (pad 37 thru_hole oval (at 15.24 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 25 /A2))
    (pad 38 thru_hole oval (at 15.24 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 26 /A1))
    (pad 39 thru_hole oval (at 15.24 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 27 /A0))
    (pad 40 thru_hole oval (at 15.24 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 +5V))
    (model Housings_DIP.3dshapes/DIP-40_W15.24mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-20_W7.62mm (layer F.Cu) (tedit 575A60A0)
    (at 158.115 77.47 90)
    (descr "20-lead dip package, row spacing 7.62 mm (300 mils)")
    (tags "dil dip 2.54 300")
    (fp_text reference U4 (at 10.16 23.495 180) (layer F.SilkS))
    (fp_text value 377 (at 3.81 0 180) (layer F.SilkS))
    (pad 1 thru_hole oval (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 45 ROMS))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 62 "Net-(U4-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 63 "Net-(U4-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 64 "Net-(U4-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 65 "Net-(U4-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 66 "Net-(U4-Pad6)"))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 67 "Net-(U4-Pad7)"))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 68 "Net-(U4-Pad8)"))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 69 "Net-(U4-Pad9)"))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 11 thru_hole oval (at 7.62 22.86 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 70 "Net-(C7-Pad1)"))
    (pad 12 thru_hole oval (at 7.62 20.32 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 78 "Net-(U4-Pad12)"))
    (pad 13 thru_hole oval (at 7.62 17.78 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 49 "Net-(P1-Pad24)"))
    (pad 14 thru_hole oval (at 7.62 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 46 "Net-(P1-Pad30)"))
    (pad 15 thru_hole oval (at 7.62 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 79 "Net-(U4-Pad15)"))
    (pad 16 thru_hole oval (at 7.62 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 60 "Net-(U1-Pad3)"))
    (pad 17 thru_hole oval (at 7.62 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 56 "Net-(P1-Pad10)"))
    (pad 18 thru_hole oval (at 7.62 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 34 "Net-(P1-Pad23)"))
    (pad 19 thru_hole oval (at 7.62 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 61 "Net-(U1-Pad4)"))
    (pad 20 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 +5V))
    (model Housings_DIP.3dshapes/DIP-20_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module flashcart-footprints:C_C (layer F.Cu) (tedit 57069E5D)
    (at 125.095 62.23 90)
    (fp_text reference C1 (at -2.54 2.54 180) (layer F.SilkS))
    (fp_text value 100nF (at 3.81 -2.54 90) (layer F.Fab) hide)
    (pad 2 thru_hole circle (at 7.62 0 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 +5V))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
  )
  (module Housings_DIP:DIP-20_W7.62mm (layer F.Cu) (tedit 575A6096)
    (at 154.94 54.61 270)
    (descr "20-lead dip package, row spacing 7.62 mm (300 mils)")
    (tags "dil dip 2.54 300")
    (fp_text reference U2 (at -2.54 24.13 360) (layer F.SilkS))
    (fp_text value 541 (at 3.81 0 360) (layer F.SilkS))
    (pad 1 thru_hole oval (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 45 ROMS))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 51 "Net-(P1-Pad20)"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 52 "Net-(P1-Pad18)"))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 53 "Net-(P1-Pad16)"))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 54 "Net-(P1-Pad14)"))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 55 "Net-(P1-Pad12)"))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 56 "Net-(P1-Pad10)"))
    (pad 8 thru_hole oval (at 0 17.78 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 34 "Net-(P1-Pad23)"))
    (pad 9 thru_hole oval (at 0 20.32 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 57 "Net-(P1-Pad8)"))
    (pad 10 thru_hole oval (at 0 22.86 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 11 thru_hole oval (at 7.62 22.86 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 27 /A0))
    (pad 12 thru_hole oval (at 7.62 20.32 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 26 /A1))
    (pad 13 thru_hole oval (at 7.62 17.78 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 25 /A2))
    (pad 14 thru_hole oval (at 7.62 15.24 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 24 /A3))
    (pad 15 thru_hole oval (at 7.62 12.7 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 23 /A4))
    (pad 16 thru_hole oval (at 7.62 10.16 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 22 /A5))
    (pad 17 thru_hole oval (at 7.62 7.62 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 21 /A6))
    (pad 18 thru_hole oval (at 7.62 5.08 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 20 /A7))
    (pad 19 thru_hole oval (at 7.62 2.54 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 12 BUSE))
    (pad 20 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 +5V))
    (model Housings_DIP.3dshapes/DIP-20_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED-5MM (layer F.Cu) (tedit 575A60D7)
    (at 157.48 107.95 90)
    (descr "LED 5mm round vertical")
    (tags "LED 5mm round vertical")
    (fp_text reference D1 (at -0.635 -4.445 180) (layer F.SilkS))
    (fp_text value BUSY (at -0.635 6.35 180) (layer F.SilkS))
    (fp_text user K (at -1.905 1.905 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0 180) (size 2 1.9) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.9 1.9) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(D1-Pad2)"))
    (model LEDs.3dshapes/LED-5MM.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module flashcart-footprints:BUS_CART (layer F.Cu) (tedit 575A61E2)
    (at 120.65 33.02)
    (descr "Connecteur Bus AT ISA 16 bits")
    (tags "CONN BUS ISA")
    (fp_text reference P1 (at 22.86 17.78) (layer F.SilkS) hide)
    (fp_text value CONN_02X18 (at 24.13 -2.54) (layer F.Fab) hide)
    (pad 35 connect rect (at 44.45 7.62) (size 1.778 15) (layers B.Cu B.Mask)
      (net 1 GND))
    (pad 33 connect rect (at 41.91 7.62) (size 1.778 15) (layers B.Cu B.Mask)
      (net 29 "Net-(P1-Pad33)"))
    (pad 31 connect rect (at 39.37 7.62) (size 1.778 15) (layers B.Cu B.Mask)
      (net 30 "Net-(P1-Pad31)"))
    (pad 29 connect rect (at 36.83 7.62) (size 1.778 15) (layers B.Cu B.Mask)
      (net 31 "Net-(P1-Pad1)"))
    (pad 27 connect rect (at 34.29 7.62) (size 1.778 15) (layers B.Cu B.Mask)
      (net 32 "Net-(P1-Pad27)"))
    (pad 25 connect rect (at 31.75 7.62) (size 1.778 15) (layers B.Cu B.Mask)
      (net 33 "Net-(P1-Pad25)"))
    (pad 23 connect rect (at 29.21 7.62) (size 1.778 15) (layers B.Cu B.Mask)
      (net 34 "Net-(P1-Pad23)"))
    (pad 21 connect rect (at 26.67 7.62) (size 1.778 15) (layers B.Cu B.Mask)
      (net 35 "Net-(P1-Pad21)"))
    (pad 19 connect rect (at 24.13 7.62) (size 1.778 15) (layers B.Cu B.Mask)
      (net 2 +5V))
    (pad 17 connect rect (at 21.59 7.62) (size 1.778 15) (layers B.Cu B.Mask)
      (net 36 "Net-(P1-Pad17)"))
    (pad 15 connect rect (at 19.05 7.62) (size 1.778 15) (layers B.Cu B.Mask)
      (net 37 "Net-(P1-Pad15)"))
    (pad 13 connect rect (at 16.51 7.62) (size 1.778 15) (layers B.Cu B.Mask)
      (net 38 "Net-(P1-Pad13)"))
    (pad 11 connect rect (at 13.97 7.62) (size 1.778 15) (layers B.Cu B.Mask)
      (net 39 "Net-(P1-Pad11)"))
    (pad 9 connect rect (at 11.43 7.62) (size 1.778 15) (layers B.Cu B.Mask)
      (net 40 "Net-(P1-Pad9)"))
    (pad 7 connect rect (at 8.89 7.62) (size 1.778 15) (layers B.Cu B.Mask)
      (net 41 "Net-(P1-Pad7)"))
    (pad 5 connect rect (at 6.35 7.62) (size 1.778 15) (layers B.Cu B.Mask)
      (net 42 "Net-(P1-Pad5)"))
    (pad 3 connect rect (at 3.81 7.62) (size 1.778 15) (layers B.Cu B.Mask)
      (net 43 "Net-(P1-Pad3)"))
    (pad 1 connect rect (at 1.27 7.62) (size 1.778 15) (layers B.Cu B.Mask)
      (net 31 "Net-(P1-Pad1)"))
    (pad 36 connect rect (at 44.45 7.62) (size 1.778 15) (layers F.Cu F.Mask)
      (net 44 "Net-(P1-Pad36)"))
    (pad 34 connect rect (at 41.91 7.62) (size 1.778 15) (layers F.Cu F.Mask)
      (net 45 ROMS))
    (pad 32 connect rect (at 39.37 7.62) (size 1.778 15) (layers F.Cu F.Mask)
      (net 85 "Net-(P1-Pad32)"))
    (pad 30 connect rect (at 36.83 7.62) (size 1.778 15) (layers F.Cu F.Mask)
      (net 46 "Net-(P1-Pad30)"))
    (pad 28 connect rect (at 34.29 7.62) (size 1.778 15) (layers F.Cu F.Mask)
      (net 47 "Net-(P1-Pad28)"))
    (pad 26 connect rect (at 31.75 7.62) (size 1.778 15) (layers F.Cu F.Mask)
      (net 48 "Net-(P1-Pad26)"))
    (pad 24 connect rect (at 29.21 7.62) (size 1.778 15) (layers F.Cu F.Mask)
      (net 49 "Net-(P1-Pad24)"))
    (pad 22 connect rect (at 26.67 7.62) (size 1.778 15) (layers F.Cu F.Mask)
      (net 50 "Net-(P1-Pad22)"))
    (pad 20 connect rect (at 24.13 7.62) (size 1.778 15) (layers F.Cu F.Mask)
      (net 51 "Net-(P1-Pad20)"))
    (pad 18 connect rect (at 21.59 7.62) (size 1.778 15) (layers F.Cu F.Mask)
      (net 52 "Net-(P1-Pad18)"))
    (pad 16 connect rect (at 19.05 7.62) (size 1.778 15) (layers F.Cu F.Mask)
      (net 53 "Net-(P1-Pad16)"))
    (pad 14 connect rect (at 16.51 7.62) (size 1.778 15) (layers F.Cu F.Mask)
      (net 54 "Net-(P1-Pad14)"))
    (pad 12 connect rect (at 13.97 7.62) (size 1.778 15) (layers F.Cu F.Mask)
      (net 55 "Net-(P1-Pad12)"))
    (pad 10 connect rect (at 11.43 7.62) (size 1.778 15) (layers F.Cu F.Mask)
      (net 56 "Net-(P1-Pad10)"))
    (pad 8 connect rect (at 8.89 7.62) (size 1.778 15) (layers F.Cu F.Mask)
      (net 57 "Net-(P1-Pad8)"))
    (pad 6 connect rect (at 6.35 7.62) (size 1.778 15) (layers F.Cu F.Mask)
      (net 58 "Net-(P1-Pad6)"))
    (pad 4 connect rect (at 3.81 7.62) (size 1.778 15) (layers F.Cu F.Mask)
      (net 59 "Net-(P1-Pad4)"))
    (pad 2 connect rect (at 1.27 7.62) (size 1.778 15) (layers F.Cu F.Mask)
      (net 1 GND))
  )
  (module Buttons_Switches_ThroughHole:SW_PUSH_SMALL (layer F.Cu) (tedit 575A60CF)
    (at 177.8 105.41 180)
    (fp_text reference SW2 (at 0 -0.762 180) (layer F.SilkS))
    (fp_text value RESET (at -8.255 -3.175 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at 3.81 -2.54 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole circle (at 3.81 2.54 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 76 "Net-(R3-Pad2)"))
    (pad 1 thru_hole circle (at -3.81 -2.54 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole circle (at -3.81 2.54 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 76 "Net-(R3-Pad2)"))
  )
  (module Housings_DIP:DIP-20_W7.62mm (layer F.Cu) (tedit 575A609B)
    (at 187.96 54.61 270)
    (descr "20-lead dip package, row spacing 7.62 mm (300 mils)")
    (tags "dil dip 2.54 300")
    (fp_text reference U1 (at -2.54 24.13 360) (layer F.SilkS))
    (fp_text value 541 (at 3.81 1.905 360) (layer F.SilkS))
    (pad 1 thru_hole oval (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 45 ROMS))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 45 ROMS))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 60 "Net-(U1-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 61 "Net-(U1-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 49 "Net-(P1-Pad24)"))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 46 "Net-(P1-Pad30)"))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 47 "Net-(P1-Pad28)"))
    (pad 8 thru_hole oval (at 0 17.78 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 48 "Net-(P1-Pad26)"))
    (pad 9 thru_hole oval (at 0 20.32 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 50 "Net-(P1-Pad22)"))
    (pad 10 thru_hole oval (at 0 22.86 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 11 thru_hole oval (at 7.62 22.86 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 19 /A8))
    (pad 12 thru_hole oval (at 7.62 20.32 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 18 /A9))
    (pad 13 thru_hole oval (at 7.62 17.78 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 17 /A10))
    (pad 14 thru_hole oval (at 7.62 15.24 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 13 /A11))
    (pad 15 thru_hole oval (at 7.62 12.7 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 14 /A12))
    (pad 16 thru_hole oval (at 7.62 10.16 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 15 /A13))
    (pad 17 thru_hole oval (at 7.62 7.62 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 16 /A14))
    (pad 18 thru_hole oval (at 7.62 5.08 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 77 "Net-(U1-Pad18)"))
    (pad 19 thru_hole oval (at 7.62 2.54 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 12 BUSE))
    (pad 20 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 +5V))
    (model Housings_DIP.3dshapes/DIP-20_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-20_W7.62mm (layer F.Cu) (tedit 575A608F)
    (at 97.79 62.23 90)
    (descr "20-lead dip package, row spacing 7.62 mm (300 mils)")
    (tags "dil dip 2.54 300")
    (fp_text reference U3 (at 10.16 -1.27 180) (layer F.SilkS))
    (fp_text value 541 (at 3.81 0.635 180) (layer F.SilkS))
    (pad 1 thru_hole oval (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 45 ROMS))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 4 /D0))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 5 /D1))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 6 /D2))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 7 /D3))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 8 /D4))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 9 /D5))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 10 /D6))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 11 /D7))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 11 thru_hole oval (at 7.62 22.86 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 36 "Net-(P1-Pad17)"))
    (pad 12 thru_hole oval (at 7.62 20.32 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 37 "Net-(P1-Pad15)"))
    (pad 13 thru_hole oval (at 7.62 17.78 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 38 "Net-(P1-Pad13)"))
    (pad 14 thru_hole oval (at 7.62 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 39 "Net-(P1-Pad11)"))
    (pad 15 thru_hole oval (at 7.62 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 40 "Net-(P1-Pad9)"))
    (pad 16 thru_hole oval (at 7.62 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 41 "Net-(P1-Pad7)"))
    (pad 17 thru_hole oval (at 7.62 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 42 "Net-(P1-Pad5)"))
    (pad 18 thru_hole oval (at 7.62 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 43 "Net-(P1-Pad3)"))
    (pad 19 thru_hole oval (at 7.62 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 12 BUSE))
    (pad 20 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 +5V))
    (model Housings_DIP.3dshapes/DIP-20_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-28_W15.24mm (layer F.Cu) (tedit 574B478E)
    (at 132.08 69.85 270)
    (descr "28-lead dip package, row spacing 15.24 mm (600 mils)")
    (tags "dil dip 2.54 600")
    (fp_text reference U5 (at -2.54 34.29 360) (layer F.SilkS))
    (fp_text value 62256 (at 4.445 0.635 360) (layer F.SilkS))
    (pad 1 thru_hole oval (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 16 /A14))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 14 /A12))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 20 /A7))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 21 /A6))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 22 /A5))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 23 /A4))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 24 /A3))
    (pad 8 thru_hole oval (at 0 17.78 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 25 /A2))
    (pad 9 thru_hole oval (at 0 20.32 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 26 /A1))
    (pad 10 thru_hole oval (at 0 22.86 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 27 /A0))
    (pad 11 thru_hole oval (at 0 25.4 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 4 /D0))
    (pad 12 thru_hole oval (at 0 27.94 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 5 /D1))
    (pad 13 thru_hole oval (at 0 30.48 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 6 /D2))
    (pad 14 thru_hole oval (at 0 33.02 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 15 thru_hole oval (at 15.24 33.02 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 7 /D3))
    (pad 16 thru_hole oval (at 15.24 30.48 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 8 /D4))
    (pad 17 thru_hole oval (at 15.24 27.94 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 9 /D5))
    (pad 18 thru_hole oval (at 15.24 25.4 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 10 /D6))
    (pad 19 thru_hole oval (at 15.24 22.86 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 11 /D7))
    (pad 20 thru_hole oval (at 15.24 20.32 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 80 "Net-(U5-Pad20)"))
    (pad 21 thru_hole oval (at 15.24 17.78 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 17 /A10))
    (pad 22 thru_hole oval (at 15.24 15.24 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 77 "Net-(U1-Pad18)"))
    (pad 23 thru_hole oval (at 15.24 12.7 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 13 /A11))
    (pad 24 thru_hole oval (at 15.24 10.16 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 18 /A9))
    (pad 25 thru_hole oval (at 15.24 7.62 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 19 /A8))
    (pad 26 thru_hole oval (at 15.24 5.08 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 15 /A13))
    (pad 27 thru_hole oval (at 15.24 2.54 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 81 "Net-(U5-Pad27)"))
    (pad 28 thru_hole oval (at 15.24 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 +5V))
    (model Housings_DIP.3dshapes/DIP-28_W15.24mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module flashcart-footprints:C_C (layer F.Cu) (tedit 57069E57)
    (at 127.635 54.61 270)
    (fp_text reference C2 (at 10.16 2.54 360) (layer F.SilkS))
    (fp_text value 100nF (at 3.81 -2.54 270) (layer F.Fab) hide)
    (pad 2 thru_hole circle (at 7.62 0 270) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 +5V))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
  )
  (module flashcart-footprints:C_C (layer F.Cu) (tedit 57069E4F)
    (at 160.655 54.61 270)
    (fp_text reference C3 (at 10.16 0 360) (layer F.SilkS))
    (fp_text value 100nF (at 3.81 -2.54 270) (layer F.Fab) hide)
    (pad 2 thru_hole circle (at 7.62 0 270) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 +5V))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
  )
  (module flashcart-footprints:C_C (layer F.Cu) (tedit 57069E48)
    (at 153.67 77.47 90)
    (fp_text reference C4 (at -2.54 0 180) (layer F.SilkS))
    (fp_text value 100nF (at 3.81 -2.54 90) (layer F.Fab) hide)
    (pad 2 thru_hole circle (at 7.62 0 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 +5V))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
  )
  (module flashcart-footprints:C_C (layer F.Cu) (tedit 57069DBF)
    (at 136.525 77.47 270)
    (fp_text reference C5 (at 10.16 0 360) (layer F.SilkS))
    (fp_text value 100nF (at -4.445 0 270) (layer F.Fab) hide)
    (pad 2 thru_hole circle (at 7.62 0 270) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 +5V))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
  )
  (module flashcart-footprints:C_C (layer F.Cu) (tedit 57069DCA)
    (at 152.4 95.885 270)
    (fp_text reference C6 (at 10.16 0.635 360) (layer F.SilkS))
    (fp_text value 100nF (at -2.54 -0.635 360) (layer F.Fab) hide)
    (pad 2 thru_hole circle (at 7.62 0 270) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 +5V))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
  )
  (module flashcart-footprints:C_C (layer F.Cu) (tedit 574B477F)
    (at 185.42 69.85 270)
    (fp_text reference C7 (at -2.54 0 360) (layer F.SilkS))
    (fp_text value 1nF (at -2.54 0 360) (layer F.SilkS))
    (pad 2 thru_hole circle (at 7.62 0 270) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 70 "Net-(C7-Pad1)"))
  )
  (module Symbols:Symbol_OSHW-Logo_SilkScreen_BIG (layer F.Cu) (tedit 57068403)
    (at 144.78 55.245)
    (descr "Symbol, OSHW-Logo, Silk Screen, BIG")
    (tags "Symbol, OSHW-Logo, Silk Screen, BIG")
    (fp_text reference REF** (at -0.29972 11.50112) (layer F.SilkS) hide)
    (fp_text value OSHW (at 0.29972 32.10052) (layer F.Fab) hide)
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 574B4787)
    (at 189.23 77.47 90)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R1 (at 5.32892 -3.50012 90) (layer F.SilkS))
    (fp_text value 68 (at 5.08 0 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 70 "Net-(C7-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 85 "Net-(P1-Pad32)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 574B479D)
    (at 157.48 99.695 90)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R2 (at 5.32892 -3.50012 90) (layer F.SilkS))
    (fp_text value 470 (at 5.08 0 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 3 "Net-(D1-Pad2)"))
    (pad 2 thru_hole circle (at 10.16 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 75 "Net-(R2-Pad2)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 574B47A3)
    (at 142.24 88.9)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R3 (at 5.32892 -3.50012) (layer F.SilkS))
    (fp_text value 10k (at 5.08 0) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 2 +5V))
    (pad 2 thru_hole circle (at 10.16 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 76 "Net-(R3-Pad2)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text endlos.net/flashrom99 (at 177.8 99.06) (layer F.SilkS))
  (gr_text "Rev. 2" (at 191.135 109.22 90) (layer F.SilkS))
  (gr_text "(c) 2016 R. Benzinger" (at 177.8 96.52) (layer F.SilkS))
  (gr_text "FlashROM 99" (at 177.8 92.71) (layer F.SilkS))
  (gr_line (start 193.515 112.29) (end 93.515 112.29) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 193.515 47.37) (end 193.515 112.29) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 93.515 47.37) (end 93.515 112.29) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 167.015 47.37) (end 193.515 47.37) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 120.015 47.37) (end 93.515 47.37) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 167.015 32.37) (end 167.015 47.37) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 120.015 32.37) (end 120.015 47.37) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 143.515 32.37) (end 120.015 32.37) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 143.515 32.37) (end 167.015 32.37) (angle 90) (layer Edge.Cuts) (width 0.15))
)
