(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "+5V")
  (net 2 "GND")
  (net 3 "Net-(D1-K)")
  (net 4 "Net-(D2-K)")
  (net 5 "Net-(J1-Pin_1)")
  (net 6 "Net-(J1-Pin_2)")
  (net 7 "Net-(Q1-B)")
  (net 8 "Net-(U2-Anode)")
  (net 9 "unconnected-(U1-Pad5)")
  (net 10 "unconnected-(U2-NC-Pad3)")
  (net 11 "unconnected-(U2-NC-Pad4)")
  (net 12 "unconnected-(U2-Pad5)")
  (net 13 "Net-(Q2-B)")
  (net 14 "Net-(U1-R_L)")
  (footprint "Diode_SMD:D_SOD-123" (layer "F.Cu")
    (at 81.28 51.816 180)
    (descr "SOD-123")
    (tags "SOD-123")
    (property "Sheetfile" "beacon-control.kicad_sch")
    (property "Sheetname" "")
    (property "Sim.Device" "D")
    (property "Sim.Pins" "1=K 2=A")
    (property "ki_description" "Diode")
    (property "ki_keywords" "diode")
    (attr smd)
    (fp_text reference "D1" (at -3.048 0.254 270) (layer "F.SilkS"))
    (fp_text value "D" (at 0 2.1 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2 180) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.65 0 180) (size 0.9 1.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(D1-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.65 0 180) (size 0.9 1.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric" (layer "F.Cu")
    (at 75.233 56.642)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "beacon-control.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C2" (at 2.999 0 90) (layer "F.SilkS"))
    (fp_text value "100n" (at 0 1.85) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.475 0) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 1 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 1.475 0) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SOD-123" (layer "F.Cu")
    (at 75.2055 49.276 180)
    (descr "SOD-123")
    (tags "SOD-123")
    (property "Sheetfile" "beacon-control.kicad_sch")
    (property "Sheetname" "")
    (property "Sim.Device" "D")
    (property "Sim.Pins" "1=K 2=A")
    (property "ki_description" "Diode")
    (property "ki_keywords" "diode")
    (attr smd)
    (fp_text reference "D2" (at -3.0265 0 270) (layer "F.SilkS"))
    (fp_text value "D" (at 0 2.1 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2 180) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.65 0 180) (size 0.9 1.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "Net-(D2-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.65 0 180) (size 0.9 1.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Relay_THT:Relay_SPDT_Omron-G5LE-1" (layer "F.Cu")
    (at 93.726 57.2055 180)
    (descr "Omron Relay SPDT, http://www.omron.com/ecb/products/pdf/en-g5le.pdf")
    (tags "Omron Relay SPDT")
    (property "Sheetfile" "beacon-control.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Omron G5LE relay, Miniature Single Pole, SPDT, 10A")
    (property "ki_keywords" "Miniature Single Pole Relay")
    (attr through_hole)
    (fp_text reference "K1" (at 9.398 19.3595 90) (layer "F.SilkS"))
    (fp_text value "G5LE-1" (at 0 20.95) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 8.7) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 2.5 2.5) (drill 1.3) (layers "*.Cu" "*.Mask")
      (net 6 "Net-(J1-Pin_2)") (pintype "passive"))
    (pad "2" thru_hole oval (at -6 2 180) (size 2.5 2.5) (drill 1.3) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pintype "passive"))
    (pad "3" thru_hole oval (at -6 14.2 180) (size 2.5 2.5) (drill 1.3) (layers "*.Cu" "*.Mask")
      (net 5 "Net-(J1-Pin_1)") (pintype "passive"))
    (pad "4" thru_hole oval (at 6 14.2 180) (size 2.5 2.5) (drill 1.3) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pintype "passive"))
    (pad "5" thru_hole oval (at 6 2 180) (size 2.5 2.5) (drill 1.3) (layers "*.Cu" "*.Mask")
      (net 3 "Net-(D1-K)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Relay_THT.3dshapes/Relay_SPDT_Omron-G5LE-1.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "F.Cu")
    (at 75.2455 54.256)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "beacon-control.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R3" (at 2.964 -0.0025 90) (layer "F.SilkS"))
    (fp_text value "2.9K" (at 0 1.82) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.4625 0) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.222222)
      (net 14 "Net-(U1-R_L)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4625 0) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.222222)
      (net 13 "Net-(Q2-B)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric" (layer "F.Cu")
    (at 110.998 54.356 -90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "beacon-control.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C1" (at -3.048 0.254 -180) (layer "F.SilkS"))
    (fp_text value "10u" (at 0 1.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.475 0 270) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 1 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 1.475 0 270) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_4.3mm_M4_Pad_Via" (layer "F.Cu")
    (at 77.978 43.103)
    (descr "Mounting Hole 4.3mm, M4")
    (tags "mounting hole 4.3mm m4")
    (property "Sheetfile" "beacon-control.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H2" (at 5.08 -2.209) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 5.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -3.225 0) (size 0.9 0.9) (drill 0.6) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at -2.280419 -2.280419) (size 0.9 0.9) (drill 0.6) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at -2.280419 2.280419) (size 0.9 0.9) (drill 0.6) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at 0 -3.225) (size 0.9 0.9) (drill 0.6) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at 0 0) (size 8.6 8.6) (drill 4.3) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at 0 3.225) (size 0.9 0.9) (drill 0.6) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at 2.280419 -2.280419) (size 0.9 0.9) (drill 0.6) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at 2.280419 2.280419) (size 0.9 0.9) (drill 0.6) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at 3.225 0) (size 0.9 0.9) (drill 0.6) (layers "*.Cu" "*.Mask"))
  )
  (footprint "TerminalBlock:TerminalBlock_bornier-2_P5.08mm" (layer "F.Cu")
    (at 116.586 42.164 -90)
    (descr "simple 2-pin terminal block, pitch 5.08mm, revamped version of bornier2")
    (tags "terminal block bornier2")
    (property "Sheetfile" "beacon-control.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic screw terminal, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "screw terminal")
    (attr through_hole)
    (fp_text reference "J1" (at 6.604 4.826 90) (layer "F.SilkS"))
    (fp_text value "Screw_Terminal_01x02" (at 2.54 5.08 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 3 3) (drill 1.52) (layers "*.Cu" "*.Mask")
      (net 5 "Net-(J1-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 5.08 0 270) (size 3 3) (drill 1.52) (layers "*.Cu" "*.Mask")
      (net 6 "Net-(J1-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/TerminalBlock.3dshapes/TerminalBlock_bornier-2_P5.08mm.wrl"
      (offset (xyz 2.539999962 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "F.Cu")
    (at 75.2455 59.0305)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "beacon-control.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R2" (at 2.9025 0.1515 90) (layer "F.SilkS"))
    (fp_text value "2.9K" (at 0 1.82) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.4625 0) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.222222)
      (net 14 "Net-(U1-R_L)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4625 0) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.222222)
      (net 7 "Net-(Q1-B)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "F.Cu")
    (at 80.8505 58.4505)
    (descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "Sheetfile" "beacon-control.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "0.1A Ic, 45V Vce, PNP Transistor, SOT-23")
    (property "ki_keywords" "PNP transistor")
    (attr smd)
    (fp_text reference "Q1" (at 2.7155 0.7315 90) (layer "F.SilkS"))
    (fp_text value "MMBT5401LT3G" (at 0 2.4) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 -0.95) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "Net-(Q1-B)") (pinfunction "B") (pintype "input"))
    (pad "2" smd roundrect (at -0.9375 0.95) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+5V") (pinfunction "E") (pintype "passive"))
    (pad "3" smd roundrect (at 0.9375 0) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(D1-K)") (pinfunction "C") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "F.Cu")
    (at 80.8505 54.8665 180)
    (descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "Sheetfile" "beacon-control.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "0.1A Ic, 45V Vce, PNP Transistor, SOT-23")
    (property "ki_keywords" "PNP transistor")
    (attr smd)
    (fp_text reference "Q2" (at -2.7495 -0.68 90) (layer "F.SilkS"))
    (fp_text value "MMBT5401LT3G" (at 0 2.4) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 -0.95 180) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "Net-(Q2-B)") (pinfunction "B") (pintype "input"))
    (pad "2" smd roundrect (at -0.9375 0.95 180) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+5V") (pinfunction "E") (pintype "passive"))
    (pad "3" smd roundrect (at 0.9375 0 180) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "Net-(D2-K)") (pinfunction "C") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "F.Cu")
    (at 75.2455 51.816 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "beacon-control.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R1" (at -2.964 -0.1515 90) (layer "F.SilkS"))
    (fp_text value "62" (at 0 1.82) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.4625 0 180) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.222222)
      (net 4 "Net-(D2-K)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4625 0 180) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.222222)
      (net 8 "Net-(U2-Anode)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_4.3mm_M4_Pad_Via" (layer "F.Cu")
    (at 107.442 43.103)
    (descr "Mounting Hole 4.3mm, M4")
    (tags "mounting hole 4.3mm m4")
    (property "Sheetfile" "beacon-control.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H1" (at 0 -5.3) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 5.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -3.225 0) (size 0.9 0.9) (drill 0.6) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at -2.280419 -2.280419) (size 0.9 0.9) (drill 0.6) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at -2.280419 2.280419) (size 0.9 0.9) (drill 0.6) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at 0 -3.225) (size 0.9 0.9) (drill 0.6) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at 0 0) (size 8.6 8.6) (drill 4.3) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at 0 3.225) (size 0.9 0.9) (drill 0.6) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at 2.280419 -2.280419) (size 0.9 0.9) (drill 0.6) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at 2.280419 2.280419) (size 0.9 0.9) (drill 0.6) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at 3.225 0) (size 0.9 0.9) (drill 0.6) (layers "*.Cu" "*.Mask"))
  )
  (footprint "TerminalBlock:TerminalBlock_bornier-2_P5.08mm" (layer "F.Cu")
    (at 116.586 52.832 -90)
    (descr "simple 2-pin terminal block, pitch 5.08mm, revamped version of bornier2")
    (tags "terminal block bornier2")
    (property "Sheetfile" "beacon-control.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic screw terminal, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "screw terminal")
    (attr through_hole)
    (fp_text reference "J2" (at 6.096 5.842 90) (layer "F.SilkS"))
    (fp_text value "Screw_Terminal_01x02" (at 2.54 5.08 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 3 3) (drill 1.52) (layers "*.Cu" "*.Mask")
      (net 1 "+5V") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 5.08 0 270) (size 3 3) (drill 1.52) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/TerminalBlock.3dshapes/TerminalBlock_bornier-2_P5.08mm.wrl"
      (offset (xyz 2.539999962 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "wham-bs-footprints:Versalink Transciever-Oscar-2022" (layer "F.Cu")
    (at 72.55 55.138 90)
    (property "Sheetfile" "beacon-control.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U1" (at 0.274 -9.304 270) (layer "F.SilkS"))
    (fp_text value "VersalinkRX" (at -0.1 3.54 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -3.81 -2.7 90) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 14 "Net-(U1-R_L)") (pinfunction "V_O") (pintype "output"))
    (pad "2" thru_hole circle (at -1.25 -2.7 90) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "+5V") (pinfunction "GND") (pintype "power_in"))
    (pad "3" thru_hole circle (at 1.29 -2.7 90) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "VCC") (pintype "power_in"))
    (pad "4" thru_hole circle (at 3.83 -2.7 90) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 14 "Net-(U1-R_L)") (pinfunction "R_L") (pintype "output"))
    (pad "5" thru_hole circle (at -3.81 -10.32 90) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 9 "unconnected-(U1-Pad5)") (pinfunction "5") (pintype "no_connect"))
    (pad "8" thru_hole circle (at 3.81 -10.32 90) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask"))
  )
  (footprint "wham-bs-footprints:Versalink Transciever-Oscar-2022" (layer "F.Cu")
    (at 72.55 44.958 90)
    (property "Sheetfile" "beacon-control.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U2" (at 3.556 1.11 90) (layer "F.SilkS"))
    (fp_text value "VersalinkTX" (at -0.1 3.54 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -3.81 -2.7 90) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(U2-Anode)") (pinfunction "Anode") (pintype "input"))
    (pad "2" thru_hole circle (at -1.25 -2.7 90) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Cathode") (pintype "input"))
    (pad "3" thru_hole circle (at 1.29 -2.7 90) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 10 "unconnected-(U2-NC-Pad3)") (pinfunction "NC") (pintype "no_connect"))
    (pad "4" thru_hole circle (at 3.83 -2.7 90) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 11 "unconnected-(U2-NC-Pad4)") (pinfunction "NC") (pintype "no_connect"))
    (pad "5" thru_hole circle (at -3.81 -10.32 90) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 12 "unconnected-(U2-Pad5)") (pinfunction "5") (pintype "no_connect"))
    (pad "8" thru_hole circle (at 3.81 -10.32 90) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask"))
  )
  (footprint "wham-bs-footprints:WHAM_LOGO_SMALLER-oscar" (layer "B.Cu")
    (at 93.726 49.022 180)
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "G***" (at 0 0) (layer "B.SilkS") hide)
    (fp_text value "LOGO" (at 0.75 0) (layer "B.SilkS") hide)
  )
  (gr_rect (start 60.198 36.83) (end 120.65 60.706)
    (fill none) (layer "Edge.Cuts"))
  (gr_text "Beacons, my beloved" (at 60.706 38.354) (layer "F.Cu"))
  (gr_text "Hey!\nHow did I get here?" (at 86.36 49.784) (layer "F.Cu"))
  (gr_text "Beacon Control\nVersion: Alpha\nEverett Penne \nJan 19, 2024" (at 108.966 59.944 90) (layer "F.SilkS"))
  (gr_text "+V" (at 112.522 51.562 90) (layer "F.SilkS"))
  (gr_text "FIBER OUT" (at 65.786 49.276 90) (layer "F.SilkS"))
  (gr_text "Relay" (at 115.316 39.116) (layer "F.SilkS"))
  (gr_text "FIBER IN" (at 65.786 58.42 90) (layer "F.SilkS"))
  (gr_text "GND" (at 112.522 59.69 90) (layer "F.SilkS"))
  (dimension (type aligned) (layer "B.SilkS")
    (pts (xy 77.978 42.926) (xy 107.442 42.926))
    (height -5.08)
    (gr_text "1.2 in" (at 92.71 37.846) (layer "B.SilkS"))
    (format (prefix "") (suffix "") (units 0) (units_format 1) (precision 1))
    (style (thickness 0.2) (arrow_length 1.27) (text_position_mode 1) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (zone (net 2) (net_name "GND") (layer "B.Cu") (hatch edge 0.5)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 59.944 64.008)
        (xy 59.944 33.02)
        (xy 125.73 33.02)
        (xy 125.73 63.754)
      )
    )
  )
)
