(kicad_pcb (version 4) (host pcbnew 4.0.1-stable)
  (general
    (links 14)
    (no_connects 0)
    (area 99.674999 99.674999 110.325001 112.825001)
    (thickness 1.6)
    (drawings 27)
    (tracks 45)
    (zones 0)
    (modules 13)
    (nets 8)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal hide)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.75)
    (user_trace_width 0.5)
    (user_trace_width 0.6)
    (user_trace_width 0.75)
    (trace_clearance 0.2)
    (zone_clearance 0.3556)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 VCC)
  (net 2 GND)
  (net 3 "Net-(C2-Pad1)")
  (net 4 "Net-(D2-Pad1)")
  (net 5 "Net-(SW1-Pad3)")
  (net 6 "Net-(U1-Pad3)")
  (net 7 "Net-(P1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(P1-Pad1)")
    (add_net "Net-(SW1-Pad3)")
    (add_net "Net-(U1-Pad3)")
    (add_net VCC)
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 59244439)
    (at 101.5 106 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 1 -2.75 90) (layer F.SilkS))
    (fp_text value 1uF (at 0.75 -5 180) (layer F.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5924442F)
    (at 105 107.25 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at 6.25 0 270) (layer F.SilkS))
    (fp_text value 1uF (at 8.5 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 592443EE)
    (at 108.5 106.25 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference D2 (at 1.25 4.25 90) (layer F.SilkS))
    (fp_text value BAT54C (at 0 2.75 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 1.00076 90) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D2-Pad1)"))
    (pad 2 smd rect (at 0.95 1.00076 90) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D2-Pad1)"))
    (pad 3 smd rect (at 0 -0.99822 90) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_SMD:SW_SPDT_PCM12 locked (layer F.Cu) (tedit 59244365)
    (at 105 110.625)
    (descr "Ultraminiature Surface Mount Slide Switch")
    (attr smd)
    (fp_text reference SW1 (at -6.25 -1 90) (layer F.SilkS))
    (fp_text value SWITCH_INV (at 0 4.5) (layer F.Fab))
    (pad "" np_thru_hole circle (at -1.5 0.325) (size 0.9 0.9) (drill 0.9) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 1.5 0.325) (size 0.9 0.9) (drill 0.9) (layers *.Cu *.Mask))
    (pad 1 smd rect (at -2.25 -1.425) (size 0.7 1.5) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(P1-Pad1)"))
    (pad 2 smd rect (at 0.75 -1.425) (size 0.7 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 2.25 -1.425) (size 0.7 1.5) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(SW1-Pad3)"))
    (pad "" smd rect (at -3.65 1.425) (size 1 0.8) (layers F.Cu F.Paste F.Mask))
    (pad "" smd rect (at 3.65 1.425) (size 1 0.8) (layers F.Cu F.Paste F.Mask))
    (pad "" smd rect (at 3.65 -0.775) (size 1 0.8) (layers F.Cu F.Paste F.Mask))
    (pad "" smd rect (at -3.65 -0.775) (size 1 0.8) (layers F.Cu F.Paste F.Mask))
  )
  (module TO_SOT_Packages_SMD:SOT-23-5 (layer F.Cu) (tedit 59247CBF)
    (at 103.5 101.75)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U1 (at -4.65 -2.65 270) (layer F.SilkS))
    (fp_text value ZXLD383 (at -7.5 1.75) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(U1-Pad3)"))
    (pad 4 smd rect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D2-Pad1)"))
    (pad 5 smd rect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:LED-XP-D_CREE_Hand_Soldering (layer F.Cu) (tedit 592445BE)
    (at 105 105)
    (descr http://www.cree.com/led-components/media/documents/XLampXBD.pdf)
    (tags "LED XP-D CREE Hand Soldering")
    (attr smd)
    (fp_text reference D1 (at 7.75 2.25 90) (layer F.SilkS))
    (fp_text value LED (at 1.75 -6) (layer F.Fab))
    (pad 2 smd rect (at 1.33 0) (size 1 2.3) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 1 smd rect (at -1.33 0) (size 1 2.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 0 0) (size 0.9 2.3) (layers F.Cu F.Paste F.Mask))
    (model LEDs.3dshapes/LED-XP-G_CREE.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:Conn_Battery_Pad_4mm (layer B.Cu) (tedit 592445B9)
    (at 105 105)
    (descr "Battery Pad 4mm")
    (tags "Battery Pad 4mm")
    (fp_text reference P2 (at 9.25 0 90) (layer B.SilkS))
    (fp_text value BAT+ (at -2 -6) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 4 4) (layers B.Cu B.Paste B.Mask)
      (net 1 VCC))
  )
  (module my_components:Hole_1.1mm (layer F.Cu) (tedit 592443CD)
    (at 109 101)
    (descr "Hole 1.1mm")
    (tags "Hole 1.1mm")
    (fp_text reference REF** (at 6.25 1.5) (layer F.SilkS))
    (fp_text value Hole_1.1mm (at 6.25 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
  )
  (module my_components:Hole_1.1mm (layer F.Cu) (tedit 59244396)
    (at 101 109)
    (descr "Hole 1.1mm")
    (tags "Hole 1.1mm")
    (fp_text reference REF** (at -7.75 1) (layer F.SilkS))
    (fp_text value Hole_1.1mm (at -7.75 -0.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
  )
  (module my_components:Hole_1.1mm (layer F.Cu) (tedit 5924439C)
    (at 109 109)
    (descr "Hole 1.1mm")
    (tags "Hole 1.1mm")
    (fp_text reference REF** (at 7.5 1.5) (layer F.SilkS))
    (fp_text value Hole_1.1mm (at 7.5 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
  )
  (module my_components:Hole_1.1mm (layer F.Cu) (tedit 592443D9)
    (at 101 101)
    (descr "Hole 1.1mm")
    (tags "Hole 1.1mm")
    (fp_text reference REF** (at -6.5 1.5) (layer F.SilkS))
    (fp_text value Hole_1.1mm (at -6.25 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
  )
  (module my_components:Conn_Wire_Pad_0.8mm (layer F.Cu) (tedit 592480B6)
    (at 105 111)
    (descr "Wire Pad 0.8mm")
    (tags "Wire Pad 0.8mm")
    (fp_text reference P1 (at -2.75 2.5 180) (layer F.SilkS))
    (fp_text value BAT- (at 0.5 2.75) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(P1-Pad1)"))
  )
  (module my_components:Inductor_1210_SMD (layer F.Cu) (tedit 59247B2C)
    (at 107.5 102.5 315)
    (descr "Inductor, SMD1210")
    (tags "Inductor SMD1210")
    (attr smd)
    (fp_text reference L1 (at -0.106066 -4.419417 315) (layer F.SilkS))
    (fp_text value 4.7uH (at -0.141421 -5.939697 315) (layer F.Fab))
    (pad 2 smd rect (at 1.4 0 315) (size 1.4 2.2) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D2-Pad1)"))
    (pad 1 smd rect (at -1.4 0 315) (size 1.4 2.2) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
  )
  (gr_arc (start 100.5 111.5) (end 100.5 112.25) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 109.5 111.5) (end 110.25 111.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text + (at 107.4 105) (layer F.SilkS))
  (gr_text Flashlight (at 107.9 105 90) (layer B.SilkS))
  (gr_text "Single\nCell" (at 101.6 105.3 90) (layer B.SilkS))
  (gr_line (start 100.5 112.25) (end 109.5 112.25) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 100.5 99.75) (end 109.5 99.75) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 99.75 100.5) (end 99.75 111.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 110.25 100.5) (end 110.25 111.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 109.5 100.5) (end 109.5 99.75) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 100.5 100.5) (end 99.75 100.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name VCC) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3556))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 110.25 112.75) (xy 99.75 112.75) (xy 99.75 99.75) (xy 110.25 99.75) (xy 110.25 112.75)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.3556))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 104 105.75) (xy 105.25 106.75) (xy 105.25 108.25) (xy 106.5 108.25) (xy 106.5 110.75)
        (xy 103.25 110.75) (xy 103.25 107.25) (xy 102.25 106.25) (xy 100.25 106.25) (xy 100 106)
        (xy 100 102.25) (xy 101 101.25) (xy 104 101.25) (xy 104 105.75)
      )
    )
  )
)
