(kicad_pcb (version 20171130) (host pcbnew 5.1.8)
  (general
    (thickness 1.6002)
    (drawings 21)
    (tracks 200)
    (zones 0)
    (modules 22)
    (nets 32)
  )
  (page USLetter)
  (title_block
    (title "Main Board")
    (date 2018-08-03)
    (rev v2.0.0)
    (company "Rave Saber")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user hide)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.2032)
    (user_trace_width 1.3716)
    (trace_clearance 0.2032)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2032)
    (via_size 0.762)
    (via_drill 0.508)
    (via_min_size 0.762)
    (via_min_drill 0.508)
    (uvia_size 0.762)
    (uvia_drill 0.508)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.15)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.99974 2.99974)
    (pad_drill 1.19888)
    (pad_to_mask_clearance 0.0508)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +BATT)
  (net 2 "Net-(D1-Pad1)")
  (net 3 GND)
  (net 4 VCC)
  (net 5 /RESET)
  (net 6 "Net-(U2-Pad15)")
  (net 7 "Net-(U2-Pad16)")
  (net 8 /DATA)
  (net 9 /BUTTON)
  (net 10 "Net-(U2-Pad5)")
  (net 11 /CLK)
  (net 12 "Net-(U2-Pad6)")
  (net 13 /XTAL1)
  (net 14 "Net-(U2-Pad23)")
  (net 15 /XTAL2)
  (net 16 "Net-(U2-Pad24)")
  (net 17 "Net-(U2-Pad11)")
  (net 18 "Net-(U2-Pad25)")
  (net 19 "Net-(U2-Pad12)")
  (net 20 "Net-(U2-Pad26)")
  (net 21 "Net-(U2-Pad13)")
  (net 22 "Net-(U2-Pad27)")
  (net 23 "Net-(U2-Pad14)")
  (net 24 "Net-(U2-Pad28)")
  (net 25 /FTDI_TX)
  (net 26 /FTDI_RX)
  (net 27 /MISO)
  (net 28 "Net-(J3-Pad3)")
  (net 29 "Net-(J3-Pad2)")
  (net 30 "Net-(J3-Pad6)")
  (net 31 "Net-(J4-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2032)
    (trace_width 0.2032)
    (via_dia 0.762)
    (via_drill 0.508)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (diff_pair_width 0.2032)
    (diff_pair_gap 0.254)
    (add_net +BATT)
    (add_net /BUTTON)
    (add_net /CLK)
    (add_net /DATA)
    (add_net /FTDI_RX)
    (add_net /FTDI_TX)
    (add_net /MISO)
    (add_net /RESET)
    (add_net /XTAL1)
    (add_net /XTAL2)
    (add_net GND)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(J3-Pad2)")
    (add_net "Net-(J3-Pad3)")
    (add_net "Net-(J3-Pad6)")
    (add_net "Net-(J4-Pad2)")
    (add_net "Net-(U2-Pad11)")
    (add_net "Net-(U2-Pad12)")
    (add_net "Net-(U2-Pad13)")
    (add_net "Net-(U2-Pad14)")
    (add_net "Net-(U2-Pad15)")
    (add_net "Net-(U2-Pad16)")
    (add_net "Net-(U2-Pad23)")
    (add_net "Net-(U2-Pad24)")
    (add_net "Net-(U2-Pad25)")
    (add_net "Net-(U2-Pad26)")
    (add_net "Net-(U2-Pad27)")
    (add_net "Net-(U2-Pad28)")
    (add_net "Net-(U2-Pad5)")
    (add_net "Net-(U2-Pad6)")
    (add_net VCC)
  )
  (module Logos:AntiFA_Logo (layer B.Cu) (tedit 5B646F82)
    (at 116.332 121.412 180)
    (descr "Imported from AntiFA_Logo.svg")
    (tags svg2mod)
    (attr virtual)
    (fp_text reference svg2mod (at 0 9.821333 180) (layer B.SilkS) hide)
    (fp_text value G*** (at 0 -9.821333 180) (layer B.SilkS) hide)
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Vertical_SMD_Pin1Left (layer F.Cu) (tedit 59FED5CC)
    (at 110.367 94.996)
    (descr "surface-mounted straight pin header, 1x06, 2.54mm pitch, single row, style 1 (pin 1 left)")
    (tags "Surface mounted pin header SMD 1x06 2.54mm single row style1 pin1 left")
    (attr smd)
    (fp_text reference J3 (at 0.377 -0.508) (layer F.SilkS))
    (fp_text value "FTDI SERIAL" (at -3.687 0 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 6 smd rect (at 1.655 6.35) (size 2.51 1) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(J3-Pad6)"))
    (pad 4 smd rect (at 1.655 1.27) (size 2.51 1) (layers F.Cu F.Paste F.Mask)
      (net 25 /FTDI_TX))
    (pad 2 smd rect (at 1.655 -3.81) (size 2.51 1) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(J3-Pad2)"))
    (pad 5 smd rect (at -1.655 3.81) (size 2.51 1) (layers F.Cu F.Paste F.Mask)
      (net 26 /FTDI_RX))
    (pad 3 smd rect (at -1.655 -1.27) (size 2.51 1) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(J3-Pad3)"))
    (pad 1 smd rect (at -1.655 -6.35) (size 2.51 1) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x06_P2.54mm_Vertical_SMD_Pin1Left.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:CP_Elec_16x17.5 (layer F.Cu) (tedit 5A841F9D)
    (at 118.364 77.216 180)
    (descr "SMT capacitor, aluminium electrolytic, 16x17.5, Vishay 1616 http://www.vishay.com/docs/28395/150crz.pdf")
    (tags "Capacitor Electrolytic")
    (attr smd)
    (fp_text reference C2 (at 10.16 7.112 180) (layer F.SilkS))
    (fp_text value 1500uF (at -7.366 9.35 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 6.25 0 180) (size 7.8 9.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 1 smd rect (at -6.25 0 180) (size 7.8 9.6) (layers F.Cu F.Paste F.Mask)
      (net 4 VCC))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/CP_Elec_16x17.5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 113.425 109.728 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C4 (at 3.951 0 180) (layer F.SilkS))
    (fp_text value 1uF (at 6.237 0 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 VCC))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-220-5_P3.4x3.7mm_StaggerOdd_Lead3.8mm_Vertical (layer F.Cu) (tedit 5AF05A31)
    (at 116.332 45.212 180)
    (descr "TO-220-5, Vertical, RM 1.7mm, Pentawatt, Multiwatt-5, staggered type-1, see http://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/ltc-legacy-to-220/to-220_5_05-08-1421.pdf?domain=www.linear.com, https://www.diodes.com/assets/Package-Files/TO220-5.pdf")
    (tags "TO-220-5 Vertical RM 1.7mm Pentawatt Multiwatt-5 staggered type-1")
    (fp_text reference U1 (at 3.81 3.683 180) (layer F.SilkS))
    (fp_text value LM2576TV-5G (at 3.4 2.15 180) (layer F.Fab))
    (fp_text user %R (at 3.4 -9.32 180) (layer F.Fab))
    (pad 5 thru_hole oval (at 6.8 0 180) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 4 thru_hole oval (at 5.1 -3.7 180) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask)
      (net 4 VCC))
    (pad 3 thru_hole oval (at 3.4 0 180) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 2 thru_hole oval (at 1.7 -3.7 180) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad1)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 +BATT))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-220-5_P3.4x3.7mm_StaggerOdd_Lead3.8mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Inductor:Wuerth WE-LHMI SMD" (layer F.Cu) (tedit 5B6DE5FB)
    (at 115.57 60.96)
    (fp_text reference L1 (at -7.366 4.064) (layer F.SilkS))
    (fp_text value 47uH (at -7.366 -4.826 90) (layer F.Fab))
    (pad 2 smd rect (at 6.25 0 180) (size 4.5 5) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(D1-Pad1)"))
    (pad 1 smd rect (at -6.25 0) (size 4.5 5) (layers F.Cu F.Paste F.Mask)
      (net 4 VCC))
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 113.425 111.252 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C5 (at 3.951 0 180) (layer F.SilkS))
    (fp_text value 100nF (at 2.681 -1.27 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 VCC))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_SMD:SW_SPST_TL3305A (layer F.Cu) (tedit 5ABC3A97)
    (at 110.998 130.81 180)
    (descr https://www.e-switch.com/system/asset/product_line/data_sheet/213/TL3305.pdf)
    (tags "TL3305 Series Tact Switch")
    (attr smd)
    (fp_text reference SW2 (at 0 0 180) (layer F.SilkS))
    (fp_text value Reset (at 0 3.2 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at -3.6 1.5 180) (size 1.6 1.4) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 2 smd rect (at 3.6 1.5 180) (size 1.6 1.4) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 1 smd rect (at -3.6 -1.5 180) (size 1.6 1.4) (layers F.Cu F.Paste F.Mask)
      (net 5 /RESET))
    (pad 1 smd rect (at 3.6 -1.5 180) (size 1.6 1.4) (layers F.Cu F.Paste F.Mask)
      (net 5 /RESET))
    (model ${KISYS3DMOD}/Button_Switch_SMD.3dshapes/SW_SPST_TL3305A.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_SMD:SW_SPST_TL3305A (layer F.Cu) (tedit 5ABC3A97)
    (at 124.46 138.938 90)
    (descr https://www.e-switch.com/system/asset/product_line/data_sheet/213/TL3305.pdf)
    (tags "TL3305 Series Tact Switch")
    (attr smd)
    (fp_text reference SW1 (at 1.016 0 180) (layer F.SilkS))
    (fp_text value Button (at 0 3.429 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at -3.6 1.5 90) (size 1.6 1.4) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 2 smd rect (at 3.6 1.5 90) (size 1.6 1.4) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 1 smd rect (at -3.6 -1.5 90) (size 1.6 1.4) (layers F.Cu F.Paste F.Mask)
      (net 9 /BUTTON))
    (pad 1 smd rect (at 3.6 -1.5 90) (size 1.6 1.4) (layers F.Cu F.Paste F.Mask)
      (net 9 /BUTTON))
    (model ${KISYS3DMOD}/Button_Switch_SMD.3dshapes/SW_SPST_TL3305A.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:CP_Elec_8x10 (layer F.Cu) (tedit 5A841F9D)
    (at 124.206 48.26)
    (descr "SMT capacitor, aluminium electrolytic, 8x10, Nichicon ")
    (tags "Capacitor Electrolytic")
    (attr smd)
    (fp_text reference C1 (at 4.318 -5.08) (layer F.SilkS))
    (fp_text value 100uF (at 0 5.2) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 3.25 0) (size 3.5 2.5) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 1 smd rect (at -3.25 0) (size 3.5 2.5) (layers F.Cu F.Paste F.Mask)
      (net 1 +BATT))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/CP_Elec_8x10.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 113.425 108.204 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C3 (at 3.951 0 180) (layer F.SilkS))
    (fp_text value 10uF (at 1.919 1.524 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 VCC))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 108.712 116.445 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C6 (at -0.113 1.524 90) (layer F.SilkS))
    (fp_text value 20pF (at 3.443 1.524 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 /XTAL1))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 108.712 123.303 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C7 (at -0.141 -1.43 90) (layer F.SilkS))
    (fp_text value 20pF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 /XTAL2))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical_SMD_Pin1Left (layer F.Cu) (tedit 59FED5CC)
    (at 123.952 90.424 270)
    (descr "surface-mounted straight pin header, 1x04, 2.54mm pitch, single row, style 1 (pin 1 left)")
    (tags "Surface mounted pin header SMD 1x04 2.54mm single row style1 pin1 left")
    (attr smd)
    (fp_text reference J2 (at 0.508 0.254) (layer F.SilkS))
    (fp_text value LED (at 0 6.14 270) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 4 smd rect (at 1.655 3.81 270) (size 2.51 1) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 2 smd rect (at 1.655 -1.27 270) (size 2.51 1) (layers F.Cu F.Paste F.Mask)
      (net 11 /CLK))
    (pad 3 smd rect (at -1.655 1.27 270) (size 2.51 1) (layers F.Cu F.Paste F.Mask)
      (net 8 /DATA))
    (pad 1 smd rect (at -1.655 -3.81 270) (size 2.51 1) (layers F.Cu F.Paste F.Mask)
      (net 4 VCC))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical_SMD_Pin1Left.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x03_P2.54mm_Vertical_SMD (layer F.Cu) (tedit 59FED5CC)
    (at 110.998 139.192 90)
    (descr "surface-mounted straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Surface mounted pin header SMD 2x03 2.54mm double row")
    (attr smd)
    (fp_text reference J4 (at 0 -1.27 180) (layer F.SilkS))
    (fp_text value ISP (at 0 -4.445 90) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 6 smd rect (at 2.525 2.54 90) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 5 smd rect (at -2.525 2.54 90) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 5 /RESET))
    (pad 4 smd rect (at 2.525 0 90) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 8 /DATA))
    (pad 3 smd rect (at -2.525 0 90) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 11 /CLK))
    (pad 2 smd rect (at 2.525 -2.54 90) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(J4-Pad2)"))
    (pad 1 smd rect (at -2.525 -2.54 90) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 27 /MISO))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x03_P2.54mm_Vertical_SMD.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Wire:SolderWirePad_1x02_P3.81mm_Drill1.2mm (layer F.Cu) (tedit 5AEE5EF3)
    (at 122.555 40.64)
    (descr "Wire solder connection")
    (tags connector)
    (attr virtual)
    (fp_text reference J1 (at 5.969 -2.286) (layer F.SilkS))
    (fp_text value BATT (at 0 -2.54 180) (layer F.Fab))
    (fp_text user %R (at 1.905 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 3.81 0) (size 2.99974 2.99974) (drill 1.19888) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 1 thru_hole rect (at 0 0) (size 2.99974 2.99974) (drill 1.19888) (layers *.Cu *.Mask)
      (net 1 +BATT))
  )
  (module Connector_Wire:SolderWirePad_1x02_P3.81mm_Drill1.2mm (layer F.Cu) (tedit 5AEE5EF3)
    (at 118.618 138.049 270)
    (descr "Wire solder connection")
    (tags connector)
    (attr virtual)
    (fp_text reference J5 (at 4.953 -2.286) (layer F.SilkS))
    (fp_text value "External Button" (at 7.62 0.127) (layer F.Fab))
    (fp_text user %R (at 1.905 0 270) (layer F.Fab))
    (pad 2 thru_hole circle (at 3.81 0 270) (size 2.99974 2.99974) (drill 1.19888) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.99974 2.99974) (drill 1.19888) (layers *.Cu *.Mask)
      (net 9 /BUTTON))
  )
  (module Crystal:Crystal_SMD_HC49-SD (layer F.Cu) (tedit 5A1AD52C)
    (at 112.395 120.015 270)
    (descr "SMD Crystal HC-49-SD http://cdn-reichelt.de/documents/datenblatt/B400/xxx-HC49-SMD.pdf, 11.4x4.7mm^2 package")
    (tags "SMD SMT crystal")
    (attr smd)
    (fp_text reference Y1 (at -6.731 3.683) (layer F.SilkS))
    (fp_text value 16Mhz (at 0.127 -0.127) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 4.25 0 270) (size 4.5 2) (layers F.Cu F.Paste F.Mask)
      (net 15 /XTAL2))
    (pad 1 smd rect (at -4.25 0 270) (size 4.5 2) (layers F.Cu F.Paste F.Mask)
      (net 13 /XTAL1))
    (model ${KISYS3DMOD}/Crystal.3dshapes/Crystal_SMD_HC49-SD.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SMA_Handsoldering (layer F.Cu) (tedit 58643398)
    (at 127 58.42 90)
    (descr "Diode SMA (DO-214AC) Handsoldering")
    (tags "Diode SMA (DO-214AC) Handsoldering")
    (attr smd)
    (fp_text reference D1 (at -5.715 0.635 180) (layer F.SilkS))
    (fp_text value 3A (at 0 2.6 90) (layer F.Fab))
    (fp_text user %R (at 0 -2.5 90) (layer F.Fab))
    (pad 2 smd rect (at 2.5 0 90) (size 3.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 1 smd rect (at -2.5 0 90) (size 3.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DIP:DIP-28_W8.89mm_SMDSocket_LongPads (layer F.Cu) (tedit 5A02E8C5)
    (at 122.555 114.935)
    (descr "28-lead though-hole mounted DIP package, row spacing 8.89 mm (350 mils), SMDSocket, LongPads")
    (tags "THT DIP DIL PDIP 2.54mm 8.89mm 350mil SMDSocket LongPads")
    (attr smd)
    (fp_text reference U2 (at -2.921 -18.923) (layer F.SilkS))
    (fp_text value ATmega168A-PU (at 1.651 -10.795 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 28 smd rect (at 4.445 -16.51) (size 3.1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(U2-Pad28)"))
    (pad 14 smd rect (at -4.445 16.51) (size 3.1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(U2-Pad14)"))
    (pad 27 smd rect (at 4.445 -13.97) (size 3.1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(U2-Pad27)"))
    (pad 13 smd rect (at -4.445 13.97) (size 3.1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(U2-Pad13)"))
    (pad 26 smd rect (at 4.445 -11.43) (size 3.1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(U2-Pad26)"))
    (pad 12 smd rect (at -4.445 11.43) (size 3.1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(U2-Pad12)"))
    (pad 25 smd rect (at 4.445 -8.89) (size 3.1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(U2-Pad25)"))
    (pad 11 smd rect (at -4.445 8.89) (size 3.1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(U2-Pad11)"))
    (pad 24 smd rect (at 4.445 -6.35) (size 3.1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(U2-Pad24)"))
    (pad 10 smd rect (at -4.445 6.35) (size 3.1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 15 /XTAL2))
    (pad 23 smd rect (at 4.445 -3.81) (size 3.1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(U2-Pad23)"))
    (pad 9 smd rect (at -4.445 3.81) (size 3.1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 13 /XTAL1))
    (pad 22 smd rect (at 4.445 -1.27) (size 3.1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 8 smd rect (at -4.445 1.27) (size 3.1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 21 smd rect (at 4.445 1.27) (size 3.1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 4 VCC))
    (pad 7 smd rect (at -4.445 -1.27) (size 3.1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 4 VCC))
    (pad 20 smd rect (at 4.445 3.81) (size 3.1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 4 VCC))
    (pad 6 smd rect (at -4.445 -3.81) (size 3.1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(U2-Pad6)"))
    (pad 19 smd rect (at 4.445 6.35) (size 3.1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 11 /CLK))
    (pad 5 smd rect (at -4.445 -6.35) (size 3.1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(U2-Pad5)"))
    (pad 18 smd rect (at 4.445 8.89) (size 3.1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 27 /MISO))
    (pad 4 smd rect (at -4.445 -8.89) (size 3.1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 9 /BUTTON))
    (pad 17 smd rect (at 4.445 11.43) (size 3.1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 8 /DATA))
    (pad 3 smd rect (at -4.445 -11.43) (size 3.1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 26 /FTDI_RX))
    (pad 16 smd rect (at 4.445 13.97) (size 3.1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(U2-Pad16)"))
    (pad 2 smd rect (at -4.445 -13.97) (size 3.1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 25 /FTDI_TX))
    (pad 15 smd rect (at 4.445 16.51) (size 3.1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(U2-Pad15)"))
    (pad 1 smd rect (at -4.445 -16.51) (size 3.1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 5 /RESET))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-28_W8.89mm_SMDSocket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Symbol:OSHW-Logo2_24.3x20mm_SilkScreen (layer B.Cu) (tedit 0)
    (at 117.602 59.69 180)
    (descr "Open Source Hardware Symbol")
    (tags "Logo Symbol OSHW")
    (attr virtual)
    (fp_text reference REF** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value OSHW-Logo2_24.3x20mm_SilkScreen (at 0.75 0 180) (layer B.Fab) hide)
  )
  (module Symbol:KiCad-Logo_6mm_SilkScreen (layer B.Cu) (tedit 0)
    (at 109.22 97.536 90)
    (descr "KiCad Logo")
    (tags "Logo KiCad")
    (attr virtual)
    (fp_text reference REF** (at 0 0 90) (layer B.SilkS) hide)
    (fp_text value KiCad-Logo_6mm_SilkScreen (at 0.75 0 90) (layer B.Fab) hide)
  )
  (gr_text VCC (at 127.762 94.234 90) (layer F.SilkS))
  (gr_text CLK (at 125.222 95.25 90) (layer F.SilkS))
  (gr_text DAT (at 122.682 92.964 90) (layer F.SilkS))
  (gr_text GND (at 118.364 92.964 90) (layer F.SilkS))
  (gr_text GND (at 113.792 88.646) (layer F.SilkS))
  (gr_text "RAVE SABER\nv3.0.0" (at 117.856 82.804) (layer B.SilkS))
  (gr_text BATT (at 124.46 43.688) (layer B.SilkS))
  (gr_text "EXT\nBTN" (at 122.682 140.208) (layer B.SilkS))
  (gr_text "CERN OHL v1.2\nGPL v3.0" (at 117.856 71.628) (layer B.SilkS))
  (gr_text "Pavan Rikhi, 2021-04-20\nhttps://github.com/Rave-Saber/" (at 126.238 89.408 90) (layer B.SilkS))
  (gr_text 1 (at 106.934 143.002) (layer F.SilkS))
  (gr_text - (at 128.778 40.64) (layer B.SilkS))
  (gr_text + (at 119.888 40.64) (layer B.SilkS))
  (gr_text - (at 128.778 40.64) (layer F.SilkS))
  (gr_text + (at 119.888 40.64) (layer F.SilkS))
  (dimension 107.95 (width 0.3) (layer Cmts.User)
    (gr_text "4.2500 in" (at 96.96 90.805 90) (layer Cmts.User))
    (feature1 (pts (xy 105.41 36.83) (xy 98.473579 36.83)))
    (feature2 (pts (xy 105.41 144.78) (xy 98.473579 144.78)))
    (crossbar (pts (xy 99.06 144.78) (xy 99.06 36.83)))
    (arrow1a (pts (xy 99.06 36.83) (xy 99.646421 37.956504)))
    (arrow1b (pts (xy 99.06 36.83) (xy 98.473579 37.956504)))
    (arrow2a (pts (xy 99.06 144.78) (xy 99.646421 143.653496)))
    (arrow2b (pts (xy 99.06 144.78) (xy 98.473579 143.653496)))
  )
  (dimension 24.639245 (width 0.3) (layer Cmts.User)
    (gr_text "0.9700 in" (at 117.729622 28.38) (layer Cmts.User))
    (feature1 (pts (xy 130.049245 36.83) (xy 130.049245 29.893579)))
    (feature2 (pts (xy 105.41 36.83) (xy 105.41 29.893579)))
    (crossbar (pts (xy 105.41 30.48) (xy 130.049245 30.48)))
    (arrow1a (pts (xy 130.049245 30.48) (xy 128.922741 31.066421)))
    (arrow1b (pts (xy 130.049245 30.48) (xy 128.922741 29.893579)))
    (arrow2a (pts (xy 105.41 30.48) (xy 106.536504 31.066421)))
    (arrow2b (pts (xy 105.41 30.48) (xy 106.536504 29.893579)))
  )
  (gr_line (start 105.41 36.83) (end 130.048 36.83) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 105.41 144.78) (end 105.41 36.83) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 130.048 144.78) (end 130.048 36.83) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 130.048 144.78) (end 105.41 144.78) (layer Edge.Cuts) (width 0.15))
  (zone (net 3) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.635))
    (polygon
      (pts
        (xy 130.048 36.83) (xy 105.41 36.83) (xy 105.41 86.36) (xy 130.048 86.36)
      )
    )
  )
  (zone (net 3) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.635))
    (polygon
      (pts
        (xy 105.41 86.868) (xy 130.048 86.868) (xy 130.048 144.78) (xy 105.41 144.78)
      )
    )
  )
)
