(kicad_pcb (version 4) (host pcbnew 4.0.2+dfsg1-stable)
  (general
    (links 81)
    (no_connects 0)
    (area 17.751667 15.846666 99.088334 84.493)
    (thickness 1.6)
    (drawings 27)
    (tracks 370)
    (zones 0)
    (modules 42)
    (nets 37)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.381)
    (user_trace_width 1.016)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(D1-Pad1)")
  (net 2 "Net-(D1-Pad2)")
  (net 3 "Net-(D2-Pad1)")
  (net 4 "Net-(D2-Pad2)")
  (net 5 "Net-(D3-Pad1)")
  (net 6 "Net-(D3-Pad2)")
  (net 7 "Net-(JP1-Pad1)")
  (net 8 +5V)
  (net 9 "Net-(JP2-Pad1)")
  (net 10 "Net-(P1-Pad1)")
  (net 11 "Net-(P1-Pad2)")
  (net 12 GND)
  (net 13 +3V3)
  (net 14 "Net-(P3-Pad1)")
  (net 15 "Net-(P3-Pad2)")
  (net 16 "Net-(P3-Pad3)")
  (net 17 +12V)
  (net 18 "Net-(P4-Pad3)")
  (net 19 "Net-(Q1-Pad3)")
  (net 20 "Net-(Q2-Pad2)")
  (net 21 LED0_IND)
  (net 22 "Net-(Q3-Pad3)")
  (net 23 "Net-(Q4-Pad2)")
  (net 24 LED1_IND)
  (net 25 "Net-(Q5-Pad3)")
  (net 26 "Net-(Q6-Pad2)")
  (net 27 LED2_IND)
  (net 28 "Net-(Q7-Pad2)")
  (net 29 "Net-(Q8-Pad2)")
  (net 30 "Net-(Q9-Pad2)")
  (net 31 "Net-(Q1-Pad1)")
  (net 32 "Net-(Q3-Pad1)")
  (net 33 "Net-(Q5-Pad1)")
  (net 34 "Net-(R2-Pad1)")
  (net 35 "Net-(R5-Pad1)")
  (net 36 "Net-(R8-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +12V)
    (add_net +3V3)
    (add_net +5V)
    (add_net GND)
    (add_net LED0_IND)
    (add_net LED1_IND)
    (add_net LED2_IND)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(JP1-Pad1)")
    (add_net "Net-(JP2-Pad1)")
    (add_net "Net-(P1-Pad1)")
    (add_net "Net-(P1-Pad2)")
    (add_net "Net-(P3-Pad1)")
    (add_net "Net-(P3-Pad2)")
    (add_net "Net-(P3-Pad3)")
    (add_net "Net-(P4-Pad3)")
    (add_net "Net-(Q1-Pad1)")
    (add_net "Net-(Q1-Pad3)")
    (add_net "Net-(Q2-Pad2)")
    (add_net "Net-(Q3-Pad1)")
    (add_net "Net-(Q3-Pad3)")
    (add_net "Net-(Q4-Pad2)")
    (add_net "Net-(Q5-Pad1)")
    (add_net "Net-(Q5-Pad3)")
    (add_net "Net-(Q6-Pad2)")
    (add_net "Net-(Q7-Pad2)")
    (add_net "Net-(Q8-Pad2)")
    (add_net "Net-(Q9-Pad2)")
    (add_net "Net-(R2-Pad1)")
    (add_net "Net-(R5-Pad1)")
    (add_net "Net-(R8-Pad1)")
  )
  (module Potentiometers:Potentiometer_VishaySpectrol-Econtrim-Type36P (layer F.Cu) (tedit 5446FD75)
    (at 78.232 64.77)
    (descr "Potentiometer, Trimmer, Spectrol Type 36P, Econtrim, Rev A, 02 Aug 2010,")
    (tags "Potentiometer, Trimmer, Spectrol Type 36P, Econtrim, Rev A, 02 Aug 2010,")
    (fp_text reference RV2 (at 6.30936 -5.56006) (layer F.SilkS))
    (fp_text value 10K (at 2.49936 3.32994) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.49936 -3.50012) (size 2.49936 2.49936) (drill 1.19888) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(Q4-Pad2)"))
    (pad 3 thru_hole circle (at 4.99872 0) (size 2.49936 2.49936) (drill 1.19888) (layers *.Cu *.Mask F.SilkS)
      (net 35 "Net-(R5-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 2.49936 2.49936) (drill 1.19888) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(Q4-Pad2)"))
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 57FC0BAA)
    (at 56.746 79.375 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at -0.127 -2.54 270) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0 -3.1 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(P1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(P1-Pad2)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module LEDs:LED-3MM (layer F.Cu) (tedit 57FC0B8E)
    (at 69.342 75.184)
    (descr "LED 3mm round vertical")
    (tags "LED  3mm round vertical")
    (fp_text reference D1 (at 1.27 -2.667) (layer F.SilkS))
    (fp_text value LED (at 1.3 -2.9) (layer F.Fab))
    (fp_text user K (at -1.69 1.74) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 90) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(D1-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(D1-Pad2)"))
    (model LEDs.3dshapes/LED-3MM.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module LEDs:LED-3MM (layer F.Cu) (tedit 57FC0B92)
    (at 75.184 75.184)
    (descr "LED 3mm round vertical")
    (tags "LED  3mm round vertical")
    (fp_text reference D2 (at 1.27 -2.667) (layer F.SilkS))
    (fp_text value LED (at 1.3 -2.9) (layer F.Fab))
    (fp_text user K (at -1.69 1.74) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 90) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(D2-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(D2-Pad2)"))
    (model LEDs.3dshapes/LED-3MM.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module LEDs:LED-3MM (layer F.Cu) (tedit 57FC0B95)
    (at 81.026 75.184)
    (descr "LED 3mm round vertical")
    (tags "LED  3mm round vertical")
    (fp_text reference D3 (at 1.397 -2.794) (layer F.SilkS))
    (fp_text value LED (at 1.3 -2.9) (layer F.Fab))
    (fp_text user K (at -1.69 1.74) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 90) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(D3-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(D3-Pad2)"))
    (model LEDs.3dshapes/LED-3MM.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Connect:GS2 (layer F.Cu) (tedit 0)
    (at 59.69 67.564)
    (descr "Pontet Goute de soudure")
    (attr virtual)
    (fp_text reference JP1 (at 1.778 0 90) (layer F.SilkS))
    (fp_text value Jumper_NO_Small (at 1.524 0 90) (layer F.Fab))
    (pad 1 smd rect (at 0 -0.635) (size 1.27 0.9652) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(JP1-Pad1)"))
    (pad 2 smd rect (at 0 0.635) (size 1.27 0.9652) (layers F.Cu F.Paste F.Mask)
      (net 8 +5V))
  )
  (module Connect:GS2 (layer F.Cu) (tedit 0)
    (at 63.754 67.564)
    (descr "Pontet Goute de soudure")
    (attr virtual)
    (fp_text reference JP2 (at 1.778 0 90) (layer F.SilkS))
    (fp_text value Jumper_NO_Small (at 1.524 0 90) (layer F.Fab))
    (pad 1 smd rect (at 0 -0.635) (size 1.27 0.9652) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(JP2-Pad1)"))
    (pad 2 smd rect (at 0 0.635) (size 1.27 0.9652) (layers F.Cu F.Paste F.Mask)
      (net 8 +5V))
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 57FC0BAA)
    (at 63.246 79.375 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at -0.127 -2.54 270) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0 -3.1 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(P1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(P1-Pad2)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 0)
    (at 93.98 25.146 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P2 (at 0 -5.1 180) (layer F.SilkS))
    (fp_text value CONN_01X03 (at 0 -3.1 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 GND))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 +3V3))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 +5V))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04 (layer F.Cu) (tedit 57FC0BFF)
    (at 30.861 20.955 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P3 (at 0 9.906 270) (layer F.SilkS))
    (fp_text value CONN_01X04 (at 0 -3.1 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(P3-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(P3-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(P3-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 +12V))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x04.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 0)
    (at 22.86 72.39 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P4 (at 0 -5.1 180) (layer F.SilkS))
    (fp_text value CONN_01X03 (at 0 -3.1 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 GND))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 +12V))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(P4-Pad3)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 57FC0C05)
    (at 22.86 61.214 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P7 (at 0 -2.794 180) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0 -3.1 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 GND))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 +12V))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module TO_SOT_Packages_THT:TO-92_Inline_Narrow_Oval (layer F.Cu) (tedit 57FC0BF0)
    (at 72.898 22.352)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.6mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q2 (at 0 -3.81) (layer F.SilkS))
    (fp_text value BC413 (at 0 3) (layer F.Fab))
    (pad 2 thru_hole oval (at 1.27 0 180) (size 0.89916 1.50114) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(Q2-Pad2)"))
    (pad 3 thru_hole oval (at 2.54 0 180) (size 0.89916 1.50114) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 12 GND))
    (pad 1 thru_hole oval (at 0 0 180) (size 0.89916 1.50114) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 21 LED0_IND))
    (model TO_SOT_Packages_THT.3dshapes/TO-92_Inline_Narrow_Oval.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module TO_SOT_Packages_THT:TO-92_Inline_Narrow_Oval (layer F.Cu) (tedit 57FC0BF3)
    (at 78.994 22.352)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.6mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q4 (at 0 -3.81) (layer F.SilkS))
    (fp_text value BC413 (at 0 3) (layer F.Fab))
    (pad 2 thru_hole oval (at 1.27 0 180) (size 0.89916 1.50114) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(Q4-Pad2)"))
    (pad 3 thru_hole oval (at 2.54 0 180) (size 0.89916 1.50114) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 12 GND))
    (pad 1 thru_hole oval (at 0 0 180) (size 0.89916 1.50114) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 24 LED1_IND))
    (model TO_SOT_Packages_THT.3dshapes/TO-92_Inline_Narrow_Oval.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module TO_SOT_Packages_THT:TO-92_Inline_Narrow_Oval (layer F.Cu) (tedit 57FC0BF7)
    (at 84.836 22.352)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.6mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q6 (at 0 -3.81) (layer F.SilkS))
    (fp_text value BC413 (at 0 3) (layer F.Fab))
    (pad 2 thru_hole oval (at 1.27 0 180) (size 0.89916 1.50114) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(Q6-Pad2)"))
    (pad 3 thru_hole oval (at 2.54 0 180) (size 0.89916 1.50114) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 12 GND))
    (pad 1 thru_hole oval (at 0 0 180) (size 0.89916 1.50114) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 27 LED2_IND))
    (model TO_SOT_Packages_THT.3dshapes/TO-92_Inline_Narrow_Oval.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module TO_SOT_Packages_THT:TO-92_Inline_Narrow_Oval (layer F.Cu) (tedit 57FC0BA4)
    (at 69.342 80.518)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.6mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q7 (at -1.651 -2.286) (layer F.SilkS))
    (fp_text value BC413 (at 0 3) (layer F.Fab))
    (pad 2 thru_hole oval (at 1.27 0 180) (size 0.89916 1.50114) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 28 "Net-(Q7-Pad2)"))
    (pad 3 thru_hole oval (at 2.54 0 180) (size 0.89916 1.50114) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 12 GND))
    (pad 1 thru_hole oval (at 0 0 180) (size 0.89916 1.50114) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(D1-Pad1)"))
    (model TO_SOT_Packages_THT.3dshapes/TO-92_Inline_Narrow_Oval.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module TO_SOT_Packages_THT:TO-92_Inline_Narrow_Oval (layer F.Cu) (tedit 57FC0BA2)
    (at 75.184 80.518)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.6mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q8 (at -1.524 -2.159) (layer F.SilkS))
    (fp_text value BC413 (at 0 3) (layer F.Fab))
    (pad 2 thru_hole oval (at 1.27 0 180) (size 0.89916 1.50114) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 29 "Net-(Q8-Pad2)"))
    (pad 3 thru_hole oval (at 2.54 0 180) (size 0.89916 1.50114) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 12 GND))
    (pad 1 thru_hole oval (at 0 0 180) (size 0.89916 1.50114) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(D2-Pad1)"))
    (model TO_SOT_Packages_THT.3dshapes/TO-92_Inline_Narrow_Oval.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module TO_SOT_Packages_THT:TO-92_Inline_Narrow_Oval (layer F.Cu) (tedit 57FC0BA7)
    (at 81.026 80.518)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.6mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q9 (at -1.27 -2.54) (layer F.SilkS))
    (fp_text value BC413 (at 0 3) (layer F.Fab))
    (pad 2 thru_hole oval (at 1.27 0 180) (size 0.89916 1.50114) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 30 "Net-(Q9-Pad2)"))
    (pad 3 thru_hole oval (at 2.54 0 180) (size 0.89916 1.50114) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 12 GND))
    (pad 1 thru_hole oval (at 0 0 180) (size 0.89916 1.50114) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(D3-Pad1)"))
    (model TO_SOT_Packages_THT.3dshapes/TO-92_Inline_Narrow_Oval.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM7mm (layer F.Cu) (tedit 57FC0B53)
    (at 35.56 65.786)
    (descr "Resistor, Axial,  RM 7.62mm, 1/3W,")
    (tags "Resistor Axial RM 7.62mm 1/3W R3")
    (fp_text reference R1 (at -2.286 0) (layer F.SilkS))
    (fp_text value 10K (at 3.81 3.81) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 31 "Net-(Q1-Pad1)"))
    (pad 2 thru_hole circle (at 7.62 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 21 LED0_IND))
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM7mm (layer F.Cu) (tedit 57FC0BE1)
    (at 80.264 34.798 90)
    (descr "Resistor, Axial,  RM 7.62mm, 1/3W,")
    (tags "Resistor Axial RM 7.62mm 1/3W R3")
    (fp_text reference R2 (at 9.652 0 180) (layer F.SilkS))
    (fp_text value 2K (at 3.81 3.81 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 34 "Net-(R2-Pad1)"))
    (pad 2 thru_hole circle (at 7.62 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 12 GND))
  )
  (module Custom_Footprints:Current_Sense_Resistor (layer F.Cu) (tedit 57DE1991)
    (at 58.928 21.59 180)
    (fp_text reference R3 (at -0.1 2.4 180) (layer F.SilkS))
    (fp_text value R (at 0.3 -2.9 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 5.715 0 180) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(Q1-Pad3)"))
    (pad 2 thru_hole circle (at -5.715 0 180) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 12 GND))
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM7mm (layer F.Cu) (tedit 57FC0B5B)
    (at 35.56 69.342)
    (descr "Resistor, Axial,  RM 7.62mm, 1/3W,")
    (tags "Resistor Axial RM 7.62mm 1/3W R3")
    (fp_text reference R4 (at -2.286 0) (layer F.SilkS))
    (fp_text value 10K (at 3.81 3.81) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 32 "Net-(Q3-Pad1)"))
    (pad 2 thru_hole circle (at 7.62 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 24 LED1_IND))
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM7mm (layer F.Cu) (tedit 57FC0BD2)
    (at 76.962 34.798 90)
    (descr "Resistor, Axial,  RM 7.62mm, 1/3W,")
    (tags "Resistor Axial RM 7.62mm 1/3W R3")
    (fp_text reference R5 (at 9.652 0 180) (layer F.SilkS))
    (fp_text value 2K (at 3.81 3.81 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 35 "Net-(R5-Pad1)"))
    (pad 2 thru_hole circle (at 7.62 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 12 GND))
  )
  (module Custom_Footprints:Current_Sense_Resistor (layer F.Cu) (tedit 57DE1991)
    (at 58.928 36.83 180)
    (fp_text reference R6 (at -0.1 2.4 180) (layer F.SilkS))
    (fp_text value R (at 0.3 -2.9 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 5.715 0 180) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(Q3-Pad3)"))
    (pad 2 thru_hole circle (at -5.715 0 180) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 12 GND))
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM7mm (layer F.Cu) (tedit 57FC0B62)
    (at 35.56 72.898)
    (descr "Resistor, Axial,  RM 7.62mm, 1/3W,")
    (tags "Resistor Axial RM 7.62mm 1/3W R3")
    (fp_text reference R7 (at -2.286 0) (layer F.SilkS))
    (fp_text value 10K (at 3.81 3.81) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 33 "Net-(Q5-Pad1)"))
    (pad 2 thru_hole circle (at 7.62 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 27 LED2_IND))
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM7mm (layer F.Cu) (tedit 57FC0BEB)
    (at 83.566 34.798 90)
    (descr "Resistor, Axial,  RM 7.62mm, 1/3W,")
    (tags "Resistor Axial RM 7.62mm 1/3W R3")
    (fp_text reference R8 (at 9.652 0 180) (layer F.SilkS))
    (fp_text value 2K (at 3.81 3.81 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 36 "Net-(R8-Pad1)"))
    (pad 2 thru_hole circle (at 7.62 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 12 GND))
  )
  (module Custom_Footprints:Current_Sense_Resistor (layer F.Cu) (tedit 57DE1991)
    (at 58.928 52.07 180)
    (fp_text reference R9 (at -0.1 2.4 180) (layer F.SilkS))
    (fp_text value R (at 0.3 -2.9 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 5.715 0 180) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(Q5-Pad3)"))
    (pad 2 thru_hole circle (at -5.715 0 180) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 12 GND))
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM7mm (layer F.Cu) (tedit 57FC0B81)
    (at 57.912 75.565)
    (descr "Resistor, Axial,  RM 7.62mm, 1/3W,")
    (tags "Resistor Axial RM 7.62mm 1/3W R3")
    (fp_text reference R10 (at -0.508 2.032) (layer F.SilkS))
    (fp_text value 4.7K (at 3.81 3.81) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 11 "Net-(P1-Pad2)"))
    (pad 2 thru_hole circle (at 7.62 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 13 +3V3))
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM7mm (layer F.Cu) (tedit 57FC0B86)
    (at 57.912 72.263)
    (descr "Resistor, Axial,  RM 7.62mm, 1/3W,")
    (tags "Resistor Axial RM 7.62mm 1/3W R3")
    (fp_text reference R11 (at 10.16 0.127) (layer F.SilkS))
    (fp_text value 4.7K (at 3.81 3.81) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 10 "Net-(P1-Pad1)"))
    (pad 2 thru_hole circle (at 7.62 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 13 +3V3))
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM7mm (layer F.Cu) (tedit 57FC0BB8)
    (at 87.122 68.58 270)
    (descr "Resistor, Axial,  RM 7.62mm, 1/3W,")
    (tags "Resistor Axial RM 7.62mm 1/3W R3")
    (fp_text reference R12 (at 10.414 0 270) (layer F.SilkS))
    (fp_text value 330 (at 3.81 3.81 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 2 "Net-(D1-Pad2)"))
    (pad 2 thru_hole circle (at 7.62 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 8 +5V))
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM7mm (layer F.Cu) (tedit 57FC0BBD)
    (at 90.424 76.2 90)
    (descr "Resistor, Axial,  RM 7.62mm, 1/3W,")
    (tags "Resistor Axial RM 7.62mm 1/3W R3")
    (fp_text reference R13 (at -2.794 0 90) (layer F.SilkS))
    (fp_text value 330 (at 3.81 3.81 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 8 +5V))
    (pad 2 thru_hole circle (at 7.62 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 4 "Net-(D2-Pad2)"))
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM7mm (layer F.Cu) (tedit 57FC0BC2)
    (at 93.726 76.2 90)
    (descr "Resistor, Axial,  RM 7.62mm, 1/3W,")
    (tags "Resistor Axial RM 7.62mm 1/3W R3")
    (fp_text reference R14 (at -2.794 0 90) (layer F.SilkS))
    (fp_text value 330 (at 3.81 3.81 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 8 +5V))
    (pad 2 thru_hole circle (at 7.62 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 6 "Net-(D3-Pad2)"))
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM7mm (layer F.Cu) (tedit 57FC0B6C)
    (at 46.228 65.786)
    (descr "Resistor, Axial,  RM 7.62mm, 1/3W,")
    (tags "Resistor Axial RM 7.62mm 1/3W R3")
    (fp_text reference R15 (at 10.287 0) (layer F.SilkS))
    (fp_text value 50K (at 3.81 3.81) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 28 "Net-(Q7-Pad2)"))
    (pad 2 thru_hole circle (at 7.62 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 21 LED0_IND))
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM7mm (layer F.Cu) (tedit 57FC0B70)
    (at 46.228 69.342)
    (descr "Resistor, Axial,  RM 7.62mm, 1/3W,")
    (tags "Resistor Axial RM 7.62mm 1/3W R3")
    (fp_text reference R16 (at 10.287 0) (layer F.SilkS))
    (fp_text value 50K (at 3.81 3.81) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 29 "Net-(Q8-Pad2)"))
    (pad 2 thru_hole circle (at 7.62 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 24 LED1_IND))
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM7mm (layer F.Cu) (tedit 57FC0B77)
    (at 46.228 72.898)
    (descr "Resistor, Axial,  RM 7.62mm, 1/3W,")
    (tags "Resistor Axial RM 7.62mm 1/3W R3")
    (fp_text reference R17 (at 7.747 2.159) (layer F.SilkS))
    (fp_text value 50K (at 3.81 3.81) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 30 "Net-(Q9-Pad2)"))
    (pad 2 thru_hole circle (at 7.62 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 27 LED2_IND))
  )
  (module Potentiometers:Potentiometer_VishaySpectrol-Econtrim-Type36P (layer F.Cu) (tedit 5446FD75)
    (at 69.85 64.77)
    (descr "Potentiometer, Trimmer, Spectrol Type 36P, Econtrim, Rev A, 02 Aug 2010,")
    (tags "Potentiometer, Trimmer, Spectrol Type 36P, Econtrim, Rev A, 02 Aug 2010,")
    (fp_text reference RV1 (at 6.30936 -5.56006) (layer F.SilkS))
    (fp_text value 10K (at 2.49936 3.32994) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.49936 -3.50012) (size 2.49936 2.49936) (drill 1.19888) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(Q2-Pad2)"))
    (pad 3 thru_hole circle (at 4.99872 0) (size 2.49936 2.49936) (drill 1.19888) (layers *.Cu *.Mask F.SilkS)
      (net 34 "Net-(R2-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 2.49936 2.49936) (drill 1.19888) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(Q2-Pad2)"))
  )
  (module Potentiometers:Potentiometer_VishaySpectrol-Econtrim-Type36P (layer F.Cu) (tedit 57FC0C73)
    (at 86.614 64.77)
    (descr "Potentiometer, Trimmer, Spectrol Type 36P, Econtrim, Rev A, 02 Aug 2010,")
    (tags "Potentiometer, Trimmer, Spectrol Type 36P, Econtrim, Rev A, 02 Aug 2010,")
    (fp_text reference RV3 (at 4.953 -5.588) (layer F.SilkS))
    (fp_text value 10K (at 2.49936 3.32994) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.49936 -3.50012) (size 2.49936 2.49936) (drill 1.19888) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(Q6-Pad2)"))
    (pad 3 thru_hole circle (at 4.99872 0) (size 2.49936 2.49936) (drill 1.19888) (layers *.Cu *.Mask F.SilkS)
      (net 36 "Net-(R8-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 2.49936 2.49936) (drill 1.19888) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(Q6-Pad2)"))
  )
  (module Housings_SSOP:TSSOP-10_3x3mm_Pitch0.5mm (layer F.Cu) (tedit 54130A77)
    (at 61.722 62.484)
    (descr "TSSOP10: plastic thin shrink small outline package; 10 leads; body width 3 mm; (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot552-1_po.pdf)")
    (tags "SSOP 0.5")
    (attr smd)
    (fp_text reference U1 (at 0 -2.55) (layer F.SilkS))
    (fp_text value PCA9633 (at 0 2.55) (layer F.Fab))
    (pad 1 smd rect (at -2.15 -1) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 21 LED0_IND))
    (pad 2 smd rect (at -2.15 -0.5) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 24 LED1_IND))
    (pad 3 smd rect (at -2.15 0) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 27 LED2_IND))
    (pad 4 smd rect (at -2.15 0.5) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(P4-Pad3)"))
    (pad 5 smd rect (at -2.15 1) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(JP2-Pad1)"))
    (pad 6 smd rect (at 2.15 1) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 12 GND))
    (pad 7 smd rect (at 2.15 0.5) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(JP1-Pad1)"))
    (pad 8 smd rect (at 2.15 0) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(P1-Pad2)"))
    (pad 9 smd rect (at 2.15 -0.5) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(P1-Pad1)"))
    (pad 10 smd rect (at 2.15 -1) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 8 +5V))
    (model Housings_SSOP.3dshapes/TSSOP-10_3x3mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-14_W7.62mm (layer F.Cu) (tedit 54130A77)
    (at 76.708 39.37)
    (descr "14-lead dip package, row spacing 7.62 mm (300 mils)")
    (tags "dil dip 2.54 300")
    (fp_text reference U2 (at 0 -5.22) (layer F.SilkS))
    (fp_text value LM324AN (at 0 -3.72) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(Q2-Pad2)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 34 "Net-(R2-Pad1)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(Q1-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 8 +5V))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(Q3-Pad3)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 35 "Net-(R5-Pad1)"))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(Q4-Pad2)"))
    (pad 8 thru_hole oval (at 7.62 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(Q6-Pad2)"))
    (pad 9 thru_hole oval (at 7.62 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 36 "Net-(R8-Pad1)"))
    (pad 10 thru_hole oval (at 7.62 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(Q5-Pad3)"))
    (pad 11 thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 12 GND))
    (pad 12 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS))
    (pad 13 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS))
    (pad 14 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS))
    (model Housings_DIP.3dshapes/DIP-14_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Power_Integrations:TO-220 (layer F.Cu) (tedit 0)
    (at 44.704 23.114)
    (descr "Non Isolated JEDEC TO-220 Package")
    (tags "Power Integration YN Package")
    (fp_text reference Q1 (at 0 -4.318) (layer F.SilkS))
    (fp_text value BUT11A (at 0 -4.318) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 0) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(P3-Pad1)"))
    (pad 3 thru_hole oval (at 2.54 0) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(Q1-Pad3)"))
    (pad 1 thru_hole oval (at -2.54 0) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask F.SilkS)
      (net 31 "Net-(Q1-Pad1)"))
  )
  (module Power_Integrations:TO-220 (layer F.Cu) (tedit 0)
    (at 44.704 38.354)
    (descr "Non Isolated JEDEC TO-220 Package")
    (tags "Power Integration YN Package")
    (fp_text reference Q3 (at 0 -4.318) (layer F.SilkS))
    (fp_text value BUT11A (at 0 -4.318) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 0) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(P3-Pad2)"))
    (pad 3 thru_hole oval (at 2.54 0) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(Q3-Pad3)"))
    (pad 1 thru_hole oval (at -2.54 0) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask F.SilkS)
      (net 32 "Net-(Q3-Pad1)"))
  )
  (module Power_Integrations:TO-220 (layer F.Cu) (tedit 0)
    (at 44.704 53.594)
    (descr "Non Isolated JEDEC TO-220 Package")
    (tags "Power Integration YN Package")
    (fp_text reference Q5 (at 0 -4.318) (layer F.SilkS))
    (fp_text value BUT11A (at 0 -4.318) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 0) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(P3-Pad3)"))
    (pad 3 thru_hole oval (at 2.54 0) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(Q5-Pad3)"))
    (pad 1 thru_hole oval (at -2.54 0) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask F.SilkS)
      (net 33 "Net-(Q5-Pad1)"))
  )
  (gr_text 12V (at 23.368 24.892 90) (layer F.SilkS))
  (gr_text SCL (at 59.182 82.169) (layer F.SilkS))
  (gr_text SDA (at 64.77 82.169) (layer F.SilkS))
  (gr_text GND (at 90.043 25.273) (layer F.SilkS))
  (gr_text 3V3 (at 90.678 22.733) (layer F.SilkS))
  (gr_text 5V (at 91.059 20.193) (layer F.SilkS))
  (gr_text LED2 (at 25.908 25.273 90) (layer F.SilkS))
  (gr_text LED1 (at 28.321 25.273 90) (layer F.SilkS))
  (gr_text LED0 (at 30.861 25.146 90) (layer F.SilkS))
  (gr_text GND (at 26.67 72.39) (layer F.SilkS))
  (gr_text 12V (at 26.67 70.104) (layer F.SilkS))
  (gr_text OUT3 (at 27.432 67.31) (layer F.SilkS))
  (gr_text GND (at 26.797 61.722) (layer F.SilkS))
  (gr_text 12V (at 26.67 58.674) (layer F.SilkS))
  (gr_text "Rev C" (at 28.702 80.264) (layer F.SilkS))
  (gr_text "David Lenfesty" (at 88.9 43.307 90) (layer F.SilkS))
  (gr_text "3 Channel RGB PWM LED Driver" (at 94.361 46.355 90) (layer F.SilkS))
  (gr_line (start 20.32 83.312) (end 20.32 68.58) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 96.52 83.312) (end 20.32 83.312) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 96.52 68.58) (end 96.52 83.312) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 20.32 68.58) (end 20.32 17.78) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 96.52 17.78) (end 96.52 68.58) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 71.12 17.78) (end 96.52 17.78) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 20.32 17.78) (end 71.12 17.78) (angle 90) (layer Edge.Cuts) (width 0.1))
  (zone (net 17) (net_name +12V) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 24.511 20.32) (xy 24.511 27.432) (xy 24.638 27.94) (xy 24.638 58.42) (xy 23.876 59.69)
        (xy 21.844 59.69) (xy 21.082 58.42) (xy 21.082 20.193) (xy 21.463 19.558) (xy 21.717 19.177)
        (xy 24.384 19.177) (xy 24.511 20.32)
      )
    )
  )
  (zone (net 12) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 66.675 24.13) (xy 66.04 24.765) (xy 66.04 25.527) (xy 66.675 25.527) (xy 66.675 25.4)
        (xy 67.945 23.495) (xy 67.945 18.415) (xy 95.885 18.415) (xy 95.885 82.55) (xy 20.955 82.55)
        (xy 20.955 64.77) (xy 21.336 64.741425) (xy 21.336 63.5) (xy 20.955 63.5) (xy 20.955 18.415)
        (xy 66.675 18.415) (xy 66.675 24.13)
      )
    )
    (polygon
      (pts        (xy 46.355 62.23) (xy 26.67 63.5) (xy 24.384 63.5) (xy 24.384 64.512825) (xy 46.355 62.865)
        (xy 58.136277 58.447021) (xy 57.828953 57.78847) (xy 46.355 62.23)
      )
    )
    (polygon
      (pts        (xy 66.04 42.037) (xy 66.04 54.61) (xy 58.96989 57.346817) (xy 59.355653 57.989755) (xy 66.675 55.245)
        (xy 66.675 42.037) (xy 66.04 42.037)
      )
    )
    (polygon
      (pts        (xy 66.04 26.162) (xy 66.04 41.275) (xy 66.675 41.275) (xy 66.675 26.162) (xy 66.04 26.162)
      )
    )
  )
)
