(kicad_pcb (version 4) (host pcbnew "(2015-01-16 BZR 5376)-product")
  (general
    (links 36)
    (no_connects 0)
    (area 27.118619 37.721 107.881381 92.129)
    (thickness 1.6)
    (drawings 9)
    (tracks 131)
    (zones 0)
    (modules 20)
    (nets 35)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.254)
    (trace_clearance 0.254)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.254)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.889)
    (via_drill 0.635)
    (via_min_size 0.889)
    (via_min_drill 0.508)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /SwitchGrounds)
  (net 2 /YLimit)
  (net 3 /Z0Stepper0)
  (net 4 /Z0Stepper1)
  (net 5 /Z0Stepper2)
  (net 6 /Z0Stepper3)
  (net 7 /LManipGrounds)
  (net 8 /LManipVac)
  (net 9 /Z0Limit)
  (net 10 /Z1Limit)
  (net 11 /Z2Limit)
  (net 12 /CollisionLimit)
  (net 13 /Z1Stepper0)
  (net 14 /Z1Stepper1)
  (net 15 /Z1Stepper2)
  (net 16 /Z1Stepper3)
  (net 17 /LManipAir)
  (net 18 /SManipGrounds)
  (net 19 /SManipVac)
  (net 20 /SManipAir)
  (net 21 /Z2Stepper0)
  (net 22 /Z2Stepper1)
  (net 23 /Z2Stepper2)
  (net 24 /Z2Stepper3)
  (net 25 /LEDGND)
  (net 26 /LEDVCC)
  (net 27 /PressureGND)
  (net 28 /PressureVCC)
  (net 29 /PressureSignal)
  (net 30 "Net-(P14-Pad1)")
  (net 31 "Net-(P17-Pad1)")
  (net 32 "Net-(P18-Pad1)")
  (net 33 "Net-(P19-Pad1)")
  (net 34 "Net-(P20-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.889)
    (via_drill 0.635)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net /CollisionLimit)
    (add_net /LEDGND)
    (add_net /LEDVCC)
    (add_net /LManipAir)
    (add_net /LManipGrounds)
    (add_net /LManipVac)
    (add_net /PressureGND)
    (add_net /PressureSignal)
    (add_net /PressureVCC)
    (add_net /SManipAir)
    (add_net /SManipGrounds)
    (add_net /SManipVac)
    (add_net /SwitchGrounds)
    (add_net /YLimit)
    (add_net /Z0Limit)
    (add_net /Z0Stepper0)
    (add_net /Z0Stepper1)
    (add_net /Z0Stepper2)
    (add_net /Z0Stepper3)
    (add_net /Z1Limit)
    (add_net /Z1Stepper0)
    (add_net /Z1Stepper1)
    (add_net /Z1Stepper2)
    (add_net /Z1Stepper3)
    (add_net /Z2Limit)
    (add_net /Z2Stepper0)
    (add_net /Z2Stepper1)
    (add_net /Z2Stepper2)
    (add_net /Z2Stepper3)
    (add_net "Net-(P14-Pad1)")
    (add_net "Net-(P17-Pad1)")
    (add_net "Net-(P18-Pad1)")
    (add_net "Net-(P19-Pad1)")
    (add_net "Net-(P20-Pad1)")
  )
  (module Socket_Strips:Socket_Strip_Straight_1x02 (layer F.Cu) (tedit 588BD847)
    (at 34 55 90)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P1 (at 0 -5.1 90) (layer F.SilkS) hide)
    (fp_text value YLIMIT (at 1 3 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 /SwitchGrounds))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 /YLimit))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x02.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x04 (layer F.Cu) (tedit 588BD80B)
    (at 47 44)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P2 (at 0 -5.1) (layer F.SilkS) hide)
    (fp_text value Z0STEPPER (at 4 3) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 /Z0Stepper0))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 /Z0Stepper1))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 /Z0Stepper2))
    (pad 4 thru_hole oval (at 7.62 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 6 /Z0Stepper3))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x04.wrl
      (at (xyz 0.15 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x02 (layer F.Cu) (tedit 588BD833)
    (at 55 86 180)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P3 (at 0 -5.1 180) (layer F.SilkS) hide)
    (fp_text value LMANIPVAC (at 1 3 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 7 /LManipGrounds))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 8 /LManipVac))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x02.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x02 (layer F.Cu) (tedit 588BD84A)
    (at 34 63 90)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P4 (at 0 -5.1 90) (layer F.SilkS) hide)
    (fp_text value Z0LIMIT (at 1 3 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 /SwitchGrounds))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 /Z0Limit))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x02.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_2x15 (layer F.Cu) (tedit 588BD844)
    (at 51 63)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P5 (at 0 -5.1) (layer F.SilkS) hide)
    (fp_text value RIBBON (at -3.5 1.25 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 /Z0Stepper0))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 /Z0Stepper1))
    (pad 3 thru_hole oval (at 2.54 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 /Z0Stepper2))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 6 /Z0Stepper3))
    (pad 5 thru_hole oval (at 5.08 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 /SwitchGrounds))
    (pad 6 thru_hole oval (at 5.08 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 /YLimit))
    (pad 7 thru_hole oval (at 7.62 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 /Z0Limit))
    (pad 8 thru_hole oval (at 7.62 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 10 /Z1Limit))
    (pad 9 thru_hole oval (at 10.16 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 11 /Z2Limit))
    (pad 10 thru_hole oval (at 10.16 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 12 /CollisionLimit))
    (pad 11 thru_hole oval (at 12.7 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 13 /Z1Stepper0))
    (pad 12 thru_hole oval (at 12.7 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 14 /Z1Stepper1))
    (pad 13 thru_hole oval (at 15.24 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 15 /Z1Stepper2))
    (pad 14 thru_hole oval (at 15.24 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 16 /Z1Stepper3))
    (pad 15 thru_hole oval (at 17.78 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 7 /LManipGrounds))
    (pad 16 thru_hole oval (at 17.78 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 8 /LManipVac))
    (pad 17 thru_hole oval (at 20.32 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 17 /LManipAir))
    (pad 18 thru_hole oval (at 20.32 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 18 /SManipGrounds))
    (pad 19 thru_hole oval (at 22.86 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 19 /SManipVac))
    (pad 20 thru_hole oval (at 22.86 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 20 /SManipAir))
    (pad 21 thru_hole oval (at 25.4 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 21 /Z2Stepper0))
    (pad 22 thru_hole oval (at 25.4 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 22 /Z2Stepper1))
    (pad 23 thru_hole oval (at 27.94 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 /Z2Stepper2))
    (pad 24 thru_hole oval (at 27.94 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 24 /Z2Stepper3))
    (pad 25 thru_hole oval (at 30.48 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 25 /LEDGND))
    (pad 26 thru_hole oval (at 30.48 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 26 /LEDVCC))
    (pad 27 thru_hole oval (at 33.02 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 27 /PressureGND))
    (pad 28 thru_hole oval (at 33.02 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 28 /PressureVCC))
    (pad 29 thru_hole oval (at 35.56 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 29 /PressureSignal))
    (pad 30 thru_hole oval (at 35.56 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 30 "Net-(P14-Pad1)"))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_2x15.wrl
      (at (xyz 0.7 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x04 (layer F.Cu) (tedit 588BD80E)
    (at 65 44)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P6 (at 0 -5.1) (layer F.SilkS) hide)
    (fp_text value Z1STEPPER (at 4 3) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 13 /Z1Stepper0))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 14 /Z1Stepper1))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 15 /Z1Stepper2))
    (pad 4 thru_hole oval (at 7.62 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 16 /Z1Stepper3))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x04.wrl
      (at (xyz 0.15 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x02 (layer F.Cu) (tedit 588BD827)
    (at 91 86 180)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P7 (at 0 -5.1 180) (layer F.SilkS) hide)
    (fp_text value LED (at 1 3 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 25 /LEDGND))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 26 /LEDVCC))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x02.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x02 (layer F.Cu) (tedit 588BD831)
    (at 64 86 180)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P8 (at 0 -5.1 180) (layer F.SilkS) hide)
    (fp_text value LMANIPAIR (at 1 3 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 7 /LManipGrounds))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 17 /LManipAir))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x02.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x02 (layer F.Cu) (tedit 588BD84E)
    (at 34 71 90)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P9 (at 0 -5.1 90) (layer F.SilkS) hide)
    (fp_text value Z1LIMIT (at 1 3 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 /SwitchGrounds))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 10 /Z1Limit))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x02.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x02 (layer F.Cu) (tedit 588BD82E)
    (at 73 86 180)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P10 (at 0 -5.1 180) (layer F.SilkS) hide)
    (fp_text value SMANIPVAC (at 1 3 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 18 /SManipGrounds))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 19 /SManipVac))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x02.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x03 (layer F.Cu) (tedit 588BD820)
    (at 101 60 270)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P11 (at 0 -5.1 270) (layer F.SilkS) hide)
    (fp_text value PRESSURE (at 3 3 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 27 /PressureGND))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 28 /PressureVCC))
    (pad 3 thru_hole oval (at 5.08 0 270) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 29 /PressureSignal))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x03.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x04 (layer F.Cu) (tedit 588BD812)
    (at 83 44)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P12 (at 0 -5.1) (layer F.SilkS) hide)
    (fp_text value Z2STEPPER (at 4 3) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 21 /Z2Stepper0))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 22 /Z2Stepper1))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 /Z2Stepper2))
    (pad 4 thru_hole oval (at 7.62 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 24 /Z2Stepper3))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x04.wrl
      (at (xyz 0.15 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x02 (layer F.Cu) (tedit 588BD852)
    (at 34 79 90)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P13 (at 0 -5.1 90) (layer F.SilkS) hide)
    (fp_text value Z2LIMIT (at 1 3 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 /SwitchGrounds))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 11 /Z2Limit))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x02.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x01 (layer F.Cu) (tedit 588BD823)
    (at 101 74)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P14 (at 0 -5.1) (layer F.SilkS) hide)
    (fp_text value SPARE (at -3 0 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask)
      (net 30 "Net-(P14-Pad1)"))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x02 (layer F.Cu) (tedit 588BD82A)
    (at 82 86 180)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P15 (at 0 -5.1 180) (layer F.SilkS) hide)
    (fp_text value SMANIPAIR (at 1 3 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 18 /SManipGrounds))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 20 /SManipAir))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x02.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x02 (layer F.Cu) (tedit 588BD837)
    (at 46 86 180)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P16 (at 0 -5.1 180) (layer F.SilkS) hide)
    (fp_text value COLLIMIT (at 1 3 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 /SwitchGrounds))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 12 /CollisionLimit))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x02.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_Pad (layer F.Cu) (tedit 588BCFC7)
    (at 34 44)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (fp_text reference P17 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MOUNT (at 0 4.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask)
      (net 31 "Net-(P17-Pad1)"))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_Pad (layer F.Cu) (tedit 588BCFA6)
    (at 101 44)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (fp_text reference P18 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MOUNT (at 0 4.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask)
      (net 32 "Net-(P18-Pad1)"))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_Pad (layer F.Cu) (tedit 588BCFA0)
    (at 34 86)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (fp_text reference P19 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MOUNT (at 0 4.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask)
      (net 33 "Net-(P19-Pad1)"))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_Pad (layer F.Cu) (tedit 588BCF9A)
    (at 101 86)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (fp_text reference P20 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MOUNT (at 0 4.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask)
      (net 34 "Net-(P20-Pad1)"))
  )
  (gr_text 20170127 (at 95.4024 82.423 90) (layer F.SilkS))
  (gr_text 30 (at 86.487 68.5292) (layer F.SilkS))
  (gr_text 29 (at 86.5124 59.9186) (layer F.SilkS))
  (gr_text 2 (at 49.8348 68.4022) (layer F.SilkS))
  (gr_text 1 (at 49.8094 59.2836) (layer F.SilkS))
  (gr_line (start 30 90) (end 30 40) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 105 90) (end 30 90) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 105 40) (end 105 90) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 30 40) (end 105 40) (angle 90) (layer Edge.Cuts) (width 0.1))
)
