(kicad_pcb (version 20171130) (host pcbnew "(5.1.10)-1")
  (general
    (thickness 1.6)
    (drawings 538)
    (tracks 1629)
    (zones 0)
    (modules 63)
    (nets 132)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (1 In1.Cu signal)
    (2 In2.Cu signal hide)
    (31 B.Cu signal hide)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user hide)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.2032)
    (trace_clearance 0.1524)
    (zone_clearance 0.254)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFEFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(D1-Pad2)")
  (net 3 /SERVIDEO)
  (net 4 /MSW)
  (net 5 /Y1)
  (net 6 /Y0)
  (net 7 /X1)
  (net 8 /X0)
  (net 9 /IRQ)
  (net 10 /KSEL2)
  (net 11 /KSEL1)
  (net 12 /SPKR)
  (net 13 /RGB2)
  (net 14 /RGB4)
  (net 15 /RGB8)
  (net 16 /AD7)
  (net 17 /AD6)
  (net 18 /AD5)
  (net 19 /AD4)
  (net 20 /AD3)
  (net 21 /AD2)
  (net 22 /AD1)
  (net 23 /AD0)
  (net 24 /S0)
  (net 25 /R-W)
  (net 26 /INH)
  (net 27 /M2SEL)
  (net 28 /DMA)
  (net 29 /MDI-MDO)
  (net 30 /RESET)
  (net 31 /RGB1)
  (net 32 /C060-67)
  (net 33 /PDLTRIG)
  (net 34 /MD0)
  (net 35 /MD1)
  (net 36 /MD2)
  (net 37 /MD3)
  (net 38 /MD4)
  (net 39 /MD5)
  (net 40 /MD6)
  (net 41 /MD7)
  (net 42 /RAMWE)
  (net 43 /A13)
  (net 44 /A14)
  (net 45 /A15)
  (net 46 /SYNC)
  (net 47 /WINDOW)
  (net 48 /RMBK)
  (net 49 /S5)
  (net 50 /S4)
  (net 51 /S3)
  (net 52 /S2)
  (net 53 /S1)
  (net 54 /RAS)
  (net 55 /CASM)
  (net 56 /CASA)
  (net 57 /PH#)
  (net 58 /Q3)
  (net 59 /CREF)
  (net 60 /7M)
  (net 61 /14M)
  (net 62 /RA0)
  (net 63 /RA1)
  (net 64 /RA2)
  (net 65 /RA3)
  (net 66 /RA4)
  (net 67 /RA5)
  (net 68 /RA6)
  (net 69 /RA7)
  (net 70 /A0)
  (net 71 /A1)
  (net 72 /A2)
  (net 73 /A3)
  (net 74 /A4)
  (net 75 /A5)
  (net 76 /A6)
  (net 77 /A7)
  (net 78 /A8)
  (net 79 /A9)
  (net 80 /A10)
  (net 81 /A11)
  (net 82 /A12)
  (net 83 /RAF0)
  (net 84 /RAF1)
  (net 85 /RAF2)
  (net 86 /RAF3)
  (net 87 /RAF4)
  (net 88 /RAF5)
  (net 89 /RAF6)
  (net 90 /RAF7)
  (net 91 /CASA.B)
  (net 92 /CASM.B)
  (net 93 /RAS.B)
  (net 94 /RWE.B)
  (net 95 "Net-(R14-Pad2)")
  (net 96 /UM4-14)
  (net 97 "Net-(R15-Pad2)")
  (net 98 /UM4-10)
  (net 99 /BA0)
  (net 100 /BA1)
  (net 101 /BA2)
  (net 102 /BA3)
  (net 103 /BA4)
  (net 104 /BA5)
  (net 105 /BA6)
  (net 106 /BA7)
  (net 107 /BA8)
  (net 108 /BA9)
  (net 109 /BA10)
  (net 110 /BA11)
  (net 111 /BA12)
  (net 112 /BA13)
  (net 113 /BA14)
  (net 114 /BA15)
  (net 115 /D0)
  (net 116 /D1)
  (net 117 /D2)
  (net 118 /D3)
  (net 119 /D4)
  (net 120 /D5)
  (net 121 /D6)
  (net 122 /D7)
  (net 123 /ROMEN)
  (net 124 /ABEN)
  (net 125 /ABDIR)
  (net 126 /FLIP7)
  (net 127 /FLIP6)
  (net 128 /DBEN)
  (net 129 /DBDIR)
  (net 130 "Net-(J7-Pad20)")
  (net 131 +5V)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.2032)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /14M)
    (add_net /7M)
    (add_net /A0)
    (add_net /A1)
    (add_net /A10)
    (add_net /A11)
    (add_net /A12)
    (add_net /A13)
    (add_net /A14)
    (add_net /A15)
    (add_net /A2)
    (add_net /A3)
    (add_net /A4)
    (add_net /A5)
    (add_net /A6)
    (add_net /A7)
    (add_net /A8)
    (add_net /A9)
    (add_net /ABDIR)
    (add_net /ABEN)
    (add_net /AD0)
    (add_net /AD1)
    (add_net /AD2)
    (add_net /AD3)
    (add_net /AD4)
    (add_net /AD5)
    (add_net /AD6)
    (add_net /AD7)
    (add_net /BA0)
    (add_net /BA1)
    (add_net /BA10)
    (add_net /BA11)
    (add_net /BA12)
    (add_net /BA13)
    (add_net /BA14)
    (add_net /BA15)
    (add_net /BA2)
    (add_net /BA3)
    (add_net /BA4)
    (add_net /BA5)
    (add_net /BA6)
    (add_net /BA7)
    (add_net /BA8)
    (add_net /BA9)
    (add_net /C060-67)
    (add_net /CASA)
    (add_net /CASA.B)
    (add_net /CASM)
    (add_net /CASM.B)
    (add_net /CREF)
    (add_net /D0)
    (add_net /D1)
    (add_net /D2)
    (add_net /D3)
    (add_net /D4)
    (add_net /D5)
    (add_net /D6)
    (add_net /D7)
    (add_net /DBDIR)
    (add_net /DBEN)
    (add_net /DMA)
    (add_net /FLIP6)
    (add_net /FLIP7)
    (add_net /INH)
    (add_net /IRQ)
    (add_net /KSEL1)
    (add_net /KSEL2)
    (add_net /M2SEL)
    (add_net /MD0)
    (add_net /MD1)
    (add_net /MD2)
    (add_net /MD3)
    (add_net /MD4)
    (add_net /MD5)
    (add_net /MD6)
    (add_net /MD7)
    (add_net /MDI-MDO)
    (add_net /MSW)
    (add_net /PDLTRIG)
    (add_net /PH#)
    (add_net /Q3)
    (add_net /R-W)
    (add_net /RA0)
    (add_net /RA1)
    (add_net /RA2)
    (add_net /RA3)
    (add_net /RA4)
    (add_net /RA5)
    (add_net /RA6)
    (add_net /RA7)
    (add_net /RAF0)
    (add_net /RAF1)
    (add_net /RAF2)
    (add_net /RAF3)
    (add_net /RAF4)
    (add_net /RAF5)
    (add_net /RAF6)
    (add_net /RAF7)
    (add_net /RAMWE)
    (add_net /RAS)
    (add_net /RAS.B)
    (add_net /RESET)
    (add_net /RGB1)
    (add_net /RGB2)
    (add_net /RGB4)
    (add_net /RGB8)
    (add_net /RMBK)
    (add_net /ROMEN)
    (add_net /RWE.B)
    (add_net /S0)
    (add_net /S1)
    (add_net /S2)
    (add_net /S3)
    (add_net /S4)
    (add_net /S5)
    (add_net /SERVIDEO)
    (add_net /SPKR)
    (add_net /SYNC)
    (add_net /UM4-10)
    (add_net /UM4-14)
    (add_net /WINDOW)
    (add_net /X0)
    (add_net /X1)
    (add_net /Y0)
    (add_net /Y1)
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(J7-Pad20)")
    (add_net "Net-(R14-Pad2)")
    (add_net "Net-(R15-Pad2)")
  )
  (net_class Power ""
    (clearance 0.3048)
    (trace_width 0.3048)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net GND)
  )
  (module "My Libraries:BE10v2" (layer F.Cu) (tedit 5FBC8857)
    (at 90.424 38.608)
    (descr "Imported from BE5.svg")
    (tags svg2mod)
    (attr virtual)
    (fp_text reference svg2mod (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value G*** (at 0 13.047999) (layer F.SilkS) hide)
  )
  (module Symbol:OSHW-Symbol_6.7x6mm_SilkScreen (layer F.Cu) (tedit 0)
    (at 97.79 61.976)
    (descr "Open Source Hardware Symbol")
    (tags "Logo Symbol OSHW")
    (attr virtual)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value OSHW-Symbol_6.7x6mm_SilkScreen (at 0.75 0) (layer F.Fab) hide)
  )
  (module Symbol:KiCad-Logo_8mm_SilkScreen (layer B.Cu) (tedit 0)
    (at 129.794 107.442)
    (descr "KiCad Logo")
    (tags "Logo KiCad")
    (attr virtual)
    (fp_text reference REF** (at 0 6.35) (layer B.SilkS) hide)
    (fp_text value KiCad-Logo_8mm_SilkScreen (at 0 -6.35) (layer B.Fab) hide)
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 153.416 139.7 270)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J8 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value "VGC Extra 2" (at 0 7.41 90) (layer F.Fab))
    (fp_text user %R (at 0 2.54) (layer F.Fab))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 /M2SEL))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 111 /BA12))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 152.654 73.914)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C11 (at 2.667 0 90) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.68) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.95 0) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.95 0) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 131 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 100.33 139.7 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J6 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value "VGC Extra 1" (at 0 7.41 90) (layer F.Fab))
    (fp_text user %R (at 0 2.54) (layer F.Fab))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 /R-W))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 /RESET))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /IRQ))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x20_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 107.95 40.767 90)
    (descr "Through hole straight pin header, 2x20, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x20 2.54mm double row")
    (fp_text reference J7 (at 1.27 -2.33 90) (layer F.SilkS) hide)
    (fp_text value Bald-Ext-1 (at 1.27 50.59 90) (layer F.Fab))
    (fp_text user %R (at 1.27 24.13) (layer F.Fab))
    (pad 40 thru_hole oval (at 2.54 48.26 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 39 thru_hole oval (at 0 48.26 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 57 /PH#))
    (pad 38 thru_hole oval (at 2.54 45.72 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 37 thru_hole oval (at 0 45.72 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 36 thru_hole oval (at 2.54 43.18 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 /MD7))
    (pad 35 thru_hole oval (at 0 43.18 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 69 /RA7))
    (pad 34 thru_hole oval (at 2.54 40.64 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 /MD6))
    (pad 33 thru_hole oval (at 0 40.64 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 68 /RA6))
    (pad 32 thru_hole oval (at 2.54 38.1 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 /MD5))
    (pad 31 thru_hole oval (at 0 38.1 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 67 /RA5))
    (pad 30 thru_hole oval (at 2.54 35.56 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 29 thru_hole oval (at 0 35.56 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 66 /RA4))
    (pad 28 thru_hole oval (at 2.54 33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 /MD4))
    (pad 27 thru_hole oval (at 0 33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 26 thru_hole oval (at 2.54 30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 /MD3))
    (pad 25 thru_hole oval (at 0 30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 65 /RA3))
    (pad 24 thru_hole oval (at 2.54 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 /MD2))
    (pad 23 thru_hole oval (at 0 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 64 /RA2))
    (pad 22 thru_hole oval (at 2.54 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 21 thru_hole oval (at 0 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 63 /RA1))
    (pad 20 thru_hole oval (at 2.54 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 130 "Net-(J7-Pad20)"))
    (pad 19 thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 18 thru_hole oval (at 2.54 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 /MD1))
    (pad 17 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 62 /RA0))
    (pad 16 thru_hole oval (at 2.54 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 /MD0))
    (pad 15 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 /AD0))
    (pad 14 thru_hole oval (at 2.54 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 13 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 /AD1))
    (pad 12 thru_hole oval (at 2.54 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /AD2))
    (pad 11 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 10 thru_hole oval (at 2.54 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /AD4))
    (pad 9 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 /AD3))
    (pad 8 thru_hole oval (at 2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /AD6))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /AD5))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /AD7))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 61 /14M))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x20_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DIP:DIP-18_W7.62mm_Socket_LongPads (layer F.Cu) (tedit 5A02E8C5)
    (at 135.001 48.006)
    (descr "18-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket, LongPads")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket LongPads")
    (fp_text reference U7 (at -2.413 -1.27) (layer F.SilkS))
    (fp_text value DRAM64KX4 (at 3.81 22.65) (layer F.Fab))
    (fp_text user %R (at 3.81 10.16) (layer F.Fab))
    (pad 18 thru_hole oval (at 7.62 0) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 9 thru_hole oval (at 0 20.32) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 131 +5V))
    (pad 17 thru_hole oval (at 7.62 2.54) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 /MD3))
    (pad 8 thru_hole oval (at 0 17.78) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 84 /RAF1))
    (pad 16 thru_hole oval (at 7.62 5.08) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 92 /CASM.B))
    (pad 7 thru_hole oval (at 0 15.24) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 85 /RAF2))
    (pad 15 thru_hole oval (at 7.62 7.62) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 /MD2))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 83 /RAF0))
    (pad 14 thru_hole oval (at 7.62 10.16) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 96 /UM4-14))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 93 /RAS.B))
    (pad 13 thru_hole oval (at 7.62 12.7) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 86 /RAF3))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 94 /RWE.B))
    (pad 12 thru_hole oval (at 7.62 15.24) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 87 /RAF4))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 /MD1))
    (pad 11 thru_hole oval (at 7.62 17.78) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 88 /RAF5))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 /MD0))
    (pad 10 thru_hole oval (at 7.62 20.32) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 98 /UM4-10))
    (pad 1 thru_hole rect (at 0 0) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-18_W7.62mm_Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x11_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 129.54 77.216 270)
    (descr "Through hole straight pin header, 1x11, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x11 2.54mm single row")
    (fp_text reference JP8 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value P64-74 (at 0 27.73 90) (layer F.Fab))
    (fp_text user %R (at 0 12.7) (layer F.Fab))
    (pad 11 thru_hole oval (at 0 25.4 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 /C060-67))
    (pad 10 thru_hole oval (at 0 22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 /PDLTRIG))
    (pad 9 thru_hole oval (at 0 20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 /MD0))
    (pad 8 thru_hole oval (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 /MD1))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 /MD2))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 /MD3))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 /MD4))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 /MD5))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 /MD6))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 /MD7))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 /RAMWE))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x11_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 139.7 73.533 90)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference J12 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value CLKS (at 0 9.95 90) (layer F.Fab))
    (fp_text user %R (at 0 3.81) (layer F.Fab))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 60 /7M))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 59 /CREF))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 58 /Q3))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 57 /PH#))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 96.52 127)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference JP1 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value "RGB Binary" (at 0 9.95) (layer F.Fab))
    (fp_text user %R (at 0 3.81 90) (layer F.Fab))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /RGB2))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 /RGB1))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /RGB8))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /RGB4))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x11_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 158.75 106.68 180)
    (descr "Through hole straight pin header, 1x11, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x11 2.54mm single row")
    (fp_text reference JP15 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value P64-74 (at 0 27.73) (layer F.Fab))
    (fp_text user %R (at 0 12.7 90) (layer F.Fab))
    (pad 11 thru_hole oval (at 0 25.4 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 62 /RA0))
    (pad 10 thru_hole oval (at 0 22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 63 /RA1))
    (pad 9 thru_hole oval (at 0 20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 64 /RA2))
    (pad 8 thru_hole oval (at 0 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 65 /RA3))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 66 /RA4))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 67 /RA5))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 68 /RA6))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 69 /RA7))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 99 /BA0))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 100 /BA1))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 101 /BA2))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x11_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 172.72 36.83)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference J11 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value PWR (at 0 9.95) (layer F.Fab))
    (fp_text user %R (at 0 3.81 90) (layer F.Fab))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 131 +5V))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 131 +5V))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 142.748 86.868)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C10 (at 0 1.68) (layer B.SilkS))
    (fp_text value 10uF (at 0 -1.68) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.95 0) (size 1 1.45) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.95 0) (size 1 1.45) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 131 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D8.0mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0)
    (at 166.37 39.751 180)
    (descr "CP, Radial series, Radial, pin pitch=5.00mm, , diameter=8mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 5.00mm  diameter 8mm Electrolytic Capacitor")
    (fp_text reference C2 (at -2.159 2.667) (layer F.SilkS))
    (fp_text value 100uF (at 2.5 5.25) (layer F.Fab))
    (fp_text user %R (at 2.5 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 131 +5V))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D8.0mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_Array_Convex_4x0612 (layer B.Cu) (tedit 5B82E1AD)
    (at 132.08 73.152 90)
    (descr "Precision Thin Film Chip Resistor Array, VISHAY (see http://www.vishay.com/docs/28770/acasat.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference RN9 (at 0 2.8 270) (layer B.SilkS))
    (fp_text value 100 (at 0 -2.8 270) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 5 smd rect (at 0.7 -1.27 90) (size 0.7 0.64) (layers B.Cu B.Paste B.Mask)
      (net 94 /RWE.B))
    (pad 6 smd rect (at 0.7 -0.4 90) (size 0.7 0.5) (layers B.Cu B.Paste B.Mask)
      (net 93 /RAS.B))
    (pad 8 smd rect (at 0.7 1.27 90) (size 0.7 0.64) (layers B.Cu B.Paste B.Mask)
      (net 92 /CASM.B))
    (pad 7 smd rect (at 0.7 0.4 90) (size 0.7 0.5) (layers B.Cu B.Paste B.Mask)
      (net 91 /CASA.B))
    (pad 4 smd rect (at -0.7 -1.27 90) (size 0.7 0.64) (layers B.Cu B.Paste B.Mask)
      (net 42 /RAMWE))
    (pad 2 smd rect (at -0.7 0.4 90) (size 0.7 0.5) (layers B.Cu B.Paste B.Mask)
      (net 56 /CASA))
    (pad 3 smd rect (at -0.7 -0.4 90) (size 0.7 0.5) (layers B.Cu B.Paste B.Mask)
      (net 54 /RAS))
    (pad 1 smd rect (at -0.7 1.27 90) (size 0.7 0.64) (layers B.Cu B.Paste B.Mask)
      (net 55 /CASM))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_Array_Convex_4x0612.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_Array_Convex_4x0612 (layer F.Cu) (tedit 5B82E1AD)
    (at 162.052 64.389 180)
    (descr "Precision Thin Film Chip Resistor Array, VISHAY (see http://www.vishay.com/docs/28770/acasat.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference RN8 (at -2.286 -1.27 270) (layer F.SilkS))
    (fp_text value 100 (at 0 2.8 180) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.7 -1.27 180) (size 0.7 0.64) (layers F.Cu F.Paste F.Mask)
      (net 63 /RA1))
    (pad 3 smd rect (at -0.7 0.4 180) (size 0.7 0.5) (layers F.Cu F.Paste F.Mask)
      (net 64 /RA2))
    (pad 2 smd rect (at -0.7 -0.4 180) (size 0.7 0.5) (layers F.Cu F.Paste F.Mask)
      (net 67 /RA5))
    (pad 4 smd rect (at -0.7 1.27 180) (size 0.7 0.64) (layers F.Cu F.Paste F.Mask)
      (net 66 /RA4))
    (pad 7 smd rect (at 0.7 -0.4 180) (size 0.7 0.5) (layers F.Cu F.Paste F.Mask)
      (net 88 /RAF5))
    (pad 8 smd rect (at 0.7 -1.27 180) (size 0.7 0.64) (layers F.Cu F.Paste F.Mask)
      (net 84 /RAF1))
    (pad 6 smd rect (at 0.7 0.4 180) (size 0.7 0.5) (layers F.Cu F.Paste F.Mask)
      (net 85 /RAF2))
    (pad 5 smd rect (at 0.7 1.27 180) (size 0.7 0.64) (layers F.Cu F.Paste F.Mask)
      (net 87 /RAF4))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_Array_Convex_4x0612.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_Array_Convex_4x0612 (layer F.Cu) (tedit 5B82E1AD)
    (at 162.052 59.436 180)
    (descr "Precision Thin Film Chip Resistor Array, VISHAY (see http://www.vishay.com/docs/28770/acasat.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference RN7 (at -0.127 2.54) (layer F.SilkS))
    (fp_text value 100 (at 0 2.8) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.7 -1.27 180) (size 0.7 0.64) (layers F.Cu F.Paste F.Mask)
      (net 62 /RA0))
    (pad 3 smd rect (at -0.7 0.4 180) (size 0.7 0.5) (layers F.Cu F.Paste F.Mask)
      (net 68 /RA6))
    (pad 2 smd rect (at -0.7 -0.4 180) (size 0.7 0.5) (layers F.Cu F.Paste F.Mask)
      (net 65 /RA3))
    (pad 4 smd rect (at -0.7 1.27 180) (size 0.7 0.64) (layers F.Cu F.Paste F.Mask)
      (net 69 /RA7))
    (pad 7 smd rect (at 0.7 -0.4 180) (size 0.7 0.5) (layers F.Cu F.Paste F.Mask)
      (net 86 /RAF3))
    (pad 8 smd rect (at 0.7 -1.27 180) (size 0.7 0.64) (layers F.Cu F.Paste F.Mask)
      (net 83 /RAF0))
    (pad 6 smd rect (at 0.7 0.4 180) (size 0.7 0.5) (layers F.Cu F.Paste F.Mask)
      (net 89 /RAF6))
    (pad 5 smd rect (at 0.7 1.27 180) (size 0.7 0.64) (layers F.Cu F.Paste F.Mask)
      (net 90 /RAF7))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_Array_Convex_4x0612.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x10_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 158.75 132.08 180)
    (descr "Through hole straight pin header, 1x10, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x10 2.54mm single row")
    (fp_text reference JP16 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value P54-63 (at 0 25.19) (layer F.Fab))
    (fp_text user %R (at 0 11.43 90) (layer F.Fab))
    (pad 10 thru_hole oval (at 0 22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 102 /BA3))
    (pad 9 thru_hole oval (at 0 20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 103 /BA4))
    (pad 8 thru_hole oval (at 0 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 104 /BA5))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 105 /BA6))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 106 /BA7))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 107 /BA8))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 108 /BA9))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 109 /BA10))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 110 /BA11))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 111 /BA12))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x10_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x10_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 154.94 77.216 270)
    (descr "Through hole straight pin header, 1x10, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x10 2.54mm single row")
    (fp_text reference JP12 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value P54-63 (at 0 25.19 90) (layer F.Fab))
    (fp_text user %R (at 0 11.43) (layer F.Fab))
    (pad 10 thru_hole oval (at 0 22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 54 /RAS))
    (pad 9 thru_hole oval (at 0 20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 55 /CASM))
    (pad 8 thru_hole oval (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 56 /CASA))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 57 /PH#))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 58 /Q3))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 59 /CREF))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 60 /7M))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 131 +5V))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 61 /14M))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x10_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x11_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 129.54 135.89 90)
    (descr "Through hole straight pin header, 1x11, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x11 2.54mm single row")
    (fp_text reference JP11 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value P64-74 (at 0 27.73 90) (layer F.Fab))
    (fp_text user %R (at 0 12.7) (layer F.Fab))
    (pad 11 thru_hole oval (at 0 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 112 /BA13))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 113 /BA14))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 114 /BA15))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 /SYNC))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 /WINDOW))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 48 /RMBK))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 /S5))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 50 /S4))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 51 /S3))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 52 /S2))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 53 /S1))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x11_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x10_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 104.14 135.89 90)
    (descr "Through hole straight pin header, 1x10, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x10 2.54mm single row")
    (fp_text reference JP7 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value P54-63 (at 0 25.19 90) (layer F.Fab))
    (fp_text user %R (at 0 11.43) (layer F.Fab))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 /S0))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 /R-W))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 /INH))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 /M2SEL))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 /DMA))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 123 /ROMEN))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 /MDI-MDO))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 /RESET))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 /RGB1))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x10_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x11_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 100.33 106.68)
    (descr "Through hole straight pin header, 1x11, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x11 2.54mm single row")
    (fp_text reference JP4 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value P64-74 (at 0 27.73) (layer F.Fab))
    (fp_text user %R (at 0 12.7 90) (layer F.Fab))
    (pad 11 thru_hole oval (at 0 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /RGB2))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /RGB4))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /RGB8))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /AD7))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /AD6))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /AD5))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /AD4))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 /AD3))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /AD2))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 /AD1))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 /AD0))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x11_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x10_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 100.33 81.28)
    (descr "Through hole straight pin header, 1x10, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x10 2.54mm single row")
    (fp_text reference JP3 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value P54-63 (at 0 25.19) (layer F.Fab))
    (fp_text user %R (at 0 11.43 90) (layer F.Fab))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /SERVIDEO))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /MSW))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /Y1))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /Y0))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /X1))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /X0))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /IRQ))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /KSEL2))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /KSEL1))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /SPKR))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x10_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x05_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 179.197 82.55)
    (descr "Through hole straight pin header, 2x05, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x05 2.54mm double row")
    (fp_text reference J10 (at 1.27 -2.33) (layer F.SilkS) hide)
    (fp_text value Data (at 1.27 13.335) (layer F.SilkS) hide)
    (fp_text user %R (at 1.27 5.08 90) (layer F.Fab))
    (pad 10 thru_hole oval (at 2.54 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 122 /D7))
    (pad 9 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 121 /D6))
    (pad 8 thru_hole oval (at 2.54 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 7 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 119 /D4))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 120 /D5))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 118 /D3))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 117 /D2))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 116 /D1))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 115 /D0))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x05_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_Array_Convex_4x0612 (layer F.Cu) (tedit 5B82E1AD)
    (at 167.578 89.408 180)
    (descr "Precision Thin Film Chip Resistor Array, VISHAY (see http://www.vishay.com/docs/28770/acasat.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference RN6 (at 0 -2.8) (layer F.SilkS))
    (fp_text value R_Pack04 (at 0 2.8) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.7 -1.27 180) (size 0.7 0.64) (layers F.Cu F.Paste F.Mask)
      (net 122 /D7))
    (pad 3 smd rect (at -0.7 0.4 180) (size 0.7 0.5) (layers F.Cu F.Paste F.Mask)
      (net 120 /D5))
    (pad 2 smd rect (at -0.7 -0.4 180) (size 0.7 0.5) (layers F.Cu F.Paste F.Mask)
      (net 121 /D6))
    (pad 4 smd rect (at -0.7 1.27 180) (size 0.7 0.64) (layers F.Cu F.Paste F.Mask)
      (net 119 /D4))
    (pad 7 smd rect (at 0.7 -0.4 180) (size 0.7 0.5) (layers F.Cu F.Paste F.Mask)
      (net 40 /MD6))
    (pad 8 smd rect (at 0.7 -1.27 180) (size 0.7 0.64) (layers F.Cu F.Paste F.Mask)
      (net 41 /MD7))
    (pad 6 smd rect (at 0.7 0.4 180) (size 0.7 0.5) (layers F.Cu F.Paste F.Mask)
      (net 39 /MD5))
    (pad 5 smd rect (at 0.7 1.27 180) (size 0.7 0.64) (layers F.Cu F.Paste F.Mask)
      (net 38 /MD4))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_Array_Convex_4x0612.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_Array_Convex_4x0612 (layer B.Cu) (tedit 5B82E1AD)
    (at 168.91 133.604 180)
    (descr "Precision Thin Film Chip Resistor Array, VISHAY (see http://www.vishay.com/docs/28770/acasat.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference RN5 (at 0 2.8) (layer B.SilkS))
    (fp_text value R_Pack04 (at 0 -2.8) (layer B.Fab))
    (fp_text user %R (at 0 0 -90) (layer B.Fab))
    (pad 1 smd rect (at -0.7 1.27 180) (size 0.7 0.64) (layers B.Cu B.Paste B.Mask)
      (net 82 /A12))
    (pad 3 smd rect (at -0.7 -0.4 180) (size 0.7 0.5) (layers B.Cu B.Paste B.Mask)
      (net 44 /A14))
    (pad 2 smd rect (at -0.7 0.4 180) (size 0.7 0.5) (layers B.Cu B.Paste B.Mask)
      (net 43 /A13))
    (pad 4 smd rect (at -0.7 -1.27 180) (size 0.7 0.64) (layers B.Cu B.Paste B.Mask)
      (net 45 /A15))
    (pad 7 smd rect (at 0.7 0.4 180) (size 0.7 0.5) (layers B.Cu B.Paste B.Mask)
      (net 112 /BA13))
    (pad 8 smd rect (at 0.7 1.27 180) (size 0.7 0.64) (layers B.Cu B.Paste B.Mask)
      (net 111 /BA12))
    (pad 6 smd rect (at 0.7 -0.4 180) (size 0.7 0.5) (layers B.Cu B.Paste B.Mask)
      (net 113 /BA14))
    (pad 5 smd rect (at 0.7 -1.27 180) (size 0.7 0.64) (layers B.Cu B.Paste B.Mask)
      (net 114 /BA15))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_Array_Convex_4x0612.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_Array_Convex_4x0612 (layer B.Cu) (tedit 5B82E1AD)
    (at 169.418 115.57 180)
    (descr "Precision Thin Film Chip Resistor Array, VISHAY (see http://www.vishay.com/docs/28770/acasat.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference RN4 (at 0 2.8) (layer B.SilkS))
    (fp_text value R_Pack04 (at 0 -2.8) (layer B.Fab))
    (fp_text user %R (at 0 0 -90) (layer B.Fab))
    (pad 1 smd rect (at -0.7 1.27 180) (size 0.7 0.64) (layers B.Cu B.Paste B.Mask)
      (net 74 /A4))
    (pad 3 smd rect (at -0.7 -0.4 180) (size 0.7 0.5) (layers B.Cu B.Paste B.Mask)
      (net 76 /A6))
    (pad 2 smd rect (at -0.7 0.4 180) (size 0.7 0.5) (layers B.Cu B.Paste B.Mask)
      (net 75 /A5))
    (pad 4 smd rect (at -0.7 -1.27 180) (size 0.7 0.64) (layers B.Cu B.Paste B.Mask)
      (net 77 /A7))
    (pad 7 smd rect (at 0.7 0.4 180) (size 0.7 0.5) (layers B.Cu B.Paste B.Mask)
      (net 104 /BA5))
    (pad 8 smd rect (at 0.7 1.27 180) (size 0.7 0.64) (layers B.Cu B.Paste B.Mask)
      (net 103 /BA4))
    (pad 6 smd rect (at 0.7 -0.4 180) (size 0.7 0.5) (layers B.Cu B.Paste B.Mask)
      (net 105 /BA6))
    (pad 5 smd rect (at 0.7 -1.27 180) (size 0.7 0.64) (layers B.Cu B.Paste B.Mask)
      (net 106 /BA7))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_Array_Convex_4x0612.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_Array_Convex_4x0612 (layer F.Cu) (tedit 5B82E1AD)
    (at 167.64 84.074 180)
    (descr "Precision Thin Film Chip Resistor Array, VISHAY (see http://www.vishay.com/docs/28770/acasat.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference RN3 (at 0 -2.8) (layer F.SilkS))
    (fp_text value R_Pack04 (at 0 2.8) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.7 -1.27 180) (size 0.7 0.64) (layers F.Cu F.Paste F.Mask)
      (net 118 /D3))
    (pad 3 smd rect (at -0.7 0.4 180) (size 0.7 0.5) (layers F.Cu F.Paste F.Mask)
      (net 116 /D1))
    (pad 2 smd rect (at -0.7 -0.4 180) (size 0.7 0.5) (layers F.Cu F.Paste F.Mask)
      (net 117 /D2))
    (pad 4 smd rect (at -0.7 1.27 180) (size 0.7 0.64) (layers F.Cu F.Paste F.Mask)
      (net 115 /D0))
    (pad 7 smd rect (at 0.7 -0.4 180) (size 0.7 0.5) (layers F.Cu F.Paste F.Mask)
      (net 36 /MD2))
    (pad 8 smd rect (at 0.7 -1.27 180) (size 0.7 0.64) (layers F.Cu F.Paste F.Mask)
      (net 37 /MD3))
    (pad 6 smd rect (at 0.7 0.4 180) (size 0.7 0.5) (layers F.Cu F.Paste F.Mask)
      (net 35 /MD1))
    (pad 5 smd rect (at 0.7 1.27 180) (size 0.7 0.64) (layers F.Cu F.Paste F.Mask)
      (net 34 /MD0))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_Array_Convex_4x0612.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_Array_Convex_4x0612 (layer B.Cu) (tedit 5B82E1AD)
    (at 168.91 128.27 180)
    (descr "Precision Thin Film Chip Resistor Array, VISHAY (see http://www.vishay.com/docs/28770/acasat.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference RN2 (at 0 2.8) (layer B.SilkS))
    (fp_text value R_Pack04 (at 0 -2.8) (layer B.Fab))
    (fp_text user %R (at 0 0 -90) (layer B.Fab))
    (pad 1 smd rect (at -0.7 1.27 180) (size 0.7 0.64) (layers B.Cu B.Paste B.Mask)
      (net 78 /A8))
    (pad 3 smd rect (at -0.7 -0.4 180) (size 0.7 0.5) (layers B.Cu B.Paste B.Mask)
      (net 80 /A10))
    (pad 2 smd rect (at -0.7 0.4 180) (size 0.7 0.5) (layers B.Cu B.Paste B.Mask)
      (net 79 /A9))
    (pad 4 smd rect (at -0.7 -1.27 180) (size 0.7 0.64) (layers B.Cu B.Paste B.Mask)
      (net 81 /A11))
    (pad 7 smd rect (at 0.7 0.4 180) (size 0.7 0.5) (layers B.Cu B.Paste B.Mask)
      (net 108 /BA9))
    (pad 8 smd rect (at 0.7 1.27 180) (size 0.7 0.64) (layers B.Cu B.Paste B.Mask)
      (net 107 /BA8))
    (pad 6 smd rect (at 0.7 -0.4 180) (size 0.7 0.5) (layers B.Cu B.Paste B.Mask)
      (net 109 /BA10))
    (pad 5 smd rect (at 0.7 -1.27 180) (size 0.7 0.64) (layers B.Cu B.Paste B.Mask)
      (net 110 /BA11))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_Array_Convex_4x0612.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_Array_Convex_4x0612 (layer B.Cu) (tedit 5B82E1AD)
    (at 169.418 109.474 180)
    (descr "Precision Thin Film Chip Resistor Array, VISHAY (see http://www.vishay.com/docs/28770/acasat.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference RN1 (at 0 2.8) (layer B.SilkS))
    (fp_text value R_Pack04 (at 0 -2.8) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -0.7 1.27 180) (size 0.7 0.64) (layers B.Cu B.Paste B.Mask)
      (net 70 /A0))
    (pad 3 smd rect (at -0.7 -0.4 180) (size 0.7 0.5) (layers B.Cu B.Paste B.Mask)
      (net 72 /A2))
    (pad 2 smd rect (at -0.7 0.4 180) (size 0.7 0.5) (layers B.Cu B.Paste B.Mask)
      (net 71 /A1))
    (pad 4 smd rect (at -0.7 -1.27 180) (size 0.7 0.64) (layers B.Cu B.Paste B.Mask)
      (net 73 /A3))
    (pad 7 smd rect (at 0.7 0.4 180) (size 0.7 0.5) (layers B.Cu B.Paste B.Mask)
      (net 100 /BA1))
    (pad 8 smd rect (at 0.7 1.27 180) (size 0.7 0.64) (layers B.Cu B.Paste B.Mask)
      (net 99 /BA0))
    (pad 6 smd rect (at 0.7 -0.4 180) (size 0.7 0.5) (layers B.Cu B.Paste B.Mask)
      (net 101 /BA2))
    (pad 5 smd rect (at 0.7 -1.27 180) (size 0.7 0.64) (layers B.Cu B.Paste B.Mask)
      (net 102 /BA3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_Array_Convex_4x0612.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x10_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 180.34 109.982)
    (descr "Through hole straight pin header, 2x10, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x10 2.54mm double row")
    (fp_text reference J9 (at 1.27 -2.33) (layer F.SilkS) hide)
    (fp_text value Address (at 1.524 26.035) (layer F.SilkS) hide)
    (fp_text user %R (at 1.27 11.43 90) (layer F.Fab))
    (pad 20 thru_hole oval (at 2.54 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 /A15))
    (pad 19 thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 /A14))
    (pad 18 thru_hole oval (at 2.54 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 /A13))
    (pad 17 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 82 /A12))
    (pad 16 thru_hole oval (at 2.54 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 81 /A11))
    (pad 15 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 14 thru_hole oval (at 2.54 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 79 /A9))
    (pad 13 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 80 /A10))
    (pad 12 thru_hole oval (at 2.54 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 11 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 78 /A8))
    (pad 10 thru_hole oval (at 2.54 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 77 /A7))
    (pad 9 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 76 /A6))
    (pad 8 thru_hole oval (at 2.54 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 75 /A5))
    (pad 7 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 73 /A3))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 74 /A4))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 72 /A2))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 71 /A1))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 70 /A0))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x10_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 173.228 74.041 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J5 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value DBEN (at 0 9.144 180) (layer F.SilkS) hide)
    (fp_text user %R (at 0 2.54) (layer F.Fab))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 128 /DBEN))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 131 +5V))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 173.228 77.724 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J4 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value DBDIR (at 0 9.398 180) (layer F.SilkS) hide)
    (fp_text user %R (at 0 2.54) (layer F.Fab))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 129 /DBDIR))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 131 +5V))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 178.308 68.453 270)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J3 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value FLIP (at 0 7.41 90) (layer F.Fab))
    (fp_text user %R (at 0 2.54) (layer F.Fab))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 127 /FLIP6))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 126 /FLIP7))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 167.767 101.727 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J2 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value ABEN (at 0 7.41 90) (layer F.Fab))
    (fp_text user %R (at 0 2.54) (layer F.Fab))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 124 /ABEN))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 131 +5V))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 167.767 98.044 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J1 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value ABDIR (at 0 7.41 90) (layer F.Fab))
    (fp_text user %R (at 0 2.54) (layer F.Fab))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 125 /ABDIR))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 131 +5V))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DIP:DIP-18_W7.62mm_Socket_LongPads (layer F.Cu) (tedit 5A02E8C5)
    (at 148.844 48.006)
    (descr "18-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket, LongPads")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket LongPads")
    (fp_text reference U9 (at -2.4765 -1.3335) (layer F.SilkS))
    (fp_text value DRAM64KX4 (at 3.81 22.65) (layer F.Fab))
    (fp_text user %R (at 3.81 10.16) (layer F.Fab))
    (pad 18 thru_hole oval (at 7.62 0) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 9 thru_hole oval (at 0 20.32) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 131 +5V))
    (pad 17 thru_hole oval (at 7.62 2.54) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 /MD7))
    (pad 8 thru_hole oval (at 0 17.78) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 84 /RAF1))
    (pad 16 thru_hole oval (at 7.62 5.08) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 92 /CASM.B))
    (pad 7 thru_hole oval (at 0 15.24) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 85 /RAF2))
    (pad 15 thru_hole oval (at 7.62 7.62) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 /MD6))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 83 /RAF0))
    (pad 14 thru_hole oval (at 7.62 10.16) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 96 /UM4-14))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 93 /RAS.B))
    (pad 13 thru_hole oval (at 7.62 12.7) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 86 /RAF3))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 94 /RWE.B))
    (pad 12 thru_hole oval (at 7.62 15.24) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 87 /RAF4))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 /MD5))
    (pad 11 thru_hole oval (at 7.62 17.78) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 88 /RAF5))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 /MD4))
    (pad 10 thru_hole oval (at 7.62 20.32) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 98 /UM4-10))
    (pad 1 thru_hole rect (at 0 0) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-18_W7.62mm_Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm (layer B.Cu) (tedit 5D9F72B1)
    (at 167.64 87.63 180)
    (descr "SOIC, 20 Pin (JEDEC MS-013AC, https://www.analog.com/media/en/package-pcb-resources/package/233848rw_20.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (attr smd)
    (fp_text reference U8 (at 0 7.35) (layer B.SilkS))
    (fp_text value 74HCT245 (at 0 -7.35) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 20 smd roundrect (at 4.65 5.715 180) (size 2.05 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 131 +5V))
    (pad 19 smd roundrect (at 4.65 4.445 180) (size 2.05 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 128 /DBEN))
    (pad 18 smd roundrect (at 4.65 3.175 180) (size 2.05 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 34 /MD0))
    (pad 17 smd roundrect (at 4.65 1.905 180) (size 2.05 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 35 /MD1))
    (pad 16 smd roundrect (at 4.65 0.635 180) (size 2.05 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 36 /MD2))
    (pad 15 smd roundrect (at 4.65 -0.635 180) (size 2.05 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 37 /MD3))
    (pad 14 smd roundrect (at 4.65 -1.905 180) (size 2.05 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 38 /MD4))
    (pad 13 smd roundrect (at 4.65 -3.175 180) (size 2.05 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 39 /MD5))
    (pad 12 smd roundrect (at 4.65 -4.445 180) (size 2.05 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 40 /MD6))
    (pad 11 smd roundrect (at 4.65 -5.715 180) (size 2.05 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 41 /MD7))
    (pad 10 smd roundrect (at -4.65 -5.715 180) (size 2.05 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 9 smd roundrect (at -4.65 -4.445 180) (size 2.05 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 122 /D7))
    (pad 8 smd roundrect (at -4.65 -3.175 180) (size 2.05 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 121 /D6))
    (pad 7 smd roundrect (at -4.65 -1.905 180) (size 2.05 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 120 /D5))
    (pad 6 smd roundrect (at -4.65 -0.635 180) (size 2.05 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 119 /D4))
    (pad 5 smd roundrect (at -4.65 0.635 180) (size 2.05 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 118 /D3))
    (pad 4 smd roundrect (at -4.65 1.905 180) (size 2.05 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 117 /D2))
    (pad 3 smd roundrect (at -4.65 3.175 180) (size 2.05 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 116 /D1))
    (pad 2 smd roundrect (at -4.65 4.445 180) (size 2.05 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 115 /D0))
    (pad 1 smd roundrect (at -4.65 5.715 180) (size 2.05 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 129 /DBDIR))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-20W_7.5x12.8mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-14_3.9x8.7mm_P1.27mm (layer F.Cu) (tedit 5D9F72B1)
    (at 176.022 61.341)
    (descr "SOIC, 14 Pin (JEDEC MS-012AB, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_14.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (attr smd)
    (fp_text reference U6 (at -2.794 -5.207) (layer F.SilkS))
    (fp_text value 74HCT86 (at 0 5.28) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 14 smd roundrect (at 2.475 -3.81) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 131 +5V))
    (pad 13 smd roundrect (at 2.475 -2.54) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 12 smd roundrect (at 2.475 -1.27) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 11 smd roundrect (at 2.475 0) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 10 smd roundrect (at 2.475 1.27) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 9 smd roundrect (at 2.475 2.54) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 8 smd roundrect (at 2.475 3.81) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 7 smd roundrect (at -2.475 3.81) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 6 smd roundrect (at -2.475 2.54) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 97 "Net-(R15-Pad2)"))
    (pad 5 smd roundrect (at -2.475 1.27) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 126 /FLIP7))
    (pad 4 smd roundrect (at -2.475 0) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 69 /RA7))
    (pad 3 smd roundrect (at -2.475 -1.27) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 95 "Net-(R14-Pad2)"))
    (pad 2 smd roundrect (at -2.475 -2.54) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 127 /FLIP6))
    (pad 1 smd roundrect (at -2.475 -3.81) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 68 /RA6))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-14_3.9x8.7mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm (layer F.Cu) (tedit 5D9F72B1)
    (at 169.164 112.268 180)
    (descr "SOIC, 20 Pin (JEDEC MS-013AC, https://www.analog.com/media/en/package-pcb-resources/package/233848rw_20.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (attr smd)
    (fp_text reference U5 (at 0 -7.35) (layer F.SilkS))
    (fp_text value 74HCT245 (at 0 7.35) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 20 smd roundrect (at 4.65 -5.715 180) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 131 +5V))
    (pad 19 smd roundrect (at 4.65 -4.445 180) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 124 /ABEN))
    (pad 18 smd roundrect (at 4.65 -3.175 180) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 106 /BA7))
    (pad 17 smd roundrect (at 4.65 -1.905 180) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 105 /BA6))
    (pad 16 smd roundrect (at 4.65 -0.635 180) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 104 /BA5))
    (pad 15 smd roundrect (at 4.65 0.635 180) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 103 /BA4))
    (pad 14 smd roundrect (at 4.65 1.905 180) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 102 /BA3))
    (pad 13 smd roundrect (at 4.65 3.175 180) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 101 /BA2))
    (pad 12 smd roundrect (at 4.65 4.445 180) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 100 /BA1))
    (pad 11 smd roundrect (at 4.65 5.715 180) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 99 /BA0))
    (pad 10 smd roundrect (at -4.65 5.715 180) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 9 smd roundrect (at -4.65 4.445 180) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 70 /A0))
    (pad 8 smd roundrect (at -4.65 3.175 180) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 71 /A1))
    (pad 7 smd roundrect (at -4.65 1.905 180) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 72 /A2))
    (pad 6 smd roundrect (at -4.65 0.635 180) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 73 /A3))
    (pad 5 smd roundrect (at -4.65 -0.635 180) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 74 /A4))
    (pad 4 smd roundrect (at -4.65 -1.905 180) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 75 /A5))
    (pad 3 smd roundrect (at -4.65 -3.175 180) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 76 /A6))
    (pad 2 smd roundrect (at -4.65 -4.445 180) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 77 /A7))
    (pad 1 smd roundrect (at -4.65 -5.715 180) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 125 /ABDIR))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-20W_7.5x12.8mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DIP:DIP-18_W7.62mm_Socket_LongPads (layer F.Cu) (tedit 5A02E8C5)
    (at 107.315 48.006)
    (descr "18-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket, LongPads")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket LongPads")
    (fp_text reference U4 (at -1.016 -2.0955) (layer F.SilkS))
    (fp_text value DRAM64KX4 (at 3.81 22.65) (layer F.Fab))
    (fp_text user %R (at 3.81 10.16) (layer F.Fab))
    (pad 18 thru_hole oval (at 7.62 0) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 9 thru_hole oval (at 0 20.32) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 131 +5V))
    (pad 17 thru_hole oval (at 7.62 2.54) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 /AD7))
    (pad 8 thru_hole oval (at 0 17.78) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 84 /RAF1))
    (pad 16 thru_hole oval (at 7.62 5.08) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 91 /CASA.B))
    (pad 7 thru_hole oval (at 0 15.24) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 85 /RAF2))
    (pad 15 thru_hole oval (at 7.62 7.62) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 /AD6))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 83 /RAF0))
    (pad 14 thru_hole oval (at 7.62 10.16) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 89 /RAF6))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 93 /RAS.B))
    (pad 13 thru_hole oval (at 7.62 12.7) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 86 /RAF3))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 94 /RWE.B))
    (pad 12 thru_hole oval (at 7.62 15.24) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 87 /RAF4))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 /AD5))
    (pad 11 thru_hole oval (at 7.62 17.78) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 88 /RAF5))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 /AD4))
    (pad 10 thru_hole oval (at 7.62 20.32) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 90 /RAF7))
    (pad 1 thru_hole rect (at 0 0) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-18_W7.62mm_Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm (layer F.Cu) (tedit 5D9F72B1)
    (at 169.164 130.302 180)
    (descr "SOIC, 20 Pin (JEDEC MS-013AC, https://www.analog.com/media/en/package-pcb-resources/package/233848rw_20.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (attr smd)
    (fp_text reference U3 (at 0 -7.35) (layer F.SilkS))
    (fp_text value 74HCT245 (at 0 7.35) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 20 smd roundrect (at 4.65 -5.715 180) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 131 +5V))
    (pad 19 smd roundrect (at 4.65 -4.445 180) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 124 /ABEN))
    (pad 18 smd roundrect (at 4.65 -3.175 180) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 114 /BA15))
    (pad 17 smd roundrect (at 4.65 -1.905 180) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 113 /BA14))
    (pad 16 smd roundrect (at 4.65 -0.635 180) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 112 /BA13))
    (pad 15 smd roundrect (at 4.65 0.635 180) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 111 /BA12))
    (pad 14 smd roundrect (at 4.65 1.905 180) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 110 /BA11))
    (pad 13 smd roundrect (at 4.65 3.175 180) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 109 /BA10))
    (pad 12 smd roundrect (at 4.65 4.445 180) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 108 /BA9))
    (pad 11 smd roundrect (at 4.65 5.715 180) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 107 /BA8))
    (pad 10 smd roundrect (at -4.65 5.715 180) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 9 smd roundrect (at -4.65 4.445 180) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 78 /A8))
    (pad 8 smd roundrect (at -4.65 3.175 180) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 79 /A9))
    (pad 7 smd roundrect (at -4.65 1.905 180) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 80 /A10))
    (pad 6 smd roundrect (at -4.65 0.635 180) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 81 /A11))
    (pad 5 smd roundrect (at -4.65 -0.635 180) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 82 /A12))
    (pad 4 smd roundrect (at -4.65 -1.905 180) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 43 /A13))
    (pad 3 smd roundrect (at -4.65 -3.175 180) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 44 /A14))
    (pad 2 smd roundrect (at -4.65 -4.445 180) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 45 /A15))
    (pad 1 smd roundrect (at -4.65 -5.715 180) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 125 /ABDIR))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-20W_7.5x12.8mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DIP:DIP-18_W7.62mm_Socket_LongPads (layer F.Cu) (tedit 5A02E8C5)
    (at 121.158 48.006)
    (descr "18-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket, LongPads")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket LongPads")
    (fp_text reference U2 (at -2.54 -1.27) (layer F.SilkS))
    (fp_text value DRAM64KX4 (at 3.81 22.65) (layer F.Fab))
    (fp_text user %R (at 3.81 10.16) (layer F.Fab))
    (pad 18 thru_hole oval (at 7.62 0) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 9 thru_hole oval (at 0 20.32) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 131 +5V))
    (pad 17 thru_hole oval (at 7.62 2.54) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 /AD3))
    (pad 8 thru_hole oval (at 0 17.78) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 84 /RAF1))
    (pad 16 thru_hole oval (at 7.62 5.08) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 91 /CASA.B))
    (pad 7 thru_hole oval (at 0 15.24) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 85 /RAF2))
    (pad 15 thru_hole oval (at 7.62 7.62) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 /AD2))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 83 /RAF0))
    (pad 14 thru_hole oval (at 7.62 10.16) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 89 /RAF6))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 93 /RAS.B))
    (pad 13 thru_hole oval (at 7.62 12.7) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 86 /RAF3))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 94 /RWE.B))
    (pad 12 thru_hole oval (at 7.62 15.24) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 87 /RAF4))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 /AD1))
    (pad 11 thru_hole oval (at 7.62 17.78) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 88 /RAF5))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 /AD0))
    (pad 10 thru_hole oval (at 7.62 20.32) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 90 /RAF7))
    (pad 1 thru_hole rect (at 0 0) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-18_W7.62mm_Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_LCC:PLCC-84_THT-Socket (layer F.Cu) (tedit 5A02ECC8)
    (at 129.54 91.313)
    (descr "PLCC, 84 pins, through hole")
    (tags "plcc leaded")
    (fp_text reference U1 (at 0 -3.77) (layer F.SilkS))
    (fp_text value Apple_MEGA_II (at 0 34.25) (layer F.Fab))
    (fp_text user %R (at 0 15.24) (layer F.Fab))
    (pad 72 thru_hole circle (at 15.24 5.08) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 64 /RA2))
    (pad 70 thru_hole circle (at 15.24 7.62) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 66 /RA4))
    (pad 68 thru_hole circle (at 15.24 10.16) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 68 /RA6))
    (pad 66 thru_hole circle (at 15.24 12.7) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 99 /BA0))
    (pad 64 thru_hole circle (at 15.24 15.24) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 101 /BA2))
    (pad 62 thru_hole circle (at 15.24 17.78) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 103 /BA4))
    (pad 60 thru_hole circle (at 15.24 20.32) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 105 /BA6))
    (pad 58 thru_hole circle (at 15.24 22.86) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 107 /BA8))
    (pad 56 thru_hole circle (at 15.24 25.4) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 109 /BA10))
    (pad 54 thru_hole circle (at 15.24 27.94) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 111 /BA12))
    (pad 73 thru_hole circle (at 12.7 5.08) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 63 /RA1))
    (pad 71 thru_hole circle (at 12.7 7.62) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 65 /RA3))
    (pad 69 thru_hole circle (at 12.7 10.16) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 67 /RA5))
    (pad 67 thru_hole circle (at 12.7 12.7) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 69 /RA7))
    (pad 65 thru_hole circle (at 12.7 15.24) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 100 /BA1))
    (pad 63 thru_hole circle (at 12.7 17.78) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 102 /BA3))
    (pad 61 thru_hole circle (at 12.7 20.32) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 104 /BA5))
    (pad 59 thru_hole circle (at 12.7 22.86) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 106 /BA7))
    (pad 57 thru_hole circle (at 12.7 25.4) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 108 /BA9))
    (pad 55 thru_hole circle (at 12.7 27.94) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 110 /BA11))
    (pad 53 thru_hole circle (at 12.7 30.48) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 112 /BA13))
    (pad 51 thru_hole circle (at 10.16 30.48) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 114 /BA15))
    (pad 49 thru_hole circle (at 7.62 30.48) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 47 /WINDOW))
    (pad 47 thru_hole circle (at 5.08 30.48) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 49 /S5))
    (pad 45 thru_hole circle (at 2.54 30.48) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 51 /S3))
    (pad 43 thru_hole circle (at 0 30.48) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 53 /S1))
    (pad 41 thru_hole circle (at -2.54 30.48) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 /R-W))
    (pad 39 thru_hole circle (at -5.08 30.48) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 /M2SEL))
    (pad 37 thru_hole circle (at -7.62 30.48) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 123 /ROMEN))
    (pad 35 thru_hole circle (at -10.16 30.48) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 /RESET))
    (pad 33 thru_hole circle (at -12.7 30.48) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 52 thru_hole circle (at 10.16 27.94) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 113 /BA14))
    (pad 50 thru_hole circle (at 7.62 27.94) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 46 /SYNC))
    (pad 48 thru_hole circle (at 5.08 27.94) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 48 /RMBK))
    (pad 46 thru_hole circle (at 2.54 27.94) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 50 /S4))
    (pad 44 thru_hole circle (at 0 27.94) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 52 /S2))
    (pad 42 thru_hole circle (at -2.54 27.94) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 /S0))
    (pad 40 thru_hole circle (at -5.08 27.94) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 /INH))
    (pad 38 thru_hole circle (at -7.62 27.94) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 /DMA))
    (pad 36 thru_hole circle (at -10.16 27.94) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 /MDI-MDO))
    (pad 34 thru_hole circle (at -12.7 27.94) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 /RGB1))
    (pad 32 thru_hole circle (at -15.24 27.94) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 /RGB2))
    (pad 30 thru_hole circle (at -15.24 25.4) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 /RGB8))
    (pad 28 thru_hole circle (at -15.24 22.86) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 /AD6))
    (pad 26 thru_hole circle (at -15.24 20.32) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 /AD4))
    (pad 24 thru_hole circle (at -15.24 17.78) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 /AD2))
    (pad 22 thru_hole circle (at -15.24 15.24) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 /AD0))
    (pad 20 thru_hole circle (at -15.24 12.7) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 /MSW))
    (pad 18 thru_hole circle (at -15.24 10.16) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 /Y0))
    (pad 16 thru_hole circle (at -15.24 7.62) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 /X0))
    (pad 14 thru_hole circle (at -15.24 5.08) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 /KSEL2))
    (pad 12 thru_hole circle (at -15.24 2.54) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 /SPKR))
    (pad 31 thru_hole circle (at -12.7 25.4) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 /RGB4))
    (pad 29 thru_hole circle (at -12.7 22.86) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 /AD7))
    (pad 27 thru_hole circle (at -12.7 20.32) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 /AD5))
    (pad 25 thru_hole circle (at -12.7 17.78) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 /AD3))
    (pad 23 thru_hole circle (at -12.7 15.24) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 /AD1))
    (pad 21 thru_hole circle (at -12.7 12.7) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /SERVIDEO))
    (pad 19 thru_hole circle (at -12.7 10.16) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 /Y1))
    (pad 17 thru_hole circle (at -12.7 7.62) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 /X1))
    (pad 15 thru_hole circle (at -12.7 5.08) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 /IRQ))
    (pad 13 thru_hole circle (at -12.7 2.54) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 /KSEL1))
    (pad 75 thru_hole circle (at 12.7 0) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 77 thru_hole circle (at 10.16 0) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 131 +5V))
    (pad 79 thru_hole circle (at 7.62 0) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 59 /CREF))
    (pad 81 thru_hole circle (at 5.08 0) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 57 /PH#))
    (pad 83 thru_hole circle (at 2.54 0) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 55 /CASM))
    (pad 11 thru_hole circle (at -12.7 0) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 /C060-67))
    (pad 9 thru_hole circle (at -10.16 0) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 /MD0))
    (pad 7 thru_hole circle (at -7.62 0) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 /MD2))
    (pad 5 thru_hole circle (at -5.08 0) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 /MD4))
    (pad 3 thru_hole circle (at -2.54 0) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 /MD6))
    (pad 1 thru_hole rect (at 0 0) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 /RAMWE))
    (pad 74 thru_hole circle (at 15.24 2.54) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 62 /RA0))
    (pad 76 thru_hole circle (at 12.7 2.54) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 61 /14M))
    (pad 78 thru_hole circle (at 10.16 2.54) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 60 /7M))
    (pad 80 thru_hole circle (at 7.62 2.54) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 58 /Q3))
    (pad 82 thru_hole circle (at 5.08 2.54) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 56 /CASA))
    (pad 84 thru_hole circle (at 2.54 2.54) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 /RAS))
    (pad 10 thru_hole circle (at -10.16 2.54) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 /PDLTRIG))
    (pad 8 thru_hole circle (at -7.62 2.54) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 /MD1))
    (pad 6 thru_hole circle (at -5.08 2.54) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 /MD3))
    (pad 4 thru_hole circle (at -2.54 2.54) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 /MD5))
    (pad 2 thru_hole circle (at 0 2.54) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 /MD7))
    (model ${KISYS3DMOD}/Package_LCC.3dshapes/PLCC-84_THT-Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "My Libraries:Harwin-S1751-46-Test-Point" (layer F.Cu) (tedit 5F9F0FC9)
    (at 159.385 72.136 270)
    (fp_text reference TP98 (at 2.54 0 180) (layer F.SilkS))
    (fp_text value TestPoint (at 0 -1.778 90) (layer F.Fab))
    (pad 1 smd rect (at 0 0 270) (size 3.45 1.85) (layers F.Cu F.Paste F.Mask)
      (net 97 "Net-(R15-Pad2)"))
    (model "C:/Users/balde/Dropbox/KiCad/Downloaded Libraries/s1751-46.stp"
      (offset (xyz 0 0.825 2))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module "My Libraries:Harwin-S1751-46-Test-Point" (layer F.Cu) (tedit 5F9F0FC9)
    (at 161.798 49.911 90)
    (fp_text reference TP97 (at 1.016 1.778 90) (layer F.SilkS))
    (fp_text value TestPoint (at 0 -1.778 90) (layer F.Fab))
    (pad 1 smd rect (at 0 0 90) (size 3.45 1.85) (layers F.Cu F.Paste F.Mask)
      (net 95 "Net-(R14-Pad2)"))
    (model "C:/Users/balde/Dropbox/KiCad/Downloaded Libraries/s1751-46.stp"
      (offset (xyz 0 0.825 2))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 161.798 69.596 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R15 (at -1.016 1.651 90) (layer F.SilkS))
    (fp_text value 100 (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.243902)
      (net 97 "Net-(R15-Pad2)"))
    (pad 1 smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.243902)
      (net 98 /UM4-10))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 161.798 53.848 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R14 (at -0.508 2.159 180) (layer F.SilkS))
    (fp_text value 100 (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.243902)
      (net 95 "Net-(R14-Pad2)"))
    (pad 1 smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.243902)
      (net 96 /UM4-14))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 174.4745 51.054)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at -0.1035 1.778) (layer F.SilkS))
    (fp_text value 1k (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.243902)
      (net 2 "Net-(D1-Pad2)"))
    (pad 1 smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.243902)
      (net 131 +5V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_2.5mm (layer F.Cu) (tedit 56D1B4CB)
    (at 92.456 144.78)
    (descr "Mounting Hole 2.5mm, no annular")
    (tags "mounting hole 2.5mm no annular")
    (attr virtual)
    (fp_text reference H4 (at 0 -3.5) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 3.5) (layer F.Fab))
    (fp_text user %R (at 0 -3.556) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.5mm (layer F.Cu) (tedit 56D1B4CB)
    (at 92.6465 35.052)
    (descr "Mounting Hole 2.5mm, no annular")
    (tags "mounting hole 2.5mm no annular")
    (attr virtual)
    (fp_text reference H3 (at 0 -3.5) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 3.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.5mm (layer F.Cu) (tedit 56D1B4CB)
    (at 185.674 35.052)
    (descr "Mounting Hole 2.5mm, no annular")
    (tags "mounting hole 2.5mm no annular")
    (attr virtual)
    (fp_text reference H2 (at 0 -3.5) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 3.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.5mm (layer F.Cu) (tedit 56D1B4CB)
    (at 185.674 144.78)
    (descr "Mounting Hole 2.5mm, no annular")
    (tags "mounting hole 2.5mm no annular")
    (attr virtual)
    (fp_text reference H1 (at 0 -3.5) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 3.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask))
  )
  (module LED_SMD:LED_1206_3216Metric (layer F.Cu) (tedit 5F68FEF1)
    (at 179.324 51.054 180)
    (descr "LED SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D1 (at 0 -1.82) (layer F.SilkS))
    (fp_text value PWR (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 2 "Net-(D1-Pad2)"))
    (pad 1 smd roundrect (at -1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 1 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 152.654 68.453)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C9 (at 0 1.68 180) (layer B.SilkS))
    (fp_text value 1uF (at 0 -1.68 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd roundrect (at 0.95 0) (size 1 1.45) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.95 0) (size 1 1.45) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 131 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 164.592 79.756)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C8 (at 0 1.68) (layer B.SilkS))
    (fp_text value 1uF (at 0 -1.68) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.95 0) (size 1 1.45) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.95 0) (size 1 1.45) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 131 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 111.252 68.326)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C7 (at 0 1.68) (layer B.SilkS))
    (fp_text value 1uF (at 0 -1.68) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.95 0) (size 1 1.45) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.95 0) (size 1 1.45) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 131 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 138.811 68.453)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C6 (at 0 1.68) (layer B.SilkS))
    (fp_text value 1uF (at 0 -1.68) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.95 0) (size 1 1.45) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.95 0) (size 1 1.45) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 131 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 122.174 71.12)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C5 (at 0 1.68 180) (layer B.SilkS))
    (fp_text value 1uF (at 0 -1.68 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd roundrect (at 0.95 0) (size 1 1.45) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.95 0) (size 1 1.45) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 131 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 165.354 120.142)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C4 (at 0 -1.68) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.68) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.95 0) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.95 0) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 131 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 165.608 138.176)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C3 (at 0 1.778) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.68) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.95 0) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.95 0) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 131 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 177.927 55.372 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at -2.667 1.016) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.68) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.95 0 180) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.95 0 180) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 131 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text 2 (at 129.54 95.885) (layer B.SilkS))
  (gr_text 44 (at 129.54 116.84 180) (layer B.SilkS))
  (gr_text 1 (at 129.54 88.9 -90) (layer B.SilkS))
  (gr_text 5 (at 124.46 88.9 -90) (layer B.SilkS))
  (gr_text 11 (at 116.84 88.9 -90) (layer B.SilkS))
  (gr_text 12 (at 111.76 93.98) (layer B.SilkS))
  (gr_text 24 (at 111.76 109.22) (layer B.SilkS))
  (gr_text 32 (at 111.76 119.38) (layer B.SilkS))
  (gr_text 39 (at 124.46 124.46 -90) (layer B.SilkS))
  (gr_text 43 (at 129.54 124.46 -90) (layer B.SilkS))
  (gr_text 53 (at 142.24 124.46 -90) (layer B.SilkS))
  (gr_text 54 (at 147.32 119.38 180) (layer B.SilkS))
  (gr_text "This board (and this project) would not \nhappen without the help of\n\nrjhelms.\n\nThank you!" (at 96.52 39.878 90) (layer B.SilkS))
  (gr_text "gd MEGA-][\n@baldengineer\nrev1" (at 93.472 77.47 90) (layer F.SilkS))
  (gr_text 5V (at 139.573 89.288857 270) (layer B.SilkS))
  (gr_text 5V (at 139.573 89.273143 -90) (layer F.SilkS))
  (gr_text 5V (at 165.862 41.656 180) (layer B.SilkS))
  (gr_text PDL (at 106.553 73.66 270) (layer B.SilkS))
  (gr_text PDL (at 106.553 73.66 -90) (layer F.SilkS))
  (gr_text C060 (at 104.013 73.406 270) (layer B.SilkS))
  (gr_text C060 (at 104.013 73.406 -90) (layer F.SilkS))
  (gr_text RAS (at 131.572 73.802857 -90) (layer F.SilkS))
  (gr_text CASM (at 133.985 73.231428 -90) (layer F.SilkS))
  (gr_text CASA (at 136.4615 73.374285 -90) (layer F.SilkS))
  (gr_text RAMWE (at 128.9685 72.683809 -90) (layer F.SilkS))
  (gr_text 10 (at 161.4805 126.896928 -90) (layer F.SilkS))
  (gr_text 11 (at 161.4805 129.690928 -90) (layer F.SilkS))
  (gr_text 13 (at 161.4805 132.738928 -90) (layer F.SilkS))
  (gr_text U9 (at 152.654 50.038) (layer B.SilkS))
  (gr_text U7 (at 138.938 50.038) (layer B.SilkS))
  (gr_text U2 (at 124.968 50.038) (layer B.SilkS))
  (gr_text U4 (at 110.998 50.292) (layer B.SilkS))
  (gr_text 7 (at 112.903 43.473834 270) (layer B.SilkS))
  (gr_text AD1 (at 123.2535 44.402406 270) (layer B.SilkS))
  (gr_text AD3 (at 118.11 44.402406 270) (layer B.SilkS))
  (gr_text PH# (at 156.21 44.521453 270) (layer B.SilkS))
  (gr_text RA1 (at 133.4135 44.402406 270) (layer B.SilkS))
  (gr_text RA2 (at 136.017 44.402406 270) (layer B.SilkS))
  (gr_text RA3 (at 138.4935 44.402406 270) (layer B.SilkS))
  (gr_text RA4 (at 143.5735 44.402406 270) (layer B.SilkS))
  (gr_text RA6 (at 148.6535 44.402406 270) (layer B.SilkS))
  (gr_text RA5 (at 146.2405 44.402406 270) (layer B.SilkS))
  (gr_text AD0 (at 125.857 44.402406 270) (layer B.SilkS))
  (gr_text RA7 (at 151.3205 44.402406 270) (layer B.SilkS))
  (gr_text RA0 (at 128.3335 44.402406 270) (layer B.SilkS))
  (gr_text MD1 (at 128.143 34.417 90) (layer B.SilkS))
  (gr_text AD4 (at 117.983 34.559857 90) (layer B.SilkS))
  (gr_text MD2 (at 135.6995 34.417 90) (layer B.SilkS))
  (gr_text MD0 (at 125.6665 34.417 90) (layer B.SilkS))
  (gr_text AD6 (at 115.443 34.559857 90) (layer B.SilkS))
  (gr_text AD2 (at 120.5865 34.559857 90) (layer B.SilkS))
  (gr_text NC (at 130.81 35.570119 180) (layer B.SilkS))
  (gr_text MD3 (at 138.2395 34.417 90) (layer B.SilkS))
  (gr_text 14M (at 108.0135 34.44081 90) (layer B.SilkS))
  (gr_text MD4 (at 140.843 34.417 90) (layer B.SilkS))
  (gr_text MD7 (at 151.13 34.417 90) (layer B.SilkS))
  (gr_text MD5 (at 145.923 34.417 90) (layer B.SilkS))
  (gr_text MD6 (at 148.463 34.417 90) (layer B.SilkS))
  (gr_text 5V (at 175.768 39.116 180) (layer B.SilkS))
  (gr_text 5V (at 175.768 36.576 180) (layer B.SilkS))
  (gr_text Flip7 (at 181.356 68.199 90) (layer B.SilkS))
  (gr_text Flip6 (at 169.545 69.088) (layer B.SilkS))
  (gr_text DB (at 181.102 75.946 90) (layer B.SilkS))
  (gr_text EN (at 175.514 71.628 180) (layer B.SilkS))
  (gr_text 5V (at 170.053 74.295) (layer B.SilkS))
  (gr_text 5V (at 170.18 77.978) (layer B.SilkS))
  (gr_text DIR (at 175.768 80.264 180) (layer B.SilkS))
  (gr_text D7 (at 184.880309 92.71) (layer B.SilkS))
  (gr_text D3 (at 184.880309 85.2805) (layer B.SilkS))
  (gr_text D5 (at 184.880309 87.5665) (layer B.SilkS))
  (gr_text D1 (at 184.880309 82.6135) (layer B.SilkS))
  (gr_text D2 (at 176.117309 84.8995) (layer B.SilkS))
  (gr_text D0 (at 176.117309 82.55) (layer B.SilkS))
  (gr_text D6 (at 176.117309 92.71) (layer B.SilkS))
  (gr_text D4 (at 176.117309 89.9795) (layer B.SilkS))
  (gr_text 5V (at 164.973 98.044 180) (layer B.SilkS))
  (gr_text 5V (at 165.1 101.727 180) (layer B.SilkS))
  (gr_text AB (at 175.895 99.949 90) (layer B.SilkS))
  (gr_text EN (at 170.307 95.504 180) (layer B.SilkS))
  (gr_text DIR (at 170.307 104.394 180) (layer B.SilkS))
  (gr_text Data (at 180.562191 96.0755 180) (layer B.SilkS))
  (gr_text Address (at 181.641691 136.2075 180) (layer B.SilkS))
  (gr_text "A10\n" (at 176.815808 125.349) (layer B.SilkS))
  (gr_text A8 (at 177.291999 122.682) (layer B.SilkS))
  (gr_text A6 (at 177.291999 120.2055) (layer B.SilkS))
  (gr_text A0 (at 177.291999 109.982) (layer B.SilkS))
  (gr_text A14 (at 176.815808 132.969) (layer B.SilkS))
  (gr_text A2 (at 177.291999 112.5855) (layer B.SilkS))
  (gr_text A4 (at 177.291999 115.189) (layer B.SilkS))
  (gr_text A12 (at 176.815808 130.556) (layer B.SilkS))
  (gr_text A15 (at 186.499499 132.969) (layer B.SilkS))
  (gr_text A13 (at 186.499499 130.2385) (layer B.SilkS))
  (gr_text A3 (at 186.023309 115.1255) (layer B.SilkS))
  (gr_text A7 (at 186.023309 120.269) (layer B.SilkS))
  (gr_text A1 (at 186.023309 110.1725) (layer B.SilkS))
  (gr_text A11 (at 186.499499 127.762) (layer B.SilkS))
  (gr_text A5 (at 186.023309 117.7925) (layer B.SilkS))
  (gr_text A9 (at 186.023309 125.095) (layer B.SilkS))
  (gr_text SYNC (at 147.193 131.722691 270) (layer B.SilkS))
  (gr_text BA13 (at 154.8765 131.675072 270) (layer B.SilkS))
  (gr_text BA15 (at 149.606 131.675072 270) (layer B.SilkS))
  (gr_text BA14 (at 152.3365 131.675072 270) (layer B.SilkS))
  (gr_text BA12 (at 150.876 143.756 270) (layer B.SilkS))
  (gr_text M2SEL (at 148.1455 144.256 270) (layer B.SilkS))
  (gr_text MDI-MDO (at 111.8235 129.841644 90) (layer B.SilkS))
  (gr_text DMA (at 116.9035 131.865453 90) (layer B.SilkS))
  (gr_text ROMEN (at 114.4905 130.794025 90) (layer B.SilkS))
  (gr_text RW (at 124.7775 132.294025 90) (layer B.SilkS))
  (gr_text M2SEL (at 119.4435 130.984501 90) (layer B.SilkS))
  (gr_text INH (at 122.047 132.079739 90) (layer B.SilkS))
  (gr_text ~RES (at 109.2835 131.936882 90) (layer B.SilkS))
  (gr_text S3 (at 134.62 132.413072 270) (layer B.SilkS))
  (gr_text S1 (at 129.54 132.413072 270) (layer B.SilkS))
  (gr_text S5 (at 139.7 132.413072 270) (layer B.SilkS))
  (gr_text RMBK (at 142.1765 131.294024 270) (layer B.SilkS))
  (gr_text S2 (at 131.953 132.413072 270) (layer B.SilkS))
  (gr_text S0 (at 126.9365 132.413072 270) (layer B.SilkS))
  (gr_text WNDW (at 144.78 131.198786 270) (layer B.SilkS))
  (gr_text S4 (at 137.033 132.413072 270) (layer B.SilkS))
  (gr_text ROMEN (at 114.3635 140.715501 90) (layer B.SilkS))
  (gr_text RW (at 124.6505 139.215501 90) (layer B.SilkS))
  (gr_text DMA (at 116.7765 139.644072 90) (layer B.SilkS))
  (gr_text M2SEL (at 119.3165 140.525025 90) (layer B.SilkS))
  (gr_text INH (at 121.92 139.429787 90) (layer B.SilkS))
  (gr_text ~RES (at 109.1565 139.572644 90) (layer B.SilkS))
  (gr_text MDI-MDO (at 111.6965 141.667882 90) (layer B.SilkS))
  (gr_text S5 (at 139.573 139.096453 270) (layer B.SilkS))
  (gr_text S3 (at 134.493 139.096453 270) (layer B.SilkS))
  (gr_text RMBK (at 142.0495 140.2155 270) (layer B.SilkS))
  (gr_text S2 (at 131.826 139.096453 270) (layer B.SilkS))
  (gr_text S0 (at 126.8095 139.096453 270) (layer B.SilkS))
  (gr_text S4 (at 136.906 139.096453 270) (layer B.SilkS))
  (gr_text S1 (at 129.413 139.096453 270) (layer B.SilkS))
  (gr_text WNDW (at 144.653 140.310738 270) (layer B.SilkS))
  (gr_text IRQ (at 100.3935 143.1925 90) (layer B.SilkS))
  (gr_text ~RES (at 102.997 143.025833 90) (layer B.SilkS))
  (gr_text RW (at 105.6005 143.382976 90) (layer B.SilkS))
  (gr_text RGB8 (at 92.5195 129.667) (layer B.SilkS))
  (gr_text "RGB1\n" (at 92.5195 132.334) (layer B.SilkS))
  (gr_text RGB4 (at 92.5195 127.1905) (layer B.SilkS))
  (gr_text RGB2 (at 92.5195 135.255) (layer B.SilkS))
  (gr_text AD6 (at 96.646786 121.92) (layer B.SilkS))
  (gr_text AD5 (at 96.646786 119.5705) (layer B.SilkS))
  (gr_text AD2 (at 96.646786 111.887) (layer B.SilkS))
  (gr_text AD1 (at 96.646786 109.347) (layer B.SilkS))
  (gr_text AD3 (at 96.646786 114.4905) (layer B.SilkS))
  (gr_text AD4 (at 96.646786 116.967) (layer B.SilkS))
  (gr_text AD0 (at 96.646786 106.807) (layer B.SilkS))
  (gr_text AD7 (at 96.646786 124.46) (layer B.SilkS))
  (gr_text X1 (at 97.099167 94.234) (layer B.SilkS))
  (gr_text MSW (at 96.4325 101.6635) (layer B.SilkS))
  (gr_text SERVID (at 95.45631 104.2035) (layer B.SilkS))
  (gr_text Y0 (at 97.146786 96.7105) (layer B.SilkS))
  (gr_text SPKR (at 96.075357 81.407) (layer B.SilkS))
  (gr_text KSEL2 (at 95.742024 83.947) (layer B.SilkS))
  (gr_text IRQ (at 96.789643 89.0905) (layer B.SilkS))
  (gr_text Y1 (at 97.146786 99.314) (layer B.SilkS))
  (gr_text X0 (at 97.099167 91.6305) (layer B.SilkS))
  (gr_text KSEL1 (at 95.742024 86.5505) (layer B.SilkS))
  (gr_text Y0 (at 103.703572 96.7105) (layer B.SilkS))
  (gr_text Y1 (at 103.703572 99.314) (layer B.SilkS))
  (gr_text KSEL1 (at 105.108334 86.5505) (layer B.SilkS))
  (gr_text X0 (at 103.751191 91.6305) (layer B.SilkS))
  (gr_text X1 (at 103.751191 94.234) (layer B.SilkS))
  (gr_text MSW (at 104.417857 101.6635) (layer B.SilkS))
  (gr_text SERVID (at 105.394048 104.2035) (layer B.SilkS))
  (gr_text IRQ (at 104.060715 89.0905) (layer B.SilkS))
  (gr_text AD1 (at 104.203572 109.4105) (layer B.SilkS))
  (gr_text AD6 (at 104.203572 121.9835) (layer B.SilkS))
  (gr_text AD3 (at 104.203572 114.554) (layer B.SilkS))
  (gr_text AD5 (at 104.203572 119.634) (layer B.SilkS))
  (gr_text AD4 (at 104.203572 117.0305) (layer B.SilkS))
  (gr_text AD0 (at 104.203572 106.8705) (layer B.SilkS))
  (gr_text AD2 (at 104.203572 111.9505) (layer B.SilkS))
  (gr_text AD7 (at 104.203572 124.5235) (layer B.SilkS))
  (gr_text SPKR (at 104.775 81.407) (layer B.SilkS))
  (gr_text KSEL2 (at 105.108334 83.947) (layer B.SilkS))
  (gr_text RGB2 (at 104.775 132.207) (layer B.SilkS))
  (gr_text RGB8 (at 104.775 127.0635) (layer B.SilkS))
  (gr_text RGB4 (at 104.775 129.6035) (layer B.SilkS))
  (gr_text 14M (at 152.2095 81.00219 270) (layer B.SilkS))
  (gr_text RAS (at 132.08 80.883143 270) (layer B.SilkS))
  (gr_text 7M (at 147.2565 80.526 270) (layer B.SilkS))
  (gr_text PH# (at 139.573 81.00219 270) (layer B.SilkS))
  (gr_text CASM (at 134.493 81.454571 270) (layer B.SilkS))
  (gr_text 5V (at 149.733 80.383143 270) (layer B.SilkS))
  (gr_text Q3 (at 142.1765 80.478381 270) (layer B.SilkS))
  (gr_text CASA (at 136.9695 81.311714 270) (layer B.SilkS))
  (gr_text CREF (at 144.8435 81.359333 270) (layer B.SilkS))
  (gr_text MD5 (at 122.047 81.026 270) (layer B.SilkS))
  (gr_text MD2 (at 114.173 81.026 270) (layer B.SilkS))
  (gr_text MD0 (at 109.2835 81.026 270) (layer B.SilkS))
  (gr_text MD6 (at 124.46 81.026 270) (layer B.SilkS))
  (gr_text MD3 (at 116.7765 81.026 270) (layer B.SilkS))
  (gr_text MD1 (at 111.6965 81.026 270) (layer B.SilkS))
  (gr_text MD7 (at 126.9365 81.026 270) (layer B.SilkS))
  (gr_text MD4 (at 119.38 81.026 270) (layer B.SilkS))
  (gr_text RAMWE (at 129.4765 82.00219 270) (layer B.SilkS))
  (gr_text BA12 (at 162.8775 132.2705) (layer B.SilkS))
  (gr_text BA11 (at 162.8775 129.8575) (layer B.SilkS))
  (gr_text BA9 (at 162.33769 124.3965) (layer B.SilkS))
  (gr_text BA3 (at 162.33769 109.1565) (layer B.SilkS))
  (gr_text BA5 (at 162.33769 114.3) (layer B.SilkS))
  (gr_text BA10 (at 162.8775 127.0635) (layer B.SilkS))
  (gr_text RA6 (at 162.33769 96.4565) (layer B.SilkS))
  (gr_text BA4 (at 162.33769 111.8235) (layer B.SilkS))
  (gr_text BA8 (at 162.33769 121.92) (layer B.SilkS))
  (gr_text RA7 (at 162.33769 99.1235) (layer B.SilkS))
  (gr_text BA6 (at 162.33769 116.84) (layer B.SilkS))
  (gr_text BA7 (at 162.33769 119.38) (layer B.SilkS))
  (gr_text BA2 (at 162.33769 106.7435) (layer B.SilkS))
  (gr_text BA0 (at 162.33769 101.5365) (layer B.SilkS))
  (gr_text BA1 (at 162.33769 104.2035) (layer B.SilkS))
  (gr_text BA10 (at 154.559 127.0635) (layer B.SilkS))
  (gr_text BA5 (at 155.035191 114.3) (layer B.SilkS))
  (gr_text BA3 (at 155.035191 109.1565) (layer B.SilkS))
  (gr_text BA9 (at 155.035191 124.3965) (layer B.SilkS))
  (gr_text BA1 (at 155.035191 104.2035) (layer B.SilkS))
  (gr_text BA0 (at 155.035191 101.5365) (layer B.SilkS))
  (gr_text RA6 (at 155.035191 96.4565) (layer B.SilkS))
  (gr_text BA8 (at 155.035191 121.92) (layer B.SilkS))
  (gr_text RA3 (at 155.035191 88.9635) (layer B.SilkS))
  (gr_text BA7 (at 155.035191 119.38) (layer B.SilkS))
  (gr_text BA4 (at 155.035191 111.8235) (layer B.SilkS))
  (gr_text RA7 (at 155.035191 99.1235) (layer B.SilkS))
  (gr_text RA4 (at 155.035191 91.5035) (layer B.SilkS))
  (gr_text BA2 (at 155.035191 106.7435) (layer B.SilkS))
  (gr_text BA6 (at 155.035191 116.84) (layer B.SilkS))
  (gr_text RA5 (at 155.035191 93.9165) (layer B.SilkS))
  (gr_text RA1 (at 155.035191 83.8835) (layer B.SilkS))
  (gr_text RA0 (at 155.035191 81.28) (layer B.SilkS))
  (gr_text RA2 (at 155.035191 86.36) (layer B.SilkS))
  (gr_text 64 (at 147.32 106.68 180) (layer B.SilkS))
  (gr_arc (start 91.948 145.288) (end 89.662 145.288) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 186.182 145.288) (end 186.182 147.574) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 186.182 34.544) (end 188.468 34.544) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 92.202 34.544) (end 92.202 32.258) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 89.662 145.288) (end 89.916 34.544) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 186.182 147.574) (end 91.948 147.574) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 188.468 34.544) (end 188.468 145.288) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 92.202 32.258) (end 186.182 32.258) (layer Edge.Cuts) (width 0.05))
  (gr_text A15 (at 186.562881 132.969) (layer F.SilkS))
  (gr_text A14 (at 176.81581 132.969) (layer F.SilkS))
  (gr_text A12 (at 176.81581 130.556) (layer F.SilkS))
  (gr_text A13 (at 186.562881 130.2385) (layer F.SilkS))
  (gr_text A11 (at 186.562881 127.762) (layer F.SilkS))
  (gr_text A9 (at 186.086691 125.095) (layer F.SilkS))
  (gr_text "A10\n" (at 176.81581 125.349) (layer F.SilkS))
  (gr_text A8 (at 177.292001 122.682) (layer F.SilkS))
  (gr_text A6 (at 177.292001 120.2055) (layer F.SilkS))
  (gr_text A7 (at 186.086691 120.269) (layer F.SilkS))
  (gr_text A5 (at 186.086691 117.7925) (layer F.SilkS))
  (gr_text A3 (at 186.086691 115.1255) (layer F.SilkS))
  (gr_text A4 (at 177.292001 115.189) (layer F.SilkS))
  (gr_text A1 (at 186.086691 110.1725) (layer F.SilkS))
  (gr_text A2 (at 177.292001 112.5855) (layer F.SilkS))
  (gr_text A0 (at 177.292001 109.982) (layer F.SilkS))
  (gr_text Address (at 181.641691 136.0805) (layer F.SilkS))
  (gr_text Data (at 180.562191 95.9485) (layer F.SilkS))
  (gr_text D1 (at 184.689691 82.6135) (layer F.SilkS))
  (gr_text D3 (at 184.689691 85.2805) (layer F.SilkS))
  (gr_text D5 (at 184.689691 87.5665) (layer F.SilkS))
  (gr_text D7 (at 184.689691 92.71) (layer F.SilkS))
  (gr_text D6 (at 176.180691 92.71) (layer F.SilkS))
  (gr_text D4 (at 176.180691 89.9795) (layer F.SilkS))
  (gr_text D2 (at 176.180691 84.8995) (layer F.SilkS))
  (gr_text D0 (at 176.180691 82.55) (layer F.SilkS))
  (gr_text BA1 (at 162.27431 104.2035) (layer F.SilkS))
  (gr_text BA0 (at 162.27431 101.5365) (layer F.SilkS))
  (gr_text RA6 (at 162.27431 96.4565) (layer F.SilkS))
  (gr_text BA8 (at 162.27431 121.92) (layer F.SilkS))
  (gr_text RA3 (at 162.27431 88.9635) (layer F.SilkS))
  (gr_text RA7 (at 162.27431 99.1235) (layer F.SilkS))
  (gr_text RA4 (at 162.27431 91.5035) (layer F.SilkS))
  (gr_text RA5 (at 162.27431 93.9165) (layer F.SilkS))
  (gr_text RA1 (at 162.27431 83.8835) (layer F.SilkS))
  (gr_text RA0 (at 162.27431 81.28) (layer F.SilkS))
  (gr_text RA2 (at 162.27431 86.36) (layer F.SilkS))
  (gr_text BA10 (at 154.559 127.0635) (layer F.SilkS))
  (gr_text BA9 (at 155.035191 124.3965) (layer F.SilkS))
  (gr_text BA8 (at 155.035191 121.92) (layer F.SilkS))
  (gr_text BA7 (at 155.035191 119.38) (layer F.SilkS))
  (gr_text BA6 (at 155.035191 116.84) (layer F.SilkS))
  (gr_text BA5 (at 155.035191 114.3) (layer F.SilkS))
  (gr_text BA4 (at 155.035191 111.8235) (layer F.SilkS))
  (gr_text BA3 (at 155.035191 109.1565) (layer F.SilkS))
  (gr_text BA2 (at 155.035191 106.7435) (layer F.SilkS))
  (gr_text BA1 (at 155.035191 104.2035) (layer F.SilkS))
  (gr_text RA7 (at 155.035191 99.1235) (layer F.SilkS))
  (gr_text BA0 (at 155.035191 101.5365) (layer F.SilkS))
  (gr_text RA6 (at 155.035191 96.4565) (layer F.SilkS))
  (gr_text RA5 (at 155.035191 93.9165) (layer F.SilkS))
  (gr_text RA4 (at 155.035191 91.5035) (layer F.SilkS))
  (gr_text RA3 (at 155.035191 88.9635) (layer F.SilkS))
  (gr_text RA2 (at 155.035191 86.36) (layer F.SilkS))
  (gr_text RA1 (at 155.035191 83.8835) (layer F.SilkS))
  (gr_text RA0 (at 155.035191 81.28) (layer F.SilkS))
  (gr_text RAMWE (at 129.4765 82.00219 -90) (layer F.SilkS))
  (gr_text 14M (at 152.2095 81.00219 -90) (layer F.SilkS))
  (gr_text CREF (at 144.8435 81.359333 -90) (layer F.SilkS))
  (gr_text CASA (at 136.9695 81.311714 -90) (layer F.SilkS))
  (gr_text RAS (at 132.08 80.883143 -90) (layer F.SilkS))
  (gr_text 7M (at 147.2565 80.526 -90) (layer F.SilkS))
  (gr_text PH# (at 139.573 81.00219 -90) (layer F.SilkS))
  (gr_text CASM (at 134.493 81.454571 -90) (layer F.SilkS))
  (gr_text 5V (at 149.733 80.383143 -90) (layer F.SilkS))
  (gr_text Q3 (at 142.1765 80.478381 -90) (layer F.SilkS))
  (gr_text MD5 (at 121.8565 73.66 -90) (layer F.SilkS))
  (gr_text MD2 (at 113.9825 73.66 -90) (layer F.SilkS))
  (gr_text MD0 (at 109.093 73.66 -90) (layer F.SilkS))
  (gr_text MD6 (at 124.2695 73.66 -90) (layer F.SilkS))
  (gr_text MD3 (at 116.586 73.66 -90) (layer F.SilkS))
  (gr_text MD1 (at 111.506 73.66 -90) (layer F.SilkS))
  (gr_text MD7 (at 126.746 73.66 -90) (layer F.SilkS))
  (gr_text MD4 (at 119.1895 73.66 -90) (layer F.SilkS))
  (gr_text MD7 (at 126.9365 81.026 -90) (layer F.SilkS))
  (gr_text MD6 (at 124.46 81.026 -90) (layer F.SilkS))
  (gr_text MD5 (at 122.047 81.026 -90) (layer F.SilkS))
  (gr_text MD4 (at 119.38 81.026 -90) (layer F.SilkS))
  (gr_text MD3 (at 116.7765 81.026 -90) (layer F.SilkS))
  (gr_text MD2 (at 114.173 81.026 -90) (layer F.SilkS))
  (gr_text MD1 (at 111.6965 81.026 -90) (layer F.SilkS))
  (gr_text MD0 (at 109.2835 81.026 -90) (layer F.SilkS))
  (gr_text Y0 (at 97.020072 96.7105) (layer F.SilkS))
  (gr_text Y1 (at 97.020072 99.314) (layer F.SilkS))
  (gr_text KSEL1 (at 95.61531 86.5505) (layer F.SilkS))
  (gr_text X0 (at 96.972453 91.6305) (layer F.SilkS))
  (gr_text X1 (at 96.972453 94.234) (layer F.SilkS))
  (gr_text MSW (at 96.305786 101.6635) (layer F.SilkS))
  (gr_text SERVID (at 95.329596 104.2035) (layer F.SilkS))
  (gr_text IRQ (at 96.662929 89.0905) (layer F.SilkS))
  (gr_text SPKR (at 95.948643 81.407) (layer F.SilkS))
  (gr_text KSEL2 (at 95.61531 83.947) (layer F.SilkS))
  (gr_text SPKR (at 104.521 81.407) (layer F.SilkS))
  (gr_text KSEL2 (at 104.854334 83.947) (layer F.SilkS))
  (gr_text IRQ (at 103.806715 89.0905) (layer F.SilkS))
  (gr_text MSW (at 104.163857 101.6635) (layer F.SilkS))
  (gr_text X1 (at 103.497191 94.234) (layer F.SilkS))
  (gr_text Y1 (at 103.449572 99.314) (layer F.SilkS))
  (gr_text Y0 (at 103.449572 96.7105) (layer F.SilkS))
  (gr_text KSEL1 (at 104.854334 86.5505) (layer F.SilkS))
  (gr_text X0 (at 103.497191 91.6305) (layer F.SilkS))
  (gr_text SERVID (at 105.140048 104.2035) (layer F.SilkS))
  (gr_text AD1 (at 96.520072 109.347) (layer F.SilkS))
  (gr_text AD6 (at 96.520072 121.92) (layer F.SilkS))
  (gr_text AD3 (at 96.520072 114.4905) (layer F.SilkS))
  (gr_text AD5 (at 96.520072 119.5705) (layer F.SilkS))
  (gr_text AD4 (at 96.520072 116.967) (layer F.SilkS))
  (gr_text AD0 (at 96.520072 106.807) (layer F.SilkS))
  (gr_text AD2 (at 96.520072 111.887) (layer F.SilkS))
  (gr_text AD7 (at 96.520072 124.46) (layer F.SilkS))
  (gr_text AD0 (at 103.949572 106.8705) (layer F.SilkS))
  (gr_text AD1 (at 103.949572 109.4105) (layer F.SilkS))
  (gr_text AD2 (at 103.949572 111.9505) (layer F.SilkS))
  (gr_text AD3 (at 103.949572 114.554) (layer F.SilkS))
  (gr_text AD4 (at 103.949572 117.0305) (layer F.SilkS))
  (gr_text AD5 (at 103.949572 119.634) (layer F.SilkS))
  (gr_text AD6 (at 103.949572 121.9835) (layer F.SilkS))
  (gr_text AD7 (at 103.949572 124.5235) (layer F.SilkS))
  (gr_text "RGB1\n" (at 92.3925 132.334) (layer F.SilkS))
  (gr_text RGB2 (at 92.3925 135.255) (layer F.SilkS))
  (gr_text RGB4 (at 92.3925 127.1905) (layer F.SilkS))
  (gr_text RGB8 (at 92.3925 129.667) (layer F.SilkS))
  (gr_text S3 (at 134.493 139.033547 -90) (layer F.SilkS))
  (gr_text S1 (at 129.413 139.033547 -90) (layer F.SilkS))
  (gr_text S5 (at 139.573 139.033547 -90) (layer F.SilkS))
  (gr_text RMBK (at 142.0495 140.152594 -90) (layer F.SilkS))
  (gr_text S2 (at 131.826 139.033547 -90) (layer F.SilkS))
  (gr_text S0 (at 126.8095 139.033547 -90) (layer F.SilkS))
  (gr_text WNDW (at 144.653 140.247832 -90) (layer F.SilkS))
  (gr_text S4 (at 136.906 139.033547 -90) (layer F.SilkS))
  (gr_text ROMEN (at 114.4905 130.937381 90) (layer F.SilkS))
  (gr_text RW (at 124.7775 132.437381 90) (layer F.SilkS))
  (gr_text DMA (at 116.9035 132.008809 90) (layer F.SilkS))
  (gr_text M2SEL (at 119.4435 131.127857 90) (layer F.SilkS))
  (gr_text INH (at 122.047 132.223095 90) (layer F.SilkS))
  (gr_text ~RES (at 109.2835 132.080238 90) (layer F.SilkS))
  (gr_text MDI-MDO (at 111.8235 129.985 90) (layer F.SilkS))
  (gr_text BA12 (at 150.876 143.518 270) (layer F.SilkS))
  (gr_text M2SEL (at 148.1455 144.018 270) (layer F.SilkS))
  (gr_text BA13 (at 154.8765 131.722928 -90) (layer F.SilkS))
  (gr_text BA14 (at 152.3365 131.722928 -90) (layer F.SilkS))
  (gr_text BA15 (at 149.606 131.722928 -90) (layer F.SilkS))
  (gr_text SYNC (at 147.193 131.675309 -90) (layer F.SilkS))
  (gr_text WNDW (at 144.78 131.437214 -90) (layer F.SilkS))
  (gr_text RMBK (at 142.1765 131.532452 -90) (layer F.SilkS))
  (gr_text S5 (at 139.7 132.6515 -90) (layer F.SilkS))
  (gr_text S4 (at 137.033 132.6515 -90) (layer F.SilkS))
  (gr_text S3 (at 134.62 132.6515 -90) (layer F.SilkS))
  (gr_text S2 (at 131.953 132.6515 -90) (layer F.SilkS))
  (gr_text S1 (at 129.54 132.6515 -90) (layer F.SilkS))
  (gr_text S0 (at 126.9365 132.6515 -90) (layer F.SilkS))
  (gr_text RGB8 (at 104.521 127.0635) (layer F.SilkS))
  (gr_text RGB4 (at 104.521 129.6035) (layer F.SilkS))
  (gr_text RGB2 (at 104.521 132.207) (layer F.SilkS))
  (gr_text ~RES (at 109.1565 139.509738 90) (layer F.SilkS))
  (gr_text MDI-MDO (at 111.6965 141.604976 90) (layer F.SilkS))
  (gr_text ROMEN (at 114.3635 140.652595 90) (layer F.SilkS))
  (gr_text DMA (at 116.7765 139.581166 90) (layer F.SilkS))
  (gr_text M2SEL (at 119.3165 140.462119 90) (layer F.SilkS))
  (gr_text INH (at 121.92 139.366881 90) (layer F.SilkS))
  (gr_text RW (at 124.6505 139.152595 90) (layer F.SilkS))
  (gr_text RW (at 105.6005 143.129024 90) (layer F.SilkS))
  (gr_text ~RES (at 102.997 143.486167 90) (layer F.SilkS))
  (gr_text IRQ (at 100.3935 143.3195 90) (layer F.SilkS))
  (gr_text 7M (at 147.955 70.8025) (layer F.SilkS))
  (gr_text CREF (at 144.907 70.80525) (layer F.SilkS))
  (gr_text Q3 (at 142.113 70.8025) (layer F.SilkS))
  (gr_text PH# (at 139.0015 70.8025) (layer F.SilkS))
  (gr_text 7 (at 112.903 43.053 -90) (layer F.SilkS))
  (gr_text PH# (at 156.21 44.378547 -90) (layer F.SilkS))
  (gr_text RA7 (at 151.3205 44.2595 -90) (layer F.SilkS))
  (gr_text RA6 (at 148.6535 44.2595 -90) (layer F.SilkS))
  (gr_text RA5 (at 146.2405 44.2595 -90) (layer F.SilkS))
  (gr_text RA4 (at 143.5735 44.2595 -90) (layer F.SilkS))
  (gr_text RA3 (at 138.4935 44.2595 -90) (layer F.SilkS))
  (gr_text RA2 (at 136.017 44.2595 -90) (layer F.SilkS))
  (gr_text RA1 (at 133.4135 44.2595 -90) (layer F.SilkS))
  (gr_text RA0 (at 128.3335 44.2595 -90) (layer F.SilkS))
  (gr_text AD0 (at 125.857 44.2595 -90) (layer F.SilkS))
  (gr_text AD1 (at 123.2535 44.2595 -90) (layer F.SilkS))
  (gr_text AD3 (at 118.11 44.2595 -90) (layer F.SilkS))
  (gr_text MD7 (at 151.13 34.671 90) (layer F.SilkS))
  (gr_text MD6 (at 148.463 34.671 90) (layer F.SilkS))
  (gr_text MD5 (at 145.923 34.671 90) (layer F.SilkS))
  (gr_text MD4 (at 140.843 34.671 90) (layer F.SilkS))
  (gr_text NC (at 130.81 35.687) (layer F.SilkS))
  (gr_text MD3 (at 138.2395 34.671 90) (layer F.SilkS))
  (gr_text MD2 (at 135.6995 34.671 90) (layer F.SilkS))
  (gr_text MD1 (at 128.143 34.671 90) (layer F.SilkS))
  (gr_text MD0 (at 125.6665 34.671 90) (layer F.SilkS))
  (gr_text AD2 (at 120.5865 34.528143 90) (layer F.SilkS))
  (gr_text AD4 (at 117.983 34.528143 90) (layer F.SilkS))
  (gr_text AD6 (at 115.443 34.528143 90) (layer F.SilkS))
  (gr_text 14M (at 108.0135 34.647191 90) (layer F.SilkS))
  (gr_text AB (at 175.895 99.949 90) (layer F.SilkS))
  (gr_text DIR (at 170.307 104.394) (layer F.SilkS))
  (gr_text EN (at 170.307 95.758) (layer F.SilkS))
  (gr_text 5V (at 164.846 98.171) (layer F.SilkS))
  (gr_text 5V (at 164.719 101.854) (layer F.SilkS))
  (gr_text 5V (at 175.768 39.116) (layer F.SilkS))
  (gr_text 5V (at 175.768 36.576) (layer F.SilkS))
  (gr_text Flip6 (at 169.545 69.088) (layer F.SilkS))
  (gr_text Flip7 (at 181.356 68.199 90) (layer F.SilkS))
  (gr_text 5V (at 170.307 74.295) (layer F.SilkS))
  (gr_text DB (at 181.102 75.946 90) (layer F.SilkS))
  (gr_text 5V (at 170.18 77.978) (layer F.SilkS))
  (gr_text DIR (at 175.768 80.264) (layer F.SilkS))
  (gr_text EN (at 175.768 71.628) (layer F.SilkS))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.381))
    (polygon
      (pts
        (xy 190.5 149.86) (xy 86.36 149.86) (xy 86.36 27.94) (xy 190.5 27.94)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.381))
    (polygon
      (pts
        (xy 190.5 149.86) (xy 86.36 149.86) (xy 86.36 27.94) (xy 190.5 27.94)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.381))
    (polygon
      (pts
        (xy 190.5 149.86) (xy 86.36 149.86) (xy 86.36 27.94) (xy 190.5 27.94)
      )
    )
  )
  (zone (net 131) (net_name +5V) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.381))
    (polygon
      (pts
        (xy 190.5 149.86) (xy 86.36 149.86) (xy 86.36 27.94) (xy 190.5 27.94)
      )
    )
  )
)
