(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 8)
    (no_connects 0)
    (area 125.117619 87.7795 188.781 114.6512)
    (thickness 1.6)
    (drawings 50)
    (tracks 80)
    (zones 0)
    (modules 24)
    (nets 9)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.5)
    (trace_clearance 0.2)
    (zone_clearance 0)
    (zone_45_only yes)
    (trace_min 0.127)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.2606 2.2606)
    (pad_drill 2.2606)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010e0_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(1NI1-Pad1)")
  (net 2 "Net-(1PI1-Pad1)")
  (net 3 "Net-(2NI1-Pad1)")
  (net 4 "Net-(2PI1-Pad1)")
  (net 5 "Net-(3NI1-Pad1)")
  (net 6 "Net-(3PI1-Pad1)")
  (net 7 "Net-(4NI1-Pad1)")
  (net 8 "Net-(4PI1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.5)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(1NI1-Pad1)")
    (add_net "Net-(1PI1-Pad1)")
    (add_net "Net-(2NI1-Pad1)")
    (add_net "Net-(2PI1-Pad1)")
    (add_net "Net-(3NI1-Pad1)")
    (add_net "Net-(3PI1-Pad1)")
    (add_net "Net-(4NI1-Pad1)")
    (add_net "Net-(4PI1-Pad1)")
  )
  (net_class "FAA board" ""
    (clearance 0.2)
    (trace_width 0.5)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module bribrary:normal_pads (layer F.Cu) (tedit 599E030F)
    (at 172.593 97.917 90)
    (fp_text reference 2PO1 (at 0.8255 10.668 90) (layer F.SilkS) hide)
    (fp_text value 2PO (at -2.9845 13.208 90) (layer F.Fab))
    (pad 1 smd rect (at -2.54 -3.81 90) (size 0.75 2.25) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(2PI1-Pad1)"))
  )
  (module bribrary:normal_pads (layer F.Cu) (tedit 598E13BA)
    (at 172.593 100.457 90)
    (fp_text reference 3PO1 (at -0.6985 9.398 90) (layer F.SilkS) hide)
    (fp_text value 3PO (at 1.2065 8.128 90) (layer F.Fab))
    (pad 1 smd rect (at -2.54 -3.81 90) (size 0.75 2.25) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(3PI1-Pad1)"))
  )
  (module bribrary:normal_pads (layer F.Cu) (tedit 599E02DD)
    (at 172.593 101.727 90)
    (fp_text reference 3NO1 (at -4.953 7.493 90) (layer F.SilkS) hide)
    (fp_text value 3NO (at -0.508 6.223 90) (layer F.Fab))
    (pad 1 smd rect (at -2.54 -3.81 90) (size 0.75 2.25) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(3NI1-Pad1)"))
  )
  (module bribrary:normal_pads (layer F.Cu) (tedit 598E13BC)
    (at 172.593 99.187 90)
    (fp_text reference 2NO1 (at -0.889 4.318 90) (layer F.SilkS) hide)
    (fp_text value 2NO (at 4.191 6.223 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -2.54 -3.81 90) (size 0.75 2.25) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(2NI1-Pad1)"))
  )
  (module bribrary:normal_pads (layer F.Cu) (tedit 599E0314)
    (at 172.593 95.377 90)
    (fp_text reference 1PO1 (at 3.683 5.588 90) (layer F.SilkS) hide)
    (fp_text value 1PO (at -0.127 8.763 90) (layer F.Fab))
    (pad 1 smd rect (at -2.54 -3.81 90) (size 0.75 2.25) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(1PI1-Pad1)"))
  )
  (module bribrary:normal_pads (layer F.Cu) (tedit 599E031D)
    (at 172.593 92.837 90)
    (fp_text reference 4PO1 (at 0.127 13.208 90) (layer F.SilkS) hide)
    (fp_text value 4PO (at -3.048 15.113 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -2.54 -3.81 90) (size 0.75 2.25) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(4PI1-Pad1)"))
  )
  (module bribrary:wire_bond_pad (layer F.Cu) (tedit 599E02FC)
    (at 155.4734 100.9904)
    (fp_text reference 1NI1 (at 24.2316 6.3246) (layer F.SilkS) hide)
    (fp_text value Ch1- (at -0.5334 -10.1854) (layer F.Fab))
    (pad 1 smd rect (at -0.9 -2) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(1NI1-Pad1)"))
  )
  (module bribrary:normal_pads (layer F.Cu) (tedit 599E0311)
    (at 172.593 96.647 90)
    (fp_text reference 1NO1 (at -1.2065 5.588 90) (layer F.SilkS) hide)
    (fp_text value 1NO (at 3.8735 8.128 90) (layer F.Fab))
    (pad 1 smd rect (at -2.54 -3.81 90) (size 0.75 2.25) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(1NI1-Pad1)"))
  )
  (module bribrary:wire_bond_pad (layer F.Cu) (tedit 599E02FF)
    (at 155.4734 99.3902)
    (fp_text reference 1PI1 (at 25.5016 9.1948) (layer F.SilkS) hide)
    (fp_text value Ch1+ (at -0.5334 -6.6802) (layer F.Fab))
    (pad 1 smd rect (at -0.9 -2) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(1PI1-Pad1)"))
  )
  (module bribrary:wire_bond_pad (layer F.Cu) (tedit 599E02F9)
    (at 155.4734 104.267)
    (fp_text reference 2NI1 (at 24.8666 1.143) (layer F.SilkS) hide)
    (fp_text value Ch2- (at 0.1016 2.413) (layer F.Fab))
    (pad 1 smd rect (at -0.9 -2) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(2NI1-Pad1)"))
  )
  (module bribrary:wire_bond_pad (layer F.Cu) (tedit 599E030C)
    (at 156.5656 99.7204 90)
    (fp_text reference 2PI1 (at -2.5146 27.5844 90) (layer F.SilkS) hide)
    (fp_text value Ch3+ (at -8.8646 -0.9906 180) (layer F.Fab))
    (pad 1 smd rect (at -0.9 -2 90) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(2PI1-Pad1)"))
  )
  (module bribrary:wire_bond_pad (layer F.Cu) (tedit 599E0309)
    (at 143.51 104.394)
    (fp_text reference 3NI1 (at 34.3154 5.9944) (layer F.SilkS) hide)
    (fp_text value Ch3- (at 0.0254 2.8194) (layer F.Fab))
    (pad 1 smd rect (at -0.9 -2) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(3NI1-Pad1)"))
  )
  (module bribrary:wire_bond_pad (layer F.Cu) (tedit 599E02D9)
    (at 143.51 102.616)
    (fp_text reference 3PI1 (at 31.7754 2.5908) (layer F.SilkS) hide)
    (fp_text value Ch3+ (at 0.0254 3.2258) (layer F.Fab))
    (pad 1 smd rect (at -0.9 -2) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(3PI1-Pad1)"))
  )
  (module bribrary:wire_bond_pad (layer F.Cu) (tedit 599E0318)
    (at 143.51 100.838)
    (fp_text reference 4NI1 (at 31.242 -9.7282) (layer F.SilkS) hide)
    (fp_text value Ch4- (at 0.127 -7.1882) (layer F.Fab))
    (pad 1 smd rect (at -0.9 -2) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(4NI1-Pad1)"))
  )
  (module bribrary:normal_pads (layer F.Cu) (tedit 598E13C3)
    (at 172.593 94.107 90)
    (fp_text reference 4NO1 (at 4.1275 11.938 90) (layer F.SilkS) hide)
    (fp_text value 4NO (at -2.8575 10.033 90) (layer F.Fab))
    (pad 1 smd rect (at -2.54 -3.81 90) (size 0.75 2.25) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(4NI1-Pad1)"))
  )
  (module bribrary:wire_bond_pad (layer F.Cu) (tedit 599E031A)
    (at 143.51 99.06)
    (fp_text reference 4PI1 (at 33.782 -9.2964) (layer F.SilkS) hide)
    (fp_text value Ch4+ (at 0.127 -6.7564) (layer F.Fab))
    (pad 1 smd rect (at -0.9 -2) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(4PI1-Pad1)"))
  )
  (module bribrary:2hole (layer F.Cu) (tedit 59B18B37)
    (at 128.27 107.442)
    (fp_text reference * (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value "#2 hole" (at 0 -0.5) (layer F.Fab))
    (pad "" thru_hole circle (at 0 0) (size 2.2606 2.2606) (drill 2.2606) (layers *.Cu *.Mask))
  )
  (module bribrary:0screw (layer F.Cu) (tedit 59B2CDA4)
    (at 162.941 91.948)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value "#0 screw" (at 0 -0.508) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6129 1.6129) (drill 1.6129) (layers *.Cu *.Mask))
  )
  (module bribrary:0screw (layer F.Cu) (tedit 599E02AE)
    (at 135.509 91.948)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value "#0 screw" (at 0 -0.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6129 1.6129) (drill 1.6129) (layers *.Cu *.Mask))
  )
  (module bribrary:0screw (layer F.Cu) (tedit 599E02B9)
    (at 135.509 107.442)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value "#0 screw" (at 0 -0.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6129 1.6129) (drill 1.6129) (layers *.Cu *.Mask))
  )
  (module bribrary:0screw (layer F.Cu) (tedit 599E02B4)
    (at 162.941 107.442)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value "#0 screw" (at 0 -0.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6129 1.6129) (drill 1.6129) (layers *.Cu *.Mask))
  )
  (module bribrary:supercdms_logo (layer F.Cu) (tedit 0)
    (at 153.543 113.157 180)
    (fp_text reference LOGO (at 0 5 180) (layer F.SilkS) hide)
    (fp_text value "" (at 0 0 180) (layer F.SilkS))
  )
  (module bribrary:0screw (layer F.Cu) (tedit 59971088)
    (at 168.783 107.315)
    (fp_text reference * (at 0 0.5) (layer F.SilkS))
    (fp_text value "#0 screw" (at 0 -0.5) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 1.6129 1.6129) (drill 1.6129) (layers *.Cu *.Mask))
  )
  (module bribrary:0screw (layer F.Cu) (tedit 59971088)
    (at 168.783 92.329)
    (fp_text reference * (at 0 0.5) (layer F.SilkS))
    (fp_text value "#0 screw" (at 0 -0.5) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 1.6129 1.6129) (drill 1.6129) (layers *.Cu *.Mask))
  )
  (gr_line (start 125.476 110.49) (end 170.18 110.49) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 125.476 104.648) (end 125.476 110.49) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 128.524 104.648) (end 125.476 104.648) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 128.524 89.154) (end 128.524 104.648) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 128.778 88.9) (end 128.524 89.154) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text "Detector Readout\nMk. 1.3.2\n" (at 148.209 90.932 180) (layer F.SilkS))
  (gr_text CH3- (at 153.416 109.474 180) (layer F.SilkS))
  (gr_text CH3+ (at 153.416 106.934 180) (layer F.SilkS))
  (gr_text CH4- (at 142.875 109.474 180) (layer F.SilkS))
  (gr_text CH4+ (at 143.002 106.934 180) (layer F.SilkS))
  (gr_text CH2- (at 153.416 92.583 180) (layer F.SilkS))
  (gr_text CH2+ (at 153.416 89.789 180) (layer F.SilkS))
  (gr_text CH1- (at 143.256 92.71 180) (layer F.SilkS))
  (gr_text "CH1+\n" (at 143.002 89.789 180) (layer F.SilkS))
  (gr_line (start 150.622 100.076) (end 150.622 101.6) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 151.257 100.076) (end 150.622 100.076) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 149.86 100.076) (end 151.257 100.076) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 149.225 101.346) (end 149.225 100.076) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 149.098 101.473) (end 149.225 101.346) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 148.971 101.6) (end 149.098 101.473) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 148.336 101.6) (end 148.971 101.6) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 148.082 101.346) (end 148.336 101.6) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 148.082 100.076) (end 148.082 101.346) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 147.574 100.33) (end 147.32 100.076) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 147.574 101.346) (end 147.574 100.33) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 147.32 101.6) (end 147.574 101.346) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 146.558 101.6) (end 147.32 101.6) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 146.304 101.346) (end 146.558 101.6) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 146.304 100.33) (end 146.304 101.346) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 146.558 100.076) (end 146.304 100.33) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 147.32 100.076) (end 146.558 100.076) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 150.749 96.52) (end 150.749 98.044) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 151.384 96.52) (end 150.749 96.52) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 150.114 96.52) (end 151.384 96.52) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 149.479 97.79) (end 149.479 96.52) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 149.225 98.044) (end 149.479 97.79) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 148.59 98.044) (end 149.225 98.044) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 148.336 97.79) (end 148.59 98.044) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 148.336 96.52) (end 148.336 97.79) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 146.812 98.044) (end 147.701 98.044) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 146.431 97.663) (end 146.812 98.044) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 146.431 96.901) (end 146.431 97.663) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 146.812 96.52) (end 146.431 96.901) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 147.701 96.52) (end 146.812 96.52) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 153.67 104.14) (end 153.67 95.25) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 153.67 95.25) (end 144.78 95.25) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 144.78 95.25) (end 144.78 104.14) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 144.78 104.14) (end 153.67 104.14) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 170.18 110.49) (end 170.18 88.9) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 170.18 88.9) (end 128.524 88.9) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 0) (net_name "") (layer B.Mask) (hatch edge 0.508)
    (connect_pads yes (clearance 0))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 10))
    (polygon
      (pts
        (xy 170.18 110.49) (xy 125.476 110.49) (xy 125.476 104.648) (xy 128.524 104.648) (xy 128.524 88.9)
        (xy 170.18 88.9)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads yes (clearance 0))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 10))
    (polygon
      (pts
        (xy 141.478 93.472) (xy 170.18 93.472) (xy 170.18 106.172) (xy 141.478 106.172) (xy 141.478 110.49)
        (xy 125.476 110.49) (xy 125.476 104.648) (xy 128.524 104.648) (xy 128.524 88.9) (xy 141.478 88.9)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 10))
    (polygon
      (pts
        (xy 170.18 110.49) (xy 125.476 110.49) (xy 125.476 104.648) (xy 128.524 104.648) (xy 128.524 88.9)
        (xy 170.18 88.9)
      )
    )
    (polygon
      (pts        (xy 143.51 93.98) (xy 143.51 105.41) (xy 154.94 105.41) (xy 154.94 93.98)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 10))
    (polygon
      (pts
        (xy 170.18 93.472) (xy 155.321 93.472) (xy 155.321 90.932) (xy 141.478 90.932) (xy 141.478 107.696)
        (xy 155.321 107.696) (xy 155.321 106.172) (xy 170.18 106.172) (xy 170.18 110.49) (xy 125.476 110.49)
        (xy 125.476 104.648) (xy 128.524 104.648) (xy 128.524 88.9) (xy 170.18 88.9)
      )
    )
  )
)
