(kicad_pcb (version 4) (host pcbnew 4.0.7-e2-6376~60~ubuntu17.10.1)
  (general
    (links 26)
    (no_connects 0)
    (area 171.374999 114.478999 200.227001 151.459001)
    (thickness 1.6)
    (drawings 21)
    (tracks 90)
    (zones 0)
    (modules 14)
    (nets 21)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.5)
    (user_trace_width 0.75)
    (user_trace_width 1)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J2-Pad1)")
  (net 2 "Net-(J2-Pad2)")
  (net 3 "Net-(J3-Pad1)")
  (net 4 "Net-(J3-Pad2)")
  (net 5 "Net-(J4-Pad1)")
  (net 6 "Net-(J4-Pad2)")
  (net 7 "Net-(J8-Pad1)")
  (net 8 "Net-(J8-Pad2)")
  (net 9 "Net-(J8-Pad3)")
  (net 10 "Net-(J8-Pad4)")
  (net 11 /+ve)
  (net 12 /-ve)
  (net 13 "Net-(J10-Pad1)")
  (net 14 "Net-(J10-Pad3)")
  (net 15 "Net-(J6-Pad2)")
  (net 16 "Net-(J10-Pad2)")
  (net 17 "Net-(J7-Pad2)")
  (net 18 "Net-(J9-Pad1)")
  (net 19 "Net-(J9-Pad2)")
  (net 20 "Net-(J9-Pad3)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /+ve)
    (add_net /-ve)
    (add_net "Net-(J10-Pad1)")
    (add_net "Net-(J10-Pad2)")
    (add_net "Net-(J10-Pad3)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(J3-Pad2)")
    (add_net "Net-(J4-Pad1)")
    (add_net "Net-(J4-Pad2)")
    (add_net "Net-(J6-Pad2)")
    (add_net "Net-(J7-Pad2)")
    (add_net "Net-(J8-Pad1)")
    (add_net "Net-(J8-Pad2)")
    (add_net "Net-(J8-Pad3)")
    (add_net "Net-(J8-Pad4)")
    (add_net "Net-(J9-Pad1)")
    (add_net "Net-(J9-Pad2)")
    (add_net "Net-(J9-Pad3)")
  )
  (net_class Heater ""
    (clearance 0.2)
    (trace_width 0.5)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module KiCad/Connectors_JST.pretty:JST_PH_B2B-PH-K_02x2.00mm_Straight (layer F.Cu) (tedit 5AAE9361)
    (at 189.738 137.414 90)
    (descr "JST PH series connector, B2B-PH-K, top entry type, through hole, Datasheet: http://www.jst-mfg.com/product/pdf/eng/ePH.pdf")
    (tags "connector jst ph")
    (fp_text reference J2 (at 5.08 0.508 180) (layer F.SilkS) hide)
    (fp_text value Thermistor (at 1.016 -3.302 90) (layer F.SilkS))
    (fp_text user %R (at 1 1.5 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.2 1.7) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 "Net-(J2-Pad1)"))
    (pad 2 thru_hole oval (at 2 0 90) (size 1.2 1.7) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 "Net-(J2-Pad2)"))
    (model Connectors_JST.3dshapes/JST_PH_B2B-PH-K_02x2.00mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiCad/Connectors_JST.pretty:JST_PH_B3B-PH-K_03x2.00mm_Straight (layer F.Cu) (tedit 5AAE8B3F)
    (at 174.625 142.494 90)
    (descr "JST PH series connector, B3B-PH-K, top entry type, through hole, Datasheet: http://www.jst-mfg.com/product/pdf/eng/ePH.pdf")
    (tags "connector jst ph")
    (fp_text reference J5 (at 7.112 0 180) (layer F.SilkS) hide)
    (fp_text value Probe (at 3.048 -5.334 90) (layer F.SilkS) hide)
    (fp_text user %R (at 2 1.5 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.2 1.7) (drill 0.7) (layers *.Cu *.Mask)
      (net 13 "Net-(J10-Pad1)"))
    (pad 2 thru_hole oval (at 2 0 90) (size 1.2 1.7) (drill 0.7) (layers *.Cu *.Mask)
      (net 14 "Net-(J10-Pad3)"))
    (pad 3 thru_hole oval (at 4 0 90) (size 1.2 1.7) (drill 0.7) (layers *.Cu *.Mask)
      (net 16 "Net-(J10-Pad2)"))
    (model Connectors_JST.3dshapes/JST_PH_B3B-PH-K_03x2.00mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiCad/Pin_Headers.pretty:Pin_Header_Straight_2x11_Pitch2.00mm (layer F.Cu) (tedit 5AAE8B22)
    (at 181.737 117.602)
    (descr "Through hole straight pin header, 2x11, 2.00mm pitch, double rows")
    (tags "Through hole pin header THT 2x11 2.00mm double row")
    (fp_text reference J9 (at 1 -2.12) (layer F.SilkS) hide)
    (fp_text value CONN_02X11 (at 1 22.12) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(J9-Pad1)"))
    (pad 2 thru_hole oval (at 2 0) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(J9-Pad2)"))
    (pad 3 thru_hole oval (at 0 2) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(J9-Pad3)"))
    (pad 4 thru_hole oval (at 2 2) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(J4-Pad2)"))
    (pad 5 thru_hole oval (at 0 4) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(J7-Pad2)"))
    (pad 6 thru_hole oval (at 2 4) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(J4-Pad1)"))
    (pad 7 thru_hole oval (at 0 6) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(J10-Pad2)"))
    (pad 8 thru_hole oval (at 2 6) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(J3-Pad2)"))
    (pad 9 thru_hole oval (at 0 8) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(J6-Pad2)"))
    (pad 10 thru_hole oval (at 2 8) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(J3-Pad1)"))
    (pad 11 thru_hole oval (at 0 10) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(J10-Pad1)"))
    (pad 12 thru_hole oval (at 2 10) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(J2-Pad2)"))
    (pad 13 thru_hole oval (at 0 12) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(J10-Pad3)"))
    (pad 14 thru_hole oval (at 2 12) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(J2-Pad1)"))
    (pad 15 thru_hole oval (at 0 14) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(J8-Pad1)"))
    (pad 16 thru_hole oval (at 2 14) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 /-ve))
    (pad 17 thru_hole oval (at 0 16) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(J8-Pad2)"))
    (pad 18 thru_hole oval (at 2 16) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 /-ve))
    (pad 19 thru_hole oval (at 0 18) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(J8-Pad3)"))
    (pad 20 thru_hole oval (at 2 18) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 /+ve))
    (pad 21 thru_hole oval (at 0 20) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(J8-Pad4)"))
    (pad 22 thru_hole oval (at 2 20) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 /+ve))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x11_Pitch2.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiCad/Connectors_JST.pretty:JST_XH_B02B-XH-A_02x2.50mm_Straight (layer F.Cu) (tedit 5AAE8B35)
    (at 189.23 147.828 90)
    (descr "JST XH series connector, B02B-XH-A, top entry type, through hole")
    (tags "connector jst xh tht top vertical 2.50mm")
    (fp_text reference J1 (at 5.842 0.508 180) (layer F.SilkS) hide)
    (fp_text value Heater (at 1.25 4.5 90) (layer F.SilkS) hide)
    (fp_text user %R (at 1.25 2.5 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask)
      (net 11 /+ve))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask)
      (net 12 /-ve))
    (model Connectors_JST.3dshapes/JST_XH_B02B-XH-A_02x2.50mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiCad/Connectors_JST.pretty:JST_PH_B3B-PH-K_03x2.00mm_Straight (layer F.Cu) (tedit 5AAE8B1E)
    (at 174.625 122.682 90)
    (descr "JST PH series connector, B3B-PH-K, top entry type, through hole, Datasheet: http://www.jst-mfg.com/product/pdf/eng/ePH.pdf")
    (tags "connector jst ph")
    (fp_text reference J7 (at 7.112 0.254 180) (layer F.SilkS) hide)
    (fp_text value "X Min ES" (at 2.032 -5.334 90) (layer F.SilkS) hide)
    (fp_text user %R (at 2 1.5 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.2 1.7) (drill 0.7) (layers *.Cu *.Mask)
      (net 13 "Net-(J10-Pad1)"))
    (pad 2 thru_hole oval (at 2 0 90) (size 1.2 1.7) (drill 0.7) (layers *.Cu *.Mask)
      (net 17 "Net-(J7-Pad2)"))
    (pad 3 thru_hole oval (at 4 0 90) (size 1.2 1.7) (drill 0.7) (layers *.Cu *.Mask)
      (net 16 "Net-(J10-Pad2)"))
    (model Connectors_JST.3dshapes/JST_PH_B3B-PH-K_03x2.00mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiCad/Connectors_JST.pretty:JST_PH_B2B-PH-K_02x2.00mm_Straight (layer F.Cu) (tedit 5AAE9367)
    (at 189.738 129.032 90)
    (descr "JST PH series connector, B2B-PH-K, top entry type, through hole, Datasheet: http://www.jst-mfg.com/product/pdf/eng/ePH.pdf")
    (tags "connector jst ph")
    (fp_text reference J3 (at 5.08 0.508 180) (layer F.SilkS) hide)
    (fp_text value "FAN 1" (at 1.016 -3.302 90) (layer F.SilkS))
    (fp_text user %R (at 1 1.5 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.2 1.7) (drill 0.7) (layers *.Cu *.Mask)
      (net 3 "Net-(J3-Pad1)"))
    (pad 2 thru_hole oval (at 2 0 90) (size 1.2 1.7) (drill 0.7) (layers *.Cu *.Mask)
      (net 4 "Net-(J3-Pad2)"))
    (model Connectors_JST.3dshapes/JST_PH_B2B-PH-K_02x2.00mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiCad/Connectors_JST.pretty:JST_PH_B2B-PH-K_02x2.00mm_Straight (layer F.Cu) (tedit 5AAE8B25)
    (at 189.738 120.65 90)
    (descr "JST PH series connector, B2B-PH-K, top entry type, through hole, Datasheet: http://www.jst-mfg.com/product/pdf/eng/ePH.pdf")
    (tags "connector jst ph")
    (fp_text reference J4 (at 5.588 0.254 180) (layer F.SilkS) hide)
    (fp_text value "FAN 2 (PWM)" (at 1 3.8 90) (layer F.SilkS) hide)
    (fp_text user %R (at 1 1.5 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.2 1.7) (drill 0.7) (layers *.Cu *.Mask)
      (net 5 "Net-(J4-Pad1)"))
    (pad 2 thru_hole oval (at 2 0 90) (size 1.2 1.7) (drill 0.7) (layers *.Cu *.Mask)
      (net 6 "Net-(J4-Pad2)"))
    (model Connectors_JST.3dshapes/JST_PH_B2B-PH-K_02x2.00mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiCad/Connectors_JST.pretty:JST_PH_B3B-PH-K_03x2.00mm_Straight (layer F.Cu) (tedit 5AAE8B44)
    (at 174.625 132.588 90)
    (descr "JST PH series connector, B3B-PH-K, top entry type, through hole, Datasheet: http://www.jst-mfg.com/product/pdf/eng/ePH.pdf")
    (tags "connector jst ph")
    (fp_text reference J6 (at 7.112 0 180) (layer F.SilkS) hide)
    (fp_text value "X Max ES" (at 2.032 -5.334 90) (layer F.SilkS) hide)
    (fp_text user %R (at 2 1.5 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.2 1.7) (drill 0.7) (layers *.Cu *.Mask)
      (net 13 "Net-(J10-Pad1)"))
    (pad 2 thru_hole oval (at 2 0 90) (size 1.2 1.7) (drill 0.7) (layers *.Cu *.Mask)
      (net 15 "Net-(J6-Pad2)"))
    (pad 3 thru_hole oval (at 4 0 90) (size 1.2 1.7) (drill 0.7) (layers *.Cu *.Mask)
      (net 16 "Net-(J10-Pad2)"))
    (model Connectors_JST.3dshapes/JST_PH_B3B-PH-K_03x2.00mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiCad/Connectors_JST.pretty:JST_PH_B4B-PH-K_04x2.00mm_Straight (layer F.Cu) (tedit 5AAE987A)
    (at 196.596 136.398 90)
    (descr "JST PH series connector, B4B-PH-K, top entry type, through hole, Datasheet: http://www.jst-mfg.com/product/pdf/eng/ePH.pdf")
    (tags "connector jst ph")
    (fp_text reference J8 (at 3.048 -2.794 90) (layer F.SilkS) hide)
    (fp_text value Stepper (at 3.302 -2.794 90) (layer F.SilkS))
    (fp_text user %R (at 3 1.5 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.2 1.7) (drill 0.7) (layers *.Cu *.Mask)
      (net 7 "Net-(J8-Pad1)"))
    (pad 2 thru_hole oval (at 2 0 90) (size 1.2 1.7) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 "Net-(J8-Pad2)"))
    (pad 3 thru_hole oval (at 4 0 90) (size 1.2 1.7) (drill 0.7) (layers *.Cu *.Mask)
      (net 9 "Net-(J8-Pad3)"))
    (pad 4 thru_hole oval (at 6 0 90) (size 1.2 1.7) (drill 0.7) (layers *.Cu *.Mask)
      (net 10 "Net-(J8-Pad4)"))
    (model Connectors_JST.3dshapes/JST_PH_B4B-PH-K_04x2.00mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiCad/Pin_Headers.pretty:Pin_Header_Straight_1x03_Pitch2.54mm (layer B.Cu) (tedit 5AAE8B47)
    (at 178.816 147.447 270)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J10 (at 0 2.39 270) (layer B.SilkS) hide)
    (fp_text value PP20 (at 0 -7.47 270) (layer B.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(J10-Pad1)"))
    (pad 2 thru_hole oval (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(J10-Pad2)"))
    (pad 3 thru_hole oval (at 0 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(J10-Pad3)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 -0.2 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module KiCad/Mounting_Holes.pretty:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5AAECA06)
    (at 196.596 118.237)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module KiCad/Mounting_Holes.pretty:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5AAECA0A)
    (at 196.596 118.237)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module KiCad/Mounting_Holes.pretty:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5AAEC9EB)
    (at 196.596 147.828)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module KiCad/Mounting_Holes.pretty:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5AAEC9F0)
    (at 196.596 147.828)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (gr_line (start 171.45 149.098) (end 171.45 114.554) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 179.959 149.098) (end 171.45 149.098) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 185.293 149.098) (end 179.959 149.098) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 185.293 151.384) (end 185.293 149.098) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 200.152 151.384) (end 185.293 151.384) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 171.45 114.554) (end 200.152 114.554) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 200.152 114.554) (end 200.152 151.384) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text - (at 179.07 128.524 90) (layer F.SilkS))
  (gr_text S (at 183.769 145.034 180) (layer B.SilkS))
  (gr_text + (at 178.308 145.161) (layer B.SilkS))
  (gr_text - (at 181.229 145.288 180) (layer B.SilkS))
  (gr_text Heater (at 189.738 141.478) (layer F.SilkS))
  (gr_text "FAN 2 (PWM)" (at 186.436 120.65 90) (layer F.SilkS))
  (gr_text - (at 179.07 138.43 90) (layer F.SilkS))
  (gr_text - (at 178.816 118.618 90) (layer F.SilkS))
  (gr_text S (at 178.816 120.65 90) (layer F.SilkS))
  (gr_text S (at 179.324 140.208 90) (layer F.SilkS))
  (gr_text S (at 179.07 130.556 90) (layer F.SilkS))
  (gr_text + (at 179.324 142.494 90) (layer F.SilkS))
  (gr_text + (at 179.07 132.588 90) (layer F.SilkS))
  (gr_text + (at 178.816 122.682 90) (layer F.SilkS))
  (zone (net 16) (net_name "Net-(J10-Pad2)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 200.279 151.384) (xy 185.293 151.384) (xy 185.293 149.098) (xy 180.086 149.098) (xy 179.959 149.098)
        (xy 171.45 149.098) (xy 171.577 114.554) (xy 200.279 114.554)
      )
    )
  )
  (zone (net 16) (net_name "Net-(J10-Pad2)") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 200.152 151.384) (xy 185.293 151.384) (xy 185.293 149.098) (xy 179.959 149.098) (xy 171.45 149.098)
        (xy 171.45 114.554) (xy 200.152 114.554)
      )
    )
  )
)
