(kicad_pcb (version 4) (host pcbnew 4.0.7+dfsg1-1~bpo8+1)
  (general
    (links 28)
    (no_connects 0)
    (area 126.924999 55.68283 152.475001 79.7934)
    (thickness 1.6)
    (drawings 66)
    (tracks 103)
    (zones 0)
    (modules 14)
    (nets 14)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal hide)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.254)
    (trace_clearance 0.1524)
    (zone_clearance 0.1778)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.6858)
    (uvia_drill 0.3302)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.032 0.75)
    (pad_drill 0)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFF77F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(BT1-Pad1)")
  (net 3 "Net-(C1-Pad1)")
  (net 4 "Net-(C2-Pad1)")
  (net 5 "Net-(C3-Pad1)")
  (net 6 "Net-(C3-Pad2)")
  (net 7 +9V)
  (net 8 "Net-(D1-Pad2)")
  (net 9 "Net-(J1-Pad1)")
  (net 10 "Net-(J2-Pad2)")
  (net 11 "Net-(LS1-Pad1)")
  (net 12 "Net-(R2-Pad2)")
  (net 13 "Net-(SW1-Pad3)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.254)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (add_net +9V)
    (add_net GND)
    (add_net "Net-(BT1-Pad1)")
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C3-Pad2)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(LS1-Pad1)")
    (add_net "Net-(R2-Pad2)")
    (add_net "Net-(SW1-Pad3)")
  )
  (module slide_sw:batt9v_pcb (layer B.Cu) (tedit 5AB1BEC9)
    (at 139.7 70.104)
    (fp_text reference BT1 (at 0.05 -3.35) (layer B.SilkS) hide)
    (fp_text value 9VCC (at 0.05 8.3) (layer B.Fab) hide)
    (fp_text user - (at 6.604 5.842) (layer B.SilkS))
    (fp_text user + (at -6.604 6.096) (layer B.SilkS))
    (pad 2 thru_hole rect (at 11.7 0.05) (size 1 3) (drill 0.76) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole rect (at 1.15 0.05) (size 1 3) (drill 0.76) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole rect (at 6.45 4.55) (size 3 1) (drill 0.76) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at -6.55 4.55) (size 3 1) (drill 0.76) (layers *.Cu *.Mask)
      (net 2 "Net-(BT1-Pad1)"))
    (pad 1 thru_hole rect (at -1.4 0.05) (size 1 3) (drill 0.76) (layers *.Cu *.Mask)
      (net 2 "Net-(BT1-Pad1)"))
    (pad 1 thru_hole rect (at -11.7 0.05) (size 1 3) (drill 0.76) (layers *.Cu *.Mask)
      (net 2 "Net-(BT1-Pad1)"))
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5AB093B5)
    (at 128.778 64.77 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 0 1.778 90) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.75 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 1.778 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5AB0944B)
    (at 150.876 64.77 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at 0 1.524 270) (layer F.SilkS))
    (fp_text value 10pF (at 0 1.75 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 1.524 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_0805 (layer F.Cu) (tedit 5AB1A54F)
    (at 144.59712 58.35904 270)
    (descr "Diode SMD in 0805 package http://datasheets.avx.com/schottky.pdf")
    (tags "smd diode")
    (attr smd)
    (fp_text reference D1 (at -0.26416 -1.7272 270) (layer F.SilkS))
    (fp_text value 300mV (at 0 1.7 270) (layer F.Fab) hide)
    (fp_text user %R (at -0.26416 -1.7272 270) (layer F.Fab))
    (pad 1 smd rect (at -1.05 0 270) (size 0.8 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 +9V))
    (pad 2 smd rect (at 1.05 0 270) (size 0.8 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.00mm (layer F.Cu) (tedit 5AB1C369)
    (at 146.304 60.706 90)
    (descr "Through hole straight pin header, 1x02, 2.00mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.00mm single row")
    (fp_text reference J1 (at -0.254 3.81 180) (layer F.SilkS) hide)
    (fp_text value LED (at 0 4.06 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 1 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(J1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.00mm (layer F.Cu) (tedit 5AB1A74C)
    (at 131.12496 60.83808 90)
    (descr "Through hole straight pin header, 1x02, 2.00mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.00mm single row")
    (fp_text reference J2 (at 1.73736 1.143 180) (layer F.SilkS))
    (fp_text value LDR (at 0 4.06 90) (layer F.Fab) hide)
    (fp_text user %R (at 1.73736 1.143 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 +9V))
    (pad 2 thru_hole oval (at 0 2 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(J2-Pad2)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5AB09436)
    (at 146.05 63.246 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 1.778 1.524 180) (layer F.SilkS))
    (fp_text value 100 (at 0 1.75 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(J1-Pad1)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 7 +9V))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5AB1B1DC)
    (at 133.35 63.246)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 1.778 -1.27) (layer F.SilkS))
    (fp_text value 100 (at 0 1.75) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(R2-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Potentiometers:Potentiometer_Trimmer_VishaySpectrol_Econtrim-Type36M (layer B.Cu) (tedit 5AB1C039)
    (at 135.636 70.866 180)
    (descr "Potentiometer, Trimmer, Spectrol Type 36M, Econtrim, Rev A, 02 Aug 2010,")
    (tags "Potentiometer Trimmer Spectrol Type 36M Econtrim Rev A 02 Aug 2010 ")
    (fp_text reference RV1 (at 2.5 7.3 180) (layer B.SilkS) hide)
    (fp_text value 1K (at 2.5 -2.35 180) (layer B.Fab) hide)
    (pad 2 thru_hole circle (at 2.5 5 180) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 "Net-(C1-Pad1)"))
    (pad 3 thru_hole circle (at 5 0 180) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 "Net-(C1-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 10 "Net-(J2-Pad2)"))
  )
  (module Potentiometers:Potentiometer_Trimmer_VishaySpectrol_Econtrim-Type36M (layer B.Cu) (tedit 5AB1C041)
    (at 148.844 71.12 180)
    (descr "Potentiometer, Trimmer, Spectrol Type 36M, Econtrim, Rev A, 02 Aug 2010,")
    (tags "Potentiometer Trimmer Spectrol Type 36M Econtrim Rev A 02 Aug 2010 ")
    (fp_text reference RV2 (at 2.5 7.3 180) (layer B.SilkS) hide)
    (fp_text value 200 (at 2.5 -2.35 180) (layer B.Fab) hide)
    (pad 2 thru_hole circle (at 2.5 5 180) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 11 "Net-(LS1-Pad1)"))
    (pad 3 thru_hole circle (at 5 0 180) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 6 "Net-(C3-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 11 "Net-(LS1-Pad1)"))
  )
  (module slide_sw:slide_sw_spdt (layer F.Cu) (tedit 5AB09368)
    (at 138.938 56.896 180)
    (fp_text reference SW1 (at 3.048 -3.81 180) (layer F.SilkS))
    (fp_text value SPDT (at -0.05 -6.3 180) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.85 -3.75 180) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(BT1-Pad1)"))
    (pad 3 smd rect (at -1.15 -3.75 180) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(SW1-Pad3)"))
    (pad "" np_thru_hole circle (at 3.15 0 180) (size 0.86 0.86) (drill 0.8) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -3.15 0 180) (size 0.86 0.86) (drill 0.8) (layers *.Cu *.Mask))
    (pad 1 smd rect (at -3.15 -3.75 180) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D1-Pad2)"))
  )
  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 5AB1C4C5)
    (at 139.7 65.024)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U1 (at -4.064 3.048) (layer F.SilkS) hide)
    (fp_text value ICM7555 (at 0 3.5) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C1-Pad1)"))
    (pad 3 smd rect (at -2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(R2-Pad2)"))
    (pad 4 smd rect (at -2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 +9V))
    (pad 5 smd rect (at 2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C2-Pad1)"))
    (pad 6 smd rect (at 2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C1-Pad1)"))
    (pad 7 smd rect (at 2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(J2-Pad2)"))
    (pad 8 smd rect (at 2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 +9V))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module slide_sw:spkr_8 (layer F.Cu) (tedit 5AB1B726)
    (at 139.7 77.216 180)
    (fp_text reference LS1 (at 5.842 1.016 180) (layer F.SilkS))
    (fp_text value 8OHM (at -0.05 -1.55 180) (layer F.Fab) hide)
    (pad 2 smd rect (at 5.207 -0.0762 180) (size 2.032 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -5.3848 -0.1016 180) (size 2.032 0.75) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(LS1-Pad1)"))
  )
  (module Capacitors_Tantalum_SMD:CP_Tantalum_Case-B_EIA-3528-21_Hand (layer F.Cu) (tedit 5AB1A351)
    (at 139.7 74.422)
    (descr "Tantalum capacitor, Case B, EIA 3528-21, 3.5x2.8x1.9mm, Hand soldering footprint")
    (tags "capacitor tantalum smd")
    (attr smd)
    (fp_text reference C3 (at 4.826 1.778) (layer F.SilkS))
    (fp_text value 15uF (at 0 3.15) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2.15 0) (size 3.2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 2.15 0) (size 3.2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C3-Pad2)"))
    (model Capacitors_Tantalum_SMD.3dshapes/CP_Tantalum_Case-B_EIA-3528-21.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text 555 (at 136.8552 68.1736) (layer F.SilkS))
  (gr_text LDR (at 129.159 61.7474) (layer F.SilkS))
  (gr_text LED (at 150.2664 61.7728) (layer F.SilkS))
  (gr_text Pitch (at 133.096 63.246) (layer B.SilkS))
  (gr_text Volume (at 146.304 63.5) (layer B.SilkS))
  (gr_text REV: (at 137.414 77.47) (layer B.SilkS))
  (gr_text SN: (at 145.796 77.47) (layer B.SilkS))
  (gr_text "MADE IN:\nNutley - U.S.A" (at 139.065 61.1378) (layer B.SilkS))
  (gr_text SOUNDSTER (at 139.9032 58.6486) (layer B.SilkS))
  (gr_line (start 127.6858 71.4248) (end 128.2954 71.4248) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 127.6858 68.8594) (end 128.2954 68.8594) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 151.0792 71.4248) (end 151.7142 71.4248) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 151.0792 68.8594) (end 151.7142 68.8594) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 141.1732 68.8594) (end 141.1732 68.8848) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 140.5382 68.8594) (end 141.1732 68.8594) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 140.5382 71.4248) (end 141.1732 71.4248) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 140.5382 68.8594) (end 140.5382 71.4248) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 137.9728 68.8848) (end 138.6332 68.8848) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 137.9728 71.4502) (end 138.6332 71.4502) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 147.4724 74.3204) (end 147.4724 74.9808) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 144.8308 74.3204) (end 144.8308 74.9808) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 147.4724 74.9808) (end 144.8308 74.9808) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 144.8308 74.3204) (end 147.4724 74.3204) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 131.826 74.3204) (end 131.826 74.9808) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 134.4676 74.3204) (end 134.4676 74.9808) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 134.4676 74.9808) (end 131.826 74.9808) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 131.826 74.3204) (end 134.4676 74.3204) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 151.7142 71.4248) (end 151.7142 68.8594) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 151.0792 68.8594) (end 151.0792 71.4248) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 141.1732 71.4248) (end 141.1732 68.8594) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 137.9728 68.8848) (end 137.9728 71.4502) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 138.6332 71.4502) (end 138.6332 68.8848) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 128.2954 68.8594) (end 128.2954 68.8848) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 128.2954 68.8594) (end 128.2954 68.8848) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 128.2954 68.8594) (end 128.2954 68.8848) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 128.2954 68.8594) (end 128.2954 68.8848) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 128.2954 68.8594) (end 128.2954 68.8848) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 128.2954 68.8594) (end 128.2954 68.8848) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 128.2954 68.8594) (end 128.2954 68.8848) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 128.2954 68.8594) (end 128.2954 68.8848) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 128.2954 68.8594) (end 128.2954 68.8848) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 128.2954 68.8594) (end 128.2954 68.8848) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 128.2954 68.8594) (end 128.2954 68.8848) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 128.2954 68.8594) (end 128.2954 68.8848) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 128.2954 68.8594) (end 128.2954 68.8848) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 128.2954 68.8594) (end 128.2954 68.8848) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 128.2954 68.8594) (end 128.2954 68.8848) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 128.2954 68.8594) (end 128.2954 68.8848) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 127.6858 71.4248) (end 127.6858 68.8594) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 128.2954 68.8594) (end 128.2954 71.4248) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 146.05 55.88) (end 133.35 55.88) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 152.4 62.23) (end 146.05 55.88) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 152.4 72.39) (end 152.4 62.23) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 146.05 78.74) (end 152.4 72.39) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 133.35 78.74) (end 146.05 78.74) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 127 72.39) (end 133.35 78.74) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 127 62.23) (end 127 72.39) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 133.35 55.88) (end 127 62.23) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch none 0.508)
    (connect_pads (clearance 0.1778))
    (min_thickness 0.1524)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing chamfer))
    (polygon
      (pts
        (xy 127.254 62.23) (xy 127.254 72.39) (xy 133.35 78.486) (xy 146.05 78.486) (xy 152.146 72.39)
        (xy 152.146 62.23) (xy 146.05 56.134) (xy 133.35 56.134)
      )
    )
  )
  (zone (net 7) (net_name +9V) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1778))
    (min_thickness 0.1524)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 152.146 62.23) (xy 152.146 72.39) (xy 146.05 78.486) (xy 133.35 78.486) (xy 127.254 72.39)
        (xy 127.254 62.23) (xy 133.35 56.134) (xy 146.05 56.134)
      )
    )
  )
)
