<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.0">
<drawing>
<board>
<plain>
<wire x1="8.8" y1="2.54" x2="12.065" y2="0" width="0.1016" layer="20" curve="90"/>
<wire x1="8.255" y1="63.5" x2="5.715" y2="60.96" width="0.1016" layer="20" curve="90"/>
<wire x1="5.715" y1="60.96" x2="8.8" y2="2.54" width="0.1016" layer="20"/>
<wire x1="63.5" y1="60.96" x2="60.96" y2="63.5" width="0.1016" layer="20" curve="90"/>
<wire x1="57.63" y1="0" x2="60.42" y2="2.54" width="0.1016" layer="20" curve="90"/>
<wire x1="60.42" y1="2.54" x2="63.5" y2="60.96" width="0.1016" layer="20"/>
<wire x1="12.065" y1="0" x2="57.63" y2="0" width="0.1016" layer="20"/>
<wire x1="8.255" y1="63.5" x2="19.3" y2="63.5" width="0.1016" layer="20"/>
<wire x1="19.3" y1="63.5" x2="19.3" y2="67.3" width="0.1016" layer="20"/>
<wire x1="22.6" y1="67.3" x2="22.6" y2="63.5" width="0.1016" layer="20"/>
<wire x1="22.6" y1="63.5" x2="48.3" y2="63.5" width="0.1016" layer="20"/>
<wire x1="52.15" y1="63.5" x2="60.96" y2="63.5" width="0.1016" layer="20"/>
<wire x1="15.605" y1="11.43" x2="15.605" y2="6.35" width="0.1016" layer="20" curve="180"/>
<wire x1="19.415" y1="6.35" x2="19.415" y2="11.43" width="0.1016" layer="20" curve="180"/>
<wire x1="15.605" y1="11.43" x2="19.415" y2="11.43" width="0.1016" layer="20"/>
<wire x1="19.415" y1="6.35" x2="15.605" y2="6.35" width="0.1016" layer="20"/>
<wire x1="51.22" y1="53.87" x2="56.3" y2="53.87" width="0.1016" layer="20" curve="180"/>
<wire x1="56.3" y1="58.95" x2="51.22" y2="58.95" width="0.1016" layer="20" curve="180"/>
<wire x1="51.22" y1="53.87" x2="51.22" y2="58.95" width="0.1016" layer="20"/>
<wire x1="56.3" y1="58.95" x2="56.3" y2="53.87" width="0.1016" layer="20"/>
<wire x1="19.3" y1="67.3" x2="12.9" y2="67.3" width="0.1016" layer="20"/>
<wire x1="12.9" y1="67.3" x2="12.3" y2="67.9" width="0.1016" layer="20"/>
<wire x1="12.3" y1="67.9" x2="12.3" y2="87.665" width="0.1016" layer="20"/>
<wire x1="12.3" y1="87.665" x2="13" y2="88.365" width="0.1016" layer="20"/>
<wire x1="13" y1="88.365" x2="16.665" y2="88.365" width="0.1016" layer="20"/>
<wire x1="16.665" y1="88.365" x2="17.5" y2="89.2" width="0.1016" layer="20" curve="90"/>
<wire x1="17.5" y1="89.2" x2="17.5" y2="91.1" width="0.1016" layer="20"/>
<wire x1="17.5" y1="91.1" x2="20.2" y2="93.6" width="0.1016" layer="20" curve="-90"/>
<wire x1="20.2" y1="93.6" x2="20.6" y2="93.6" width="0.1016" layer="20"/>
<wire x1="20.6" y1="93.6" x2="23.1" y2="91.5" width="0.1016" layer="20" curve="-90"/>
<wire x1="23.1" y1="91.5" x2="23.1" y2="89.5" width="0.1016" layer="20"/>
<wire x1="23.1" y1="89.5" x2="23.9" y2="88.465" width="0.1016" layer="20" curve="90"/>
<wire x1="23.9" y1="88.465" x2="30.7" y2="88.465" width="0.1016" layer="20"/>
<wire x1="30.7" y1="88.465" x2="31.6" y2="87.565" width="0.1016" layer="20"/>
<wire x1="31.6" y1="87.565" x2="31.6" y2="78.1" width="0.1016" layer="20"/>
<wire x1="31.6" y1="78.1" x2="32.7" y2="77" width="0.1016" layer="20"/>
<wire x1="32.7" y1="77" x2="32.7" y2="68.9" width="0.1016" layer="20"/>
<wire x1="32.7" y1="68.9" x2="31.2" y2="67.3" width="0.1016" layer="20"/>
<wire x1="31.2" y1="67.3" x2="22.6" y2="67.3" width="0.1016" layer="20"/>
<wire x1="40.12" y1="79.995" x2="49.73" y2="90.14" width="0.1016" layer="20" curve="-90"/>
<wire x1="49.73" y1="90.14" x2="59.59" y2="80.345" width="0.1016" layer="20" curve="-90"/>
<wire x1="56.08" y1="67.83" x2="56.915" y2="68.465" width="0.1016" layer="20" curve="90"/>
<wire x1="56.915" y1="68.465" x2="56.915" y2="73.445" width="0.1016" layer="20"/>
<wire x1="56.08" y1="67.83" x2="52.15" y2="67.83" width="0.1016" layer="20"/>
<wire x1="52.15" y1="67.83" x2="52.15" y2="63.5" width="0.1016" layer="20"/>
<wire x1="48.3" y1="63.5" x2="48.3" y2="67.83" width="0.1016" layer="20"/>
<wire x1="48.3" y1="67.83" x2="43.58" y2="67.83" width="0.1016" layer="20"/>
<wire x1="43.58" y1="67.83" x2="42.945" y2="68.465" width="0.1016" layer="20" curve="-90"/>
<wire x1="42.945" y1="68.465" x2="42.945" y2="73.545" width="0.1016" layer="20"/>
<wire x1="59.59" y1="80.345" x2="56.915" y2="73.445" width="0.1016" layer="20" curve="-39.093859"/>
<wire x1="40.12" y1="79.995" x2="42.945" y2="73.545" width="0.1016" layer="20" curve="39"/>
<hole x="19.7" y="63.9" drill="0.5"/>
<hole x="20.5" y="63.9" drill="0.5"/>
<hole x="21.4" y="63.9" drill="0.5"/>
<hole x="22.2" y="63.9" drill="0.5"/>
<hole x="22.2" y="67" drill="0.5"/>
<hole x="21.3" y="67" drill="0.5"/>
<hole x="20.5" y="67" drill="0.5"/>
<hole x="19.7" y="67" drill="0.5"/>
<text>Yowie Wah</text>
<text>v 1.0
</text>
<text>graybloomfield.com/guitar
</text>
<text>2018
</text>
<hole x="48.75" y="63.75" drill="0.4"/>
<hole x="49.5" y="63.75" drill="0.4"/>
<hole x="50.25" y="63.75" drill="0.4"/>
<hole x="51" y="63.75" drill="0.4"/>
<hole x="51.75" y="63.75" drill="0.4"/>
<hole x="51.75" y="67.5" drill="0.4"/>
<hole x="51" y="67.5" drill="0.4"/>
<hole x="50.25" y="67.5" drill="0.4"/>
<hole x="49.5" y="67.5" drill="0.4"/>
<hole x="48.75" y="67.5" drill="0.4"/>
</plain>
<libraries>
<library name="jacks">
<packages>
<package name="DC_TS">
</package>
</packages>
</library>
<library name="resistors">
<packages>
<package name="0.3&quot;.B">
<description>0.3"  (7.62mm) lead spacing, 1/4W (flat)</description>
</package>
</packages>
</library>
<library name="inductors">
<packages>
<package name="IND.2">
</package>
</packages>
</library>
<library name="caps-film">
<packages>
<package name="0.2&quot;.SML">
<description>0.2" (5.08mm) spacing
&lt;p&gt;
&lt;b&gt; 
10pf - 180n&lt;/b&gt;</description>
</package>
<package name="0.2&quot;.MED">
<description>0.2" (5.08mm) spacing
&lt;p&gt;
&lt;b&gt;220n-680n caps&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="transistors-BJT">
<packages>
<package name="TO92">
</package>
</packages>
</library>
<library name="diodes">
<packages>
<package name="DO41-2">
<description>&lt;b&gt;DO-41 0.2" pad spacing&lt;/b&gt;</description>
</package>
<package name="3MM_2">
</package>
</packages>
</library>
<library name="caps-elec">
<packages>
<package name="0633">
<description>0.2" (5.08mm) spacing</description>
</package>
<package name="0503">
<description>0.1" (2.54mm) spacing, for routing 10mil trace b/w pads</description>
</package>
</packages>
</library>
<library name="switches">
<packages>
<package name="2P4T.MINI">
<description>&lt;b&gt;Mini&lt;/b&gt;
&lt;br&gt; &lt;a href="http://smallbear-electronics.mybigcommerce.com/rotary-switch-miniature-2p4t/"&gt;http://smallbear-electronics.mybigcommerce.com/rotary-switch-miniature-2p4t/&lt;/a&gt;</description>
</package>
<package name="3PDT.LUGS">
<description>&lt;b&gt; Latching Footswitch, Solder Lugs&lt;/b&gt;
&lt;br&gt;&lt;a href="http://smallbear-electronics.mybigcommerce.com/cic-blue-3pdt/"&gt;http://smallbear-electronics.mybigcommerce.com/cic-blue-3pdt/&lt;/a&gt;
&lt;p&gt;
&lt;b&gt;Momentary Footswitch, Solder Lugs&lt;/b&gt;
&lt;br&gt;&lt;a href="http://smallbear-electronics.mybigcommerce.com/cic-blue-3pdt-momentary/"&gt;http://smallbear-electronics.mybigcommerce.com/cic-blue-3pdt-momentary/&lt;/a&gt;</description>
</package>
</packages>
</library>
<library name="supply pins">
<packages>
<package name="PAD2">
<description>&lt;b&gt;Round Pad (no label) - 76mil Diameter, 39mil Drill&lt;b&gt;</description>
</package>
<package name="PAD4">
<description>&lt;b&gt;Square (no label) - 76mil Diameter, 39mil Drill&lt;b&gt;</description>
</package>
<package name="PAD1">
<description>&lt;b&gt;Round Pad (w/label) - 80mil Diameter, 47mil Drill&lt;b&gt;</description>
</package>
<package name="PAD3">
<description>&lt;b&gt;Square Pad (w/label) - 80mil Diameter, 47mil Drill&lt;b&gt;</description>
</package>
</packages>
</library>
<library name="potentiometers">
<packages>
<package name="16MM_PADS.1">
<description>&lt;b&gt;16mm / Solder Lug&lt;/b&gt;
&lt;p&gt;
For wired potentiometers
&lt;p&gt;
&lt;a href="http://smallbear-electronics.mybigcommerce.com/alpha-single-gang-16mm-solder-terms-linear-audio-taper/"&gt;http://smallbear-electronics.mybigcommerce.com/alpha-single-gang-16mm-solder-terms-linear-audio-taper/&lt;/a&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="9V" library="jacks" package="DC_TS" value="DC_TS"/>
<element name="R7" library="resistors" package="0.3&quot;.B" value="1M"/>
<element name="R9" library="resistors" package="0.3&quot;.B" value="68k"/>
<element name="R2" library="resistors" package="0.3&quot;.B" value="22k"/>
<element name="R11" library="resistors" package="0.3&quot;.B" value="220"/>
<element name="R10" library="resistors" package="0.3&quot;.B" value="1k8"/>
<element name="R3" library="resistors" package="0.3&quot;.B" value="470k"/>
<element name="L1" library="inductors" package="IND.2" value=""/>
<element name="C3" library="caps-film" package="0.2&quot;.SML" value="10n"/>
<element name="C2" library="caps-film" package="0.2&quot;.SML" value="220n"/>
<element name="Q1" library="transistors-BJT" package="TO92" value="2N5088"/>
<element name="Q2" library="transistors-BJT" package="TO92" value="2N5088"/>
<element name="D1" library="diodes" package="DO41-2" value=""/>
<element name="C10" library="caps-film" package="0.2&quot;.MED" value="100n"/>
<element name="C8" library="caps-elec" package="0633" value="100uF"/>
<element name="R4" library="resistors" package="0.3&quot;.B" value="100k"/>
<element name="R5" library="resistors" package="0.3&quot;.B" value="100k"/>
<element name="R6" library="resistors" package="0.3&quot;.B" value="470k"/>
<element name="R1" library="resistors" package="0.3&quot;.B" value="1k"/>
<element name="C9" library="caps-elec" package="0503" value="4u7"/>
<element name="C1" library="caps-film" package="0.2&quot;.SML" value="220n"/>
<element name="C7" library="caps-film" package="0.2&quot;.SML" value="4n7"/>
<element name="C6" library="caps-film" package="0.2&quot;.SML" value="6n8"/>
<element name="C5" library="caps-film" package="0.2&quot;.SML" value="10n"/>
<element name="C4" library="caps-film" package="0.2&quot;.SML" value="15n"/>
<element name="R8" library="resistors" package="0.3&quot;.B" value="10k"/>
<element name="FQ" library="switches" package="2P4T.MINI" value=""/>
<element name="A" library="supply pins" package="PAD1" value="PADS.RND_LBL"/>
<element name="S.A" library="supply pins" package="PAD4" value="PADS.SQR_NL">
<attribute name="L" value="A"/>
<attribute name="M" value="Centre Freq"/>
</element>
<element name="S.1" library="supply pins" package="PAD2" value="PADS.RND_NL">
<attribute name="L" value="1"/>
</element>
<element name="S.2" library="supply pins" package="PAD2" value="PADS.RND_NL">
<attribute name="L" value="2"/>
</element>
<element name="S.3" library="supply pins" package="PAD2" value="PADS.RND_NL">
<attribute name="L" value="3"/>
</element>
<element name="S.4" library="supply pins" package="PAD2" value="PADS.RND_NL">
<attribute name="L" value="4"/>
</element>
<element name="A4" library="supply pins" package="PAD1" value="PADS.RND_LBL"/>
<element name="A3" library="supply pins" package="PAD1" value="PADS.RND_LBL"/>
<element name="A2" library="supply pins" package="PAD1" value="PADS.RND_LBL"/>
<element name="A1" library="supply pins" package="PAD1" value="PADS.RND_LBL"/>
<element name="IN" library="supply pins" package="PAD1" value="PADS.RND_LBL"/>
<element name="U$13" library="supply pins" package="PAD1" value="PADS.RND_LBL">
<attribute name="MLABEL" value="G"/>
</element>
<element name="U$14" library="supply pins" package="PAD1" value="PADS.RND_LBL">
<attribute name="MLABEL" value="G"/>
</element>
<element name="G" library="supply pins" package="PAD1" value="PADS.RND_LBL"/>
<element name="SWEEP" library="potentiometers" package="16MM_PADS.1" value="100k"/>
<element name="R12" library="resistors" package="0.3&quot;.B" value="10M">
<attribute name="NAME"/>
</element>
<element name="R13" library="resistors" package="0.3&quot;.B" value="10M"/>
<element name="R14" library="resistors" package="0.3&quot;.B" value="10M"/>
<element name="OUT" library="supply pins" package="PAD1" value="PADS.RND_LBL"/>
<element name="DIST2" library="supply pins" package="PAD2" value="PADS.RND_NL">
<attribute name="NLABEL" value="2"/>
</element>
<element name="DIST1" library="supply pins" package="PAD4" value="PADS.SQR_NL">
<attribute name="MLABEL" value="Distort"/>
<attribute name="NLABEL" value="1"/>
</element>
<element name="SW_1" library="switches" package="3PDT.LUGS" value=""/>
<element name="CLR" library="resistors" package="0.3&quot;.B" value="CLR"/>
<element name="D2" library="diodes" package="3MM_2" value="LED.3"/>
<element name="SND" library="supply pins" package="PAD1" value="PADS.RND_LBL">
<attribute name="MLABEL" value="P. In"/>
</element>
<element name="O" library="supply pins" package="PAD1" value="PADS.RND_LBL">
<attribute name="MLABEL" value="J. O"/>
</element>
<element name="GND" library="supply pins" package="PAD1" value="PADS.RND_LBL">
<attribute name="MLABEL" value="G"/>
</element>
<element name="I" library="supply pins" package="PAD1" value="PADS.RND_LBL">
<attribute name="MLABEL" value="J. In"/>
</element>
<element name="RTN" library="supply pins" package="PAD1" value="PADS.RND_LBL">
<attribute name="MLABEL" value="P. O"/>
</element>
<element name="9+" library="jacks" package="DC_TS" value="DC_TS">
<attribute name="NAME"/>
<attribute name="NAME"/>
</element>
<element name="GND7" library="supply pins" package="PAD1" value="PADS.RND_LBL">
<attribute name="MLABEL" value="G"/>
</element>
<element name="U$2" library="supply pins" package="PAD3" value="PADS.SQR_LBL">
<attribute name="MLABEL" value="9+"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="C8" pad="-"/>
<contactref element="C10" pad="1"/>
<contactref element="9V" pad="GND"/>
<contactref element="R5" pad="2"/>
<contactref element="C9" pad="-"/>
<contactref element="R7" pad="1"/>
<contactref element="R8" pad="2"/>
<contactref element="U$13" pad="1"/>
<contactref element="U$14" pad="1"/>
<contactref element="G" pad="1"/>
<contactref element="SWEEP" pad="1"/>
<contactref element="DIST1" pad="P$1"/>
</signal>
<signal name="N$4">
<contactref element="D1" pad="A"/>
<contactref element="9V" pad="PWR"/>
</signal>
<signal name="VCC">
<contactref element="C10" pad="2"/>
<contactref element="D1" pad="C"/>
<contactref element="C8" pad="+"/>
<contactref element="R2" pad="2"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="IN">
<contactref element="R7" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="IN" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="C3" pad="1"/>
<contactref element="R9" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="R9" pad="2"/>
<contactref element="Q1" pad="2"/>
<contactref element="R10" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="Q1" pad="1"/>
<contactref element="R2" pad="1"/>
<contactref element="R3" pad="2"/>
<contactref element="R6" pad="2"/>
<contactref element="C2" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="R11" pad="2"/>
<contactref element="Q1" pad="3"/>
</signal>
<signal name="N$7">
<contactref element="R4" pad="2"/>
<contactref element="R3" pad="1"/>
<contactref element="L1" pad="5"/>
<contactref element="L1" pad="8"/>
<contactref element="L1" pad="6"/>
<contactref element="L1" pad="12"/>
<contactref element="L1" pad="11"/>
<contactref element="L1" pad="3"/>
<contactref element="L1" pad="9"/>
<contactref element="L1" pad="4"/>
<contactref element="L1" pad="A"/>
<contactref element="L1" pad="7"/>
<contactref element="L1" pad="10"/>
<contactref element="L1" pad="13"/>
<contactref element="R5" pad="1"/>
<contactref element="C9" pad="+"/>
</signal>
<signal name="N$8">
<contactref element="R6" pad="1"/>
<contactref element="Q2" pad="2"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="N$9">
<contactref element="R1" pad="2"/>
<contactref element="Q2" pad="1"/>
</signal>
<signal name="LPLANE">
<contactref element="C7" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="L1" pad="B"/>
<contactref element="L1" pad="18"/>
<contactref element="L1" pad="24"/>
<contactref element="L1" pad="17"/>
<contactref element="L1" pad="23"/>
<contactref element="L1" pad="15"/>
<contactref element="L1" pad="21"/>
<contactref element="L1" pad="16"/>
<contactref element="L1" pad="19"/>
<contactref element="L1" pad="22"/>
<contactref element="L1" pad="14"/>
<contactref element="L1" pad="20"/>
<contactref element="R4" pad="1"/>
<contactref element="R10" pad="1"/>
</signal>
<signal name="SW.A">
<contactref element="R8" pad="1"/>
<contactref element="Q2" pad="3"/>
<contactref element="S.A" pad="P$1"/>
</signal>
<signal name="N$12">
<contactref element="A4" pad="1"/>
<contactref element="FQ" pad="A4"/>
</signal>
<signal name="N$13">
<contactref element="A3" pad="1"/>
<contactref element="FQ" pad="A3"/>
</signal>
<signal name="N$14">
<contactref element="A2" pad="1"/>
<contactref element="FQ" pad="A2"/>
</signal>
<signal name="N$15">
<contactref element="A1" pad="1"/>
<contactref element="FQ" pad="A1"/>
</signal>
<signal name="A1">
<contactref element="C7" pad="1"/>
<contactref element="S.1" pad="P$1"/>
<contactref element="R12" pad="2"/>
</signal>
<signal name="OUT">
<contactref element="C2" pad="1"/>
<contactref element="SWEEP" pad="3"/>
<contactref element="OUT" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="SWEEP" pad="2"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="A">
<contactref element="FQ" pad="A"/>
<contactref element="A" pad="1"/>
</signal>
<signal name="A2">
<contactref element="R12" pad="1"/>
<contactref element="R13" pad="2"/>
<contactref element="C6" pad="1"/>
<contactref element="S.2" pad="P$1"/>
</signal>
<signal name="A3">
<contactref element="R13" pad="1"/>
<contactref element="R14" pad="2"/>
<contactref element="C5" pad="1"/>
<contactref element="S.3" pad="P$1"/>
</signal>
<signal name="A4">
<contactref element="C4" pad="1"/>
<contactref element="R14" pad="1"/>
<contactref element="S.4" pad="P$1"/>
</signal>
<signal name="N$6">
<contactref element="R11" pad="1"/>
<contactref element="DIST2" pad="P$1"/>
</signal>
<signal name="J.IN">
<contactref element="I" pad="1"/>
<contactref element="SW_1" pad="A1"/>
<contactref element="SW_1" pad="C3"/>
</signal>
<signal name="PCB.IN">
<contactref element="SW_1" pad="A2"/>
<contactref element="SND" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="SW_1" pad="B1"/>
<contactref element="D2" pad="P$1"/>
</signal>
<signal name="N$16">
<contactref element="D2" pad="ANODE"/>
<contactref element="CLR" pad="1"/>
</signal>
<signal name="J.OUT">
<contactref element="O" pad="1"/>
<contactref element="SW_1" pad="C2"/>
</signal>
<signal name="PCB.OUT">
<contactref element="RTN" pad="1"/>
<contactref element="SW_1" pad="C1"/>
<contactref element="SW_1" pad="B3"/>
</signal>
<signal name="G2">
<contactref element="SW_1" pad="B2"/>
<contactref element="GND" pad="1"/>
<contactref element="SW_1" pad="A3"/>
<contactref element="9+" pad="GND"/>
<contactref element="GND7" pad="1"/>
</signal>
<signal name="N$17">
<contactref element="9+" pad="PWR"/>
<contactref element="CLR" pad="2"/>
<contactref element="U$2" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
