(kicad_pcb (version 20171130) (host pcbnew "(5.1.4)-1")
  (general
    (thickness 1.6)
    (drawings 44)
    (tracks 201)
    (zones 0)
    (modules 21)
    (nets 24)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user)
    (35 F.Paste user hide)
    (36 B.SilkS user hide)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.15 3.25)
    (pad_drill 0)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 12V)
  (net 3 5V)
  (net 4 "Net-(D1-Pad2)")
  (net 5 "Net-(D1-Pad1)")
  (net 6 EN1)
  (net 7 RST)
  (net 8 LED)
  (net 9 NC_1)
  (net 10 NC_2)
  (net 11 NC_3)
  (net 12 NC_6)
  (net 13 NC_5)
  (net 14 NC_4)
  (net 15 A_IN)
  (net 16 "Net-(JP2-Pad1)")
  (net 17 "Net-(JP3-Pad2)")
  (net 18 A_CTRL)
  (net 19 SCL)
  (net 20 SDA)
  (net 21 AIN_EXT)
  (net 22 AIN_POT)
  (net 23 PRESNET)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net 12V)
    (add_net 5V)
    (add_net AIN_EXT)
    (add_net AIN_POT)
    (add_net A_CTRL)
    (add_net A_IN)
    (add_net EN1)
    (add_net GND)
    (add_net LED)
    (add_net NC_1)
    (add_net NC_2)
    (add_net NC_3)
    (add_net NC_4)
    (add_net NC_5)
    (add_net NC_6)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(JP2-Pad1)")
    (add_net "Net-(JP3-Pad2)")
    (add_net PRESNET)
    (add_net RST)
    (add_net SCL)
    (add_net SDA)
  )
  (module DPS1200FB_lib:SOT223-4 (layer B.Cu) (tedit 5F6278EF)
    (at 28.9 24.1 180)
    (fp_text reference U1 (at -0.025 4.754) (layer Cmts.User) hide)
    (fp_text value LM7805_TO220 (at 8.865 -4.365) (layer B.Fab) hide)
    (pad 1 smd rect (at -2.9 2.3 180) (size 2.15 0.95) (layers B.Cu B.Paste B.Mask)
      (net 2 12V))
    (pad 2 smd rect (at -2.9 0 180) (size 2.15 0.95) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -2.9 -2.3 180) (size 2.15 0.95) (layers B.Cu B.Paste B.Mask)
      (net 3 5V))
    (pad 4 smd rect (at 2.9 0 180) (size 2.15 3.25) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
  )
  (module DPS1200FB_lib:SOIC8 (layer F.Cu) (tedit 5F614B9F)
    (at 30.2 22.9 90)
    (fp_text reference U2 (at 0.585455 4.225535 270) (layer Cmts.User) hide)
    (fp_text value ATtiny45-20PU (at 15.3181 -6.13234 270) (layer F.Fab) hide)
    (pad 8 smd rect (at 3.7084 -1.905 90) (size 1.5494 0.5334) (layers F.Cu F.Paste F.Mask)
      (net 3 5V))
    (pad 7 smd rect (at 3.7084 -0.635 90) (size 1.5494 0.5334) (layers F.Cu F.Paste F.Mask)
      (net 19 SCL))
    (pad 6 smd rect (at 3.7084 0.635 90) (size 1.5494 0.5334) (layers F.Cu F.Paste F.Mask)
      (net 8 LED))
    (pad 5 smd rect (at 3.7084 1.905 90) (size 1.5494 0.5334) (layers F.Cu F.Paste F.Mask)
      (net 20 SDA))
    (pad 4 smd rect (at -3.7084 1.905 90) (size 1.5494 0.5334) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -3.7084 0.635 90) (size 1.5494 0.5334) (layers F.Cu F.Paste F.Mask)
      (net 18 A_CTRL))
    (pad 2 smd rect (at -3.7084 -0.635 90) (size 1.5494 0.5334) (layers F.Cu F.Paste F.Mask)
      (net 15 A_IN))
    (pad 1 smd rect (at -3.7084 -1.905 90) (size 1.5494 0.5334) (layers F.Cu F.Paste F.Mask)
      (net 7 RST))
  )
  (module DPS1200FB_lib:6_pin_SMD_2.54 (layer B.Cu) (tedit 5F6148CF)
    (at 32.8 20.7)
    (descr "surface-mounted straight socket strip, 2x06, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated")
    (tags "Surface mounted socket strip SMD 2x06 2.54mm double row")
    (attr smd)
    (fp_text reference J4 (at 17.1 5.1 -90) (layer Cmts.User) hide)
    (fp_text value Card_Bot_Pins (at 9 6.6 -90) (layer B.Fab) hide)
    (fp_text user %R (at 14.9 5.9 -90) (layer B.Fab) hide)
    (pad 6 smd rect (at 2.52 -6.35) (size 3 1) (layers B.Cu B.Paste B.Mask)
      (net 19 SCL))
    (pad 5 smd rect (at 2.52 -3.81) (size 3 1) (layers B.Cu B.Paste B.Mask)
      (net 20 SDA))
    (pad 4 smd rect (at 2.52 -1.27) (size 3 1) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 2.52 1.27) (size 3 1) (layers B.Cu B.Paste B.Mask)
      (net 12 NC_6))
    (pad 2 smd rect (at 2.52 3.81) (size 3 1) (layers B.Cu B.Paste B.Mask)
      (net 13 NC_5))
    (pad 1 smd rect (at 2.52 6.35) (size 3 1) (layers B.Cu B.Paste B.Mask)
      (net 14 NC_4))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_2x06_P2.54mm_Vertical_SMD.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 32.1 15.825 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at 4.525 -4.5 180) (layer Cmts.User) hide)
    (fp_text value 22K (at 2.575 -0.1 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 23 PRESNET))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 12V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 27.9 15.825 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R2 (at -4.625 0.9 90) (layer Cmts.User) hide)
    (fp_text value 4.7K (at -4.025 -1.7 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 16 "Net-(JP2-Pad1)"))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 3 5V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 30 15.825 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R4 (at -4.825 2.4 90) (layer Cmts.User) hide)
    (fp_text value 4.7K (at 2.575 -1.5 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 17 "Net-(JP3-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 3 5V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 23.7 15.825 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R5 (at -3.825 2.7 90) (layer Cmts.User) hide)
    (fp_text value 10K (at 2.575 0.4 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 7 RST))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 3 5V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 25.8 15.825 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R6 (at -3.725 2.6 90) (layer Cmts.User) hide)
    (fp_text value 10K (at -4.225 5.8 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 3 5V))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 18 A_CTRL))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Potentiometer_SMD:Potentiometer_Bourns_TC33X_Vertical (layer F.Cu) (tedit 5C165D15)
    (at 18.1 19.2)
    (descr "Potentiometer, Bourns, TC33X, Vertical, https://www.bourns.com/pdfs/TC33.pdf")
    (tags "Potentiometer Bourns TC33X Vertical")
    (attr smd)
    (fp_text reference RV1 (at 0 -2.5) (layer Cmts.User) hide)
    (fp_text value 1M_POT (at 0 2.5) (layer F.Fab) hide)
    (fp_text user "Wiper may be\nanywhere within\ncircle shown" (at -0.1 0.1) (layer Cmts.User))
    (fp_text user %R (at -0.1 -0.7) (layer F.Fab))
    (pad 2 smd rect (at 1.45 0) (size 1.5 1.6) (layers F.Cu F.Paste F.Mask)
      (net 22 AIN_POT))
    (pad 3 smd rect (at -1.8 1) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.8 -1) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 3 5V))
    (model ${KISYS3DMOD}/Potentiometer_SMD.3dshapes/Potentiometer_Bourns_TC33X_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 22.6 25.625 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R3 (at 0 -1.65 90) (layer Cmts.User) hide)
    (fp_text value 1K (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 5 "Net-(D1-Pad1)"))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Jumper:SolderJumper-2_P1.3mm_Bridged_Pad1.0x1.5mm (layer B.Cu) (tedit 5C756AB2)
    (at 25.8 16.25 90)
    (descr "SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, bridged with 1 copper strip")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP4 (at 0 1.8 90) (layer Cmts.User) hide)
    (fp_text value A_CTRL_JMP (at 0 -1.9 90) (layer B.Fab) hide)
    (pad 2 smd rect (at 0.65 0 90) (size 1 1.5) (layers B.Cu B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.65 0 90) (size 1 1.5) (layers B.Cu B.Mask)
      (net 18 A_CTRL))
  )
  (module Jumper:SolderJumper-2_P1.3mm_Bridged_Pad1.0x1.5mm (layer B.Cu) (tedit 5C756AB2)
    (at 31.7 17.3 180)
    (descr "SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, bridged with 1 copper strip")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP3 (at 0 1.8) (layer Cmts.User) hide)
    (fp_text value SDA_JMP (at 0 -1.9) (layer B.Fab) hide)
    (pad 2 smd rect (at 0.65 0 180) (size 1 1.5) (layers B.Cu B.Mask)
      (net 17 "Net-(JP3-Pad2)"))
    (pad 1 smd rect (at -0.65 0 180) (size 1 1.5) (layers B.Cu B.Mask)
      (net 20 SDA))
  )
  (module Jumper:SolderJumper-2_P1.3mm_Bridged_Pad1.0x1.5mm (layer B.Cu) (tedit 5C756AB2)
    (at 31.7 14.8)
    (descr "SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, bridged with 1 copper strip")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP2 (at 0 1.8) (layer Cmts.User) hide)
    (fp_text value SCL_JMP (at 0 -1.9) (layer B.Fab) hide)
    (pad 2 smd rect (at 0.65 0) (size 1 1.5) (layers B.Cu B.Mask)
      (net 19 SCL))
    (pad 1 smd rect (at -0.65 0) (size 1 1.5) (layers B.Cu B.Mask)
      (net 16 "Net-(JP2-Pad1)"))
  )
  (module Jumper:SolderJumper-2_P1.3mm_Bridged_Pad1.0x1.5mm (layer B.Cu) (tedit 5C756AB2)
    (at 21.75 26.8 180)
    (descr "SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, bridged with 1 copper strip")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP1 (at 0 1.8) (layer Cmts.User) hide)
    (fp_text value LED_JMP (at 0 -1.9) (layer B.Fab) hide)
    (pad 2 smd rect (at 0.65 0 180) (size 1 1.5) (layers B.Cu B.Mask)
      (net 4 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -0.65 0 180) (size 1 1.5) (layers B.Cu B.Mask)
      (net 8 LED))
  )
  (module DPS1200FB_lib:3_pin_SMD_2.54 (layer B.Cu) (tedit 5F614913)
    (at 14.6 20.7)
    (descr "surface-mounted straight socket strip, 2x06, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated")
    (tags "Surface mounted socket strip SMD 2x06 2.54mm double row")
    (attr smd)
    (fp_text reference J2 (at 0 5.08 -90) (layer Cmts.User) hide)
    (fp_text value A_IN_PIN (at -2.54 2.54 -90) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 -90) (layer B.Fab) hide)
    (pad 3 smd rect (at 2.52 1.27) (size 3 1) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.52 3.81) (size 3 1) (layers B.Cu B.Paste B.Mask)
      (net 21 AIN_EXT))
    (pad 1 smd rect (at 2.52 6.35) (size 3 1) (layers B.Cu B.Paste B.Mask)
      (net 3 5V))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_2x06_P2.54mm_Vertical_SMD.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module DPS1200FB_lib:6_pin_SMD_2.54 (layer F.Cu) (tedit 5F6148CF)
    (at 32.8 20.7)
    (descr "surface-mounted straight socket strip, 2x06, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated")
    (tags "Surface mounted socket strip SMD 2x06 2.54mm double row")
    (attr smd)
    (fp_text reference J3 (at 14 3.1 90) (layer Cmts.User) hide)
    (fp_text value Card_Top_Pins (at 10.3 5.7 90) (layer F.Fab) hide)
    (fp_text user %R (at 14.3 8.6 90) (layer F.Fab) hide)
    (pad 6 smd rect (at 2.52 6.35) (size 3 1) (layers F.Cu F.Paste F.Mask)
      (net 9 NC_1))
    (pad 5 smd rect (at 2.52 3.81) (size 3 1) (layers F.Cu F.Paste F.Mask)
      (net 2 12V))
    (pad 4 smd rect (at 2.52 1.27) (size 3 1) (layers F.Cu F.Paste F.Mask)
      (net 23 PRESNET))
    (pad 3 smd rect (at 2.52 -1.27) (size 3 1) (layers F.Cu F.Paste F.Mask)
      (net 10 NC_2))
    (pad 2 smd rect (at 2.52 -3.81) (size 3 1) (layers F.Cu F.Paste F.Mask)
      (net 11 NC_3))
    (pad 1 smd rect (at 2.52 -6.35) (size 3 1) (layers F.Cu F.Paste F.Mask)
      (net 6 EN1))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_2x06_P2.54mm_Vertical_SMD.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 17 15.4 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J1 (at 0 -2.33 90) (layer Cmts.User) hide)
    (fp_text value EN_JMP (at 5.8 -2.7 90) (layer F.Fab) hide)
    (fp_text user %R (at 3.4 -1.1) (layer F.Fab) hide)
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 EN1))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B4B45C9)
    (at 20.7 25.6 90)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (attr smd)
    (fp_text reference D1 (at 0 -1.65 90) (layer Cmts.User) hide)
    (fp_text value LED (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 4 "Net-(D1-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 5 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 23.725 21.2)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C2 (at 0 -1.65) (layer Cmts.User) hide)
    (fp_text value 1uf (at 0 1.65) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 3 5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Jumper:SolderJumper-3_P1.3mm_Bridged2Bar12_Pad1.0x1.5mm_NumberLabels (layer B.Cu) (tedit 5C756B16)
    (at 20.2 23.5 270)
    (descr "SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, pads 1-2 Bridged2Bar with 2 copper strip, labeled with numbers")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP5 (at 0 1.8 90) (layer Cmts.User) hide)
    (fp_text value AIN_SEL_JMP (at 0 -1.9 90) (layer B.Fab) hide)
    (fp_text user 3 (at 1.4 -2 90) (layer Cmts.User) hide)
    (fp_text user 1 (at -1.5 -2.1 90) (layer Cmts.User) hide)
    (pad 1 smd rect (at -1.3 0 270) (size 1 1.5) (layers B.Cu B.Mask)
      (net 22 AIN_POT))
    (pad 3 smd rect (at 1.3 0 270) (size 1 1.5) (layers B.Cu B.Mask)
      (net 21 AIN_EXT))
    (pad 2 smd rect (at 0 0 270) (size 1 1.5) (layers B.Cu B.Mask)
      (net 15 A_IN))
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 23.7 19.1 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C1 (at 0 -1.65) (layer Cmts.User) hide)
    (fp_text value 10uf (at 0 1.65) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 12V))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text +5V (at 26.7 13.9) (layer F.SilkS))
  (gr_text +12V (at 32 13.9) (layer F.SilkS))
  (gr_text +5V (at 16.2 26) (layer B.SilkS))
  (gr_text ANA (at 16.1 23.5) (layer B.SilkS))
  (gr_text GND (at 16.1 21) (layer B.SilkS))
  (gr_text LM7805 (at 29.1 20.4) (layer B.SilkS))
  (gr_text EXT/TMP (at 22.9 24.9) (layer B.SilkS))
  (gr_text POT (at 22.1 22.2) (layer B.SilkS))
  (gr_text LED (at 23.9 27.4) (layer B.SilkS))
  (gr_text SCL (at 29.4 14.1) (layer B.SilkS))
  (gr_text SDA (at 31 18.8) (layer B.SilkS))
  (gr_text ACTL (at 25.8 18.3) (layer B.SilkS))
  (gr_text ASEL (at 20.2 20.9) (layer B.SilkS))
  (gr_text ^P28 (at 34.7 25.6) (layer B.SilkS))
  (gr_text ^P27 (at 36.1 26 180) (layer B.SilkS))
  (gr_text ^P29 (at 35.9 20.9 180) (layer B.SilkS))
  (gr_text ^P30 (at 34.4 20.5) (layer B.SilkS))
  (gr_text ^P31 (at 36 15.8 180) (layer B.SilkS))
  (gr_text ^P32 (at 34.5 15.4) (layer B.SilkS))
  (gr_text "ATTINY 45/85" (at 27 22.9 90) (layer F.SilkS))
  (gr_text "R1.0\nSEPT 2020\n" (at 25.4 27.6 270) (layer F.SilkS))
  (gr_text P34 (at 33.2 16.9 270) (layer F.SilkS))
  (gr_text P35 (at 33.2 19.5 270) (layer F.SilkS))
  (gr_text P36 (at 33.3 21.9 270) (layer F.SilkS))
  (gr_text P38 (at 33.3 27 270) (layer F.SilkS))
  (gr_text P37 (at 33.3 24.5 270) (layer F.SilkS))
  (gr_text 22K (at 32.1 17.9) (layer F.SilkS))
  (gr_text 4.7K (at 27.7 17.9) (layer F.SilkS))
  (gr_text 4.7K (at 30.1 17.9) (layer F.SilkS))
  (gr_text 10K (at 25.8 17.9) (layer F.SilkS))
  (gr_text 10K (at 23.8 17.9) (layer F.SilkS))
  (gr_text "1M_POT\n\n" (at 20.9 19.4 270) (layer F.SilkS))
  (gr_text EN_SW (at 21.8 15.4 270) (layer F.SilkS))
  (gr_text 10uf (at 26.3 19.3) (layer F.SilkS))
  (gr_text 1uf (at 23.8 22.1) (layer F.SilkS))
  (gr_text P33 (at 33.3 14.4 270) (layer F.SilkS))
  (gr_text 1K (at 23.8 27 270) (layer F.SilkS))
  (gr_text LED> (at 21.2 22.8 270) (layer F.SilkS))
  (gr_text "M. Neiderhauser\nPSU Fan Ctrl\nDPS1200FB\n" (at 17.7 27.5 270) (layer F.SilkS))
  (gr_line (start 15.3 13.5) (end 37.1 13.5) (layer Edge.Cuts) (width 0.12))
  (gr_line (start 15.3 27.8) (end 15.3 13.5) (layer Edge.Cuts) (width 0.12))
  (gr_line (start 37.1 27.8) (end 15.3 27.8) (layer Edge.Cuts) (width 0.12))
  (gr_line (start 37.1 13.5) (end 37.1 27.8) (layer Edge.Cuts) (width 0.12))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 15.4 13.7) (xy 37 13.7) (xy 37 27.7) (xy 15.4 27.7)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 15.4 13.7) (xy 37 13.7) (xy 37 27.7) (xy 15.4 27.7)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 17.1 17.4) (xy 17.1 21) (xy 18.6 21) (xy 18.6 17.4)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 18.6 18.2) (xy 18.6 17.4) (xy 20.4 17.4) (xy 20.4 18.2)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 18.6 21) (xy 20 21) (xy 20 20.2) (xy 18.6 20.2)
      )
    )
  )
)
