(kicad_pcb (version 20171130) (host pcbnew "(5.0.0)")
  (general
    (thickness 1.6)
    (drawings 66)
    (tracks 560)
    (zones 0)
    (modules 114)
    (nets 66)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.5)
    (user_trace_width 0.25)
    (user_trace_width 1)
    (user_trace_width 0.25)
    (user_trace_width 1)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.5)
    (via_min_size 0.8)
    (via_min_drill 0.5)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.3 1.3)
    (pad_drill 0.75)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 178.562 34.925)
    (visible_elements 7FFFF7FF)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin true)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerber/"))
  )
  (net 0 "")
  (net 1 /AUDIO_L)
  (net 2 GND)
  (net 3 /AUDIO_R)
  (net 4 "Net-(C1-Pad1)")
  (net 5 +12V)
  (net 6 "Net-(D1-Pad1)")
  (net 7 "Net-(D1-Pad2)")
  (net 8 /SW_AUDIO_R)
  (net 9 /SW_AUDIO_L)
  (net 10 /AUDIO)
  (net 11 /CSYNC)
  (net 12 "Net-(C4-Pad2)")
  (net 13 /CVBS_CSYNC)
  (net 14 /R-RY)
  (net 15 /GY)
  (net 16 /B-BY)
  (net 17 /HD_CS)
  (net 18 "Net-(C2-Pad1)")
  (net 19 +5V)
  (net 20 "Net-(R3-Pad2)")
  (net 21 "Net-(R4-Pad2)")
  (net 22 "Net-(J1-Pad18)")
  (net 23 "Net-(J1-Pad16)")
  (net 24 "Net-(J1-Pad14)")
  (net 25 "Net-(J1-Pad12)")
  (net 26 "Net-(J1-Pad10)")
  (net 27 "Net-(J1-Pad8)")
  (net 28 "Net-(J1-Pad19)")
  (net 29 "Net-(J1-Pad17)")
  (net 30 "Net-(J1-Pad3)")
  (net 31 "Net-(J1-Pad1)")
  (net 32 "Net-(SW2-Pad4)")
  (net 33 "Net-(U1-Pad3)")
  (net 34 "Net-(U1-Pad5)")
  (net 35 "Net-(U1-Pad7)")
  (net 36 "Net-(J4-Pad9)")
  (net 37 "Net-(C101-Pad1)")
  (net 38 "Net-(C102-Pad1)")
  (net 39 "Net-(C103-Pad1)")
  (net 40 "Net-(C104-Pad1)")
  (net 41 "Net-(C105-Pad1)")
  (net 42 /VD)
  (net 43 /VCC+14V)
  (net 44 "Net-(C203-Pad1)")
  (net 45 /AUDIO_)
  (net 46 /Y)
  (net 47 /B-Y)
  (net 48 /R-Y)
  (net 49 /HD)
  (net 50 /VD_)
  (net 51 /G/Y)
  (net 52 /B/B-Y)
  (net 53 /R/R-Y)
  (net 54 /HD/CS)
  (net 55 "Net-(C204-Pad2)")
  (net 56 "Net-(C106-Pad1)")
  (net 57 "Net-(C106-Pad2)")
  (net 58 "Net-(C108-Pad1)")
  (net 59 "Net-(C108-Pad2)")
  (net 60 "Net-(C110-Pad1)")
  (net 61 "Net-(C110-Pad2)")
  (net 62 "Net-(C112-Pad1)")
  (net 63 "Net-(C112-Pad2)")
  (net 64 "Net-(C113-Pad1)")
  (net 65 "Net-(C113-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.5)
    (via_dia 0.8)
    (via_drill 0.5)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +12V)
    (add_net +5V)
    (add_net /AUDIO)
    (add_net /AUDIO_)
    (add_net /AUDIO_L)
    (add_net /AUDIO_R)
    (add_net /B-BY)
    (add_net /B-Y)
    (add_net /B/B-Y)
    (add_net /CSYNC)
    (add_net /CVBS_CSYNC)
    (add_net /G/Y)
    (add_net /GY)
    (add_net /HD)
    (add_net /HD/CS)
    (add_net /HD_CS)
    (add_net /R-RY)
    (add_net /R-Y)
    (add_net /R/R-Y)
    (add_net /SW_AUDIO_L)
    (add_net /SW_AUDIO_R)
    (add_net /VCC+14V)
    (add_net /VD)
    (add_net /VD_)
    (add_net /Y)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C101-Pad1)")
    (add_net "Net-(C102-Pad1)")
    (add_net "Net-(C103-Pad1)")
    (add_net "Net-(C104-Pad1)")
    (add_net "Net-(C105-Pad1)")
    (add_net "Net-(C106-Pad1)")
    (add_net "Net-(C106-Pad2)")
    (add_net "Net-(C108-Pad1)")
    (add_net "Net-(C108-Pad2)")
    (add_net "Net-(C110-Pad1)")
    (add_net "Net-(C110-Pad2)")
    (add_net "Net-(C112-Pad1)")
    (add_net "Net-(C112-Pad2)")
    (add_net "Net-(C113-Pad1)")
    (add_net "Net-(C113-Pad2)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C203-Pad1)")
    (add_net "Net-(C204-Pad2)")
    (add_net "Net-(C4-Pad2)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad10)")
    (add_net "Net-(J1-Pad12)")
    (add_net "Net-(J1-Pad14)")
    (add_net "Net-(J1-Pad16)")
    (add_net "Net-(J1-Pad17)")
    (add_net "Net-(J1-Pad18)")
    (add_net "Net-(J1-Pad19)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(J4-Pad9)")
    (add_net "Net-(R3-Pad2)")
    (add_net "Net-(R4-Pad2)")
    (add_net "Net-(SW2-Pad4)")
    (add_net "Net-(U1-Pad3)")
    (add_net "Net-(U1-Pad5)")
    (add_net "Net-(U1-Pad7)")
  )
  (module TO-220-own:TO-220-3_own (layer F.Cu) (tedit 5B72D711)
    (at 248.539 114.808 90)
    (descr "TO-220-3, Horizontal, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
    (tags "TO-220-3 Horizontal RM 2.54mm")
    (fp_text reference U1 (at 2.54 -20.447 90) (layer F.SilkS))
    (fp_text value NCP1117-12_SOT223 (at 2.54 2 90) (layer F.Fab))
    (fp_text user %R (at 2.54 -20.58 90) (layer F.Fab))
    (pad 3 thru_hole oval (at 0 0 90) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 43 /VCC+14V))
    (pad 2 thru_hole oval (at 5.08 0 90) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 5 +12V))
    (pad 1 thru_hole circle (at 2.54 0 90) (size 1.905 1.905) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad "" np_thru_hole oval (at 2.54 -16.66 90) (size 3.5 3.5) (drill 3.5) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-220-3_Horizontal_TabDown.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO-92-own:TO-92-own (layer F.Cu) (tedit 5B72B7C9)
    (at 257.81 43.18 180)
    (descr "TO-92L leads in-line (large body variant of TO-92), also known as TO-226, wide, drill 0.75mm (see https://www.diodes.com/assets/Package-Files/TO92L.pdf and http://www.ti.com/lit/an/snoa059/snoa059.pdf)")
    (tags "TO-92L Molded Narrow transistor")
    (fp_text reference Q101 (at 1.29 2.413) (layer F.SilkS))
    (fp_text value BC817-40 (at 1.29 2.79 180) (layer F.Fab))
    (fp_text user %R (at 1.29 -3.56 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 2.794 0.381 270) (size 1.3 1.3) (drill 0.75) (layers *.Cu *.Mask)
      (net 57 "Net-(C106-Pad2)"))
    (pad 3 thru_hole circle (at -0.254 0.381 270) (size 1.3 1.3) (drill 0.75) (layers *.Cu *.Mask)
      (net 5 +12V))
    (pad 2 thru_hole circle (at 1.28 -1.27 270) (size 1.3 1.3) (drill 0.75) (layers *.Cu *.Mask)
      (net 56 "Net-(C106-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92L.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO-92-own:TO-92-own (layer F.Cu) (tedit 5B72B7C9)
    (at 244.094 122.174 180)
    (descr "TO-92L leads in-line (large body variant of TO-92), also known as TO-226, wide, drill 0.75mm (see https://www.diodes.com/assets/Package-Files/TO92L.pdf and http://www.ti.com/lit/an/snoa059/snoa059.pdf)")
    (tags "TO-92L Molded Narrow transistor")
    (fp_text reference Q201 (at 1.29 2.54) (layer F.SilkS))
    (fp_text value BC817-40 (at 1.29 2.79 180) (layer F.Fab))
    (fp_text user %R (at 1.29 -3.56 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 2.794 0.381 270) (size 1.3 1.3) (drill 0.75) (layers *.Cu *.Mask)
      (net 55 "Net-(C204-Pad2)"))
    (pad 3 thru_hole circle (at -0.254 0.381 270) (size 1.3 1.3) (drill 0.75) (layers *.Cu *.Mask)
      (net 5 +12V))
    (pad 2 thru_hole circle (at 1.28 -1.27 270) (size 1.3 1.3) (drill 0.75) (layers *.Cu *.Mask)
      (net 45 /AUDIO_))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92L.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO-92-own:TO-92-own (layer F.Cu) (tedit 5B72B7C9)
    (at 254.889 97.028 180)
    (descr "TO-92L leads in-line (large body variant of TO-92), also known as TO-226, wide, drill 0.75mm (see https://www.diodes.com/assets/Package-Files/TO92L.pdf and http://www.ti.com/lit/an/snoa059/snoa059.pdf)")
    (tags "TO-92L Molded Narrow transistor")
    (fp_text reference Q114 (at 1.29 2.413) (layer F.SilkS))
    (fp_text value BC817-40 (at 1.29 2.79 180) (layer F.Fab))
    (fp_text user %R (at 1.29 -3.56 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 2.794 0.381 270) (size 1.3 1.3) (drill 0.75) (layers *.Cu *.Mask)
      (net 65 "Net-(C113-Pad2)"))
    (pad 3 thru_hole circle (at -0.254 0.381 270) (size 1.3 1.3) (drill 0.75) (layers *.Cu *.Mask)
      (net 5 +12V))
    (pad 2 thru_hole circle (at 1.28 -1.27 270) (size 1.3 1.3) (drill 0.75) (layers *.Cu *.Mask)
      (net 64 "Net-(C113-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92L.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO-92-own:TO-92-own (layer F.Cu) (tedit 5B72B7C9)
    (at 254.762 83.566 180)
    (descr "TO-92L leads in-line (large body variant of TO-92), also known as TO-226, wide, drill 0.75mm (see https://www.diodes.com/assets/Package-Files/TO92L.pdf and http://www.ti.com/lit/an/snoa059/snoa059.pdf)")
    (tags "TO-92L Molded Narrow transistor")
    (fp_text reference Q113 (at 1.29 2.413) (layer F.SilkS))
    (fp_text value BC817-40 (at 1.29 2.79 180) (layer F.Fab))
    (fp_text user %R (at 1.29 -3.56 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 2.794 0.381 270) (size 1.3 1.3) (drill 0.75) (layers *.Cu *.Mask)
      (net 63 "Net-(C112-Pad2)"))
    (pad 3 thru_hole circle (at -0.254 0.381 270) (size 1.3 1.3) (drill 0.75) (layers *.Cu *.Mask)
      (net 5 +12V))
    (pad 2 thru_hole circle (at 1.28 -1.27 270) (size 1.3 1.3) (drill 0.75) (layers *.Cu *.Mask)
      (net 62 "Net-(C112-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92L.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO-92-own:TO-92-own (layer F.Cu) (tedit 5B72B7C9)
    (at 257.81 70.104 180)
    (descr "TO-92L leads in-line (large body variant of TO-92), also known as TO-226, wide, drill 0.75mm (see https://www.diodes.com/assets/Package-Files/TO92L.pdf and http://www.ti.com/lit/an/snoa059/snoa059.pdf)")
    (tags "TO-92L Molded Narrow transistor")
    (fp_text reference Q109 (at 1.29 2.54) (layer F.SilkS))
    (fp_text value BC817-40 (at 1.29 2.79 180) (layer F.Fab))
    (fp_text user %R (at 1.29 -3.56 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 2.794 0.381 270) (size 1.3 1.3) (drill 0.75) (layers *.Cu *.Mask)
      (net 61 "Net-(C110-Pad2)"))
    (pad 3 thru_hole circle (at -0.254 0.381 270) (size 1.3 1.3) (drill 0.75) (layers *.Cu *.Mask)
      (net 5 +12V))
    (pad 2 thru_hole circle (at 1.28 -1.27 270) (size 1.3 1.3) (drill 0.75) (layers *.Cu *.Mask)
      (net 60 "Net-(C110-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92L.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO-92-own:TO-92-own (layer F.Cu) (tedit 5B72B7C9)
    (at 257.81 56.642 180)
    (descr "TO-92L leads in-line (large body variant of TO-92), also known as TO-226, wide, drill 0.75mm (see https://www.diodes.com/assets/Package-Files/TO92L.pdf and http://www.ti.com/lit/an/snoa059/snoa059.pdf)")
    (tags "TO-92L Molded Narrow transistor")
    (fp_text reference Q105 (at 1.397 2.413) (layer F.SilkS))
    (fp_text value BC817-40 (at 1.29 2.79 180) (layer F.Fab))
    (fp_text user %R (at 1.29 -3.56 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 2.794 0.381 270) (size 1.3 1.3) (drill 0.75) (layers *.Cu *.Mask)
      (net 59 "Net-(C108-Pad2)"))
    (pad 3 thru_hole circle (at -0.254 0.381 270) (size 1.3 1.3) (drill 0.75) (layers *.Cu *.Mask)
      (net 5 +12V))
    (pad 2 thru_hole circle (at 1.28 -1.27 270) (size 1.3 1.3) (drill 0.75) (layers *.Cu *.Mask)
      (net 58 "Net-(C108-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92L.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:CP_Elec_5x5.7 (layer F.Cu) (tedit 5ACCE2FE)
    (at 263.144 112.268 90)
    (descr "SMT capacitor, aluminium electrolytic, 5x5.7")
    (attr smd)
    (fp_text reference C122 (at 4.826 0.127 180) (layer F.SilkS))
    (fp_text value 10uF/25V (at 0 -3.92 90) (layer F.Fab))
    (fp_text user + (at -1.4 -0.06 90) (layer F.Fab))
    (fp_text user + (at -3.38 2.36 90) (layer F.SilkS))
    (fp_text user %R (at 0 3.92 90) (layer F.Fab))
    (pad 1 smd rect (at -2.2 0 270) (size 3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 43 /VCC+14V))
    (pad 2 smd rect (at 2.2 0 270) (size 3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/CP_Elec_5x5.7.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x07_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 221.8436 87.9094 180)
    (descr "Through hole straight pin header, 2x07, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x07 2.54mm double row")
    (fp_text reference J1 (at -0.0254 -2.3876 180) (layer F.SilkS))
    (fp_text value Conn_01x14 (at 1.27 17.57 180) (layer F.Fab))
    (fp_text user %R (at 1.27 7.62 270) (layer F.Fab))
    (pad 14 thru_hole oval (at 2.54 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 13 thru_hole oval (at 0 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 +12V))
    (pad 12 thru_hole oval (at 2.54 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 11 thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /AUDIO))
    (pad 10 thru_hole oval (at 2.54 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 9 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 /VD))
    (pad 8 thru_hole oval (at 2.54 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 7 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 54 /HD/CS))
    (pad 6 thru_hole oval (at 2.54 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 5 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 53 /R/R-Y))
    (pad 4 thru_hole oval (at 2.54 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 52 /B/B-Y))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 51 /G/Y))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x07_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 5AD3A38A)
    (at 186.817 55.88)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U1 (at 0 0) (layer F.SilkS))
    (fp_text value LM1881 (at 0 3.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 11 /CSYNC))
    (pad 2 smd rect (at -2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C1-Pad1)"))
    (pad 3 smd rect (at -2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(U1-Pad3)"))
    (pad 4 smd rect (at -2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at 2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(U1-Pad5)"))
    (pad 6 smd rect (at 2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C4-Pad2)"))
    (pad 7 smd rect (at 2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(U1-Pad7)"))
    (pad 8 smd rect (at 2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-223 (layer F.Cu) (tedit 5AD77948)
    (at 207.772 50.292)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference U2 (at 0 0) (layer F.SilkS))
    (fp_text value AZ1117-5.0 (at 0 4.5) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 4 smd rect (at 3.15 0) (size 2 3.8) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -3.15 0) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 19 +5V))
    (pad 3 smd rect (at -3.15 2.3) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 5 +12V))
    (pad 1 smd rect (at -3.15 -2.3) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module scart-conn:K-SCARTX-024 (layer F.Cu) (tedit 5AE62249)
    (at 190.373 91.313 270)
    (fp_text reference J1 (at -22.225 -2.54 270) (layer F.SilkS))
    (fp_text value SCART-F (at -26.035 2.54) (layer F.Fab))
    (pad "" np_thru_hole oval (at 22.86 2.54 270) (size 2 4.8) (drill oval 2 4.8) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 19.06 5.08 270) (size 2.2 2.2) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 31 "Net-(J1-Pad1)"))
    (pad 3 thru_hole circle (at 15.25 5.08 270) (size 2.2 2.2) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 30 "Net-(J1-Pad3)"))
    (pad 5 thru_hole circle (at 11.44 5.08 270) (size 2.2 2.2) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 7 thru_hole circle (at 7.63 5.08 270) (size 2.2 2.2) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 16 /B-BY))
    (pad 9 thru_hole circle (at 3.82 5.08 270) (size 2.2 2.2) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 11 thru_hole circle (at 0.01 5.08 270) (size 2.2 2.2) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 15 /GY))
    (pad 13 thru_hole circle (at -3.8 5.08 270) (size 2.2 2.2) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 15 thru_hole circle (at -7.61 5.08 270) (size 2.2 2.2) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 14 /R-RY))
    (pad 17 thru_hole circle (at -11.42 5.08 270) (size 2.2 2.2) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 29 "Net-(J1-Pad17)"))
    (pad 19 thru_hole circle (at -15.23 5.08 270) (size 2.2 2.2) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 28 "Net-(J1-Pad19)"))
    (pad 21 thru_hole circle (at -19.04 5.08 270) (size 2.2 2.2) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole circle (at 17.145 0 270) (size 2.2 2.2) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 3 /AUDIO_R))
    (pad 4 thru_hole circle (at 13.335 0 270) (size 2.2 2.2) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 6 thru_hole circle (at 9.525 0 270) (size 2.2 2.2) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 1 /AUDIO_L))
    (pad 8 thru_hole circle (at 5.715 0 270) (size 2.2 2.2) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 27 "Net-(J1-Pad8)"))
    (pad 10 thru_hole circle (at 1.905 0 270) (size 2.2 2.2) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(J1-Pad10)"))
    (pad 12 thru_hole circle (at -1.905 0 270) (size 2.2 2.2) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(J1-Pad12)"))
    (pad 14 thru_hole circle (at -5.715 0 270) (size 2.2 2.2) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(J1-Pad14)"))
    (pad 16 thru_hole circle (at -9.525 0 270) (size 2.2 2.2) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(J1-Pad16)"))
    (pad 18 thru_hole circle (at -13.335 0 270) (size 2.2 2.2) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(J1-Pad18)"))
    (pad 20 thru_hole circle (at -17.145 0 270) (size 2.2 2.2) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 13 /CVBS_CSYNC))
    (pad "" np_thru_hole oval (at -22.86 2.54 270) (size 2 4.8) (drill oval 2 4.8) (layers *.Cu *.SilkS *.Mask Dwgs.User Eco1.User Eco2.User))
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x07_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 205.994 58.039)
    (descr "Through hole straight pin header, 2x07, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x07 2.54mm double row")
    (fp_text reference J4 (at 0 -2.159) (layer F.SilkS))
    (fp_text value Conn_01x14 (at 1.27 17.57) (layer F.Fab))
    (fp_text user %R (at 1.27 7.62 90) (layer F.Fab))
    (pad 14 thru_hole oval (at 2.54 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 13 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 +12V))
    (pad 12 thru_hole oval (at 2.54 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 11 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /AUDIO))
    (pad 10 thru_hole oval (at 2.54 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 9 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 "Net-(J4-Pad9)"))
    (pad 8 thru_hole oval (at 2.54 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 7 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /HD_CS))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /R-RY))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /B-BY))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /GY))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x07_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module eswitch-dpdt:eswitch-dpdt-m2 (layer F.Cu) (tedit 5AB17F78)
    (at 210.312 94.234 180)
    (fp_text reference SW1 (at 2.54 2.413) (layer F.SilkS))
    (fp_text value SW_DPDT_x2 (at 2.55 -2.8 180) (layer F.Fab))
    (pad 6 thru_hole circle (at 4.83 9.4 180) (size 2.5 2.5) (drill 1.85) (layers *.Cu *.Mask)
      (net 21 "Net-(R4-Pad2)"))
    (pad 3 thru_hole circle (at 0 9.4 180) (size 2.5 2.5) (drill 1.85) (layers *.Cu *.Mask)
      (net 20 "Net-(R3-Pad2)"))
    (pad 5 thru_hole circle (at 4.83 4.7 180) (size 2.5 2.5) (drill 1.85) (layers *.Cu *.Mask)
      (net 3 /AUDIO_R))
    (pad 2 thru_hole circle (at 0 4.7 180) (size 2.5 2.5) (drill 1.85) (layers *.Cu *.Mask)
      (net 1 /AUDIO_L))
    (pad 4 thru_hole circle (at 4.83 0 180) (size 2.5 2.5) (drill 1.85) (layers *.Cu *.Mask)
      (net 8 /SW_AUDIO_R))
    (pad 1 thru_hole circle (at 0 0 180) (size 2.5 2.5) (drill 1.85) (layers *.Cu *.Mask)
      (net 9 /SW_AUDIO_L))
  )
  (module eswitch-dpdt:eswitch-dpdt-m2 (layer F.Cu) (tedit 5AB17F78)
    (at 198.501 49.53 180)
    (fp_text reference SW2 (at 2.413 2.286 180) (layer F.SilkS))
    (fp_text value SW_DPDT_x2 (at 2.55 -2.8 180) (layer F.Fab))
    (pad 6 thru_hole circle (at 4.83 9.4 180) (size 2.5 2.5) (drill 1.85) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole circle (at 0 9.4 180) (size 2.5 2.5) (drill 1.85) (layers *.Cu *.Mask)
      (net 11 /CSYNC))
    (pad 5 thru_hole circle (at 4.83 4.7 180) (size 2.5 2.5) (drill 1.85) (layers *.Cu *.Mask)
      (net 6 "Net-(D1-Pad1)"))
    (pad 2 thru_hole circle (at 0 4.7 180) (size 2.5 2.5) (drill 1.85) (layers *.Cu *.Mask)
      (net 17 /HD_CS))
    (pad 4 thru_hole circle (at 4.83 0 180) (size 2.5 2.5) (drill 1.85) (layers *.Cu *.Mask)
      (net 32 "Net-(SW2-Pad4)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 2.5 2.5) (drill 1.85) (layers *.Cu *.Mask)
      (net 13 /CVBS_CSYNC))
  )
  (module rca:RCJ-02 (layer F.Cu) (tedit 5AB16243)
    (at 205.105 119.507)
    (fp_text reference J3 (at -0.0254 -3.0734 180) (layer F.SilkS))
    (fp_text value Conn_Coaxial (at -4.15 -2.25) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.6 2.6) (drill 1.7) (layers *.Cu *.Mask)
      (net 9 /SW_AUDIO_L))
    (pad 2 thru_hole circle (at 5.15 1.6) (size 3 3) (drill 2) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at -5.15 1.6) (size 3 3) (drill 2) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module rca:RCJ-02 (layer F.Cu) (tedit 5AB16243)
    (at 205.105 105.791)
    (fp_text reference J2 (at -0.0254 -2.9718 180) (layer F.SilkS))
    (fp_text value Conn_Coaxial (at -4.15 -2.25) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.6 2.6) (drill 1.7) (layers *.Cu *.Mask)
      (net 8 /SW_AUDIO_R))
    (pad 2 thru_hole circle (at 5.15 1.6) (size 3 3) (drill 2) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at -5.15 1.6) (size 3 3) (drill 2) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module smd-jumper:SMD-JUMPER (layer F.Cu) (tedit 5AE75FAD)
    (at 199.263 57.785)
    (fp_text reference JP1 (at -1.524 1.651 180) (layer F.SilkS))
    (fp_text value 5V (at 1.397 1.651) (layer F.Fab))
    (pad 1 smd trapezoid (at -0.5 0) (size 0.8 1.27) (rect_delta -0.5 0 ) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(C2-Pad1)"))
    (pad 2 smd trapezoid (at 0.5 0) (size 0.8 1.27) (rect_delta 0.5 0 ) (layers F.Cu F.Paste F.Mask)
      (net 5 +12V))
  )
  (module smd-jumper:SMD-JUMPER (layer F.Cu) (tedit 5AE75FAD)
    (at 199.271 53.975)
    (fp_text reference JP2 (at -1.651 1.651 180) (layer F.SilkS))
    (fp_text value 12V (at 1.524 1.651) (layer F.Fab))
    (pad 1 smd trapezoid (at -0.5 0) (size 0.8 1.27) (rect_delta -0.5 0 ) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(C2-Pad1)"))
    (pad 2 smd trapezoid (at 0.5 0) (size 0.8 1.27) (rect_delta 0.5 0 ) (layers F.Cu F.Paste F.Mask)
      (net 19 +5V))
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5AB3FBE3)
    (at 181.102 56.134 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at -2.921 0 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 4.318 0.889 270) (layer F.Fab))
    (fp_text user %R (at 3.302 -1.016 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 13 /CVBS_CSYNC))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5AD3A37F)
    (at 194.056 53.975 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at -1.397 -1.778) (layer F.SilkS))
    (fp_text value 10uF (at 1.27 -1.778 180) (layer F.Fab))
    (fp_text user %R (at -1.397 -1.778 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 186.817 61.468 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at -1.27 -1.778 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 1.905 -1.778 180) (layer F.Fab))
    (fp_text user %R (at -1.143 -1.778 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D5.0mm (layer F.Cu) (tedit 5995936A)
    (at 183.388 46.99 270)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (fp_text reference D1 (at 4.191 -2.794) (layer F.SilkS))
    (fp_text value LED (at 4.699 2.413) (layer F.Fab))
    (fp_text user %R (at 1.25 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 6 "Net-(D1-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 7 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D5.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5AD3A3B1)
    (at 188.976 48.006 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at -3.175 0) (layer F.SilkS))
    (fp_text value R_LED (at -0.127 -1.651 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 5 +12V))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5AD39700)
    (at 194.056 57.785 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C4 (at -1.397 -1.778 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 1.524 -1.778 180) (layer F.Fab))
    (fp_text user %R (at -1.397 -1.778 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C4-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5AD8D9C1)
    (at 194.056 61.468 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at -1.397 -1.778) (layer F.SilkS))
    (fp_text value 680k (at 1.524 -1.778 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C4-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5AF882AC)
    (at 183.388 130.429)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference J5 (at 0.0635 -0.0635) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 4.2) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5B6C9055)
    (at 183.388 39.116)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference J6 (at 0 -0.0635) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 4.2) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5B71892B)
    (at 208.788 39.116)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference J7 (at 0 0.127) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 4.2) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 208.788 130.429)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (zone_connect 2)
    (fp_text reference J8 (at 0.0635 -0.127) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 4.2) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5ABA700E)
    (at 200.406 76.962)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference J9 (at 0.0635 -0.1905) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 4.2) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 3.8 3.8) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 200.406 61.468)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C5 (at 1.397 1.778) (layer F.SilkS))
    (fp_text value 10uF (at -1.524 1.778) (layer F.Fab))
    (fp_text user %R (at 1.397 1.778) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 +12V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5AD3A4F1)
    (at 207.899 44.577)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C6 (at -2.921 0 -90) (layer F.SilkS))
    (fp_text value 10uF (at 1.27 -1.778) (layer F.Fab))
    (fp_text user %R (at -1.27 -1.778) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 19 +5V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5AF87E5B)
    (at 210.312 80.518 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at -3.0988 0.0254) (layer F.SilkS))
    (fp_text value 475R (at 0.0508 -1.778 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 10 /AUDIO))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(R3-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5AF87E3A)
    (at 205.486 80.518 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at -3.048 0.0762) (layer F.SilkS))
    (fp_text value 475R (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 10 /AUDIO))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(R4-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5AF87E5F)
    (at 207.899 80.518 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R5 (at 3.048 0 180) (layer F.SilkS))
    (fp_text value 20K (at -3.8608 0.1016 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 10 /AUDIO))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5AB01DF7)
    (at 229.9462 100.9396 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R152 (at 0 1.651 270) (layer F.SilkS))
    (fp_text value 75 (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 42 /VD))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5AD1061B)
    (at 229.9462 87.884 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R143 (at 0 1.6002 90) (layer F.SilkS))
    (fp_text value 75 (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 54 /HD/CS))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5AD10639)
    (at 229.362 74.2696 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R129 (at 0.0254 1.651 90) (layer F.SilkS))
    (fp_text value 75 (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 53 /R/R-Y))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5AD10665)
    (at 228.854 60.88 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R115 (at -0.047 1.651 90) (layer F.SilkS))
    (fp_text value 75 (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 52 /B/B-Y))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5AB01DCD)
    (at 228.854 47.498 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R101 (at 0 1.651 270) (layer F.SilkS))
    (fp_text value 75 (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 51 /G/Y))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SOD-123 (layer F.Cu) (tedit 5AB01E09)
    (at 229.616 127.762 270)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D201 (at -0.0254 1.905 90) (layer F.SilkS))
    (fp_text value D_Zener (at 0 2.1 270) (layer F.Fab))
    (fp_text user %R (at 0 -2 270) (layer F.Fab))
    (pad 1 smd rect (at -1.65 0 270) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(C203-Pad1)"))
    (pad 2 smd rect (at 1.65 0 270) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SOD-123 (layer F.Cu) (tedit 5AB01FB6)
    (at 241.7572 102.5906 270)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D110 (at 3.1496 0.0762) (layer F.SilkS))
    (fp_text value D (at 0 2.1 270) (layer F.Fab))
    (fp_text user %R (at 0 -2 270) (layer F.Fab))
    (pad 1 smd rect (at -1.65 0 270) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(C105-Pad1)"))
    (pad 2 smd rect (at 1.65 0 270) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SOD-123 (layer F.Cu) (tedit 58645DC7)
    (at 241.7572 97.028 270)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D109 (at -2.9718 0) (layer F.SilkS))
    (fp_text value D (at 0 2.1 270) (layer F.Fab))
    (fp_text user %R (at 0 -2 270) (layer F.Fab))
    (pad 1 smd rect (at -1.65 0 270) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 5 +12V))
    (pad 2 smd rect (at 1.65 0 270) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(C105-Pad1)"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SOD-123 (layer F.Cu) (tedit 5AB01F21)
    (at 241.7572 89.154 270)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D108 (at 3.0988 0.0508) (layer F.SilkS))
    (fp_text value D (at 0 2.1 270) (layer F.Fab))
    (fp_text user %R (at 0 -2 270) (layer F.Fab))
    (pad 1 smd rect (at -1.65 0 270) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(C104-Pad1)"))
    (pad 2 smd rect (at 1.65 0 270) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SOD-123 (layer F.Cu) (tedit 58645DC7)
    (at 241.7572 83.566 270)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D107 (at -3.0226 0.0508) (layer F.SilkS))
    (fp_text value D (at 0 2.1 270) (layer F.Fab))
    (fp_text user %R (at 0 -2 270) (layer F.Fab))
    (pad 1 smd rect (at -1.65 0 270) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 5 +12V))
    (pad 2 smd rect (at 1.65 0 270) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(C104-Pad1)"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SOD-123 (layer F.Cu) (tedit 5AB01EE8)
    (at 241.7572 75.6666 270)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D106 (at 3.048 0.0254) (layer F.SilkS))
    (fp_text value D (at 0 2.1 270) (layer F.Fab))
    (fp_text user %R (at 0 -2 270) (layer F.Fab))
    (pad 1 smd rect (at -1.65 0 270) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(C103-Pad1)"))
    (pad 2 smd rect (at 1.65 0 270) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SOD-123 (layer F.Cu) (tedit 58645DC7)
    (at 241.808 70.104 270)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D105 (at -2.9718 0.0254) (layer F.SilkS))
    (fp_text value D (at 0 2.1 270) (layer F.Fab))
    (fp_text user %R (at 0 -2 270) (layer F.Fab))
    (pad 1 smd rect (at -1.65 0 270) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 5 +12V))
    (pad 2 smd rect (at 1.65 0 270) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(C103-Pad1)"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SOD-123 (layer F.Cu) (tedit 5AB01EF0)
    (at 241.7572 62.23 270)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D104 (at 3.048 0) (layer F.SilkS))
    (fp_text value D (at 0 2.1 270) (layer F.Fab))
    (fp_text user %R (at 0 -2 270) (layer F.Fab))
    (pad 1 smd rect (at -1.65 0 270) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(C102-Pad1)"))
    (pad 2 smd rect (at 1.65 0 270) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SOD-123 (layer F.Cu) (tedit 58645DC7)
    (at 241.808 56.642 270)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D103 (at -3.048 0) (layer F.SilkS))
    (fp_text value D (at 0 2.1 270) (layer F.Fab))
    (fp_text user %R (at 0 -2 270) (layer F.Fab))
    (pad 1 smd rect (at -1.65 0 270) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 5 +12V))
    (pad 2 smd rect (at 1.65 0 270) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(C102-Pad1)"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SOD-123 (layer F.Cu) (tedit 5AB01E51)
    (at 241.808 48.768 270)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D102 (at 3.175 0) (layer F.SilkS))
    (fp_text value D (at 0 2.1 270) (layer F.Fab))
    (fp_text user %R (at 0 -2 270) (layer F.Fab))
    (pad 1 smd rect (at -1.65 0 270) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(C101-Pad1)"))
    (pad 2 smd rect (at 1.65 0 270) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SOD-123 (layer F.Cu) (tedit 5AB01E56)
    (at 241.808 43.18 270)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D101 (at -3.048 0) (layer F.SilkS))
    (fp_text value D (at 0 2.1 270) (layer F.Fab))
    (fp_text user %R (at 0 -2 270) (layer F.Fab))
    (pad 1 smd rect (at -1.65 0 270) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 5 +12V))
    (pad 2 smd rect (at 1.65 0 270) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(C101-Pad1)"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:CP_Elec_4x5.7 (layer F.Cu) (tedit 58AA8612)
    (at 223.52 112.268 90)
    (descr "SMT capacitor, aluminium electrolytic, 4x5.7")
    (attr smd)
    (fp_text reference C203 (at 0 -3.048 270) (layer F.SilkS))
    (fp_text value 1uF/50V (at 0 -3.54 90) (layer F.Fab))
    (fp_text user + (at -1.1 -0.08 90) (layer F.Fab))
    (fp_text user + (at -2.77 2.01 90) (layer F.SilkS))
    (fp_text user %R (at 0 3.54 90) (layer F.Fab))
    (pad 1 smd rect (at -1.8 0 270) (size 2.6 1.6) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(C203-Pad1)"))
    (pad 2 smd rect (at 1.8 0 270) (size 2.6 1.6) (layers F.Cu F.Paste F.Mask)
      (net 10 /AUDIO))
    (model Capacitors_SMD.3dshapes/CP_Elec_4x5.7.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:CP_Elec_5x5.7 (layer F.Cu) (tedit 58AA8AEF)
    (at 235.4402 99.822 180)
    (descr "SMT capacitor, aluminium electrolytic, 5x5.7")
    (attr smd)
    (fp_text reference C105 (at 0 3.429 180) (layer F.SilkS))
    (fp_text value 10uF/50V (at 0 -3.92 180) (layer F.Fab))
    (fp_text user + (at -1.4 -0.06 180) (layer F.Fab))
    (fp_text user + (at -3.38 2.36 180) (layer F.SilkS))
    (fp_text user %R (at 0 3.92 180) (layer F.Fab))
    (pad 1 smd rect (at -2.2 0) (size 3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(C105-Pad1)"))
    (pad 2 smd rect (at 2.2 0) (size 3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 42 /VD))
    (model Capacitors_SMD.3dshapes/CP_Elec_5x5.7.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:CP_Elec_5x5.7 (layer F.Cu) (tedit 58AA8AEF)
    (at 235.458 86.36 180)
    (descr "SMT capacitor, aluminium electrolytic, 5x5.7")
    (attr smd)
    (fp_text reference C104 (at 0.127 3.429 180) (layer F.SilkS))
    (fp_text value 10uF/50V (at 0 -3.92 180) (layer F.Fab))
    (fp_text user + (at -1.4 -0.06 180) (layer F.Fab))
    (fp_text user + (at -3.38 2.36 180) (layer F.SilkS))
    (fp_text user %R (at 0 3.92 180) (layer F.Fab))
    (pad 1 smd rect (at -2.2 0) (size 3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(C104-Pad1)"))
    (pad 2 smd rect (at 2.2 0) (size 3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 54 /HD/CS))
    (model Capacitors_SMD.3dshapes/CP_Elec_5x5.7.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 248.92 127.762 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R205 (at 0 1.651 270) (layer F.SilkS))
    (fp_text value 2.7K (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 45 /AUDIO_))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5AB01E0F)
    (at 237.3884 127.762 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R204 (at 0.0254 1.7272 90) (layer F.SilkS))
    (fp_text value 68K (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0.7112 0.5588 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(C204-Pad2)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5AB01E1C)
    (at 237.3884 122.174 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R203 (at 0.1016 1.7272 90) (layer F.SilkS))
    (fp_text value 56K (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 5 +12V))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(C204-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5AB037F4)
    (at 231.648 123.4948 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R202 (at 0.033 1.651 180) (layer F.SilkS))
    (fp_text value 1K (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(C204-Pad2)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(C203-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 263.144 97.028)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R160 (at 0 -1.7) (layer F.SilkS))
    (fp_text value OPT (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 50 /VD_))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5AB01F9D)
    (at 263.144 102.616 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R159 (at 0.033 1.651 180) (layer F.SilkS))
    (fp_text value 0 (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 50 /VD_))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(C113-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5AB01F96)
    (at 258.318 102.616 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R158 (at 0 -1.651 90) (layer F.SilkS))
    (fp_text value 2.7k (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(C113-Pad1)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5AB03803)
    (at 248.666 102.616 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R157 (at 3.175 0.033) (layer F.SilkS))
    (fp_text value 33k (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 65 "Net-(C113-Pad2)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5AB01F7E)
    (at 248.666 97.028 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R156 (at -3.048 0) (layer F.SilkS))
    (fp_text value 33k (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 5 +12V))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 65 "Net-(C113-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 245.364 99.822 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R155 (at 0 1.651 90) (layer F.SilkS))
    (fp_text value 100 (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 65 "Net-(C113-Pad2)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(C105-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5AB01F5D)
    (at 263.144 83.566)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R151 (at -0.381 -1.684) (layer F.SilkS))
    (fp_text value OPT (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 49 /HD))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5AB01F6B)
    (at 263.144 89.154 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R150 (at 0.033 1.651 180) (layer F.SilkS))
    (fp_text value 0 (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 49 /HD))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 62 "Net-(C112-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5AB01F58)
    (at 258.318 89.154 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R149 (at 0 -1.651 90) (layer F.SilkS))
    (fp_text value 2.7k (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 62 "Net-(C112-Pad1)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5AB01F71)
    (at 248.666 89.154 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R148 (at 3.175 0.033) (layer F.SilkS))
    (fp_text value 33k (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(C112-Pad2)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5AD106DF)
    (at 248.666 83.566 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R147 (at -3.048 0.033) (layer F.SilkS))
    (fp_text value 33k (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 5 +12V))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(C112-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 245.364 86.36 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R146 (at 0 1.651 90) (layer F.SilkS))
    (fp_text value 100 (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(C112-Pad2)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(C104-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 261.8232 74.7776)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R142 (at 0 -1.6256) (layer F.SilkS))
    (fp_text value 100 (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 60 "Net-(C110-Pad1)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 48 /R-Y))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 256.0828 76.8096 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R135 (at 0 -1.7 180) (layer F.SilkS))
    (fp_text value 1.5k (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 60 "Net-(C110-Pad1)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5AB01F34)
    (at 248.666 75.692 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R134 (at 3.1115 0.033) (layer F.SilkS))
    (fp_text value 33k (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(C110-Pad2)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5AB01F06)
    (at 248.666 70.104 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R133 (at -3.048 0.033) (layer F.SilkS))
    (fp_text value 56k (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 5 +12V))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(C110-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 245.364 72.898 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R132 (at 0 1.651 90) (layer F.SilkS))
    (fp_text value 100 (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(C110-Pad2)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(C103-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 261.874 61.468)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R128 (at 0 -1.524) (layer F.SilkS))
    (fp_text value 100 (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 58 "Net-(C108-Pad1)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 47 /B-Y))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 256.54 63.246 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R121 (at 0 1.651 270) (layer F.SilkS))
    (fp_text value 1.5k (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 58 "Net-(C108-Pad1)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5AB01ECF)
    (at 248.666 62.23 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R120 (at 3.048 0) (layer F.SilkS))
    (fp_text value 33k (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 59 "Net-(C108-Pad2)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5AB01EB9)
    (at 248.666 56.642 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R119 (at -3.048 0.033 180) (layer F.SilkS))
    (fp_text value 56k (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 5 +12V))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 59 "Net-(C108-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 245.364 59.436 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R118 (at 0 1.651 90) (layer F.SilkS))
    (fp_text value 100 (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 59 "Net-(C108-Pad2)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(C102-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 261.8562 48.006)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R114 (at 0 -1.524) (layer F.SilkS))
    (fp_text value 100 (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(C106-Pad1)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 46 /Y))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 256.54 49.784 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R107 (at 0 1.651 270) (layer F.SilkS))
    (fp_text value 1.5k (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(C106-Pad1)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5AB01E62)
    (at 248.666 48.768 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R106 (at 3.0734 0 180) (layer F.SilkS))
    (fp_text value 33k (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(C106-Pad2)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5AB01E6C)
    (at 248.666 43.18 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R105 (at -3.048 0 180) (layer F.SilkS))
    (fp_text value 56k (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 5 +12V))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(C106-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 245.364 45.974 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R104 (at 0.127 1.524 90) (layer F.SilkS))
    (fp_text value 100 (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(C106-Pad2)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(C101-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Angled_2x25_Pitch2.54mm (layer F.Cu) (tedit 59650533)
    (at 269.1892 69.1896)
    (descr "Through hole angled pin header, 2x25, 2.54mm pitch, 6mm pin length, double rows")
    (tags "Through hole angled pin header THT 2x25 2.54mm double row")
    (fp_text reference J2 (at 0.0508 -2.2606) (layer F.SilkS))
    (fp_text value CONN_02X25 (at 5.655 63.23) (layer F.Fab))
    (fp_text user %R (at 5.31 30.48 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 /Y))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 /B-Y))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 48 /R-Y))
    (pad 7 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 8 thru_hole oval (at 2.54 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 9 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 10 thru_hole oval (at 2.54 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 11 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 12 thru_hole oval (at 2.54 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 /HD))
    (pad 13 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 14 thru_hole oval (at 2.54 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 50 /VD_))
    (pad 15 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 16 thru_hole oval (at 2.54 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 17 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 18 thru_hole oval (at 2.54 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 19 thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 20 thru_hole oval (at 2.54 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 21 thru_hole oval (at 0 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 22 thru_hole oval (at 2.54 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 23 thru_hole oval (at 0 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 24 thru_hole oval (at 2.54 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 25 thru_hole oval (at 0 30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 26 thru_hole oval (at 2.54 30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 27 thru_hole oval (at 0 33.02) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 28 thru_hole oval (at 2.54 33.02) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 29 thru_hole oval (at 0 35.56) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 30 thru_hole oval (at 2.54 35.56) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 31 thru_hole oval (at 0 38.1) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 32 thru_hole oval (at 2.54 38.1) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 33 thru_hole oval (at 0 40.64) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 34 thru_hole oval (at 2.54 40.64) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 35 thru_hole oval (at 0 43.18) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 36 thru_hole oval (at 2.54 43.18) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 37 thru_hole oval (at 0 45.72) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 38 thru_hole oval (at 2.54 45.72) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 39 thru_hole oval (at 0 48.26) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 /VCC+14V))
    (pad 40 thru_hole oval (at 2.54 48.26) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 41 thru_hole oval (at 0 50.8) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 /VCC+14V))
    (pad 42 thru_hole oval (at 2.54 50.8) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 43 thru_hole oval (at 0 53.34) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 44 thru_hole oval (at 2.54 53.34) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 45 thru_hole oval (at 0 55.88) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 46 thru_hole oval (at 2.54 55.88) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 47 thru_hole oval (at 0 58.42) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 48 thru_hole oval (at 2.54 58.42) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 /AUDIO_))
    (pad 49 thru_hole oval (at 0 60.96) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 50 thru_hole oval (at 2.54 60.96) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Angled_2x25_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5AB01E34)
    (at 248.92 122.174 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C206 (at 0 -1.684 90) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 +12V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 242.824 129.032 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C205 (at 0 1.651 180) (layer F.SilkS))
    (fp_text value 180pF (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 45 /AUDIO_))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(C204-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5AB01E01)
    (at 223.4692 103.124 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C202 (at 0.0508 1.6002 180) (layer F.SilkS))
    (fp_text value 180pF (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 10 /AUDIO))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 223.4692 106.426 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C201 (at -0.0254 1.5748 180) (layer F.SilkS))
    (fp_text value 180pF (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 10 /AUDIO))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5AB01F91)
    (at 258.318 97.028 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C119 (at 0.033 1.651 90) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 +12V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5AB01F66)
    (at 258.318 83.566 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C118 (at 0.033 1.651 90) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 +12V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5AB01FF6)
    (at 261.874 70.104 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C117 (at 0 -1.651 90) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 +12V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5AB01EA6)
    (at 261.874 56.642 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C116 (at 0 -1.6002 90) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 +12V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:CP_Elec_6.3x5.7 (layer F.Cu) (tedit 5AB01E9C)
    (at 268.0792 45.974 270)
    (descr "SMT capacitor, aluminium electrolytic, 6.3x5.7")
    (attr smd)
    (fp_text reference C115 (at -5.334 0.16) (layer F.SilkS))
    (fp_text value 100uF/16V (at 0 -4.56 270) (layer F.Fab))
    (fp_text user + (at -1.79 -0.06 270) (layer F.Fab))
    (fp_text user + (at -4.28 3.01 270) (layer F.SilkS))
    (fp_text user %R (at 0 4.56 270) (layer F.Fab))
    (pad 1 smd rect (at -2.7 0 90) (size 3.5 1.6) (layers F.Cu F.Paste F.Mask)
      (net 5 +12V))
    (pad 2 smd rect (at 2.7 0 90) (size 3.5 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/CP_Elec_6.3x5.7.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5AB01EAB)
    (at 261.874 43.18 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C114 (at 0 -1.524 90) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 +12V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5AB03806)
    (at 253.4742 102.616 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C113 (at -0.0178 -1.651 180) (layer F.SilkS))
    (fp_text value OPT (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(C113-Pad1)"))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 65 "Net-(C113-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 253.492 89.154 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C112 (at 0 -1.75 180) (layer F.SilkS))
    (fp_text value OPT (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 62 "Net-(C112-Pad1)"))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(C112-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5AB01F0C)
    (at 251.968 72.898 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C110 (at 0 -1.524 90) (layer F.SilkS))
    (fp_text value OPT (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 60 "Net-(C110-Pad1)"))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(C110-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5AB01EC9)
    (at 251.968 59.436 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C108 (at 0 -1.524 90) (layer F.SilkS))
    (fp_text value OPT (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 58 "Net-(C108-Pad1)"))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 59 "Net-(C108-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5AB01E73)
    (at 251.968 45.974 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C106 (at 0 -1.524 90) (layer F.SilkS))
    (fp_text value OPT (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(C106-Pad1)"))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(C106-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:CP_Elec_6.3x5.7 (layer F.Cu) (tedit 58AA8B43)
    (at 235.4402 72.898 180)
    (descr "SMT capacitor, aluminium electrolytic, 6.3x5.7")
    (attr smd)
    (fp_text reference C103 (at -0.0178 4.064 180) (layer F.SilkS))
    (fp_text value 47uF/25V (at 0 -4.56 180) (layer F.Fab))
    (fp_text user + (at -1.79 -0.06 180) (layer F.Fab))
    (fp_text user + (at -4.28 3.01 180) (layer F.SilkS))
    (fp_text user %R (at 0 4.56 180) (layer F.Fab))
    (pad 1 smd rect (at -2.7 0) (size 3.5 1.6) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(C103-Pad1)"))
    (pad 2 smd rect (at 2.7 0) (size 3.5 1.6) (layers F.Cu F.Paste F.Mask)
      (net 53 /R/R-Y))
    (model Capacitors_SMD.3dshapes/CP_Elec_6.3x5.7.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:CP_Elec_6.3x5.7 (layer F.Cu) (tedit 58AA8B43)
    (at 235.4402 59.436 180)
    (descr "SMT capacitor, aluminium electrolytic, 6.3x5.7")
    (attr smd)
    (fp_text reference C102 (at 0 4.064 180) (layer F.SilkS))
    (fp_text value 47uF/25V (at 0 -4.56 180) (layer F.Fab))
    (fp_text user + (at -1.79 -0.06 180) (layer F.Fab))
    (fp_text user + (at -4.28 3.01 180) (layer F.SilkS))
    (fp_text user %R (at 0 4.56 180) (layer F.Fab))
    (pad 1 smd rect (at -2.7 0) (size 3.5 1.6) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(C102-Pad1)"))
    (pad 2 smd rect (at 2.7 0) (size 3.5 1.6) (layers F.Cu F.Paste F.Mask)
      (net 52 /B/B-Y))
    (model Capacitors_SMD.3dshapes/CP_Elec_6.3x5.7.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:CP_Elec_6.3x5.7 (layer F.Cu) (tedit 58AA8B43)
    (at 235.4072 45.974 180)
    (descr "SMT capacitor, aluminium electrolytic, 6.3x5.7")
    (attr smd)
    (fp_text reference C101 (at 0 4.064 180) (layer F.SilkS))
    (fp_text value 47uF/25V (at 0 -4.56 180) (layer F.Fab))
    (fp_text user + (at -1.79 -0.06 180) (layer F.Fab))
    (fp_text user + (at -4.28 3.01 180) (layer F.SilkS))
    (fp_text user %R (at 0 4.56 180) (layer F.Fab))
    (pad 1 smd rect (at -2.7 0) (size 3.5 1.6) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(C101-Pad1)"))
    (pad 2 smd rect (at 2.7 0) (size 3.5 1.6) (layers F.Cu F.Paste F.Mask)
      (net 51 /G/Y))
    (model Capacitors_SMD.3dshapes/CP_Elec_6.3x5.7.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 261.874 51.5366)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R113 (at 0 -1.4986) (layer F.SilkS))
    (fp_text value 390 (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(C106-Pad1)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 261.874 65.024)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R127 (at 0 -1.524) (layer F.SilkS))
    (fp_text value 390 (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 58 "Net-(C108-Pad1)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 261.8232 78.4606)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R141 (at 0 -1.7) (layer F.SilkS))
    (fp_text value 390 (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 60 "Net-(C110-Pad1)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5AB02885)
    (at 257.1496 129.6924)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (zone_connect 2)
    (fp_text reference J3 (at 0 -0.0254) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 4.2) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 3.6 3.6) (drill 3.2) (layers *.Cu *.Mask)
      (zone_connect 2))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5AB0287E)
    (at 220.9038 129.9718)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (zone_connect 2)
    (fp_text reference J4 (at -0.1778 -0.0508) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 4.2) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 3.6 3.6) (drill 3.2) (layers *.Cu *.Mask)
      (zone_connect 2))
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5B728E8B)
    (at 233.426 127.762 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C204 (at 0.0254 -1.5748 90) (layer F.SilkS))
    (fp_text value 39pF (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(C204-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5AB164B7)
    (at 258.318 112.141 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C121 (at -3.302 0 180) (layer F.SilkS))
    (fp_text value 1uF/25V (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 +12V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:CP_Elec_5x5.7 (layer F.Cu) (tedit 5ACCE2F4)
    (at 253.492 112.268 270)
    (descr "SMT capacitor, aluminium electrolytic, 5x5.7")
    (attr smd)
    (fp_text reference C120 (at 4.8006 -0.0508) (layer F.SilkS))
    (fp_text value 10uF/25V (at 0 -3.92 270) (layer F.Fab))
    (fp_text user + (at -1.4 -0.06 270) (layer F.Fab))
    (fp_text user + (at -3.38 2.36 270) (layer F.SilkS))
    (fp_text user %R (at 0 3.92 270) (layer F.Fab))
    (pad 1 smd rect (at -2.2 0 90) (size 3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 5 +12V))
    (pad 2 smd rect (at 2.2 0 90) (size 3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/CP_Elec_5x5.7.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:CP_Elec_6.3x5.7 (layer F.Cu) (tedit 5AD10715)
    (at 256.54 122.0724)
    (descr "SMT capacitor, aluminium electrolytic, 6.3x5.7")
    (attr smd)
    (fp_text reference C207 (at 0 4.1656) (layer F.SilkS))
    (fp_text value 100uF/16V (at 0 -4.56) (layer F.Fab))
    (fp_text user + (at -1.79 -0.06) (layer F.Fab))
    (fp_text user + (at -4.28 3.01) (layer F.SilkS))
    (fp_text user %R (at 0 4.56) (layer F.Fab))
    (pad 1 smd rect (at -2.7 0 180) (size 3.5 1.6) (layers F.Cu F.Paste F.Mask)
      (net 5 +12V))
    (pad 2 smd rect (at 2.7 0 180) (size 3.5 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/CP_Elec_6.3x5.7.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (gr_arc (start 211.582 56.642) (end 211.582 56.134) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 211.582 74.676) (end 211.074 74.676) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_text "10x10 layout by\nJari Mikkilä\njari@mikkila.org" (at 268.8082 59.1566 90) (layer F.SilkS))
  (gr_text "2018 Martin Hejnfelt (martin@hejnfelt.com)" (at 224.9678 53.4924 90) (layer F.SilkS))
  (gr_text R/R-Y (at 235.458 77.5462) (layer F.SilkS))
  (gr_text "2018 Martin Hejnfelt\n(martin@hejnfelt.com)" (at 195.9356 130.9116) (layer F.SilkS))
  (gr_text "10x10 layout by\nJari Mikkilä\njari@mikkila.org" (at 199.4535 90.2335 90) (layer F.SilkS))
  (gr_line (start 215.9 134.62) (end 215.9 131.826) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 213.868 131.826) (end 213.868 134.62) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 215.9 121.666) (end 215.9 128.016) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 213.868 128.016) (end 213.868 121.666) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 215.9 117.602) (end 215.9 111.506) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 213.868 111.506) (end 213.868 117.602) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 215.9 107.569) (end 215.9 100.711) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 213.868 100.711) (end 213.868 107.569) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 215.9 96.647) (end 215.9 90.551) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 213.868 90.551) (end 213.868 96.647) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 215.9 80.391) (end 215.9 86.614) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 213.868 80.391) (end 213.868 86.614) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 213.868 75.184) (end 213.868 76.3905) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 215.9 76.454) (end 215.9 52.578) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 215.9 42.291) (end 215.9 48.514) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 215.9 34.925) (end 215.9 38.354) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 213.868 56.134) (end 213.868 52.578) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 213.868 48.514) (end 213.868 42.291) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 214.884 131.826) (end 215.9 131.826) (angle -180) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 214.884 128.016) (end 213.868 128.016) (angle -180) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 214.884 121.666) (end 215.9 121.666) (angle -180) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 214.884 117.602) (end 213.868 117.602) (angle -180) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 214.884 111.506) (end 215.9 111.506) (angle -180) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 214.884 107.569) (end 213.868 107.569) (angle -180) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 214.884 100.711) (end 215.9 100.711) (angle -180) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 214.884 96.647) (end 213.868 96.647) (angle -180) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 214.884 90.551) (end 215.9 90.551) (angle -180) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 214.884 86.614) (end 213.868 86.614) (angle -180) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 214.884 80.391) (end 215.9 80.391) (angle -180) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 214.884 76.454) (end 213.868 76.454) (angle -180) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 214.884 52.578) (end 215.9 52.578) (angle -180) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 214.884 48.514) (end 213.868 48.514) (angle -180) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 214.884 42.291) (end 215.9 42.291) (angle -180) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 214.884 38.354) (end 213.868 38.354) (angle -176.1859439) (layer Edge.Cuts) (width 0.15))
  (gr_text "IF-C01COMG CLONE\nSCART INPUT\n" (at 196.2912 126.0348) (layer F.SilkS))
  (gr_line (start 186.309 114.173) (end 189.357 114.173) (angle 90) (layer Edge.Cuts) (width 2))
  (gr_line (start 186.309 68.453) (end 189.357 68.453) (angle 90) (layer Edge.Cuts) (width 2))
  (gr_text 12V (at 201.168 59.309) (layer F.SilkS))
  (gr_text 5V (at 201.041 55.499) (layer F.SilkS))
  (gr_line (start 213.868 38.354) (end 213.868 34.925) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 211.582 75.184) (end 213.868 75.184) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 211.074 56.642) (end 211.074 74.676) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 213.868 56.134) (end 211.582 56.134) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text LEFT (at 199.5805 116.3955) (layer F.SilkS))
  (gr_text RIGHT (at 199.4535 102.616) (layer F.SilkS))
  (gr_line (start 213.868 34.925) (end 178.562 34.925) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 178.562 134.62) (end 178.562 34.925) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 213.868 134.62) (end 178.562 134.62) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text AUDIO (at 231.013 119.634) (layer F.SilkS))
  (gr_text G/Y (at 235.331 50.8) (layer F.SilkS))
  (gr_text B/B-Y (at 235.458 64.008) (layer F.SilkS))
  (gr_text CS (at 235.331 90.297) (layer F.SilkS))
  (gr_text VD (at 235.331 103.886) (layer F.SilkS))
  (gr_line (start 235.204 34.925) (end 215.9 34.925) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text "JVC IF-C01COMG (RGB/YPbPr)\nCLONE BASE BOARD\n" (at 221.0816 53.1368 90) (layer F.SilkS))
  (gr_line (start 275.209 34.925) (end 235.204 34.925) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 275.1582 134.62) (end 215.9 134.62) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 275.209 34.925) (end 275.1582 134.62) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 185.801 35.56) (xy 202.692 35.56) (xy 213.233 35.56) (xy 213.233 55.499) (xy 210.439 55.499)
        (xy 210.439 75.819) (xy 213.233 75.819) (xy 213.233 133.985) (xy 179.197 133.985) (xy 179.197 35.56)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 183.134 35.56) (xy 197.612 35.56) (xy 213.233 35.56) (xy 213.233 55.499) (xy 210.439 55.499)
        (xy 210.439 75.819) (xy 213.233 75.819) (xy 213.233 133.985) (xy 179.197 133.985) (xy 179.197 35.56)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 274.447 133.985) (xy 216.535 133.985) (xy 216.535 101.092) (xy 216.535 92.202) (xy 216.535 35.56)
        (xy 235.458 35.56) (xy 274.574 35.56)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 274.447 133.985) (xy 216.535 133.985) (xy 216.535 98.679) (xy 216.535 92.202) (xy 216.535 35.56)
        (xy 235.458 35.56) (xy 274.574 35.56)
      )
    )
  )
)
