(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "+5V")
  (net 2 "Earth")
  (net 3 "Net-(JP1-B)")
  (net 4 "Net-(JP2-B)")
  (net 5 "Net-(JP3-B)")
  (net 6 "Net-(JP4-B)")
  (net 7 "Net-(P1-Pin_1)")
  (net 8 "Net-(P1-Pin_2)")
  (net 9 "Net-(J1-Pin_07)")
  (net 10 "Net-(J1-Pin_08)")
  (net 11 "Net-(J1-Pin_11)")
  (net 12 "Net-(J1-Pin_12)")
  (net 13 "Net-(J1-Pin_03)")
  (net 14 "Net-(J1-Pin_05)")
  (net 15 "Net-(P1-Pin_3)")
  (net 16 "Net-(P1-Pin_4)")
  (footprint "Jumper:SolderJumper-2_P1.3mm_Open_Pad1.0x1.5mm" (layer "F.Cu")
    (at 196.49 126.492)
    (descr "SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (property "Sheetfile" "8250 disk interface board.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Solder Jumper, 2-pole, closed/bridged")
    (property "ki_keywords" "solder jumper SPST")
    (attr exclude_from_pos_files)
    (fp_text reference "JP3" (at -0.148 -2.032 180) (layer "F.SilkS"))
    (fp_text value "SolderJumper_2_Bridged" (at 0 1.9) (layer "F.Fab"))
    (pad "1" smd rect (at -0.65 0) (size 1 1.5) (layers "F.Cu" "F.Mask")
      (net 2 "Earth") (pinfunction "A") (pintype "passive"))
    (pad "2" smd rect (at 0.65 0) (size 1 1.5) (layers "F.Cu" "F.Mask")
      (net 5 "Net-(JP3-B)") (pinfunction "B") (pintype "passive"))
  )
  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal" (layer "F.Cu")
    (at 171.953 111.76 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "8250 disk interface board.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R3" (at -1.8034 0.005 180) (layer "F.SilkS"))
    (fp_text value "22k" (at 2.5654 1.7068 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 2.54 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 1 "+5V") (pintype "passive"))
    (pad "2" thru_hole oval (at 5.08 0 90) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 12 "Net-(J1-Pin_12)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "8250_feet:8250_14-pin_connector" (layer "F.Cu")
    (at 188 101.65)
    (property "Sheetfile" "8250 disk interface board.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x14, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J1" (at -20.106 -0.05 unlocked) (layer "F.SilkS"))
    (fp_text value "01x14_Servo connector" (at 1.12 3.75 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.12 5.25 unlocked) (layer "F.Fab"))
    (pad "P1-1" thru_hole oval (at 1.23 -0.05 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(J1-Pin_07)") (pinfunction "Pin_07") (pintype "passive"))
    (pad "P1-2" thru_hole oval (at -1.31 -0.05 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 10 "Net-(J1-Pin_08)") (pinfunction "Pin_08") (pintype "passive"))
    (pad "P1-3" thru_hole oval (at -3.85 -0.05 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "Earth") (pinfunction "Pin_19") (pintype "passive"))
    (pad "P1-4" thru_hole oval (at -6.39 -0.05 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "Earth") (pinfunction "Pin_10") (pintype "passive"))
    (pad "P2-1" thru_hole oval (at -8.93 -0.05 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 11 "Net-(J1-Pin_11)") (pinfunction "Pin_11") (pintype "passive"))
    (pad "P2-2" thru_hole oval (at -11.47 -0.05 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 12 "Net-(J1-Pin_12)") (pinfunction "Pin_12") (pintype "passive"))
    (pad "P2-3" thru_hole oval (at -14.01 -0.05 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "Earth") (pinfunction "Pin_13") (pintype "passive"))
    (pad "P2-4" thru_hole oval (at -16.55 -0.05 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "Earth") (pinfunction "Pin_14") (pintype "passive"))
    (pad "P3-1" thru_hole oval (at 11.39 -0.05 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 13 "Net-(J1-Pin_03)") (pinfunction "Pin_03") (pintype "passive"))
    (pad "P3-2" thru_hole oval (at 8.85 -0.05 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "Earth") (pinfunction "Pin_04") (pintype "passive"))
    (pad "P4-1" thru_hole oval (at 6.31 -0.05 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 14 "Net-(J1-Pin_05)") (pinfunction "Pin_05") (pintype "passive"))
    (pad "P4-2" thru_hole oval (at 3.77 -0.05 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "Earth") (pinfunction "Pin_06") (pintype "passive"))
    (pad "P5-1" thru_hole rect (at 16.47 -0.05 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "+5V") (pinfunction "Pin_01") (pintype "passive"))
    (pad "P5-2" thru_hole oval (at 13.93 -0.05 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "Earth") (pinfunction "Pin_02") (pintype "passive"))
  )
  (footprint "Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm" (layer "F.Cu")
    (at 204.45 106.9848 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
    (property "Sheetfile" "8250 disk interface board.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr through_hole)
    (fp_text reference "C3" (at 1.27 -2.286) (layer "F.SilkS"))
    (fp_text value "0.1 uF" (at 1.2246 -3.7592) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "Earth") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "+5V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Jumper:SolderJumper-2_P1.3mm_Open_Pad1.0x1.5mm" (layer "F.Cu")
    (at 192.94 126.492)
    (descr "SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (property "Sheetfile" "8250 disk interface board.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Solder Jumper, 2-pole, closed/bridged")
    (property "ki_keywords" "solder jumper SPST")
    (attr exclude_from_pos_files)
    (fp_text reference "JP4" (at -0.154 -2.032 180) (layer "F.SilkS"))
    (fp_text value "SolderJumper_2_Bridged" (at 0 1.9) (layer "F.Fab"))
    (pad "1" smd rect (at -0.65 0) (size 1 1.5) (layers "F.Cu" "F.Mask")
      (net 2 "Earth") (pinfunction "A") (pintype "passive"))
    (pad "2" smd rect (at 0.65 0) (size 1 1.5) (layers "F.Cu" "F.Mask")
      (net 6 "Net-(JP4-B)") (pinfunction "B") (pintype "passive"))
  )
  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal" (layer "F.Cu")
    (at 197.0786 111.7346 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "8250 disk interface board.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R4" (at -1.8288 0.0254 180) (layer "F.SilkS"))
    (fp_text value "22k" (at 2.54 1.92 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 2.54 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 1 "+5V") (pintype "passive"))
    (pad "2" thru_hole oval (at 5.08 0 90) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 10 "Net-(J1-Pin_08)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (at 73 114)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (property "Sheetfile" "8250 disk interface board.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H2" (at 0 -4.2) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 4.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Jumper:SolderJumper-2_P1.3mm_Open_Pad1.0x1.5mm" (layer "F.Cu")
    (at 203.59 126.492)
    (descr "SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (property "Sheetfile" "8250 disk interface board.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Solder Jumper, 2-pole, closed/bridged")
    (property "ki_keywords" "solder jumper SPST")
    (attr exclude_from_pos_files)
    (fp_text reference "JP1" (at -0.136 -2.032 180) (layer "F.SilkS"))
    (fp_text value "SolderJumper_2_Bridged" (at 0 1.9) (layer "F.Fab"))
    (pad "1" smd rect (at -0.65 0) (size 1 1.5) (layers "F.Cu" "F.Mask")
      (net 2 "Earth") (pinfunction "A") (pintype "passive"))
    (pad "2" smd rect (at 0.65 0) (size 1 1.5) (layers "F.Cu" "F.Mask")
      (net 3 "Net-(JP1-B)") (pinfunction "B") (pintype "passive"))
  )
  (footprint "Jumper:SolderJumper-2_P1.3mm_Open_Pad1.0x1.5mm" (layer "F.Cu")
    (at 200.04 126.492)
    (descr "SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (property "Sheetfile" "8250 disk interface board.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Solder Jumper, 2-pole, closed/bridged")
    (property "ki_keywords" "solder jumper SPST")
    (attr exclude_from_pos_files)
    (fp_text reference "JP2" (at -0.142 -2.032 180) (layer "F.SilkS"))
    (fp_text value "SolderJumper_2_Bridged" (at 0 1.9) (layer "F.Fab"))
    (pad "1" smd rect (at -0.65 0) (size 1 1.5) (layers "F.Cu" "F.Mask")
      (net 2 "Earth") (pinfunction "A") (pintype "passive"))
    (pad "2" smd rect (at 0.65 0) (size 1 1.5) (layers "F.Cu" "F.Mask")
      (net 4 "Net-(JP2-B)") (pinfunction "B") (pintype "passive"))
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (at 203 114)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (property "Sheetfile" "8250 disk interface board.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H1" (at 0 -4.2) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 4.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers "F&B.Cu" "*.Mask"))
  )
  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal" (layer "F.Cu")
    (at 194.813 106.7054 -90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "8250 disk interface board.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R2" (at 6.9342 0.0204) (layer "F.SilkS"))
    (fp_text value "200" (at 2.81 1.6714 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 2.54 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(J1-Pin_07)") (pintype "passive"))
    (pad "2" thru_hole oval (at 5.08 0 270) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 1 "+5V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal" (layer "F.Cu")
    (at 169.6212 106.68 -90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "8250 disk interface board.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R1" (at 6.858 0) (layer "F.SilkS"))
    (fp_text value "200" (at 2.54 1.92 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 2.54 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 11 "Net-(J1-Pin_11)") (pintype "passive"))
    (pad "2" thru_hole oval (at 5.08 0 270) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 1 "+5V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_DIP:DIP-14_W7.62mm_Socket_LongPads" (layer "F.Cu")
    (at 190.9572 106.7054 -90)
    (descr "14-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket, LongPads")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket LongPads")
    (property "Sheetfile" "8250 disk interface board.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Hex Inverter")
    (property "ki_keywords" "TTL not inv")
    (attr through_hole)
    (fp_text reference "U1" (at 10.404 7.625 -180) (layer "F.SilkS"))
    (fp_text value "74LS04" (at 3.81 17.57 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 7.62) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 10 "Net-(J1-Pin_08)") (pintype "input"))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 13 "Net-(J1-Pin_03)") (pintype "output"))
    (pad "3" thru_hole oval (at 0 5.08 270) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 12 "Net-(J1-Pin_12)") (pintype "input"))
    (pad "4" thru_hole oval (at 0 7.62 270) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 14 "Net-(J1-Pin_05)") (pintype "output"))
    (pad "5" thru_hole oval (at 0 10.16 270) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 3 "Net-(JP1-B)") (pintype "input"))
    (pad "6" thru_hole oval (at 0 12.7 270) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 7 "Net-(P1-Pin_1)") (pintype "output"))
    (pad "7" thru_hole oval (at 0 15.24 270) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "Earth") (pinfunction "GND") (pintype "power_in"))
    (pad "8" thru_hole oval (at 7.62 15.24 270) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(P1-Pin_2)") (pintype "output"))
    (pad "9" thru_hole oval (at 7.62 12.7 270) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(JP2-B)") (pintype "input"))
    (pad "10" thru_hole oval (at 7.62 10.16 270) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 15 "Net-(P1-Pin_3)") (pintype "output"))
    (pad "11" thru_hole oval (at 7.62 7.62 270) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 5 "Net-(JP3-B)") (pintype "input"))
    (pad "12" thru_hole oval (at 7.62 5.08 270) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 16 "Net-(P1-Pin_4)") (pintype "output"))
    (pad "13" thru_hole oval (at 7.62 2.54 270) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 6 "Net-(JP4-B)") (pintype "input"))
    (pad "14" thru_hole oval (at 7.62 0 270) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "+5V") (pinfunction "VCC") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-14_W7.62mm_Socket.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical" (layer "F.Cu")
    (at 201.158 121.666 -90)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (property "Sheetfile" "8250 disk interface board.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "P1" (at 0 -3.058 -180) (layer "F.SilkS"))
    (fp_text value "Conn_01x04" (at 0 9.95 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 3.81) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 7 "Net-(P1-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(P1-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 15 "Net-(P1-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 16 "Net-(P1-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line locked (start 207 129) (end 69 129)
    (layer "Edge.Cuts"))
  (gr_line locked (start 207 99) (end 207 129)
    (layer "Edge.Cuts"))
  (gr_line (start 69 99) (end 207 99)
    (layer "Edge.Cuts"))
  (gr_line (start 69 129) (end 69 99)
    (layer "Edge.Cuts"))
  (gr_text "MPI Servo Board\nFor Comodore 8050/8250\nDisk Drive\nPCB #314227-01\nJDTucker V 0.1\n09/24/23" (at 169.164 125.73) (layer "B.SilkS"))
  (gr_text "P2" (at 174.371 104.5972) (layer "F.SilkS"))
  (gr_text "P4" (at 192.151 104.5972) (layer "F.SilkS"))
  (gr_text "P3" (at 197.1548 104.5972) (layer "F.SilkS"))
  (gr_text "P5" (at 202.2094 104.5972) (layer "F.SilkS"))
  (gr_text "P1" (at 184.5056 104.5972) (layer "F.SilkS"))
  (zone (net 2) (net_name "Earth") (layer "B.Cu") (hatch edge 0.5)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 208.407 98.492107)
        (xy 208.327692 131.2164)
        (xy 67.9958 131.910612)
        (xy 67.914621 98.441605)
      )
    )
  )
)
