(kicad_pcb (version 4) (host pcbnew 4.0.5)
  (general
    (links 11)
    (no_connects 0)
    (area 133.274999 58.344999 191.845001 99.135001)
    (thickness 1.6)
    (drawings 21)
    (tracks 44)
    (zones 0)
    (modules 15)
    (nets 9)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.1524)
    (user_trace_width 0.35)
    (user_trace_width 2)
    (user_trace_width 3)
    (user_trace_width 4)
    (user_trace_width 5)
    (user_trace_width 6)
    (trace_clearance 0.1524)
    (zone_clearance 0.5)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (user_via 2 1)
    (user_via 3 2)
    (user_via 4 3)
    (user_via 6 5)
    (uvia_size 0.762)
    (uvia_drill 0.508)
    (uvias_allowed no)
    (uvia_min_size 0.01016)
    (uvia_min_drill 0.00254)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 5)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(12V1-Pad1)")
  (net 2 "Net-(GND1-Pad1)")
  (net 3 "Net-(GND2-Pad1)")
  (net 4 "Net-(IRF3708-Pad1)")
  (net 5 "Net-(IRF3708-Pad2)")
  (net 6 "Net-(OC1-Pad3)")
  (net 7 "Net-(OC1-Pad2)")
  (net 8 "Net-(IN1-Pad1)")
  (net_class Default "Dies ist die voreingestellte Netzklasse."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net "Net-(GND1-Pad1)")
    (add_net "Net-(IN1-Pad1)")
    (add_net "Net-(IRF3708-Pad1)")
    (add_net "Net-(OC1-Pad2)")
    (add_net "Net-(OC1-Pad3)")
  )
  (net_class Hochstrom ""
    (clearance 0.2)
    (trace_width 2)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net "Net-(12V1-Pad1)")
    (add_net "Net-(GND2-Pad1)")
    (add_net "Net-(IRF3708-Pad2)")
  )
  (module Wire_Pads:SolderWirePad_single_2mmDrill (layer F.Cu) (tedit 593EBDDC)
    (at 187.96 95.25)
    (fp_text reference REF** (at 12.065 6.35) (layer F.SilkS))
    (fp_text value SolderWirePad_single_2mmDrill (at 8.89 8.89) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.50088 4.50088) (drill 1.99898) (layers *.Cu *.Mask))
  )
  (module Wire_Pads:SolderWirePad_single_2mmDrill (layer F.Cu) (tedit 593EBDC0)
    (at 187.96 62.23)
    (fp_text reference REF** (at 2.54 -6.35) (layer F.SilkS))
    (fp_text value SolderWirePad_single_2mmDrill (at 11.43 -8.89) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.50088 4.50088) (drill 1.99898) (layers *.Cu *.Mask))
  )
  (module Wire_Pads:SolderWirePad_single_2mmDrill (layer F.Cu) (tedit 593EBDD9)
    (at 137.16 95.25)
    (fp_text reference REF** (at -11.43 6.35) (layer F.SilkS))
    (fp_text value SolderWirePad_single_2mmDrill (at -9.525 8.89) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.50088 4.50088) (drill 1.99898) (layers *.Cu *.Mask))
  )
  (module Wire_Pads:SolderWirePad_single_SMD_5x10mm (layer F.Cu) (tedit 593EC2FB)
    (at 173.99 66.04)
    (descr "Wire Pad, Square, SMD Pad,  5mm x 10mm,")
    (tags "MesurementPoint Square SMDPad 5mmx10mm ")
    (attr smd)
    (fp_text reference 12V (at 0 6.35) (layer F.SilkS))
    (fp_text value 12V (at 0 6.35) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 5 10) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(12V1-Pad1)"))
  )
  (module Wire_Pads:SolderWirePad_single_SMD_5x10mm (layer F.Cu) (tedit 593EC320)
    (at 168.91 93.98 270)
    (descr "Wire Pad, Square, SMD Pad,  5mm x 10mm,")
    (tags "MesurementPoint Square SMDPad 5mmx10mm ")
    (attr smd)
    (fp_text reference GND (at 0 -6.985 270) (layer F.SilkS))
    (fp_text value GND (at 0 -6.985 450) (layer F.Fab))
    (pad 1 smd rect (at 0 0 270) (size 5 10) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(GND1-Pad1)"))
  )
  (module Wire_Pads:SolderWirePad_single_SMD_5x10mm (layer F.Cu) (tedit 593EC2EE)
    (at 153.035 66.04)
    (descr "Wire Pad, Square, SMD Pad,  5mm x 10mm,")
    (tags "MesurementPoint Square SMDPad 5mmx10mm ")
    (attr smd)
    (fp_text reference GND (at 0 6.35) (layer F.SilkS))
    (fp_text value GND (at 0 6.35) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 5 10) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(GND2-Pad1)"))
  )
  (module TO_SOT_Packages_THT:TO-220_Vertical (layer F.Cu) (tedit 593EC392)
    (at 153.035 85.725 90)
    (descr "TO-220, Vertical, RM 2.54mm")
    (tags "TO-220 Vertical RM 2.54mm")
    (fp_text reference IRF3708 (at 8.89 0.635 180) (layer F.SilkS))
    (fp_text value NMOS_GDS (at -3.81 1.27 180) (layer F.Fab))
    (fp_text user %R (at 8.89 0.635 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(IRF3708-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(IRF3708-Pad2)"))
    (pad 3 thru_hole oval (at 5.08 0 90) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(GND2-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-220_Vertical.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-4_W7.62mm (layer F.Cu) (tedit 593EC42C)
    (at 168.91 88.9 180)
    (descr "4-lead dip package, row spacing 7.62 mm (300 mils)")
    (tags "DIL DIP PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference PC817 (at 3.81 5.08 180) (layer F.SilkS))
    (fp_text value PC817 (at 3.81 5.08 180) (layer F.Fab))
    (fp_text user %R (at 3.81 0 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(IN1-Pad1)"))
    (pad 3 thru_hole oval (at 7.62 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(OC1-Pad3)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(OC1-Pad2)"))
    (pad 4 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(12V1-Pad1)"))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-4_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0414_L11.9mm_D4.5mm_P15.24mm_Horizontal (layer F.Cu) (tedit 593EC371)
    (at 172.72 82.55)
    (descr "Resistor, Axial_DIN0414 series, Axial, Horizontal, pin pitch=15.24mm, 2W, length*diameter=11.9*4.5mm^2, http://www.vishay.com/docs/20128/wkxwrx.pdf")
    (tags "Resistor Axial_DIN0414 series Axial Horizontal pin pitch 15.24mm 2W length 11.9mm diameter 4.5mm")
    (fp_text reference 100R (at 7.62 0) (layer F.SilkS))
    (fp_text value 100R (at 7.62 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 4 "Net-(IRF3708-Pad1)"))
    (pad 2 thru_hole oval (at 15.24 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 6 "Net-(OC1-Pad3)"))
    (model Resistors_THT.3dshapes/R_Axial_DIN0414_L11.9mm_D4.5mm_P15.24mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0414_L11.9mm_D4.5mm_P15.24mm_Horizontal (layer F.Cu) (tedit 593EC37B)
    (at 187.96 77.47 180)
    (descr "Resistor, Axial_DIN0414 series, Axial, Horizontal, pin pitch=15.24mm, 2W, length*diameter=11.9*4.5mm^2, http://www.vishay.com/docs/20128/wkxwrx.pdf")
    (tags "Resistor Axial_DIN0414 series Axial Horizontal pin pitch 15.24mm 2W length 11.9mm diameter 4.5mm")
    (fp_text reference 10K (at 7.62 0 180) (layer F.SilkS))
    (fp_text value 10K (at 7.62 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 4 "Net-(IRF3708-Pad1)"))
    (pad 2 thru_hole oval (at 15.24 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 "Net-(GND2-Pad1)"))
    (model Resistors_THT.3dshapes/R_Axial_DIN0414_L11.9mm_D4.5mm_P15.24mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0414_L11.9mm_D4.5mm_P15.24mm_Horizontal (layer F.Cu) (tedit 593EC361)
    (at 172.72 87.63)
    (descr "Resistor, Axial_DIN0414 series, Axial, Horizontal, pin pitch=15.24mm, 2W, length*diameter=11.9*4.5mm^2, http://www.vishay.com/docs/20128/wkxwrx.pdf")
    (tags "Resistor Axial_DIN0414 series Axial Horizontal pin pitch 15.24mm 2W length 11.9mm diameter 4.5mm")
    (fp_text reference 680R (at 7.62 0) (layer F.SilkS))
    (fp_text value 680R (at 7.62 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 7 "Net-(OC1-Pad2)"))
    (pad 2 thru_hole oval (at 15.24 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 "Net-(GND1-Pad1)"))
    (model Resistors_THT.3dshapes/R_Axial_DIN0414_L11.9mm_D4.5mm_P15.24mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wire_Pads:SolderWirePad_single_SMD_5x10mm (layer F.Cu) (tedit 593EC338)
    (at 156.21 93.98 270)
    (descr "Wire Pad, Square, SMD Pad,  5mm x 10mm,")
    (tags "MesurementPoint Square SMDPad 5mmx10mm ")
    (attr smd)
    (fp_text reference IN+ (at 0 6.35 270) (layer F.SilkS))
    (fp_text value IN+ (at 0 6.35 270) (layer F.Fab))
    (pad 1 smd rect (at 0 0 270) (size 5 10) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(IN1-Pad1)"))
  )
  (module Wire_Pads:SolderWirePad_single_SMD_5x10mm (layer F.Cu) (tedit 593EC2CF)
    (at 167.005 66.04)
    (descr "Wire Pad, Square, SMD Pad,  5mm x 10mm,")
    (tags "MesurementPoint Square SMDPad 5mmx10mm ")
    (attr smd)
    (fp_text reference LOAD+ (at 0 6.35) (layer F.SilkS))
    (fp_text value LOAD+ (at 0 6.35) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 5 10) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(12V1-Pad1)"))
  )
  (module Wire_Pads:SolderWirePad_single_SMD_5x10mm (layer F.Cu) (tedit 593EC2E0)
    (at 160.02 66.04)
    (descr "Wire Pad, Square, SMD Pad,  5mm x 10mm,")
    (tags "MesurementPoint Square SMDPad 5mmx10mm ")
    (attr smd)
    (fp_text reference LOAD- (at 0 6.35) (layer F.SilkS))
    (fp_text value LOAD- (at 0 6.35 180) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 5 10) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(IRF3708-Pad2)"))
  )
  (module Wire_Pads:SolderWirePad_single_2mmDrill (layer F.Cu) (tedit 593EBDC7)
    (at 137.16 62.23)
    (fp_text reference REF** (at -12.065 -5.715) (layer F.SilkS))
    (fp_text value SolderWirePad_single_2mmDrill (at -10.795 -7.62) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.50088 4.50088) (drill 1.99898) (layers *.Cu *.Mask))
  )
  (gr_text "CUT OUT" (at 143.51 80.645) (layer F.SilkS))
  (dimension 58.42 (width 0.3) (layer Dwgs.User)
    (gr_text "58,420 mm" (at 162.56 48.815) (layer Dwgs.User))
    (feature1 (pts (xy 191.77 53.34) (xy 191.77 47.465)))
    (feature2 (pts (xy 133.35 53.34) (xy 133.35 47.465)))
    (crossbar (pts (xy 133.35 50.165) (xy 191.77 50.165)))
    (arrow1a (pts (xy 191.77 50.165) (xy 190.643496 50.751421)))
    (arrow1b (pts (xy 191.77 50.165) (xy 190.643496 49.578579)))
    (arrow2a (pts (xy 133.35 50.165) (xy 134.476504 50.751421)))
    (arrow2b (pts (xy 133.35 50.165) (xy 134.476504 49.578579)))
  )
  (dimension 17.78 (width 0.3) (layer Dwgs.User)
    (gr_text "17,780 mm" (at 182.88 54.53) (layer Dwgs.User))
    (feature1 (pts (xy 191.77 58.42) (xy 191.77 53.18)))
    (feature2 (pts (xy 173.99 58.42) (xy 173.99 53.18)))
    (crossbar (pts (xy 173.99 55.88) (xy 191.77 55.88)))
    (arrow1a (pts (xy 191.77 55.88) (xy 190.643496 56.466421)))
    (arrow1b (pts (xy 191.77 55.88) (xy 190.643496 55.293579)))
    (arrow2a (pts (xy 173.99 55.88) (xy 175.116504 56.466421)))
    (arrow2b (pts (xy 173.99 55.88) (xy 175.116504 55.293579)))
  )
  (dimension 40.64 (width 0.3) (layer Dwgs.User)
    (gr_text "40,640 mm" (at 153.67 54.53) (layer Dwgs.User))
    (feature1 (pts (xy 173.99 58.42) (xy 173.99 53.18)))
    (feature2 (pts (xy 133.35 58.42) (xy 133.35 53.18)))
    (crossbar (pts (xy 133.35 55.88) (xy 173.99 55.88)))
    (arrow1a (pts (xy 173.99 55.88) (xy 172.863496 56.466421)))
    (arrow1b (pts (xy 173.99 55.88) (xy 172.863496 55.293579)))
    (arrow2a (pts (xy 133.35 55.88) (xy 134.476504 56.466421)))
    (arrow2b (pts (xy 133.35 55.88) (xy 134.476504 55.293579)))
  )
  (dimension 40.64 (width 0.3) (layer Dwgs.User)
    (gr_text "40,640 mm" (at 130.095 78.74 270) (layer Dwgs.User))
    (feature1 (pts (xy 133.35 99.06) (xy 128.745 99.06)))
    (feature2 (pts (xy 133.35 58.42) (xy 128.745 58.42)))
    (crossbar (pts (xy 131.445 58.42) (xy 131.445 99.06)))
    (arrow1a (pts (xy 131.445 99.06) (xy 130.858579 97.933496)))
    (arrow1b (pts (xy 131.445 99.06) (xy 132.031421 97.933496)))
    (arrow2a (pts (xy 131.445 58.42) (xy 130.858579 59.546504)))
    (arrow2b (pts (xy 131.445 58.42) (xy 132.031421 59.546504)))
  )
  (gr_line (start 133.35 62.23) (end 133.35 95.25) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 137.16 95.25) (end 137.16 99.06) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 137.16 62.23) (end 133.35 62.23) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 187.96 95.25) (end 191.77 95.25) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 187.96 62.23) (end 187.96 58.42) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 187.96 58.42) (end 137.16 58.42) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 191.77 95.25) (end 191.77 62.23) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 187.96 99.06) (end 137.16 99.06) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 147.955 69.215) (end 139.065 69.215) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 149.86 89.535) (end 149.86 71.12) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 147.955 91.44) (end 139.065 91.44) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 147.955 71.12) (end 147.955 69.215) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 139.065 71.12) (end 137.16 71.12) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 137.16 89.535) (end 137.16 71.12) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 139.065 89.535) (end 139.065 91.44) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 147.955 89.535) (end 149.86 89.535) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 191.77 99.06) (xy 133.35 99.06) (xy 133.35 58.42) (xy 191.77 58.42)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 191.77 99.06) (xy 133.35 99.06) (xy 133.35 58.42) (xy 191.77 58.42)
      )
    )
  )
)
