(kicad_pcb (version 4) (host pcbnew 4.0.5)
  (general
    (links 88)
    (no_connects 0)
    (area 223.444999 18.9256 278.205001 69.925001)
    (thickness 1.6)
    (drawings 7)
    (tracks 359)
    (zones 0)
    (modules 33)
    (nets 55)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions false)
      (gerberprecision 5)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory GERBER/))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 "Net-(C1-Pad2)")
  (net 3 "Net-(C2-Pad1)")
  (net 4 "Net-(C2-Pad2)")
  (net 5 "Net-(C3-Pad1)")
  (net 6 "Net-(C3-Pad2)")
  (net 7 "Net-(C4-Pad2)")
  (net 8 "Net-(C5-Pad1)")
  (net 9 "Net-(C7-Pad1)")
  (net 10 "Net-(CON1-Pad1)")
  (net 11 "Net-(CON1-Pad3)")
  (net 12 "Net-(CON1-Pad4)")
  (net 13 "Net-(CON1-Pad5)")
  (net 14 "Net-(D1-Pad4)")
  (net 15 "Net-(D1-Pad1)")
  (net 16 "Net-(D1-Pad3)")
  (net 17 "Net-(D1-Pad2)")
  (net 18 "Net-(D3-Pad4)")
  (net 19 "Net-(D3-Pad3)")
  (net 20 "Net-(D4-Pad1)")
  (net 21 "Net-(IC1-Pad1)")
  (net 22 "Net-(IC1-Pad2)")
  (net 23 "Net-(IC1-Pad9)")
  (net 24 "Net-(IC1-Pad10)")
  (net 25 "Net-(IC1-Pad11)")
  (net 26 "Net-(IC1-Pad12)")
  (net 27 "Net-(IC1-Pad13)")
  (net 28 "Net-(IC1-Pad14)")
  (net 29 "Net-(IC1-Pad19)")
  (net 30 "Net-(IC1-Pad22)")
  (net 31 "Net-(IC1-Pad23)")
  (net 32 "Net-(IC1-Pad24)")
  (net 33 "Net-(IC1-Pad25)")
  (net 34 "Net-(IC1-Pad26)")
  (net 35 "Net-(IC1-Pad27)")
  (net 36 "Net-(IC1-Pad28)")
  (net 37 "Net-(IC1-Pad30)")
  (net 38 "Net-(IC1-Pad31)")
  (net 39 "Net-(IC1-Pad32)")
  (net 40 "Net-(P3-Pad2)")
  (net 41 "Net-(P3-Pad3)")
  (net 42 "Net-(Q1-Pad1)")
  (net 43 "Net-(R1-Pad2)")
  (net 44 "Net-(R3-Pad1)")
  (net 45 "Net-(R5-Pad2)")
  (net 46 "Net-(R6-Pad1)")
  (net 47 "Net-(R7-Pad1)")
  (net 48 "Net-(U3-Pad7)")
  (net 49 "Net-(U3-Pad8)")
  (net 50 "Net-(U3-Pad9)")
  (net 51 "Net-(U3-Pad10)")
  (net 52 GND)
  (net 53 VCC)
  (net 54 "Net-(D2-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C3-Pad2)")
    (add_net "Net-(C4-Pad2)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(CON1-Pad1)")
    (add_net "Net-(CON1-Pad3)")
    (add_net "Net-(CON1-Pad4)")
    (add_net "Net-(CON1-Pad5)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D1-Pad3)")
    (add_net "Net-(D1-Pad4)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad3)")
    (add_net "Net-(D3-Pad4)")
    (add_net "Net-(D4-Pad1)")
    (add_net "Net-(IC1-Pad1)")
    (add_net "Net-(IC1-Pad10)")
    (add_net "Net-(IC1-Pad11)")
    (add_net "Net-(IC1-Pad12)")
    (add_net "Net-(IC1-Pad13)")
    (add_net "Net-(IC1-Pad14)")
    (add_net "Net-(IC1-Pad19)")
    (add_net "Net-(IC1-Pad2)")
    (add_net "Net-(IC1-Pad22)")
    (add_net "Net-(IC1-Pad23)")
    (add_net "Net-(IC1-Pad24)")
    (add_net "Net-(IC1-Pad25)")
    (add_net "Net-(IC1-Pad26)")
    (add_net "Net-(IC1-Pad27)")
    (add_net "Net-(IC1-Pad28)")
    (add_net "Net-(IC1-Pad30)")
    (add_net "Net-(IC1-Pad31)")
    (add_net "Net-(IC1-Pad32)")
    (add_net "Net-(IC1-Pad9)")
    (add_net "Net-(P3-Pad2)")
    (add_net "Net-(P3-Pad3)")
    (add_net "Net-(Q1-Pad1)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R3-Pad1)")
    (add_net "Net-(R5-Pad2)")
    (add_net "Net-(R6-Pad1)")
    (add_net "Net-(R7-Pad1)")
    (add_net "Net-(U3-Pad10)")
    (add_net "Net-(U3-Pad7)")
    (add_net "Net-(U3-Pad8)")
    (add_net "Net-(U3-Pad9)")
    (add_net VCC)
  )
  (module "Personal Footprints:Capacitor_0805" (layer F.Cu) (tedit 58B52ABF)
    (at 250.825 58.42 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 0 -1.75 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.75 270) (layer F.SilkS))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Personal Footprints:Capacitor_0805" (layer F.Cu) (tedit 58B52ABF)
    (at 250.825 64.135 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at 0 -1.75 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.75 270) (layer F.SilkS))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C2-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Personal Footprints:Capacitor_0805" (layer F.Cu) (tedit 58B52ABF)
    (at 247.65 60.96 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at 0 -1.75 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.75 270) (layer F.SilkS))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C3-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Personal Footprints:Capacitor_0805" (layer F.Cu) (tedit 58B52ABF)
    (at 243.84 36.83 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C4 (at 0 -1.75 270) (layer F.SilkS))
    (fp_text value 27pF (at 0 1.75 270) (layer F.SilkS))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 52 GND))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C4-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Personal Footprints:Capacitor_0805" (layer F.Cu) (tedit 58B52ABF)
    (at 243.84 46.99 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C5 (at 0 -1.75 270) (layer F.SilkS))
    (fp_text value 27pF (at 0 1.75 270) (layer F.SilkS))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C5-Pad1)"))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 52 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Personal Footprints:Capacitor_0805" (layer F.Cu) (tedit 58B52ABF)
    (at 262.89 55.88)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C6 (at 0 -1.75) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.75) (layer F.SilkS))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 52 GND))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 53 VCC))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Personal Footprints:Capacitor_0805" (layer F.Cu) (tedit 58B52ABF)
    (at 251.46 24.13 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C7 (at 0 -1.75 270) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.75 270) (layer F.SilkS))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C7-Pad1)"))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 52 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Personal Footprints:Capacitor_0805" (layer F.Cu) (tedit 58B52ABF)
    (at 261.62 35.56 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C8 (at 0 -1.75 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.75 90) (layer F.SilkS))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 53 VCC))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 52 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Personal Footprints:MB1S_SOIC-4" (layer F.Cu) (tedit 58B52B5C)
    (at 234.95 50.8 270)
    (fp_text reference D1 (at -3.6322 0.8636 360) (layer F.SilkS))
    (fp_text value MB1S (at 4.2926 1.2192 360) (layer F.SilkS))
    (pad 4 smd rect (at -1.27 -2.1832 270) (size 1.55 2.1) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(D1-Pad4)"))
    (pad 1 smd rect (at -1.27 4.3168 270) (size 1.55 2.1) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(D1-Pad1)"))
    (pad 3 smd rect (at 1.27 -2.1832 270) (size 1.55 2.1) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(D1-Pad3)"))
    (pad 2 smd rect (at 1.27 4.3168 270) (size 1.55 2.1) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(D1-Pad2)"))
  )
  (module "Personal Footprints:MB1S_SOIC-4" (layer F.Cu) (tedit 58B52B5C)
    (at 259.08 24.13 270)
    (fp_text reference D3 (at -3.6322 0.8636 360) (layer F.SilkS))
    (fp_text value MB1S (at 4.2926 1.2192 360) (layer F.SilkS))
    (pad 4 smd rect (at -1.27 -2.1832 270) (size 1.55 2.1) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(D3-Pad4)"))
    (pad 1 smd rect (at -1.27 4.3168 270) (size 1.55 2.1) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C7-Pad1)"))
    (pad 3 smd rect (at 1.27 -2.1832 270) (size 1.55 2.1) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(D3-Pad3)"))
    (pad 2 smd rect (at 1.27 4.3168 270) (size 1.55 2.1) (layers F.Cu F.Paste F.Mask)
      (net 52 GND))
  )
  (module "Personal Footprints:LED_0603" (layer F.Cu) (tedit 58B53BE7)
    (at 273.05 44.45)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference D4 (at 0 -1.45) (layer F.SilkS))
    (fp_text value LED (at 0 1.55) (layer F.SilkS))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(D4-Pad1)"))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 53 VCC))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Personal Footprints:QFP_32" (layer F.Cu) (tedit 58B5921B)
    (at 256.54 44.45)
    (fp_text reference IC1 (at 0 -6.7) (layer F.SilkS))
    (fp_text value ATMEGA328-A (at 0 6.7) (layer F.SilkS))
    (pad 1 smd oval (at -4.5 -2.8 90) (size 0.4 2) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(IC1-Pad1)"))
    (pad 2 smd oval (at -4.5 -2 90) (size 0.4 2) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(IC1-Pad2)"))
    (pad 3 smd oval (at -4.5 -1.2 90) (size 0.4 2) (layers F.Cu F.Paste F.Mask)
      (net 52 GND))
    (pad 4 smd oval (at -4.5 -0.4 90) (size 0.4 2) (layers F.Cu F.Paste F.Mask)
      (net 53 VCC))
    (pad 5 smd oval (at -4.5 0.4 90) (size 0.4 2) (layers F.Cu F.Paste F.Mask)
      (net 52 GND))
    (pad 6 smd oval (at -4.5 1.2 90) (size 0.4 2) (layers F.Cu F.Paste F.Mask)
      (net 53 VCC))
    (pad 7 smd oval (at -4.5 2 90) (size 0.4 2) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C4-Pad2)"))
    (pad 8 smd oval (at -4.5 2.8 90) (size 0.4 2) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C5-Pad1)"))
    (pad 9 smd oval (at -2.8 4.5) (size 0.4 2) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(IC1-Pad9)"))
    (pad 10 smd oval (at -2 4.5) (size 0.4 2) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(IC1-Pad10)"))
    (pad 11 smd oval (at -1.2 4.5) (size 0.4 2) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(IC1-Pad11)"))
    (pad 12 smd oval (at -0.4 4.5) (size 0.4 2) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(IC1-Pad12)"))
    (pad 13 smd oval (at 0.4 4.5) (size 0.4 2) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(IC1-Pad13)"))
    (pad 14 smd oval (at 1.2 4.5) (size 0.4 2) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(IC1-Pad14)"))
    (pad 15 smd oval (at 2 4.5) (size 0.4 2) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(CON1-Pad4)"))
    (pad 16 smd oval (at 2.8 4.5) (size 0.4 2) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(CON1-Pad1)"))
    (pad 17 smd oval (at 4.5 2.8 90) (size 0.4 2) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(CON1-Pad3)"))
    (pad 18 smd oval (at 4.5 2 90) (size 0.4 2) (layers F.Cu F.Paste F.Mask)
      (net 53 VCC))
    (pad 19 smd oval (at 4.5 1.2 90) (size 0.4 2) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(IC1-Pad19)"))
    (pad 20 smd oval (at 4.5 0.4 90) (size 0.4 2) (layers F.Cu F.Paste F.Mask)
      (net 53 VCC))
    (pad 21 smd oval (at 4.5 -0.4 90) (size 0.4 2) (layers F.Cu F.Paste F.Mask)
      (net 52 GND))
    (pad 22 smd oval (at 4.5 -1.2 90) (size 0.4 2) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(IC1-Pad22)"))
    (pad 23 smd oval (at 4.5 -2 90) (size 0.4 2) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(IC1-Pad23)"))
    (pad 24 smd oval (at 4.5 -2.8 90) (size 0.4 2) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(IC1-Pad24)"))
    (pad 25 smd oval (at 2.8 -4.5) (size 0.4 2) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(IC1-Pad25)"))
    (pad 26 smd oval (at 2 -4.5) (size 0.4 2) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(IC1-Pad26)"))
    (pad 27 smd oval (at 1.2 -4.5) (size 0.4 2) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(IC1-Pad27)"))
    (pad 28 smd oval (at 0.4 -4.5) (size 0.4 2) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(IC1-Pad28)"))
    (pad 29 smd oval (at -0.4 -4.5) (size 0.4 2) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(CON1-Pad5)"))
    (pad 30 smd oval (at -1.2 -4.5) (size 0.4 2) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(IC1-Pad30)"))
    (pad 31 smd oval (at -2 -4.5) (size 0.4 2) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(IC1-Pad31)"))
    (pad 32 smd oval (at -2.8 -4.5) (size 0.4 2) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(IC1-Pad32)"))
  )
  (module "Personal Footprints:BCX56_SOT89" (layer F.Cu) (tedit 58B530D7)
    (at 233.68 43.18)
    (descr "SOT89-3, Housing, Handsoldering,")
    (tags "SOT89-3 Housing Handsoldering ")
    (attr smd)
    (fp_text reference Q1 (at 0.45 -3.3) (layer F.SilkS))
    (fp_text value Q_NPN_BCE (at 0.5 3.15) (layer F.SilkS))
    (pad 1 smd rect (at -1.98 -1.5 270) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(Q1-Pad1)"))
    (pad 2 smd rect (at -1.98 0 270) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(D1-Pad1)"))
    (pad 3 smd rect (at -1.98 1.5 270) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(D1-Pad2)"))
    (pad 2 smd rect (at 1.98 0 270) (size 2 4) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(D1-Pad1)"))
    (pad 2 smd trapezoid (at -0.37 0 90) (size 1.5 0.75) (rect_delta 0 0.5 ) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(D1-Pad1)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT89-3_Housing_Handsoldering.wrl
      (at (xyz 0.02 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 90))
    )
  )
  (module "Personal Footprints:Resistor_0805" (layer F.Cu) (tedit 58B57407)
    (at 227.33 36.83 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 0 -1.7 180) (layer F.SilkS))
    (fp_text value 2.2K (at 0 1.75 180) (layer F.SilkS))
    (fp_text user %R (at 0 -1.7 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(D2-Pad2)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(R1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Personal Footprints:Resistor_0805" (layer F.Cu) (tedit 58B57407)
    (at 243.205 30.48 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 0 -1.7 90) (layer F.SilkS))
    (fp_text value 2.2K (at 0 1.75 90) (layer F.SilkS))
    (fp_text user %R (at 0 -1.7 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 53 VCC))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(IC1-Pad12)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Personal Footprints:Resistor_0805" (layer F.Cu) (tedit 58B57407)
    (at 227.33 29.21)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at 0 -1.7) (layer F.SilkS))
    (fp_text value 120 (at 0 1.75) (layer F.SilkS))
    (fp_text user %R (at 0 -1.7) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(R3-Pad1)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(Q1-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Personal Footprints:Resistor_0805" (layer F.Cu) (tedit 58B57407)
    (at 228.6 22.86 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at 0 -1.7 270) (layer F.SilkS))
    (fp_text value 1K (at 0 1.75 270) (layer F.SilkS))
    (fp_text user %R (at 0 -1.7 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(D1-Pad2)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(R3-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Personal Footprints:Resistor_0805" (layer F.Cu) (tedit 58B57407)
    (at 243.84 23.495)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R5 (at 0 -1.7) (layer F.SilkS))
    (fp_text value 560 (at 0 1.75) (layer F.SilkS))
    (fp_text user %R (at 0 -1.7) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 53 VCC))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(R5-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Personal Footprints:Resistor_0805" (layer F.Cu) (tedit 58B57407)
    (at 262.89 60.96)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R6 (at 0 -1.7) (layer F.SilkS))
    (fp_text value 1K (at 0 1.75) (layer F.SilkS))
    (fp_text user %R (at 0 -1.7) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(R6-Pad1)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(IC1-Pad30)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Personal Footprints:Resistor_0805" (layer F.Cu) (tedit 58B57407)
    (at 262.89 66.04)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R7 (at 0 -1.7) (layer F.SilkS))
    (fp_text value 1K (at 0 1.75) (layer F.SilkS))
    (fp_text user %R (at 0 -1.7) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(R7-Pad1)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(IC1-Pad31)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Personal Footprints:Resistor_0805" (layer F.Cu) (tedit 58B57407)
    (at 255.27 31.75)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R8 (at 0 -1.7) (layer F.SilkS))
    (fp_text value 10K (at 0 1.75) (layer F.SilkS))
    (fp_text user %R (at 0 -1.7) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 53 VCC))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(CON1-Pad5)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Personal Footprints:Resistor_0805" (layer F.Cu) (tedit 58B57407)
    (at 266.7 44.45 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R9 (at 0 -1.7 180) (layer F.SilkS))
    (fp_text value 1K (at 0 1.75 180) (layer F.SilkS))
    (fp_text user %R (at 0 -1.7 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(D4-Pad1)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 52 GND))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Personal Footprints:SOIC-16_3.9x9.9mm_Pitch1.27mm" (layer F.Cu) (tedit 58B53AD8)
    (at 256.54 60.96)
    (descr "16-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U3 (at 0 -6) (layer F.SilkS))
    (fp_text value MAX232 (at 0 6) (layer F.SilkS))
    (pad 1 smd rect (at -2.7 -4.445) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at -2.7 -3.175) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C3-Pad1)"))
    (pad 3 smd rect (at -2.7 -1.905) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 4 smd rect (at -2.7 -0.635) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 5 smd rect (at -2.7 0.635) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C2-Pad2)"))
    (pad 6 smd rect (at -2.7 1.905) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C3-Pad2)"))
    (pad 7 smd rect (at -2.7 3.175) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(U3-Pad7)"))
    (pad 8 smd rect (at -2.7 4.445) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(U3-Pad8)"))
    (pad 9 smd rect (at 2.7 4.445) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(U3-Pad9)"))
    (pad 10 smd rect (at 2.7 3.175) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(U3-Pad10)"))
    (pad 11 smd rect (at 2.7 1.905) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(R7-Pad1)"))
    (pad 12 smd rect (at 2.7 0.635) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(R6-Pad1)"))
    (pad 13 smd rect (at 2.7 -0.635) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(P3-Pad3)"))
    (pad 14 smd rect (at 2.7 -1.905) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(P3-Pad2)"))
    (pad 15 smd rect (at 2.7 -3.175) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 52 GND))
    (pad 16 smd rect (at 2.7 -4.445) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 53 VCC))
    (model Housings_SOIC.3dshapes/SOIC-16_3.9x9.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Personal Footprints:78M05_TO-252" (layer F.Cu) (tedit 58B53417)
    (at 269.24 35.56)
    (descr TO-252-2Lead)
    (attr smd)
    (fp_text reference U4 (at 0.3 -4.54) (layer F.SilkS))
    (fp_text value LM78M05CT (at 0.25 4.81) (layer F.SilkS))
    (pad 1 smd rect (at -3.7 -2.29 270) (size 2 3.5) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C7-Pad1)"))
    (pad 3 smd rect (at -3.7 2.29 270) (size 2 3.5) (layers F.Cu F.Paste F.Mask)
      (net 53 VCC))
    (pad 2 smd rect (at 3.7 0.01 270) (size 7 7) (layers F.Cu F.Paste F.Mask)
      (net 52 GND))
    (model TO_SOT_Packages_SMD.3dshapes\TO-252-2Lead.wrl
      (at (xyz -0.1377952755905512 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module "Personal Footprints:Crystal_SMD_HC49" (layer F.Cu) (tedit 58B58908)
    (at 247.65 43.18 90)
    (descr "SMD Crystal HC-49-SD http://cdn-reichelt.de/documents/datenblatt/B400/xxx-HC49-SMD.pdf, hand-soldering, 11.4x4.7mm^2 package")
    (tags "SMD SMT crystal hand-soldering")
    (attr smd)
    (fp_text reference Y1 (at 0 -3.55 90) (layer F.SilkS))
    (fp_text value 16MHz (at 6.5024 2.24536 90) (layer F.SilkS))
    (pad 1 smd rect (at -5.9375 0 90) (size 7.875 2) (layers F.Cu F.Mask)
      (net 8 "Net-(C5-Pad1)"))
    (pad 2 smd rect (at 5.9375 0 90) (size 7.875 2) (layers F.Cu F.Mask)
      (net 7 "Net-(C4-Pad2)"))
    (model Crystals.3dshapes/Crystal_SMD_HC49-SD_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Personal Footprints:1x2_Header" (layer F.Cu) (tedit 58B59223)
    (at 232.41 58.42 180)
    (fp_text reference P1 (at 1.8 -8.3 180) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 1.8 3.2 180) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0 180) (size 1.524 1.524) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(D1-Pad4)"))
    (pad 2 thru_hole circle (at 3.5 0 180) (size 1.524 1.524) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(D1-Pad3)"))
    (pad 2 thru_hole circle (at 3.5 -5 180) (size 1.524 1.524) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(D1-Pad3)"))
    (pad 1 thru_hole circle (at 0 -5 180) (size 1.524 1.524) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(D1-Pad4)"))
  )
  (module "Personal Footprints:1x2_Header" (layer F.Cu) (tedit 58B59220)
    (at 243.205 58.42 180)
    (fp_text reference P2 (at 1.8 -8.3 180) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 1.8 3.2 180) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0 180) (size 1.524 1.524) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(D1-Pad4)"))
    (pad 2 thru_hole circle (at 3.5 0 180) (size 1.524 1.524) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(D1-Pad3)"))
    (pad 2 thru_hole circle (at 3.5 -5 180) (size 1.524 1.524) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(D1-Pad3)"))
    (pad 1 thru_hole circle (at 0 -5 180) (size 1.524 1.524) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(D1-Pad4)"))
  )
  (module "Personal Footprints:BZX84" (layer F.Cu) (tedit 58B580C4)
    (at 227.33 43.18 270)
    (descr "SOT-23, Single Diode")
    (tags SOT-23)
    (attr smd)
    (fp_text reference D2 (at 0 -2.5 270) (layer F.SilkS))
    (fp_text value BZX84C5V1 (at 0 2.5 270) (layer F.SilkS))
    (pad 2 smd rect (at -1 -0.95 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(D2-Pad2)"))
    (pad "" smd rect (at -1 0.95 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at 1 0 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(D1-Pad1)"))
    (model Diodes_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module "Personal Footprints:ISP" (layer F.Cu) (tedit 58B58A6D)
    (at 267.97 51.435)
    (fp_text reference CON1 (at -2.7 -1.27 90) (layer F.SilkS))
    (fp_text value AVR-ISP-6 (at 2.67462 2.50952) (layer F.SilkS))
    (pad 2 thru_hole circle (at 0 -2.54) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 53 VCC))
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(CON1-Pad1)"))
    (pad 4 thru_hole circle (at 2.54 -2.54) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(CON1-Pad4)"))
    (pad 3 thru_hole circle (at 2.54 0) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(CON1-Pad3)"))
    (pad 6 thru_hole circle (at 5.08 -2.54) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 52 GND))
    (pad 5 thru_hole circle (at 5.08 0) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(CON1-Pad5)"))
  )
  (module "Personal Footprints:1x3_Header" (layer F.Cu) (tedit 58B59195)
    (at 267.014 59.1161 270)
    (fp_text reference P3 (at 1.8 -8.3 270) (layer F.SilkS))
    (fp_text value CONN_01X03 (at 1.8 3.2 270) (layer F.Fab) hide)
    (pad 2 thru_hole circle (at 3.5 -5 270) (size 1.524 1.524) (drill 1) (layers *.Cu *.Mask)
      (net 40 "Net-(P3-Pad2)"))
    (pad 2 thru_hole circle (at 3.5 0 270) (size 1.524 1.524) (drill 1) (layers *.Cu *.Mask)
      (net 40 "Net-(P3-Pad2)"))
    (pad 2 thru_hole circle (at 3.5 0 270) (size 1.524 1.524) (drill 1) (layers *.Cu *.Mask)
      (net 40 "Net-(P3-Pad2)"))
    (pad 2 thru_hole circle (at 3.5 -5 270) (size 1.524 1.524) (drill 1) (layers *.Cu *.Mask)
      (net 40 "Net-(P3-Pad2)"))
    (pad 2 thru_hole circle (at 3.5 -5 270) (size 1.524 1.524) (drill 1) (layers *.Cu *.Mask)
      (net 40 "Net-(P3-Pad2)"))
    (pad 2 thru_hole circle (at 3.5 0 270) (size 1.524 1.524) (drill 1) (layers *.Cu *.Mask)
      (net 40 "Net-(P3-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.524 1.524) (drill 1) (layers *.Cu *.Mask)
      (net 52 GND))
    (pad 2 thru_hole circle (at 3.5 0 270) (size 1.524 1.524) (drill 1) (layers *.Cu *.Mask)
      (net 40 "Net-(P3-Pad2)"))
    (pad 2 thru_hole circle (at 3.5 -5 270) (size 1.524 1.524) (drill 1) (layers *.Cu *.Mask)
      (net 40 "Net-(P3-Pad2)"))
    (pad 1 thru_hole circle (at 0 -5 270) (size 1.524 1.524) (drill 1) (layers *.Cu *.Mask)
      (net 52 GND))
    (pad 3 thru_hole circle (at 7 0 270) (size 1.524 1.524) (drill 1) (layers *.Cu *.Mask)
      (net 41 "Net-(P3-Pad3)"))
    (pad 3 thru_hole circle (at 7 -5 270) (size 1.524 1.524) (drill 1) (layers *.Cu *.Mask)
      (net 41 "Net-(P3-Pad3)"))
  )
  (module "Personal Footprints:1x2_Header" (layer F.Cu) (tedit 58B57982)
    (at 267.01 23.15 270)
    (fp_text reference P4 (at 1.8 -8.3 270) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 1.8 3.2 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.524 1.524) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(D3-Pad3)"))
    (pad 2 thru_hole circle (at 3.5 0 270) (size 1.524 1.524) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(D3-Pad4)"))
    (pad 2 thru_hole circle (at 3.5 -5 270) (size 1.524 1.524) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(D3-Pad4)"))
    (pad 1 thru_hole circle (at 0 -5 270) (size 1.524 1.524) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(D3-Pad3)"))
  )
  (module "Personal Footprints:PC357" (layer F.Cu) (tedit 58B52E91)
    (at 235.79 31.71 270)
    (fp_text reference U1 (at -3.37 0 360) (layer F.SilkS))
    (fp_text value PC357 (at 3.4544 -0.0762 360) (layer F.SilkS))
    (pad 4 smd rect (at -1.27 -3.5 270) (size 0.8 1.5) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(IC1-Pad12)"))
    (pad 1 smd rect (at -1.27 3.5 270) (size 0.8 1.5) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(R1-Pad2)"))
    (pad 3 smd rect (at 1.27 -3.5 270) (size 0.8 1.5) (layers F.Cu F.Paste F.Mask)
      (net 52 GND))
    (pad 2 smd rect (at 1.27 3.5 270) (size 0.8 1.5) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(D1-Pad2)"))
  )
  (module "Personal Footprints:PC357" (layer F.Cu) (tedit 58B52E91)
    (at 235.66628 23.495 90)
    (fp_text reference U2 (at -3.37 0 180) (layer F.SilkS))
    (fp_text value PC357 (at 3.4544 -0.0762 180) (layer F.SilkS))
    (pad 4 smd rect (at -1.27 -3.5 90) (size 0.8 1.5) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(D1-Pad1)"))
    (pad 1 smd rect (at -1.27 3.5 90) (size 0.8 1.5) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(R5-Pad2)"))
    (pad 3 smd rect (at 1.27 -3.5 90) (size 0.8 1.5) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(R3-Pad1)"))
    (pad 2 smd rect (at 1.27 3.5 90) (size 0.8 1.5) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(IC1-Pad9)"))
  )
  (gr_line (start 223.52 69.85) (end 278.13 69.85) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 223.52 19.05) (end 223.52 69.85) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 278.13 19.05) (end 223.52 19.05) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 278.13 69.85) (end 278.13 19.05) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text TX (at 275.59 66.675) (layer F.SilkS))
  (gr_text RX (at 275.59 62.865) (layer F.SilkS))
  (gr_text GND (at 275.59 59.055) (layer F.SilkS))
)
