<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.4.2">
<drawing>
<board>
<plain>
<wire x1="2.54" y1="5.08" x2="31.75" y2="5.08" width="0" layer="20"/>
<wire x1="31.75" y1="5.08" x2="31.75" y2="22.86" width="0" layer="20"/>
<wire x1="31.75" y1="22.86" x2="2.54" y2="22.86" width="0" layer="20"/>
<wire x1="2.54" y1="22.86" x2="2.54" y2="5.08" width="0" layer="20"/>
</plain>
<libraries>
<library name="semicon-smd-ipc">
<description>&lt;b&gt;IPC Standard SMD Semiconductors&lt;/b&gt;&lt;p&gt;
A few devices defined according to the IPC standard.&lt;p&gt;
Based on:&lt;p&gt;
IPC-SM-782&lt;br&gt;
IRevision A, August 1993&lt;br&gt;
Includes Amendment 1, October 1996&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOD123">
<description>&lt;b&gt;SMALL OUTLINE DIODE&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="testpad">
<description>&lt;b&gt;Test Pins/Pads&lt;/b&gt;&lt;p&gt;
Cream on SMD OFF.&lt;br&gt;
new: Attribute TP_SIGNAL_NAME&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="P1-13">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="D1" library="semicon-smd-ipc" package="SOD123" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D2" library="semicon-smd-ipc" package="SOD123" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IN2" library="testpad" package="P1-13" value="PTR1PAD1-13">
<attribute name="NAME"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="IN1" library="testpad" package="P1-13" value="PTR1PAD1-13">
<attribute name="NAME"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="OUT1" library="testpad" package="P1-13" value="PTR1PAD1-13">
<attribute name="NAME"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="OUT2" library="testpad" package="P1-13" value="PTR1PAD1-13">
<attribute name="NAME"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="D1" pad="1"/>
<contactref element="D2" pad="2"/>
<contactref element="IN1" pad="TP"/>
<contactref element="OUT1" pad="TP"/>
</signal>
<signal name="N$2">
<contactref element="D1" pad="2"/>
<contactref element="D2" pad="1"/>
<contactref element="OUT2" pad="TP"/>
<contactref element="IN2" pad="TP"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
