<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<text>PWR</text>
<text>ACT</text>
<text>HB</text>
<text>COS</text>
<text>PTT</text>
<text>DMR</text>
<text>D*</text>
<text>YSF</text>
<text>P25</text>
<text>WA0EDA</text>
<text>NXD</text>
<text>CLP</text>
<text>RX</text>
<text>TX</text>
<text>CLIP</text>
<text>MODEM</text>
<text>GND</text>
<text>RESET</text>
<text>BOOT</text>
<text>HOST RXD</text>
<text>HOST TXD</text>
<text>NanoPi NEO</text>
<text>STM32-DVM-MTR2K v2.0a</text>
<text>LOAD</text>
<text>UART LEVEL SHIFT</text>
<text>+V</text>
<text>GND</text>
<text>Install to
Emulate
Aux I/O Card</text>
<text>I/O PROCESSOR</text>
<text>(C) 2019 THE REGENTS OF THE K0USY GROUP</text>
<text>ANALOG
HANDSHAKE
ENABLE</text>
<text>&gt;2</text>
<text>&gt;0</text>
<text>&gt;8</text>
<text>&gt;13</text>
<text>&lt;3</text>
<text>&lt;4</text>
<text>&lt;7</text>
<text>&lt;10</text>
<text>I/O INDICATORS</text>
<text>MODEM INDICATORS</text>
<text>N0MJS
N3XCC</text>
</plain>
<libraries>
<library name="rcl">
<packages>
<package name="R0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="C0805">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="L2012C">
<description>&lt;b&gt;INDUCTOR&lt;/b&gt;</description>
</package>
<package name="C1210">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="linear">
<packages>
<package name="SO08">
<description>&lt;b&gt;Small Outline Package 8&lt;/b&gt;&lt;br&gt;
NS Package M08A</description>
</package>
</packages>
</library>
<library name="Custom">
<packages>
<package name="5.2X3.4-4-PAD">
<description>&lt;b&gt;IQD Frequency Products SMD Package&lt;/b&gt;</description>
</package>
<package name="MPS2307_DC-TO-DC">
<description>MP2307 DC-to-DC Buck Regulator</description>
</package>
</packages>
</library>
<library name="crystal">
<description>&lt;b&gt;Crystals and Crystal Resonators&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="HC49/S">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X02/90">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X02">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="2X03">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X04">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X05">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="2X02">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="led">
<description>&lt;b&gt;LEDs&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;br&gt;
Extended by Federico Battaglin &lt;author&gt;&amp;lt;federico.rd@fdpinternational.com&amp;gt;&lt;/author&gt; with DUOLED</description>
<packages>
<package name="CHIPLED_0805">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_R971.pdf</description>
</package>
</packages>
</library>
<library name="Voltage Regulator">
<packages>
<package name="XC6206_SOT-23">
<description>&lt;hr&gt;
&lt;b&gt;XC6206 SOT-23 type package&lt;/b&gt;
&lt;hr&gt;</description>
</package>
</packages>
</library>
<library name="semicon-smd-ipc">
<description>&lt;b&gt;IPC Standard SMD Semiconductors&lt;/b&gt;&lt;p&gt;
A few devices defined according to the IPC standard.&lt;p&gt;
Based on:&lt;p&gt;
IPC-SM-782&lt;br&gt;
IRevision A, August 1993&lt;br&gt;
Includes Amendment 1, October 1996&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT23C">
<description>&lt;b&gt;SMALL OUTLINE TRANSISTOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="transistor">
<description>&lt;b&gt;Transistors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SC59-BEC">
<description>SC59 (SOT23) Motorola</description>
</package>
<package name="SOT23-BEC">
<description>TO-236 ITT Intermetall</description>
</package>
</packages>
</library>
<library name="solpad">
<description>&lt;b&gt;Solder Pads/Test Points&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="MCS10B">
<description>&lt;b&gt;SOLDER PAD&lt;/b&gt;&lt;p&gt;
drill 1.0 mm</description>
</package>
</packages>
</library>
<library name="ST Microelctronics_By_element14_Batch_1">
<description>Developed by element14 :&lt;br&gt;
element14 CAD Library consolidation.ulp
at 30/07/2012 15:32:30</description>
<packages>
<package name="QFP50P1200X1200X160-64N">
</package>
</packages>
</library>
<library name="19inch">
<description>&lt;b&gt;19-Inch Slot Eurocards&lt;/b&gt;&lt;p&gt;
100 x 160 mm with DIN 41612 connectors&lt;br&gt;
 VME-BUS-Cards - http://www.interfacebus.com/COTs_Cards_VME.html&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="VG96">
<description>&lt;b&gt;EUROCARD&lt;/b&gt;, C/ABC, 2.54</description>
</package>
</packages>
</library>
<library name="CortFun">
<packages>
<package name="EDA">
</package>
<package name="EDA_SM">
</package>
</packages>
</library>
<library name="NanoPi">
<packages>
<package name="NANOPI-NEO">
</package>
</packages>
</library>
<library name="bss138_10">
<description>&lt;b&gt;Fairchild BSS138 Field Effect Transistor&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
Version 1.0&lt;br&gt;
&amp;copy; 2015 Samuel Lourenço</description>
<packages>
<package name="SOT23">
<description>&lt;b&gt;SOT-23 Plastic Small Outline&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="diode">
<description>&lt;b&gt;Diodes&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Motorola : www.onsemi.com
&lt;li&gt;Fairchild : www.fairchildsemi.com
&lt;li&gt;Philips : www.semiconductors.com
&lt;li&gt;Vishay : www.vishay.de
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT23">
<description>&lt;B&gt;DIODE&lt;/B&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="FTDI_BASIC">
<description>&lt;h3&gt;FTDI Basic &lt;/h3&gt;
Includes tDocu labels for end pins that match the FTDI Basic connection.
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 6&lt;/li&gt;
&lt;li&gt;Pin pitch: 0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;6_Pin_Serial_Cable&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="2X3">
<description>&lt;h3&gt;Plated Through Hole - 2x3&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Aesthetics&lt;/h3&gt;
This library contiains non-functional items such as logos, build/ordering notes, frame blocks, etc. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="OSHW-LOGO-M">
<description>&lt;h3&gt;Open-Source Hardware (OSHW) Logo - Medium - Silkscreen&lt;/h3&gt;
&lt;p&gt;Silkscreen logo for open-source hardware designs.&lt;/p&gt;
&lt;p&gt;Devices using:
&lt;ul&gt;&lt;li&gt;OSHW_LOGO&lt;/li&gt;&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-IC-Microcontroller">
<description>&lt;h3&gt;SparkFun Microcontrollers&lt;/h3&gt;
This library contains microcontrollers.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TQFP32-08">
<description>&lt;B&gt;Thin Plasic Quad Flat Package&lt;/B&gt; Grid 0.8 mm</description>
</package>
</packages>
</library>
<library name="SparkFun-Clocks">
<description>&lt;h3&gt;SparkFun Clocks, Oscillators and Resonators&lt;/h3&gt;
This library contains the real-time clocks, oscillators, resonators, and crystals we use. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="RESONATOR-SMD-3.2X1.3">
<description>&lt;h3&gt;3.2x1.3mm 3-Pin SMD Resonator&lt;/h3&gt;
&lt;p&gt;&lt;a href="http://www.murata.com/~/media/webrenewal/support/library/catalog/products/timingdevice/ceralock/p16e.ashx"&gt;Example datasheet&lt;/a&gt; (CSTCE_VH3L)&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="R6" library="rcl" package="R0805" value="39K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="rcl" package="R0805" value="3.9K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC2" library="linear" package="SO08" value="MCP6002">
<attribute name="DATA_SHEET" value="&lt;a href=&quot;http://www.ti.com/lit/ds/symlink/tl084a.pdf&quot;&gt; Data sheet &lt;/a&gt;"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="rcl" package="C0805" value="680pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="rcl" package="C0805" value=".01uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="rcl" package="C0805" value=".01uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="rcl" package="R0805" value="3.3K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="rcl" package="R0805" value="22K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R12" library="rcl" package="R0805" value="39K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R15" library="rcl" package="R0805" value="3.9K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC1" library="linear" package="SO08" value="MCP6002">
<attribute name="DATA_SHEET" value="&lt;a href=&quot;http://www.ti.com/lit/ds/symlink/tl084a.pdf&quot;&gt; Data sheet &lt;/a&gt;"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C16" library="rcl" package="C0805" value="680pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C14" library="rcl" package="C0805" value=".01uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C12" library="rcl" package="C0805" value=".01uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="rcl" package="R0805" value="3.3K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="rcl" package="R0805" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="rcl" package="R0805" value="22K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="OS1" library="Custom" package="5.2X3.4-4-PAD" value="TCXO 12MHz">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C23" library="rcl" package="C0805" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C26" library="rcl" package="C0805" value="4.7uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C27" library="rcl" package="C0805" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C25" library="rcl" package="C0805" value="4.7uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C24" library="rcl" package="C0805" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L1" library="rcl" package="L2012C" value="FBead">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="rcl" package="C0805" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="rcl" package="C0805" value="4.7uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="rcl" package="C0805" value="10pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C11" library="rcl" package="C0805" value="10pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q1" library="crystal" package="HC49/S" value="8MHz">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="1667008"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C13" library="rcl" package="C0805" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="rcl" package="R0805" value="100K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R53" library="rcl" package="R0805" value="47K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C30" library="rcl" package="C0805" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R48" library="rcl" package="R0805" value="47K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED2" library="led" package="CHIPLED_0805" value="BLU">
<attribute name="NAME"/>
</element>
<element name="LED3" library="led" package="CHIPLED_0805" value="ORG">
<attribute name="NAME"/>
</element>
<element name="LED4" library="led" package="CHIPLED_0805" value="ORG">
<attribute name="NAME"/>
</element>
<element name="LED5" library="led" package="CHIPLED_0805" value="GRN">
<attribute name="NAME"/>
</element>
<element name="LED6" library="led" package="CHIPLED_0805" value="RED">
<attribute name="NAME"/>
</element>
<element name="LED7" library="led" package="CHIPLED_0805" value="YEL">
<attribute name="NAME"/>
</element>
<element name="LED8" library="led" package="CHIPLED_0805" value="YEL">
<attribute name="NAME"/>
</element>
<element name="LED9" library="led" package="CHIPLED_0805" value="YEL">
<attribute name="NAME"/>
</element>
<element name="LED10" library="led" package="CHIPLED_0805" value="YEL">
<attribute name="NAME"/>
</element>
<element name="R28" library="rcl" package="R0805" value="1K">
<attribute name="NAME"/>
</element>
<element name="R29" library="rcl" package="R0805" value="560">
<attribute name="NAME"/>
</element>
<element name="R30" library="rcl" package="R0805" value="560">
<attribute name="NAME"/>
</element>
<element name="R31" library="rcl" package="R0805" value="1K">
<attribute name="NAME"/>
</element>
<element name="R32" library="rcl" package="R0805" value="560">
<attribute name="NAME"/>
</element>
<element name="R33" library="rcl" package="R0805" value="560">
<attribute name="NAME"/>
</element>
<element name="R34" library="rcl" package="R0805" value="560">
<attribute name="NAME"/>
</element>
<element name="R35" library="rcl" package="R0805" value="560">
<attribute name="NAME"/>
</element>
<element name="R36" library="rcl" package="R0805" value="560">
<attribute name="NAME"/>
</element>
<element name="JP1" library="pinhead" package="1X02" value="LED ENABLE">
<attribute name="VALUE"/>
</element>
<element name="P1" library="Voltage Regulator" package="XC6206_SOT-23" value="XC6206P332MR">
<attribute name="NAME"/>
</element>
<element name="JP3" library="pinhead" package="2X03" value="STM32 ICSP">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="rcl" package="C1210" value="22uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C15" library="rcl" package="C1210" value="22uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C20" library="rcl" package="C0805" value="4.7uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C21" library="rcl" package="C0805" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="rcl" package="R0805" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC3" library="linear" package="SO08" value="MCP6002">
<attribute name="DATA_SHEET" value="&lt;a href=&quot;http://www.ti.com/lit/ds/symlink/tl084a.pdf&quot;&gt; Data sheet &lt;/a&gt;"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R21" library="rcl" package="R0805" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R22" library="rcl" package="R0805" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R23" library="rcl" package="R0805" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="rcl" package="R0805" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="semicon-smd-ipc" package="SOT23C" value="BAV70">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED1" library="led" package="CHIPLED_0805" value="RED">
<attribute name="NAME"/>
</element>
<element name="R25" library="rcl" package="R0805" value="560">
<attribute name="NAME"/>
</element>
<element name="C22" library="rcl" package="C0805" value="4.7uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R20" library="rcl" package="R0805" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="T11" library="transistor" package="SC59-BEC" value="N2211LT1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="T12" library="transistor" package="SOT23-BEC" value="N2111LT1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP1" library="solpad" package="MCS10B" value="MCS10B">
<attribute name="NAME"/>
</element>
<element name="TP2" library="solpad" package="MCS10B" value="MCS10B">
<attribute name="NAME"/>
</element>
<element name="TP3" library="solpad" package="MCS10B" value="MCS10B">
<attribute name="NAME"/>
</element>
<element name="TP6" library="solpad" package="MCS10B" value="MCS10B">
<attribute name="NAME"/>
</element>
<element name="TP7" library="solpad" package="MCS10B" value="MCS10B">
<attribute name="NAME"/>
</element>
<element name="+3.3V" library="solpad" package="MCS10B" value="MCS10B">
<attribute name="NAME"/>
</element>
<element name="T2" library="transistor" package="SC59-BEC" value="N2111LT1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP5" library="solpad" package="MCS10B" value="MCS10B">
<attribute name="NAME"/>
</element>
<element name="C29" library="rcl" package="C0805" value="4.7uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C28" library="rcl" package="C0805" value="4.7uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="rcl" package="C1210" value="47uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="rcl" package="C1210" value="47uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="T1" library="transistor" package="SC59-BEC" value="N2214LT1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED11" library="led" package="CHIPLED_0805" value="YEL">
<attribute name="NAME"/>
</element>
<element name="R37" library="rcl" package="R0805" value="560">
<attribute name="NAME"/>
</element>
<element name="JP4" library="pinhead" package="1X04" value="MODEM DISP">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="ST Microelctronics_By_element14_Batch_1" package="QFP50P1200X1200X160-64N" value="STM32F446RET6">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="A1" library="Custom" package="MPS2307_DC-TO-DC" value="MP2307_DC-TO-DC">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="rcl" package="C0805" value="4.7uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="+5V" library="solpad" package="MCS10B" value="MCS10B">
<attribute name="NAME"/>
</element>
<element name="GND" library="solpad" package="MCS10B" value="MCS10B">
<attribute name="NAME"/>
</element>
<element name="R16" library="rcl" package="R0805" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R17" library="rcl" package="R0805" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R13" library="rcl" package="R0805" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="19inch" package="VG96" value="MTR2K J2">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="CortFun" package="EDA" value=""/>
<element name="R9" library="rcl" package="R0805" value="3.3K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP10" library="pinhead" package="1X02/90" value="RESET">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U2" library="NanoPi" package="NANOPI-NEO" value="NanoPi NEO">
<attribute name="NAME"/>
<attribute name="VALUE" value="NanoPi NEO"/>
</element>
<element name="JP5" library="pinhead" package="1X05" value="MODEM SERIAL">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R54" library="rcl" package="R0805" value="12k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R55" library="rcl" package="R0805" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q2" library="bss138_10" package="SOT23" value="BSS138">
<attribute name="MF" value="Fairchild"/>
<attribute name="MPN" value="BSS138"/>
<attribute name="OC_NEWARK" value="67R2009"/>
<attribute name="OC_FARNELL" value="9845330"/>
<attribute name="NAME"/>
</element>
<element name="R42" library="rcl" package="R0805" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R45" library="rcl" package="R0805" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q3" library="bss138_10" package="SOT23" value="BSS138">
<attribute name="MF" value="Fairchild"/>
<attribute name="MPN" value="BSS138"/>
<attribute name="OC_NEWARK" value="67R2009"/>
<attribute name="OC_FARNELL" value="9845330"/>
<attribute name="NAME"/>
</element>
<element name="R43" library="rcl" package="R0805" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R46" library="rcl" package="R0805" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D3" library="diode" package="SOT23" value="BAT54A">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J3" library="SparkFun-Connectors" package="FTDI_BASIC" value="I/O SERIAL">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP7" library="pinhead" package="2X02" value="I/O SERIAL EN.">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP9" library="pinhead" package="1X02/90" value="BOOT">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="T8" library="transistor" package="SC59-BEC" value="N2211LT1">
<attribute name="NAME"/>
</element>
<element name="T9" library="transistor" package="SC59-BEC" value="N2211LT1">
<attribute name="NAME"/>
</element>
<element name="T7" library="transistor" package="SC59-BEC" value="N2211LT1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="T10" library="transistor" package="SC59-BEC" value="N2211LT1">
<attribute name="NAME"/>
</element>
<element name="JP2" library="pinhead" package="1X02" value="EXT PWR +7-15V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R14" library="rcl" package="R0805" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q4" library="bss138_10" package="SOT23" value="BSS138">
<attribute name="MPN" value="BSS138"/>
<attribute name="OC_FARNELL" value="9845330"/>
<attribute name="MF" value="Fairchild"/>
<attribute name="OC_NEWARK" value="67R2009"/>
<attribute name="NAME"/>
</element>
<element name="R44" library="rcl" package="R0805" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R47" library="rcl" package="R0805" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP8" library="pinhead" package="2X02" value="ANALOG HANDSHAKE ENABLE">
<attribute name="NAME"/>
</element>
<element name="R38" library="rcl" package="R0805" value="47K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="T3" library="transistor" package="SOT23-BEC" value="N2111LT1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R39" library="rcl" package="R0805" value="47K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="T4" library="transistor" package="SOT23-BEC" value="N2111LT1">
<attribute name="NAME"/>
</element>
<element name="R40" library="rcl" package="R0805" value="47K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="T5" library="transistor" package="SOT23-BEC" value="N2111LT1">
<attribute name="NAME"/>
</element>
<element name="R41" library="rcl" package="R0805" value="47K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="T6" library="transistor" package="SOT23-BEC" value="N2111LT1">
<attribute name="NAME"/>
</element>
<element name="U$2" library="SparkFun-Aesthetics" package="OSHW-LOGO-M" value=""/>
<element name="LED16" library="led" package="CHIPLED_0805" value="RED">
<attribute name="NAME"/>
</element>
<element name="R56" library="rcl" package="R0805" value="560">
<attribute name="NAME"/>
</element>
<element name="LED17" library="led" package="CHIPLED_0805" value="RED">
<attribute name="NAME"/>
</element>
<element name="R57" library="rcl" package="R0805" value="560">
<attribute name="NAME"/>
</element>
<element name="LED18" library="led" package="CHIPLED_0805" value="RED">
<attribute name="NAME"/>
</element>
<element name="R58" library="rcl" package="R0805" value="560">
<attribute name="NAME"/>
</element>
<element name="LED19" library="led" package="CHIPLED_0805" value="RED">
<attribute name="NAME"/>
</element>
<element name="R59" library="rcl" package="R0805" value="560">
<attribute name="NAME"/>
</element>
<element name="LED12" library="led" package="CHIPLED_0805" value="GRN">
<attribute name="NAME"/>
</element>
<element name="R49" library="rcl" package="R0805" value="560">
<attribute name="NAME"/>
</element>
<element name="LED13" library="led" package="CHIPLED_0805" value="GRN">
<attribute name="NAME"/>
</element>
<element name="R50" library="rcl" package="R0805" value="560">
<attribute name="NAME"/>
</element>
<element name="LED14" library="led" package="CHIPLED_0805" value="GRN">
<attribute name="NAME"/>
</element>
<element name="R51" library="rcl" package="R0805" value="560">
<attribute name="NAME"/>
</element>
<element name="LED15" library="led" package="CHIPLED_0805" value="GRN">
<attribute name="NAME"/>
</element>
<element name="R52" library="rcl" package="R0805" value="560">
<attribute name="NAME"/>
</element>
<element name="EDA1" library="CortFun" package="EDA_SM" value="EDASMALL"/>
<element name="EDA2" library="CortFun" package="EDA_SM" value="EDASMALL"/>
<element name="JP6" library="pinhead" package="1X04" value="SBC DISP">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP11" library="pinhead" package="1X02" value="AVR RESET">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="2X3" value="AVR_SPI_ICSP">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D2" library="diode" package="SOT23" value="BAT54A">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U3" library="SparkFun-IC-Microcontroller" package="TQFP32-08" value="ATMEGA328P_TQFP">
<attribute name="PROD_ID" value="IC-09069"/>
</element>
<element name="Y1" library="SparkFun-Clocks" package="RESONATOR-SMD-3.2X1.3" value="16MHz">
<attribute name="VALUE" value="16MHz"/>
<attribute name="PROD_ID" value="XTAL-08900"/>
</element>
<element name="C18" library="rcl" package="C0805" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C19" library="rcl" package="C0805" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C17" library="rcl" package="C0805" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R24" library="rcl" package="R0805" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R27" library="rcl" package="R0805" value="3.3K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R26" library="rcl" package="R0805" value="3.3K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R18" library="rcl" package="R0805" value="3.3K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R19" library="rcl" package="R0805" value="3.3K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="C10" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C16" pad="2"/>
<contactref element="C12" pad="2"/>
<contactref element="IC2" pad="4"/>
<contactref element="OS1" pad="2"/>
<contactref element="C26" pad="1"/>
<contactref element="C25" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="C9" pad="2"/>
<contactref element="C11" pad="2"/>
<contactref element="R3" pad="1"/>
<contactref element="C30" pad="1"/>
<contactref element="R48" pad="1"/>
<contactref element="IC1" pad="4"/>
<contactref element="JP1" pad="2"/>
<contactref element="JP3" pad="3"/>
<contactref element="C20" pad="1"/>
<contactref element="C21" pad="1"/>
<contactref element="JP3" pad="5"/>
<contactref element="IC3" pad="4"/>
<contactref element="R23" pad="2"/>
<contactref element="C22" pad="2"/>
<contactref element="T11" pad="E"/>
<contactref element="C29" pad="2"/>
<contactref element="C28" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="T1" pad="E"/>
<contactref element="P1" pad="1"/>
<contactref element="JP4" pad="4"/>
<contactref element="U1" pad="31"/>
<contactref element="U1" pad="47"/>
<contactref element="U1" pad="63"/>
<contactref element="U1" pad="18"/>
<contactref element="U1" pad="12"/>
<contactref element="A1" pad="GND2"/>
<contactref element="A1" pad="GND1"/>
<contactref element="C7" pad="1"/>
<contactref element="GND" pad="MP"/>
<contactref element="C13" pad="2"/>
<contactref element="JP10" pad="2"/>
<contactref element="J1" pad="A14"/>
<contactref element="J1" pad="B14"/>
<contactref element="J1" pad="C14"/>
<contactref element="J1" pad="A2"/>
<contactref element="J1" pad="B2"/>
<contactref element="J1" pad="C2"/>
<contactref element="U2" pad="A14"/>
<contactref element="U2" pad="A20"/>
<contactref element="U2" pad="A6"/>
<contactref element="U2" pad="A9"/>
<contactref element="JP5" pad="5"/>
<contactref element="R55" pad="1"/>
<contactref element="J1" pad="C21"/>
<contactref element="J1" pad="A21"/>
<contactref element="J1" pad="A8"/>
<contactref element="J1" pad="A17"/>
<contactref element="J1" pad="A18"/>
<contactref element="J1" pad="B9"/>
<contactref element="J1" pad="B18"/>
<contactref element="J1" pad="C9"/>
<contactref element="T8" pad="E"/>
<contactref element="T9" pad="E"/>
<contactref element="T7" pad="E"/>
<contactref element="T10" pad="E"/>
<contactref element="JP2" pad="2"/>
<contactref element="R14" pad="2"/>
<contactref element="R38" pad="1"/>
<contactref element="R39" pad="1"/>
<contactref element="R40" pad="1"/>
<contactref element="R41" pad="1"/>
<contactref element="C24" pad="1"/>
<contactref element="C27" pad="1"/>
<contactref element="J3" pad="GND"/>
<contactref element="J3" pad="CTS"/>
<contactref element="LED16" pad="C"/>
<contactref element="LED17" pad="C"/>
<contactref element="LED18" pad="C"/>
<contactref element="LED19" pad="C"/>
<contactref element="LED12" pad="C"/>
<contactref element="LED13" pad="C"/>
<contactref element="LED14" pad="C"/>
<contactref element="LED15" pad="C"/>
<contactref element="JP6" pad="4"/>
<contactref element="J2" pad="6"/>
<contactref element="U3" pad="5"/>
<contactref element="U3" pad="3"/>
<contactref element="U3" pad="21"/>
<contactref element="Y1" pad="2"/>
<contactref element="C19" pad="1"/>
<contactref element="C17" pad="1"/>
</signal>
<signal name="RXD_HOST">
<contactref element="U1" pad="43"/>
<contactref element="U2" pad="A8"/>
<contactref element="JP5" pad="2"/>
</signal>
<signal name="TXD_HOST">
<contactref element="U1" pad="42"/>
<contactref element="U2" pad="A10"/>
<contactref element="JP5" pad="1"/>
<contactref element="T2" pad="B"/>
</signal>
<signal name="N$24">
<contactref element="R6" pad="1"/>
<contactref element="R8" pad="2"/>
<contactref element="C8" pad="1"/>
</signal>
<signal name="N$26">
<contactref element="R5" pad="1"/>
<contactref element="R6" pad="2"/>
<contactref element="C3" pad="1"/>
</signal>
<signal name="N$41">
<contactref element="R12" pad="1"/>
<contactref element="R15" pad="2"/>
<contactref element="C14" pad="1"/>
</signal>
<signal name="N$42">
<contactref element="R15" pad="1"/>
<contactref element="C16" pad="1"/>
<contactref element="IC2" pad="5"/>
</signal>
<signal name="N$43">
<contactref element="R10" pad="1"/>
<contactref element="R12" pad="2"/>
<contactref element="C12" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="IC1" pad="7"/>
<contactref element="C15" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="IC1" pad="6"/>
</signal>
<signal name="N$25">
<contactref element="IC1" pad="5"/>
<contactref element="R8" pad="1"/>
<contactref element="C10" pad="1"/>
</signal>
<signal name="EXT_CLK">
<contactref element="C23" pad="2"/>
<contactref element="U1" pad="50"/>
</signal>
<signal name="N$1">
<contactref element="C23" pad="1"/>
<contactref element="OS1" pad="3"/>
</signal>
<signal name="TXA">
<contactref element="U1" pad="20"/>
<contactref element="IC1" pad="3"/>
</signal>
<signal name="RXA">
<contactref element="C14" pad="2"/>
<contactref element="IC2" pad="7"/>
<contactref element="IC2" pad="6"/>
<contactref element="TP3" pad="MP"/>
<contactref element="U1" pad="26"/>
</signal>
<signal name="RSSI">
<contactref element="U1" pad="27"/>
<contactref element="R53" pad="2"/>
<contactref element="C30" pad="2"/>
<contactref element="TP7" pad="MP"/>
</signal>
<signal name="PTT">
<contactref element="R32" pad="2"/>
<contactref element="T11" pad="B"/>
<contactref element="U1" pad="33"/>
</signal>
<signal name="+5V">
<contactref element="JP4" pad="1"/>
<contactref element="A1" pad="OUT"/>
<contactref element="U2" pad="A4"/>
<contactref element="U2" pad="A2"/>
<contactref element="R45" pad="1"/>
<contactref element="R46" pad="1"/>
<contactref element="R47" pad="1"/>
<contactref element="T3" pad="E"/>
<contactref element="T4" pad="E"/>
<contactref element="T5" pad="E"/>
<contactref element="T6" pad="E"/>
<contactref element="C27" pad="2"/>
<contactref element="C26" pad="2"/>
<contactref element="+5V" pad="MP"/>
<contactref element="P1" pad="3"/>
<contactref element="JP6" pad="1"/>
<contactref element="U3" pad="18"/>
<contactref element="U3" pad="4"/>
<contactref element="U3" pad="6"/>
<contactref element="C17" pad="2"/>
<contactref element="R24" pad="1"/>
<contactref element="R26" pad="2"/>
<contactref element="R27" pad="2"/>
</signal>
<signal name="VDDA">
<contactref element="L1" pad="1"/>
<contactref element="C6" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="U1" pad="13"/>
</signal>
<signal name="N$11">
<contactref element="C11" pad="1"/>
<contactref element="Q1" pad="1"/>
<contactref element="U1" pad="5"/>
</signal>
<signal name="N$12">
<contactref element="C9" pad="1"/>
<contactref element="Q1" pad="2"/>
<contactref element="U1" pad="6"/>
</signal>
<signal name="NRST">
<contactref element="JP3" pad="6"/>
<contactref element="U1" pad="7"/>
<contactref element="R11" pad="2"/>
<contactref element="C13" pad="1"/>
<contactref element="R17" pad="2"/>
<contactref element="JP10" pad="1"/>
</signal>
<signal name="+3V3">
<contactref element="L1" pad="2"/>
<contactref element="R2" pad="1"/>
<contactref element="R28" pad="2"/>
<contactref element="JP3" pad="1"/>
<contactref element="R11" pad="1"/>
<contactref element="IC3" pad="8"/>
<contactref element="R21" pad="1"/>
<contactref element="R25" pad="2"/>
<contactref element="T12" pad="E"/>
<contactref element="T2" pad="E"/>
<contactref element="U1" pad="1"/>
<contactref element="U1" pad="32"/>
<contactref element="U1" pad="48"/>
<contactref element="U1" pad="64"/>
<contactref element="U1" pad="19"/>
<contactref element="OS1" pad="4"/>
<contactref element="C21" pad="2"/>
<contactref element="C20" pad="2"/>
<contactref element="IC2" pad="8"/>
<contactref element="C29" pad="1"/>
<contactref element="R42" pad="1"/>
<contactref element="Q2" pad="1"/>
<contactref element="R43" pad="1"/>
<contactref element="Q3" pad="1"/>
<contactref element="IC1" pad="8"/>
<contactref element="C28" pad="1"/>
<contactref element="R44" pad="1"/>
<contactref element="Q4" pad="1"/>
<contactref element="C25" pad="2"/>
<contactref element="C24" pad="2"/>
<contactref element="+3.3V" pad="MP"/>
<contactref element="P1" pad="2"/>
<contactref element="JP9" pad="2"/>
<contactref element="R18" pad="2"/>
<contactref element="R19" pad="2"/>
</signal>
<signal name="N$17">
<contactref element="R5" pad="2"/>
<contactref element="TP5" pad="MP"/>
<contactref element="IC1" pad="1"/>
<contactref element="IC1" pad="2"/>
</signal>
<signal name="N$21">
<contactref element="R7" pad="2"/>
<contactref element="R9" pad="1"/>
<contactref element="IC2" pad="2"/>
<contactref element="TP1" pad="MP"/>
</signal>
<signal name="N$28">
<contactref element="IC2" pad="3"/>
<contactref element="R4" pad="1"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="N$29">
<contactref element="R4" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="RXA_R">
<contactref element="R1" pad="1"/>
<contactref element="J1" pad="A16"/>
</signal>
<signal name="RSSI_R">
<contactref element="R53" pad="1"/>
<contactref element="J1" pad="A22"/>
</signal>
<signal name="TXA_R">
<contactref element="C15" pad="1"/>
<contactref element="TP6" pad="MP"/>
<contactref element="J1" pad="C16"/>
</signal>
<signal name="PTT_R">
<contactref element="T11" pad="C"/>
<contactref element="J1" pad="A23"/>
<contactref element="JP8" pad="4"/>
<contactref element="J1" pad="B24"/>
</signal>
<signal name="INHIBIT_R">
<contactref element="T12" pad="B"/>
<contactref element="JP8" pad="2"/>
<contactref element="J1" pad="B23"/>
</signal>
<signal name="INHIBIT">
<contactref element="R48" pad="2"/>
<contactref element="T12" pad="C"/>
<contactref element="U1" pad="34"/>
</signal>
<signal name="N$30">
<contactref element="LED2" pad="A"/>
<contactref element="R28" pad="1"/>
</signal>
<signal name="N$33">
<contactref element="LED3" pad="A"/>
<contactref element="R29" pad="1"/>
</signal>
<signal name="N$34">
<contactref element="LED4" pad="A"/>
<contactref element="R30" pad="1"/>
</signal>
<signal name="N$40">
<contactref element="LED7" pad="A"/>
<contactref element="R33" pad="1"/>
</signal>
<signal name="N$44">
<contactref element="LED8" pad="A"/>
<contactref element="R34" pad="1"/>
</signal>
<signal name="N$45">
<contactref element="LED9" pad="A"/>
<contactref element="R35" pad="1"/>
</signal>
<signal name="N$46">
<contactref element="LED10" pad="A"/>
<contactref element="R36" pad="1"/>
</signal>
<signal name="N$51">
<contactref element="LED5" pad="A"/>
<contactref element="R31" pad="1"/>
</signal>
<signal name="N$52">
<contactref element="LED6" pad="A"/>
<contactref element="R32" pad="1"/>
</signal>
<signal name="N$38">
<contactref element="R29" pad="2"/>
<contactref element="T2" pad="C"/>
</signal>
<signal name="N$56">
<contactref element="LED2" pad="C"/>
<contactref element="LED3" pad="C"/>
<contactref element="LED4" pad="C"/>
<contactref element="LED5" pad="C"/>
<contactref element="LED6" pad="C"/>
<contactref element="LED7" pad="C"/>
<contactref element="LED8" pad="C"/>
<contactref element="LED9" pad="C"/>
<contactref element="LED10" pad="C"/>
<contactref element="JP1" pad="1"/>
<contactref element="LED11" pad="C"/>
</signal>
<signal name="LED_COS">
<contactref element="R31" pad="2"/>
<contactref element="U1" pad="56"/>
</signal>
<signal name="LED_DSTAR">
<contactref element="R34" pad="2"/>
<contactref element="U1" pad="58"/>
</signal>
<signal name="LED_YSF">
<contactref element="R35" pad="2"/>
<contactref element="U1" pad="59"/>
</signal>
<signal name="LED_P25">
<contactref element="R36" pad="2"/>
<contactref element="U1" pad="61"/>
</signal>
<signal name="LED_DMR">
<contactref element="R33" pad="2"/>
<contactref element="U1" pad="57"/>
</signal>
<signal name="N$6">
</signal>
<signal name="SWDIO">
<contactref element="JP3" pad="2"/>
<contactref element="U1" pad="46"/>
</signal>
<signal name="SWCLK">
<contactref element="JP3" pad="4"/>
<contactref element="U1" pad="49"/>
</signal>
<signal name="N$2">
<contactref element="C2" pad="2"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$54">
<contactref element="R21" pad="2"/>
<contactref element="R22" pad="1"/>
<contactref element="IC3" pad="6"/>
</signal>
<signal name="N$55">
<contactref element="R22" pad="2"/>
<contactref element="R23" pad="1"/>
<contactref element="IC3" pad="3"/>
</signal>
<signal name="N$19">
<contactref element="IC2" pad="1"/>
<contactref element="R10" pad="2"/>
<contactref element="R20" pad="1"/>
<contactref element="TP2" pad="MP"/>
<contactref element="R9" pad="2"/>
</signal>
<signal name="N$57">
<contactref element="R25" pad="1"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="N$58">
<contactref element="LED1" pad="C"/>
<contactref element="T1" pad="C"/>
</signal>
<signal name="N$60">
<contactref element="IC3" pad="7"/>
<contactref element="D1" pad="2"/>
</signal>
<signal name="N$61">
<contactref element="IC3" pad="1"/>
<contactref element="D1" pad="1"/>
</signal>
<signal name="N$63">
<contactref element="T1" pad="B"/>
<contactref element="C22" pad="1"/>
<contactref element="D1" pad="3"/>
</signal>
<signal name="N$59">
<contactref element="IC3" pad="5"/>
<contactref element="IC3" pad="2"/>
<contactref element="R20" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="R7" pad="1"/>
<contactref element="C4" pad="1"/>
</signal>
<signal name="LED_NXDN">
<contactref element="R37" pad="2"/>
<contactref element="U1" pad="62"/>
</signal>
<signal name="N$65">
<contactref element="LED11" pad="A"/>
<contactref element="R37" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="U1" pad="30"/>
<contactref element="C7" pad="2"/>
</signal>
<signal name="14.2V">
<contactref element="A1" pad="IN"/>
<contactref element="J1" pad="A15"/>
<contactref element="J1" pad="B15"/>
<contactref element="J1" pad="C15"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="LED_HB">
<contactref element="R30" pad="2"/>
<contactref element="U1" pad="55"/>
</signal>
<signal name="BOOT0">
<contactref element="U1" pad="60"/>
<contactref element="R13" pad="2"/>
</signal>
<signal name="GPI_3">
<contactref element="J1" pad="C28"/>
<contactref element="JP8" pad="3"/>
<contactref element="T3" pad="B"/>
</signal>
<signal name="GPO_2">
<contactref element="J1" pad="C22"/>
<contactref element="T8" pad="C"/>
<contactref element="JP8" pad="1"/>
</signal>
<signal name="N$7">
</signal>
<signal name="BOOT">
<contactref element="U2" pad="A7"/>
<contactref element="JP5" pad="3"/>
<contactref element="R16" pad="2"/>
</signal>
<signal name="RESET">
<contactref element="U2" pad="A12"/>
<contactref element="JP5" pad="4"/>
<contactref element="R17" pad="1"/>
</signal>
<signal name="N$9">
</signal>
<signal name="GND7">
</signal>
<signal name="STN5V">
<contactref element="J1" pad="C3"/>
<contactref element="R54" pad="2"/>
<contactref element="J1" pad="B3"/>
<contactref element="J1" pad="A3"/>
</signal>
<signal name="OPTID">
<contactref element="R54" pad="1"/>
<contactref element="R55" pad="2"/>
<contactref element="J1" pad="C19"/>
</signal>
<signal name="MOSI">
<contactref element="J1" pad="A7"/>
<contactref element="J2" pad="4"/>
<contactref element="U3" pad="15"/>
</signal>
<signal name="MISO">
<contactref element="J1" pad="B8"/>
<contactref element="J2" pad="1"/>
<contactref element="U3" pad="16"/>
</signal>
<signal name="SPICLK">
<contactref element="J1" pad="C8"/>
<contactref element="J2" pad="3"/>
<contactref element="U3" pad="17"/>
</signal>
<signal name="CS2">
<contactref element="J1" pad="A10"/>
<contactref element="D3" pad="1"/>
<contactref element="U3" pad="32"/>
</signal>
<signal name="CS4">
<contactref element="J1" pad="B10"/>
</signal>
<signal name="CS3">
<contactref element="J1" pad="C10"/>
</signal>
<signal name="CS1">
<contactref element="J1" pad="B11"/>
<contactref element="D3" pad="2"/>
<contactref element="U3" pad="1"/>
</signal>
<signal name="OPTIRQ">
<contactref element="J1" pad="A25"/>
<contactref element="U3" pad="12"/>
</signal>
<signal name="CARDET">
<contactref element="J1" pad="B29"/>
</signal>
<signal name="ACFAIL">
<contactref element="J1" pad="C29"/>
</signal>
<signal name="GPO_0">
<contactref element="J1" pad="B25"/>
<contactref element="T7" pad="C"/>
</signal>
<signal name="GPO_8">
<contactref element="J1" pad="C32"/>
<contactref element="T9" pad="C"/>
</signal>
<signal name="GPO_13">
<contactref element="J1" pad="B31"/>
<contactref element="T10" pad="C"/>
</signal>
<signal name="GPI_4">
<contactref element="J1" pad="A28"/>
<contactref element="T4" pad="B"/>
</signal>
<signal name="GPI_7">
<contactref element="J1" pad="C11"/>
<contactref element="T5" pad="B"/>
</signal>
<signal name="GPI_9">
<contactref element="J1" pad="C6"/>
</signal>
<signal name="GPI_10">
<contactref element="J1" pad="A24"/>
<contactref element="T6" pad="B"/>
</signal>
<signal name="TXO">
<contactref element="JP7" pad="2"/>
<contactref element="J3" pad="RXI"/>
<contactref element="U3" pad="31"/>
</signal>
<signal name="SBC_TX">
<contactref element="U2" pad="A11"/>
<contactref element="Q3" pad="2"/>
<contactref element="R43" pad="2"/>
<contactref element="JP6" pad="2"/>
</signal>
<signal name="SBC_RX">
<contactref element="U2" pad="A22"/>
<contactref element="Q2" pad="2"/>
<contactref element="R42" pad="2"/>
<contactref element="JP6" pad="3"/>
</signal>
<signal name="AVR_TX">
<contactref element="Q2" pad="3"/>
<contactref element="R45" pad="2"/>
<contactref element="JP7" pad="1"/>
</signal>
<signal name="RXI">
<contactref element="JP7" pad="4"/>
<contactref element="J3" pad="TXO"/>
<contactref element="U3" pad="30"/>
</signal>
<signal name="~SS">
<contactref element="D3" pad="3"/>
<contactref element="U3" pad="14"/>
</signal>
<signal name="LOAD">
<contactref element="R14" pad="1"/>
<contactref element="R13" pad="1"/>
<contactref element="R16" pad="1"/>
<contactref element="JP9" pad="1"/>
</signal>
<signal name="AVR_RX">
<contactref element="Q3" pad="3"/>
<contactref element="R46" pad="2"/>
<contactref element="JP7" pad="3"/>
</signal>
<signal name="OUT0">
<contactref element="T7" pad="B"/>
<contactref element="R56" pad="2"/>
<contactref element="U3" pad="2"/>
</signal>
<signal name="OUT2">
<contactref element="T8" pad="B"/>
<contactref element="R57" pad="2"/>
<contactref element="U3" pad="9"/>
</signal>
<signal name="OUT8">
<contactref element="T9" pad="B"/>
<contactref element="R58" pad="2"/>
<contactref element="U3" pad="10"/>
</signal>
<signal name="OUT13">
<contactref element="T10" pad="B"/>
<contactref element="R59" pad="2"/>
<contactref element="U3" pad="11"/>
</signal>
<signal name="IN3">
<contactref element="R38" pad="2"/>
<contactref element="T3" pad="C"/>
<contactref element="R49" pad="2"/>
<contactref element="U3" pad="23"/>
</signal>
<signal name="IN4">
<contactref element="R39" pad="2"/>
<contactref element="T4" pad="C"/>
<contactref element="R50" pad="2"/>
<contactref element="U3" pad="24"/>
</signal>
<signal name="IN7">
<contactref element="R40" pad="2"/>
<contactref element="T5" pad="C"/>
<contactref element="R51" pad="2"/>
<contactref element="U3" pad="25"/>
</signal>
<signal name="IN10">
<contactref element="R41" pad="2"/>
<contactref element="T6" pad="C"/>
<contactref element="R52" pad="2"/>
<contactref element="U3" pad="26"/>
</signal>
<signal name="GPI_12">
<contactref element="J1" pad="B22"/>
</signal>
<signal name="DISP_TX">
<contactref element="JP4" pad="2"/>
<contactref element="U1" pad="53"/>
</signal>
<signal name="DISP_RX">
<contactref element="JP4" pad="3"/>
<contactref element="U1" pad="54"/>
</signal>
<signal name="DTR">
<contactref element="J3" pad="DTR"/>
<contactref element="C18" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="LED16" pad="A"/>
<contactref element="R56" pad="1"/>
</signal>
<signal name="N$13">
<contactref element="LED17" pad="A"/>
<contactref element="R57" pad="1"/>
</signal>
<signal name="N$15">
<contactref element="LED18" pad="A"/>
<contactref element="R58" pad="1"/>
</signal>
<signal name="N$18">
<contactref element="LED19" pad="A"/>
<contactref element="R59" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="LED12" pad="A"/>
<contactref element="R49" pad="1"/>
</signal>
<signal name="N$14">
<contactref element="LED13" pad="A"/>
<contactref element="R50" pad="1"/>
</signal>
<signal name="N$16">
<contactref element="LED14" pad="A"/>
<contactref element="R51" pad="1"/>
</signal>
<signal name="N$20">
<contactref element="LED15" pad="A"/>
<contactref element="R52" pad="1"/>
</signal>
<signal name="~RESET">
<contactref element="J1" pad="B16"/>
<contactref element="JP11" pad="1"/>
</signal>
<signal name="AVR_RESET">
<contactref element="JP11" pad="2"/>
<contactref element="D2" pad="2"/>
</signal>
<signal name="SBC_DTR">
<contactref element="Q4" pad="2"/>
<contactref element="R44" pad="2"/>
<contactref element="U2" pad="A24"/>
</signal>
<signal name="SBC_SDA">
<contactref element="U2" pad="A3"/>
<contactref element="R18" pad="1"/>
<contactref element="J1" pad="C5"/>
</signal>
<signal name="SBC_SCL">
<contactref element="U2" pad="A5"/>
<contactref element="R19" pad="1"/>
<contactref element="J1" pad="C7"/>
</signal>
<signal name="AVR_PROG">
<contactref element="Q4" pad="3"/>
<contactref element="R47" pad="2"/>
<contactref element="D2" pad="1"/>
</signal>
<signal name="RST">
<contactref element="D2" pad="3"/>
<contactref element="J2" pad="5"/>
<contactref element="R24" pad="2"/>
<contactref element="U3" pad="29"/>
<contactref element="C18" pad="1"/>
</signal>
<signal name="AVR_SDA">
<contactref element="U3" pad="27"/>
<contactref element="R26" pad="1"/>
<contactref element="J1" pad="C24"/>
</signal>
<signal name="AVR_SCL">
<contactref element="U3" pad="28"/>
<contactref element="R27" pad="1"/>
<contactref element="J1" pad="C25"/>
</signal>
<signal name="XTAL1">
<contactref element="Y1" pad="1"/>
<contactref element="U3" pad="7"/>
</signal>
<signal name="XTAL2">
<contactref element="Y1" pad="3"/>
<contactref element="U3" pad="8"/>
</signal>
<signal name="AREF">
<contactref element="U3" pad="20"/>
<contactref element="C19" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
