(kicad_pcb (version 20171130) (host pcbnew "(5.0.0)")
  (general
    (thickness 1.6)
    (drawings 20)
    (tracks 109)
    (zones 0)
    (modules 16)
    (nets 9)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.254)
    (trace_clearance 0.381)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.254)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.3302)
    (via_min_drill 0.3)
    (uvia_size 0.6858)
    (uvia_drill 0.3302)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 8.6 8.6)
    (pad_drill 4.3)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 28VDC_IN)
  (net 2 GND_IN)
  (net 3 +5VDC_OUT)
  (net 4 GND_OUT)
  (net 5 +12VDC_NEW_OUT)
  (net 6 28VDC_SOURCE)
  (net 7 -12VDC_OLD_OUT)
  (net 8 +12VDC_OLD_OUT)
  (net_class Default "This is the default net class."
    (clearance 0.381)
    (trace_width 0.254)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (diff_pair_gap 0.254)
    (diff_pair_width 0.254)
    (add_net +12VDC_NEW_OUT)
    (add_net +12VDC_OLD_OUT)
    (add_net +5VDC_OUT)
    (add_net -12VDC_OLD_OUT)
    (add_net 28VDC_IN)
    (add_net 28VDC_SOURCE)
    (add_net GND_IN)
    (add_net GND_OUT)
  )
  (module TCP_power_board:JCA6024D02 (layer B.Cu) (tedit 5BCFBB1F)
    (at 100.33 128.27 90)
    (descr "DCDC-Converter, BOTHHAND, Type CFxxxx-Serie,  (Very dodgy url but was the only at hand), ")
    (tags "DCDC-Converter BOTHHAND Type CFxxxx-Serie")
    (fp_text reference U1 (at 2.286 15.494 180) (layer B.SilkS))
    (fp_text value JCA0624D02 (at 0 -15.24 90) (layer B.Fab))
    (fp_text user %R (at 0 1.97 90) (layer B.Fab))
    (pad 22 thru_hole oval (at 7.64 8.89 90) (size 2.5 1.5) (drill 0.79375) (layers *.Cu *.Mask)
      (net 1 28VDC_IN))
    (pad 2 thru_hole oval (at -7.62 11.43 90) (size 2.5 1.5) (drill 0.79375) (layers *.Cu *.Mask)
      (net 2 GND_IN))
    (pad 9 thru_hole oval (at -7.62 -6.35 90) (size 2.5 1.5) (drill 0.79375) (layers *.Cu *.Mask)
      (net 4 GND_OUT))
    (pad 11 thru_hole oval (at -7.62 -11.43 90) (size 2.5 1.5) (drill 0.79375) (layers *.Cu *.Mask)
      (net 7 -12VDC_OLD_OUT))
    (pad 3 thru_hole oval (at -7.62 8.89 90) (size 2.5 1.5) (drill 0.79375) (layers *.Cu *.Mask)
      (net 2 GND_IN))
    (pad 14 thru_hole oval (at 7.62 -11.43 90) (size 2.5 1.5) (drill 0.79375) (layers *.Cu *.Mask)
      (net 8 +12VDC_OLD_OUT))
    (pad 16 thru_hole oval (at 7.62 -6.35 90) (size 2.5 1.5) (drill 0.79375) (layers *.Cu *.Mask)
      (net 4 GND_OUT))
    (pad 23 thru_hole oval (at 7.62 11.43 90) (size 2.5 1.5) (drill 0.79375) (layers *.Cu *.Mask)
      (net 1 28VDC_IN))
    (model ${KISYS3DMOD}/Converters_DCDC_ACDC.3dshapes/DCDC-Conv_BOTHHAND_CFUDxxxx-Serie.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TCP_power_board:JCK5024S12 (layer B.Cu) (tedit 5BCF70FF)
    (at 156.845 116.84 270)
    (tags "DCDC-Converter XPpower")
    (fp_text reference U3 (at 14.224 -3.175) (layer B.SilkS))
    (fp_text value JCK5024S12 (at 0 -27.94 270) (layer B.Fab))
    (fp_text user %R (at 0 1.97 270) (layer B.Fab))
    (pad 6 thru_hole oval (at -10.16 22.86 270) (size 3.556 2.032) (drill 1.27) (layers *.Cu *.Mask))
    (pad 1 thru_hole oval (at 7.62 -22.86 270) (size 3.556 2.032) (drill 1.27) (layers *.Cu *.Mask)
      (net 1 28VDC_IN))
    (pad 3 thru_hole oval (at -7.62 -22.86 270) (size 3.556 2.032) (drill 1.27) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 22.86 270) (size 3.556 2.032) (drill 1.27) (layers *.Cu *.Mask)
      (net 4 GND_OUT))
    (pad 2 thru_hole oval (at 2.54 -22.86 270) (size 3.556 2.032) (drill 1.27) (layers *.Cu *.Mask)
      (net 2 GND_IN))
    (pad 4 thru_hole oval (at 10.16 22.86 270) (size 3.556 2.032) (drill 1.27) (layers *.Cu *.Mask)
      (net 5 +12VDC_NEW_OUT))
    (model ${KISYS3DMOD}/Converters_DCDC_ACDC.3dshapes/DCDC-Conv_BOTHHAND_CFUDxxxx-Serie.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D12.5mm_P5.00mm (layer F.Cu) (tedit 5AE50EF1)
    (at 144.145 97.155 180)
    (descr "CP, Radial series, Radial, pin pitch=5.00mm, , diameter=12.5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 5.00mm  diameter 12.5mm Electrolytic Capacitor")
    (fp_text reference C1 (at 11.049 0.127 180) (layer F.SilkS))
    (fp_text value "220uF 35V" (at 2.5 7.5 180) (layer F.Fab))
    (fp_text user %R (at 2.5 0 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 28VDC_IN))
    (pad 2 thru_hole circle (at 5 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 GND_IN))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D12.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D10.0mm_P2.50mm_P5.00mm (layer F.Cu) (tedit 5AE50EF1)
    (at 123.785 122.555 180)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm 5.00mm, , diameter=10mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm 5.00mm  diameter 10mm Electrolytic Capacitor")
    (fp_text reference C2 (at -5.247 0.127 180) (layer F.SilkS))
    (fp_text value "220uF 16V" (at 1.25 6.25 180) (layer F.Fab))
    (fp_text user %R (at 1.25 0 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 +5VDC_OUT))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 GND_OUT))
    (pad 1 thru_hole rect (at -0.670937 -1.6 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 +5VDC_OUT))
    (pad 2 thru_hole circle (at 3.170937 1.6 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 GND_OUT))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D10.0mm_P2.50mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D10.0mm_P2.50mm_P5.00mm (layer F.Cu) (tedit 5AE50EF1)
    (at 123.825 133.35 180)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm 5.00mm, , diameter=10mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm 5.00mm  diameter 10mm Electrolytic Capacitor")
    (fp_text reference C3 (at -5.207 0.254 180) (layer F.SilkS))
    (fp_text value "220uF 16V" (at 1.25 6.25 180) (layer F.Fab))
    (fp_text user %R (at 1.25 0 180) (layer F.Fab))
    (pad 2 thru_hole circle (at 3.170937 1.6 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 GND_OUT))
    (pad 1 thru_hole rect (at -0.670937 -1.6 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 +12VDC_NEW_OUT))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 GND_OUT))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 +12VDC_NEW_OUT))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D10.0mm_P2.50mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-220-2_Horizontal_TabDown (layer F.Cu) (tedit 5AC8BA0D)
    (at 163.83 93.98 270)
    (descr "TO-220-2, Horizontal, RM 5.08mm, see https://www.centralsemi.com/PDFS/CASE/TO-220-2PD.PDF")
    (tags "TO-220-2 Horizontal RM 5.08mm")
    (fp_text reference CR1 (at 9.652 -11.938) (layer F.SilkS))
    (fp_text value MBR1045 (at 2.54 2 270) (layer F.Fab))
    (fp_text user %R (at 2.54 -20.58 270) (layer F.Fab))
    (pad "" np_thru_hole oval (at 2.54 -16.66 270) (size 3.5 3.5) (drill 3.5) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at 0 0 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 28VDC_IN))
    (pad 2 thru_hole oval (at 5.08 0 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 6 28VDC_SOURCE))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-220-2_Horizontal_TabDown.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Molex:Molex_Mini-Fit_Jr_5569-02A2_2x01_P4.20mm_Horizontal (layer F.Cu) (tedit 5A15CC90)
    (at 169.23 135.89 270)
    (descr "Molex Mini-Fit Jr. Power Connectors, old mpn/engineering number: 5569-02A2, example for new mpn: 39-30-0020, 1 Pins per row, Mounting: Snap-in Plastic Peg PCB Lock (http://www.molex.com/pdm_docs/sd/039300020_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex Mini-Fit_Jr top entryplastic_peg")
    (fp_text reference J1 (at -3.81 -13.142) (layer F.SilkS))
    (fp_text value 28VDC (at 0 8.55 270) (layer F.Fab))
    (fp_text user %R (at 0 -13.2 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.7 3.7) (drill 1.8) (layers *.Cu *.Mask)
      (net 6 28VDC_SOURCE))
    (pad 2 thru_hole oval (at 0 5.5 270) (size 2.7 3.7) (drill 1.8) (layers *.Cu *.Mask)
      (net 2 GND_IN))
    (pad "" np_thru_hole circle (at 0 -7.3 270) (size 3 3) (drill 3) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_Mini-Fit_Jr_5569-02A2_2x01_P4.20mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Molex:Molex_Mini-Fit_Jr_5566-10A_2x05_P4.20mm_Vertical (layer F.Cu) (tedit 5A15CC62)
    (at 66.675 116.205 90)
    (descr "Molex Mini-Fit Jr. Power Connectors, old mpn/engineering number: 5566-10A, example for new mpn: 39-28-x10x, 5 Pins per row, Mounting:  (http://www.molex.com/pdm_docs/sd/039281043_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex Mini-Fit_Jr side entry")
    (fp_text reference J2 (at 20.701 -1.143 180) (layer F.SilkS))
    (fp_text value OldPwr (at 8.4 9.95 90) (layer F.Fab))
    (fp_text user %R (at 8.4 -1.55 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.7 3.3) (drill 1.4) (layers *.Cu *.Mask)
      (net 4 GND_OUT))
    (pad 2 thru_hole oval (at 4.2 0 90) (size 2.7 3.3) (drill 1.4) (layers *.Cu *.Mask)
      (net 4 GND_OUT))
    (pad 3 thru_hole oval (at 8.4 0 90) (size 2.7 3.3) (drill 1.4) (layers *.Cu *.Mask)
      (net 4 GND_OUT))
    (pad 4 thru_hole oval (at 12.6 0 90) (size 2.7 3.3) (drill 1.4) (layers *.Cu *.Mask)
      (net 4 GND_OUT))
    (pad 5 thru_hole oval (at 16.8 0 90) (size 2.7 3.3) (drill 1.4) (layers *.Cu *.Mask)
      (net 7 -12VDC_OLD_OUT))
    (pad 6 thru_hole oval (at 0 5.5 90) (size 2.7 3.3) (drill 1.4) (layers *.Cu *.Mask)
      (net 3 +5VDC_OUT))
    (pad 7 thru_hole oval (at 4.2 5.5 90) (size 2.7 3.3) (drill 1.4) (layers *.Cu *.Mask)
      (net 3 +5VDC_OUT))
    (pad 8 thru_hole oval (at 8.4 5.5 90) (size 2.7 3.3) (drill 1.4) (layers *.Cu *.Mask)
      (net 3 +5VDC_OUT))
    (pad 9 thru_hole oval (at 12.6 5.5 90) (size 2.7 3.3) (drill 1.4) (layers *.Cu *.Mask)
      (net 3 +5VDC_OUT))
    (pad 10 thru_hole oval (at 16.8 5.5 90) (size 2.7 3.3) (drill 1.4) (layers *.Cu *.Mask)
      (net 8 +12VDC_OLD_OUT))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_Mini-Fit_Jr_5566-10A_2x05_P4.20mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 71.12 92.71 270)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J3 (at -0.254 5.08) (layer F.SilkS))
    (fp_text value FanPwr (at 0 4.87 270) (layer F.Fab))
    (fp_text user %R (at 0 1.27) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +5VDC_OUT))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 GND_OUT))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Molex:Molex_Mini-Fit_Jr_5566-04A_2x02_P4.20mm_Vertical (layer F.Cu) (tedit 5A15CC62)
    (at 66.675 127 90)
    (descr "Molex Mini-Fit Jr. Power Connectors, old mpn/engineering number: 5566-04A, example for new mpn: 39-28-x04x, 2 Pins per row, Mounting:  (http://www.molex.com/pdm_docs/sd/039281043_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex Mini-Fit_Jr side entry")
    (fp_text reference J4 (at -4.064 -1.143 180) (layer F.SilkS))
    (fp_text value NewPwr (at 2.1 9.95 90) (layer F.Fab))
    (fp_text user %R (at 2.1 -1.55 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.7 3.3) (drill 1.4) (layers *.Cu *.Mask)
      (net 4 GND_OUT))
    (pad 2 thru_hole oval (at 4.2 0 90) (size 2.7 3.3) (drill 1.4) (layers *.Cu *.Mask)
      (net 4 GND_OUT))
    (pad 3 thru_hole oval (at 0 5.5 90) (size 2.7 3.3) (drill 1.4) (layers *.Cu *.Mask)
      (net 5 +12VDC_NEW_OUT))
    (pad 4 thru_hole oval (at 4.2 5.5 90) (size 2.7 3.3) (drill 1.4) (layers *.Cu *.Mask)
      (net 5 +12VDC_NEW_OUT))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_Mini-Fit_Jr_5566-04A_2x02_P4.20mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TCP_power_board:JCK5024S05 (layer B.Cu) (tedit 5BCF6FB5)
    (at 102.87 104.14 270)
    (tags "DCDC-Converter XPpower")
    (fp_text reference U2 (at 13.97 19.05) (layer B.SilkS))
    (fp_text value JCK5024S05 (at 0 -27.94 270) (layer B.Fab))
    (fp_text user %R (at 0 1.97 270) (layer B.Fab))
    (pad 4 thru_hole oval (at 10.16 22.86 270) (size 3.556 2.032) (drill 1.27) (layers *.Cu *.Mask)
      (net 3 +5VDC_OUT))
    (pad 2 thru_hole oval (at 2.54 -22.86 270) (size 3.556 2.032) (drill 1.27) (layers *.Cu *.Mask)
      (net 2 GND_IN))
    (pad 5 thru_hole oval (at 0 22.86 270) (size 3.556 2.032) (drill 1.27) (layers *.Cu *.Mask)
      (net 4 GND_OUT))
    (pad 3 thru_hole oval (at -7.62 -22.86 270) (size 3.556 2.032) (drill 1.27) (layers *.Cu *.Mask))
    (pad 1 thru_hole oval (at 7.62 -22.86 270) (size 3.556 2.032) (drill 1.27) (layers *.Cu *.Mask)
      (net 1 28VDC_IN))
    (pad 6 thru_hole oval (at -10.16 22.86 270) (size 3.556 2.032) (drill 1.27) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Converters_DCDC_ACDC.3dshapes/DCDC-Conv_BOTHHAND_CFUDxxxx-Serie.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-15_P15.24mm_Horizontal (layer F.Cu) (tedit 5AE50CD5)
    (at 137.16 135.89)
    (descr "Diode, DO-15 series, Axial, Horizontal, pin pitch=15.24mm, , length*diameter=7.6*3.6mm^2, , http://www.diodes.com/_files/packages/DO-15.pdf")
    (tags "Diode DO-15 series Axial Horizontal pin pitch 15.24mm  length 7.6mm diameter 3.6mm")
    (fp_text reference VR1 (at 7.62 -2.92) (layer F.SilkS))
    (fp_text value P6KE43A (at 7.62 2.92) (layer F.Fab))
    (fp_text user %R (at 8.19 0) (layer F.Fab))
    (fp_text user K (at 0 -2.2) (layer F.Fab))
    (fp_text user K (at 0 -2.2) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 28VDC_IN))
    (pad 2 thru_hole oval (at 15.24 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 GND_IN))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-15_P15.24mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 5C95825F)
    (at 85.725 108.585 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference TP1 (at 0 4.953 180) (layer F.SilkS))
    (fp_text value TP1 (at 0 4.87 180) (layer F.Fab))
    (fp_text user %R (at 0 1.27 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +5VDC_OUT))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 GND_OUT))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 5C958269)
    (at 139.7 123.19 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference TP2 (at 0 4.826 180) (layer F.SilkS))
    (fp_text value TP2 (at 0 4.87 180) (layer F.Fab))
    (fp_text user %R (at 0 1.27 270) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 GND_OUT))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 +12VDC_NEW_OUT))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_4.3mm_M4_Pad (layer F.Cu) (tedit 5C4B6F7B)
    (at 79.375 130.175)
    (descr "Mounting Hole 4.3mm, M4")
    (tags "mounting hole 4.3mm m4")
    (attr virtual)
    (fp_text reference REF1 (at 0 -5.3) (layer F.SilkS) hide)
    (fp_text value MountingHole_4.3mm_M4_Pad (at 0 5.3) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 8.6 8.6) (drill 4.3) (layers *.Cu *.Mask)
      (net 4 GND_OUT))
  )
  (module MountingHole:MountingHole_4.3mm_M4_Pad (layer F.Cu) (tedit 5C4B6F04)
    (at 155.4 99.1)
    (descr "Mounting Hole 4.3mm, M4")
    (tags "mounting hole 4.3mm m4")
    (attr virtual)
    (fp_text reference REF2 (at 0 -5.3) (layer F.SilkS) hide)
    (fp_text value MountingHole_4.3mm_M4_Pad (at 0 5.3) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 8.6 8.6) (drill 4.3) (layers *.Cu *.Mask)
      (net 4 GND_OUT))
  )
  (gr_text "BATCH: 20190322" (at 66.04 137.16) (layer F.SilkS))
  (gr_text "TCP Power Board (dual)\nPCB:  419992-1 (Rev -)\nASSY: 37695 / 729989-801 (Rev -)" (at 85.09 95.25) (layer F.SilkS))
  (gr_text 10/9 (at 76.708 116.332) (layer F.SilkS))
  (gr_text 8/7 (at 76.708 111.76) (layer F.SilkS))
  (gr_text 6/5 (at 76.708 107.696) (layer F.SilkS))
  (gr_text 4/3 (at 76.708 103.632) (layer F.SilkS))
  (gr_text 2/1 (at 76.708 99.06) (layer F.SilkS))
  (gr_text "LEGACY\nPIN #s" (at 76.708 96.012) (layer F.SilkS))
  (gr_text JCk5024S05 (at 80.01 120.65) (layer B.SilkS))
  (gr_text JCK5024S12 (at 152.4 131.064) (layer B.SilkS))
  (gr_text JCA0624D02 (at 119.38 128.524) (layer B.SilkS))
  (gr_text "B  R" (at 69.596 90.424) (layer F.SilkS))
  (gr_text GND (at 91.44 106.172) (layer F.SilkS))
  (gr_text GND (at 145.6055 120.8405) (layer F.SilkS))
  (gr_text +12VDC (at 145.4785 123.3805) (layer F.SilkS))
  (gr_text +5VDC (at 90.932 108.712) (layer F.SilkS))
  (gr_line (start 63.5 139.7) (end 63.5 88.9) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 184.15 139.7) (end 63.5 139.7) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 184.15 88.9) (end 184.15 139.7) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 63.5 88.9) (end 184.15 88.9) (layer Edge.Cuts) (width 0.1))
  (zone (net 4) (net_name GND_OUT) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 63.5 88.9) (xy 184.15 88.9) (xy 184.15 139.7) (xy 63.5 139.7)
      )
    )
  )
  (zone (net 4) (net_name GND_OUT) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 63.5 88.9) (xy 184.15 88.9) (xy 184.15 139.7) (xy 63.5 139.7)
      )
    )
  )
  (zone (net 0) (net_name "") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 183.515 90.805) (xy 184.15 90.805) (xy 167.005 90.805) (xy 167.005 102.235) (xy 184.15 102.235)
        (xy 184.15 90.805)
      )
    )
  )
)
