(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(4 "In1.Cu" signal)
		(6 "In2.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "prepreg")
				(thickness 0.1)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "In1.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 2"
				(type "core")
				(thickness 1.24)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "In2.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 3"
				(type "prepreg")
				(thickness 0.1)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "Net-(J9-In)")
	(net 2 "GND")
	(net 3 "Net-(U1-SET)")
	(net 4 "LDO+5")
	(net 5 "Net-(J10-In)")
	(net 6 "Net-(U2-SET)")
	(net 7 "LDO-5")
	(net 8 "Net-(J2-In)")
	(net 9 "Net-(C7-Pad2)")
	(net 10 "Net-(U3A--)")
	(net 11 "Net-(C12-Pad2)")
	(net 12 "Net-(J4-In)")
	(net 13 "Net-(C10-Pad2)")
	(net 14 "Net-(J6-In)")
	(net 15 "Net-(U3C--)")
	(net 16 "Net-(U3B--)")
	(net 17 "Net-(J8-In)")
	(net 18 "Net-(C13-Pad2)")
	(net 19 "Net-(U3D--)")
	(net 20 "Net-(J1-In)")
	(net 21 "Net-(J3-In)")
	(net 22 "Net-(J5-In)")
	(net 23 "Net-(J7-In)")
	(net 24 "Net-(U1-PG)")
	(net 25 "Net-(U1-ILIM)")
	(net 26 "Net-(U1-PGFB)")
	(net 27 "Net-(U2-ILIM)")
	(net 28 "Net-(U2-EN{slash}UV)")
	(net 29 "Net-(U2-PGFB)")
	(net 30 "unconnected-(U2-PG-Pad4)")
	(net 31 "unconnected-(U2-VIOC-Pad7)")
	(footprint "Package_SO:MSOP-12-1EP_3x4.039mm_P0.65mm_EP1.651x2.845mm"
		(layer "F.Cu")
		(at 104.65 105.625)
		(descr "MSOP, 12 Pin (https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/ltc-legacy-msop/05081666_g_mse12.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "MSOP SO")
		(property "Reference" "U1"
			(at 0 -2.97 0)
			(layer "F.SilkS")
		)
		(property "Value" "LT3045xMSE"
			(at 0.125 2.925 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/3045fa.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "500mA, Adjustable, Ultralow Noise, Ultrahigh PSRR Linear Regulator, MSOP-12"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MSOP*1EP*3x4.039mm*P0.65mm*")
		(sheetname "/")
		(sheetfile "LT3045_breakout.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.415 -0.71)
			(size 0.67 1.15)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at -0.415 0.71)
			(size 0.67 1.15)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.415 -0.71)
			(size 0.67 1.15)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.415 0.71)
			(size 0.67 1.15)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -2.15 -1.625)
			(size 1.45 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "Net-(J9-In)")
			(pinfunction "IN")
			(pintype "power_in")
		)
		(pad "2" smd roundrect
			(at -2.15 -0.975)
			(size 1.45 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "Net-(J9-In)")
			(pinfunction "IN")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at -2.15 -0.325)
			(size 1.45 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "Net-(J9-In)")
			(pinfunction "IN")
			(pintype "passive")
		)
		(pad "4" smd roundrect
			(at -2.15 0.325)
			(size 1.45 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "Net-(J9-In)")
			(pinfunction "EN/UV")
			(pintype "input")
		)
		(pad "5" smd roundrect
			(at -2.15 0.975)
			(size 1.45 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 24 "Net-(U1-PG)")
			(pinfunction "PG")
			(pintype "open_collector")
		)
		(pad "6" smd roundrect
			(at -2.15 1.625)
			(size 1.45 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 25 "Net-(U1-ILIM)")
			(pinfunction "ILIM")
			(pintype "passive")
		)
		(pad "7" smd roundrect
			(at 2.15 1.625)
			(size 1.45 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 26 "Net-(U1-PGFB)")
			(pinfunction "PGFB")
			(pintype "input")
		)
		(pad "8" smd roundrect
			(at 2.15 0.975)
			(size 1.45 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "Net-(U1-SET)")
			(pinfunction "SET")
			(pintype "passive")
		)
		(pad "9" smd roundrect
			(at 2.15 0.325)
			(size 1.45 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "10" smd roundrect
			(at 2.15 -0.325)
			(size 1.45 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "LDO+5")
			(pinfunction "OUTS")
			(pintype "input")
		)
		(pad "11" smd roundrect
			(at 2.15 -0.975)
			(size 1.45 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "LDO+5")
			(pinfunction "OUT")
			(pintype "power_out")
		)
		(pad "12" smd roundrect
			(at 2.15 -1.625)
			(size 1.45 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "LDO+5")
			(pinfunction "OUT")
			(pintype "passive")
		)
		(pad "13" smd rect
			(at 0 0)
			(size 1.651 2.845)
			(property pad_prop_heatsink)
			(layers "F.Cu" "F.Mask")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(zone_connect 2)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_SO.3dshapes/MSOP-12-1EP_3x4.039mm_P0.65mm_EP1.651x2.845mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Coaxial:SMA_Amphenol_132134_Vertical"
		(layer "F.Cu")
		(at 136.859524 140.07)
		(descr "https://www.amphenolrf.com/library/download/link/link_id/593003/parent/132134/")
		(tags "SMA THT Female Jack Vertical ExtendedLegs")
		(property "Reference" "J5"
			(at 0.165476 -5.095 0)
			(layer "F.SilkS")
		)
		(property "Value" "Ch3 in"
			(at 0 5 0)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, LEMO, ...)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*BNC* *SMA* *SMB* *SMC* *Cinch* *LEMO* *UMRF* *MCX* *U.FL*")
		(sheetname "/ADA4087/")
		(sheetfile "ADA4087.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2.05 2.05)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "Net-(J5-In)")
			(pinfunction "In")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at -2.54 -2.54)
			(size 2.25 2.25)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at -2.54 2.54)
			(size 2.25 2.25)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 -2.54)
			(size 2.25 2.25)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 2.54)
			(size 2.25 2.25)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_Coaxial.3dshapes/SMA_Amphenol_132134_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 91.9 104.825 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C1"
			(at 0 -1.43 90)
			(layer "F.SilkS")
		)
		(property "Value" "4.7 uF"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "LT3045_breakout.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "Net-(J9-In)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Coaxial:SMA_Amphenol_132134_Vertical"
		(layer "F.Cu")
		(at 151.874762 90.61)
		(descr "https://www.amphenolrf.com/library/download/link/link_id/593003/parent/132134/")
		(tags "SMA THT Female Jack Vertical ExtendedLegs")
		(property "Reference" "J1"
			(at 0 -4.75 0)
			(layer "F.SilkS")
		)
		(property "Value" "Ch1 In"
			(at 0 5 0)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, LEMO, ...)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*BNC* *SMA* *SMB* *SMC* *Cinch* *LEMO* *UMRF* *MCX* *U.FL*")
		(sheetname "/ADA4087/")
		(sheetfile "ADA4087.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2.05 2.05)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "Net-(J1-In)")
			(pinfunction "In")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at -2.54 -2.54)
			(size 2.25 2.25)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at -2.54 2.54)
			(size 2.25 2.25)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 -2.54)
			(size 2.25 2.25)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 2.54)
			(size 2.25 2.25)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_Coaxial.3dshapes/SMA_Amphenol_132134_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 97.65 110.175 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R3"
			(at 0 -1.43 90)
			(layer "F.SilkS")
		)
		(property "Value" "49.9k"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "LT3045_breakout.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "Net-(U1-SET)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Coaxial:SMA_Amphenol_132134_Vertical"
		(layer "F.Cu")
		(at 136.859524 90.61)
		(descr "https://www.amphenolrf.com/library/download/link/link_id/593003/parent/132134/")
		(tags "SMA THT Female Jack Vertical ExtendedLegs")
		(property "Reference" "J3"
			(at 0 -4.75 0)
			(layer "F.SilkS")
		)
		(property "Value" "Ch2 in"
			(at 0 5 0)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, LEMO, ...)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*BNC* *SMA* *SMB* *SMC* *Cinch* *LEMO* *UMRF* *MCX* *U.FL*")
		(sheetname "/ADA4087/")
		(sheetfile "ADA4087.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2.05 2.05)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "Net-(J3-In)")
			(pinfunction "In")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at -2.54 -2.54)
			(size 2.25 2.25)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at -2.54 2.54)
			(size 2.25 2.25)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 -2.54)
			(size 2.25 2.25)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 2.54)
			(size 2.25 2.25)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_Coaxial.3dshapes/SMA_Amphenol_132134_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Loop_D1.80mm_Drill1.0mm_Beaded"
		(layer "F.Cu")
		(at 82.02 123.07)
		(descr "wire loop with bead as test point, loop diameter 1.8mm, hole diameter 1.0mm")
		(tags "test point wire loop bead")
		(property "Reference" "TP3"
			(at 2.4 2.5 0)
			(layer "F.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -2.8 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "LT3045_breakout.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.7 2.5 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "Net-(J10-In)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/TestPoint.3dshapes/TestPoint_Loop_D1.80mm_Drill1.0mm_Beaded.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 97.525 131.875 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R7"
			(at 0 -1.43 90)
			(layer "F.SilkS")
		)
		(property "Value" "100k"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "LT3045_breakout.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "Net-(J10-In)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 28 "Net-(U2-EN{slash}UV)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 136.85 101.975 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R17"
			(at -0.05 -1.775 90)
			(layer "F.SilkS")
		)
		(property "Value" "2.2k"
			(at 0.15 1.675 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/ADA4087/")
		(sheetfile "ADA4087.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 11 "Net-(C12-Pad2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 21 "Net-(J3-In)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 102.325 137.7)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R6"
			(at 0 -1.43 0)
			(layer "F.SilkS")
		)
		(property "Value" "4.99k"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "LT3045_breakout.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 27 "Net-(U2-ILIM)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Coaxial:SMA_Amphenol_132134_Vertical"
		(layer "F.Cu")
		(at 121.844286 90.61)
		(descr "https://www.amphenolrf.com/library/download/link/link_id/593003/parent/132134/")
		(tags "SMA THT Female Jack Vertical ExtendedLegs")
		(property "Reference" "J4"
			(at 0 -4.75 0)
			(layer "F.SilkS")
		)
		(property "Value" "Ch2 output"
			(at 0 5 0)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, LEMO, ...)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*BNC* *SMA* *SMB* *SMC* *Cinch* *LEMO* *UMRF* *MCX* *U.FL*")
		(sheetname "/ADA4087/")
		(sheetfile "ADA4087.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2.05 2.05)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "Net-(J4-In)")
			(pinfunction "In")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at -2.54 -2.54)
			(size 2.25 2.25)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at -2.54 2.54)
			(size 2.25 2.25)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 -2.54)
			(size 2.25 2.25)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 2.54)
			(size 2.25 2.25)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_Coaxial.3dshapes/SMA_Amphenol_132134_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 93.035 131.94 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C4"
			(at 0 -1.43 90)
			(layer "F.SilkS")
		)
		(property "Value" "4.7 uF"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "LT3045_breakout.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "Net-(J10-In)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 162.2 128.3625 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C13"
			(at 0 -1.43 0)
			(layer "F.SilkS")
		)
		(property "Value" "2.7n"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/ADA4087/")
		(sheetfile "ADA4087.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 17 "Net-(J8-In)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 18 "Net-(C13-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Loop_D1.80mm_Drill1.0mm_Beaded"
		(layer "F.Cu")
		(at 120.3 126.99)
		(descr "wire loop with bead as test point, loop diameter 1.8mm, hole diameter 1.0mm")
		(tags "test point wire loop bead")
		(property "Reference" "TP2"
			(at 0.7 2.5 0)
			(layer "F.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -2.8 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "LT3045_breakout.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.7 2.5 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "LDO-5")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/TestPoint.3dshapes/TestPoint_Loop_D1.80mm_Drill1.0mm_Beaded.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Coaxial:SMA_Amphenol_132134_Vertical"
		(layer "F.Cu")
		(at 121.844286 140.07)
		(descr "https://www.amphenolrf.com/library/download/link/link_id/593003/parent/132134/")
		(tags "SMA THT Female Jack Vertical ExtendedLegs")
		(property "Reference" "J6"
			(at 0 -4.75 0)
			(layer "F.SilkS")
		)
		(property "Value" "Ch3 output"
			(at 0.045714 5.39 0)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, LEMO, ...)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*BNC* *SMA* *SMB* *SMC* *Cinch* *LEMO* *UMRF* *MCX* *U.FL*")
		(sheetname "/ADA4087/")
		(sheetfile "ADA4087.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2.05 2.05)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "Net-(J6-In)")
			(pinfunction "In")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at -2.54 -2.54)
			(size 2.25 2.25)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at -2.54 2.54)
			(size 2.25 2.25)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 -2.54)
			(size 2.25 2.25)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 2.54)
			(size 2.25 2.25)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_Coaxial.3dshapes/SMA_Amphenol_132134_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 128.35 103.9375)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C9"
			(at 0 -1.43 0)
			(layer "F.SilkS")
		)
		(property "Value" "2.7n"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/ADA4087/")
		(sheetfile "ADA4087.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 12 "Net-(J4-In)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 11 "Net-(C12-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 112.85 108.9 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R5"
			(at 0 -1.43 90)
			(layer "F.SilkS")
		)
		(property "Value" "453k"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "LT3045_breakout.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "LDO+5")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 26 "Net-(U1-PGFB)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 102.25 141.6)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R9"
			(at 0 -1.43 0)
			(layer "F.SilkS")
		)
		(property "Value" "49.9k"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "LT3045_breakout.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 29 "Net-(U2-PGFB)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 136.85 131.4 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R14"
			(at 0 -1.43 90)
			(layer "F.SilkS")
		)
		(property "Value" "2.2k"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/ADA4087/")
		(sheetfile "ADA4087.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 13 "Net-(C10-Pad2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 22 "Net-(J5-In)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 109.95 137.85 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R8"
			(at 0 -1.43 90)
			(layer "F.SilkS")
		)
		(property "Value" "49.9k"
			(at -2.625 1.48 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "LT3045_breakout.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "Net-(U2-SET)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 162.2 132.675 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R21"
			(at 0 -1.43 0)
			(layer "F.SilkS")
		)
		(property "Value" "52.3"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/ADA4087/")
		(sheetfile "ADA4087.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 18 "Net-(C13-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 162.2 103.9375 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C7"
			(at 0 -1.43 0)
			(layer "F.SilkS")
		)
		(property "Value" "2.7n"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/ADA4087/")
		(sheetfile "ADA4087.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 8 "Net-(J2-In)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 9 "Net-(C7-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 91.575 110.175 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R2"
			(at 0 -1.43 90)
			(layer "F.SilkS")
		)
		(property "Value" "750"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "LT3045_breakout.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 25 "Net-(U1-ILIM)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:TSSOP-14_4.4x5mm_P0.65mm"
		(layer "F.Cu")
		(at 144.5 116.2 -90)
		(descr "TSSOP, 14 Pin (JEDEC MO-153 Var AB-1 https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "TSSOP SO")
		(property "Reference" "U3"
			(at 0 -3.45 90)
			(layer "F.SilkS")
		)
		(property "Value" "ADA4807-4ARUZ"
			(at 0 3.45 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADA4807-1_4807-2_4807-4.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Quad Rail-to-Rail Input/Output Amplifiers, TSSOP-14"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TSSOP*4.4x5mm*P0.65mm*")
		(sheetname "/ADA4087/")
		(sheetfile "ADA4087.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.8625 -1.95 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 8 "Net-(J2-In)")
			(pintype "output")
		)
		(pad "2" smd roundrect
			(at -2.8625 -1.3 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "Net-(U3A--)")
			(pinfunction "-")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -2.8625 -0.65 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "+")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at -2.8625 0 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "LDO+5")
			(pinfunction "V+")
			(pintype "power_in")
		)
		(pad "5" smd roundrect
			(at -2.8625 0.65 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "+")
			(pintype "input")
		)
		(pad "6" smd roundrect
			(at -2.8625 1.3 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 16 "Net-(U3B--)")
			(pinfunction "-")
			(pintype "input")
		)
		(pad "7" smd roundrect
			(at -2.8625 1.95 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 12 "Net-(J4-In)")
			(pintype "output")
		)
		(pad "8" smd roundrect
			(at 2.8625 1.95 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 14 "Net-(J6-In)")
			(pintype "output")
		)
		(pad "9" smd roundrect
			(at 2.8625 1.3 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 15 "Net-(U3C--)")
			(pinfunction "-")
			(pintype "input")
		)
		(pad "10" smd roundrect
			(at 2.8625 0.65 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "+")
			(pintype "input")
		)
		(pad "11" smd roundrect
			(at 2.8625 0 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "LDO-5")
			(pinfunction "V-")
			(pintype "power_in")
		)
		(pad "12" smd roundrect
			(at 2.8625 -0.65 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "+")
			(pintype "input")
		)
		(pad "13" smd roundrect
			(at 2.8625 -1.3 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 19 "Net-(U3D--)")
			(pinfunction "-")
			(pintype "input")
		)
		(pad "14" smd roundrect
			(at 2.8625 -1.95 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 17 "Net-(J8-In)")
			(pintype "output")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_SO.3dshapes/TSSOP-14_4.4x5mm_P0.65mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 113.425 131.7)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C6"
			(at 0 -1.43 0)
			(layer "F.SilkS")
		)
		(property "Value" "10u"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "LT3045_breakout.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "LDO-5")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Coaxial:SMA_Amphenol_132134_Vertical"
		(layer "F.Cu")
		(at 166.89 140.07)
		(descr "https://www.amphenolrf.com/library/download/link/link_id/593003/parent/132134/")
		(tags "SMA THT Female Jack Vertical ExtendedLegs")
		(property "Reference" "J8"
			(at 0 -4.75 0)
			(layer "F.SilkS")
		)
		(property "Value" "Ch4 output"
			(at 0 5 0)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, LEMO, ...)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*BNC* *SMA* *SMB* *SMC* *Cinch* *LEMO* *UMRF* *MCX* *U.FL*")
		(sheetname "/ADA4087/")
		(sheetfile "ADA4087.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2.05 2.05)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "Net-(J8-In)")
			(pinfunction "In")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at -2.54 -2.54)
			(size 2.25 2.25)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at -2.54 2.54)
			(size 2.25 2.25)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 -2.54)
			(size 2.25 2.25)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 2.54)
			(size 2.25 2.25)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_Coaxial.3dshapes/SMA_Amphenol_132134_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Coaxial:SMA_Amphenol_132134_Vertical"
		(layer "F.Cu")
		(at 81.995 104.105)
		(descr "https://www.amphenolrf.com/library/download/link/link_id/593003/parent/132134/")
		(tags "SMA THT Female Jack Vertical ExtendedLegs")
		(property "Reference" "J9"
			(at -2.975 -5.675 0)
			(layer "F.SilkS")
		)
		(property "Value" "DC+5V"
			(at 0 5 0)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, LEMO, ...)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*BNC* *SMA* *SMB* *SMC* *Cinch* *LEMO* *UMRF* *MCX* *U.FL*")
		(sheetname "/")
		(sheetfile "LT3045_breakout.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2.05 2.05)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "Net-(J9-In)")
			(pinfunction "In")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at -2.54 -2.54)
			(size 2.25 2.25)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at -2.54 2.54)
			(size 2.25 2.25)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 -2.54)
			(size 2.25 2.25)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 2.54)
			(size 2.25 2.25)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_Coaxial.3dshapes/SMA_Amphenol_132134_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 113.45 105.2)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C3"
			(at 0 -1.43 0)
			(layer "F.SilkS")
		)
		(property "Value" "10u"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "LT3045_breakout.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "LDO+5")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Coaxial:SMA_Amphenol_132134_Vertical"
		(layer "F.Cu")
		(at 166.89 90.61)
		(descr "https://www.amphenolrf.com/library/download/link/link_id/593003/parent/132134/")
		(tags "SMA THT Female Jack Vertical ExtendedLegs")
		(property "Reference" "J2"
			(at 0 -4.75 0)
			(layer "F.SilkS")
		)
		(property "Value" "Ch1 output"
			(at 0 5 0)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, LEMO, ...)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*BNC* *SMA* *SMB* *SMC* *Cinch* *LEMO* *UMRF* *MCX* *U.FL*")
		(sheetname "/ADA4087/")
		(sheetfile "ADA4087.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2.05 2.05)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "Net-(J2-In)")
			(pinfunction "In")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at -2.54 -2.54)
			(size 2.25 2.25)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at -2.54 2.54)
			(size 2.25 2.25)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 -2.54)
			(size 2.25 2.25)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 2.54)
			(size 2.25 2.25)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_Coaxial.3dshapes/SMA_Amphenol_132134_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 128.35 99.35)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R18"
			(at 0 -1.43 0)
			(layer "F.SilkS")
		)
		(property "Value" "52.3"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/ADA4087/")
		(sheetfile "ADA4087.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 11 "Net-(C12-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 162.2 124.05)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R22"
			(at 0 -1.43 0)
			(layer "F.SilkS")
		)
		(property "Value" "4.42k"
			(at 0.575 1.425 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/ADA4087/")
		(sheetfile "ADA4087.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 19 "Net-(U3D--)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 17 "Net-(J8-In)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 162.2 99.35 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R12"
			(at 0 -1.43 0)
			(layer "F.SilkS")
		)
		(property "Value" "52.3"
			(at 0.125 1.475 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/ADA4087/")
		(sheetfile "ADA4087.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 9 "Net-(C7-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 151.85 124.95 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C14"
			(at 0 -1.43 90)
			(layer "F.SilkS")
		)
		(property "Value" "2.7n"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/ADA4087/")
		(sheetfile "ADA4087.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 19 "Net-(U3D--)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 18 "Net-(C13-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 95.675 104.8 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R1"
			(at 0 -1.43 90)
			(layer "F.SilkS")
		)
		(property "Value" "200 k"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "LT3045_breakout.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "Net-(J9-In)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 24 "Net-(U1-PG)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 128.35 128.3625)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C10"
			(at 0 -1.43 0)
			(layer "F.SilkS")
		)
		(property "Value" "2.7n"
			(at 0.05 1.5 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/ADA4087/")
		(sheetfile "ADA4087.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -0.05 0.025 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 14 "Net-(J6-In)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 13 "Net-(C10-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 113.625 127.75)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R10"
			(at 0 -1.43 0)
			(layer "F.SilkS")
		)
		(property "Value" "453k"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "LT3045_breakout.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "LDO-5")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 29 "Net-(U2-PGFB)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 162.2 108.525)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R13"
			(at 0 -1.43 0)
			(layer "F.SilkS")
		)
		(property "Value" "4.42k"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/ADA4087/")
		(sheetfile "ADA4087.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "Net-(U3A--)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 8 "Net-(J2-In)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 128.35 132.675)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R15"
			(at 0 -1.43 0)
			(layer "F.SilkS")
		)
		(property "Value" "52.3"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/ADA4087/")
		(sheetfile "ADA4087.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 13 "Net-(C10-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 151.85 101.975 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R11"
			(at 0 -1.43 90)
			(layer "F.SilkS")
		)
		(property "Value" "2.2k"
			(at -0.025 1.75 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/ADA4087/")
		(sheetfile "ADA4087.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 9 "Net-(C7-Pad2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 20 "Net-(J1-In)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Coaxial:SMA_Amphenol_132134_Vertical"
		(layer "F.Cu")
		(at 81.995 131.105)
		(descr "https://www.amphenolrf.com/library/download/link/link_id/593003/parent/132134/")
		(tags "SMA THT Female Jack Vertical ExtendedLegs")
		(property "Reference" "J10"
			(at -2.505 -5.152324 0)
			(layer "F.SilkS")
		)
		(property "Value" "DC-5V"
			(at 0 5 0)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, LEMO, ...)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*BNC* *SMA* *SMB* *SMC* *Cinch* *LEMO* *UMRF* *MCX* *U.FL*")
		(sheetname "/")
		(sheetfile "LT3045_breakout.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2.05 2.05)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "Net-(J10-In)")
			(pinfunction "In")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at -2.54 -2.54)
			(size 2.25 2.25)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at -2.54 2.54)
			(size 2.25 2.25)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 -2.54)
			(size 2.25 2.25)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 2.54)
			(size 2.25 2.25)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_Coaxial.3dshapes/SMA_Amphenol_132134_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 136.85 124.95 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C11"
			(at 0 -1.43 90)
			(layer "F.SilkS")
		)
		(property "Value" "2.7n"
			(at 0.34 1.795 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/ADA4087/")
		(sheetfile "ADA4087.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 15 "Net-(U3C--)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 13 "Net-(C10-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:MSOP-12-1EP_3x4.039mm_P0.65mm_EP1.651x2.845mm"
		(layer "F.Cu")
		(at 106.22 132.625)
		(descr "MSOP, 12 Pin (https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/ltc-legacy-msop/05081666_g_mse12.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "MSOP SO")
		(property "Reference" "U2"
			(at 0 -2.97 0)
			(layer "F.SilkS")
		)
		(property "Value" "LT3094xMSE"
			(at 0 2.97 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/LT3094.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "-500mA, Adjustable, Ultralow Noise, Ultrahigh PSRR RF Negative Linear Regulator, MSOP-12"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MSOP*1EP*3x4.039mm*P0.65mm*")
		(sheetname "/")
		(sheetfile "LT3045_breakout.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.415 -0.71)
			(size 0.67 1.15)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at -0.415 0.71)
			(size 0.67 1.15)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.415 -0.71)
			(size 0.67 1.15)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.415 0.71)
			(size 0.67 1.15)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -2.15 -1.625)
			(size 1.45 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "Net-(J10-In)")
			(pinfunction "IN")
			(pintype "power_in")
		)
		(pad "2" smd roundrect
			(at -2.15 -0.975)
			(size 1.45 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "Net-(J10-In)")
			(pinfunction "IN")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at -2.15 -0.325)
			(size 1.45 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 28 "Net-(U2-EN{slash}UV)")
			(pinfunction "EN/UV")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at -2.15 0.325)
			(size 1.45 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 30 "unconnected-(U2-PG-Pad4)")
			(pinfunction "PG")
			(pintype "open_collector+no_connect")
		)
		(pad "5" smd roundrect
			(at -2.15 0.975)
			(size 1.45 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 29 "Net-(U2-PGFB)")
			(pinfunction "PGFB")
			(pintype "input")
		)
		(pad "6" smd roundrect
			(at -2.15 1.625)
			(size 1.45 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 27 "Net-(U2-ILIM)")
			(pinfunction "ILIM")
			(pintype "passive")
		)
		(pad "7" smd roundrect
			(at 2.15 1.625)
			(size 1.45 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 31 "unconnected-(U2-VIOC-Pad7)")
			(pinfunction "VIOC")
			(pintype "passive+no_connect")
		)
		(pad "8" smd roundrect
			(at 2.15 0.975)
			(size 1.45 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "Net-(U2-SET)")
			(pinfunction "SET")
			(pintype "passive")
		)
		(pad "9" smd roundrect
			(at 2.15 0.325)
			(size 1.45 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "10" smd roundrect
			(at 2.15 -0.325)
			(size 1.45 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "LDO-5")
			(pinfunction "OUTS")
			(pintype "input")
		)
		(pad "11" smd roundrect
			(at 2.15 -0.975)
			(size 1.45 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "LDO-5")
			(pinfunction "OUT")
			(pintype "power_out")
		)
		(pad "12" smd roundrect
			(at 2.15 -1.625)
			(size 1.45 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "LDO-5")
			(pinfunction "OUT")
			(pintype "passive")
		)
		(pad "13" smd rect
			(at 0 0)
			(size 1.651 2.845)
			(property pad_prop_heatsink)
			(layers "F.Cu" "F.Mask")
			(net 5 "Net-(J10-In)")
			(pinfunction "IN")
			(pintype "passive")
			(zone_connect 2)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_SO.3dshapes/MSOP-12-1EP_3x4.039mm_P0.65mm_EP1.651x2.845mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 94.6125 110.175 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C2"
			(at 0 -1.43 90)
			(layer "F.SilkS")
		)
		(property "Value" "4.7 uF"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "LT3045_breakout.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "Net-(U1-SET)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Coaxial:SMA_Amphenol_132134_Vertical"
		(layer "F.Cu")
		(at 151.874762 140.07)
		(descr "https://www.amphenolrf.com/library/download/link/link_id/593003/parent/132134/")
		(tags "SMA THT Female Jack Vertical ExtendedLegs")
		(property "Reference" "J7"
			(at 0 -4.75 0)
			(layer "F.SilkS")
		)
		(property "Value" "Ch4 in"
			(at 0 5 0)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, LEMO, ...)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*BNC* *SMA* *SMB* *SMC* *Cinch* *LEMO* *UMRF* *MCX* *U.FL*")
		(sheetname "/ADA4087/")
		(sheetfile "ADA4087.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2.05 2.05)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "Net-(J7-In)")
			(pinfunction "In")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at -2.54 -2.54)
			(size 2.25 2.25)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at -2.54 2.54)
			(size 2.25 2.25)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 -2.54)
			(size 2.25 2.25)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 2.54)
			(size 2.25 2.25)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_Coaxial.3dshapes/SMA_Amphenol_132134_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 114.325 137.8 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C5"
			(at 0 -1.43 90)
			(layer "F.SilkS")
		)
		(property "Value" "4.7 uF"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "LT3045_breakout.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "Net-(U2-SET)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 113.6 112.325)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R4"
			(at 0 -1.43 0)
			(layer "F.SilkS")
		)
		(property "Value" "49.9k"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "LT3045_breakout.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 26 "Net-(U1-PGFB)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 136.85 107.75 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C12"
			(at 0 -1.575 90)
			(layer "F.SilkS")
		)
		(property "Value" "2.7n"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/ADA4087/")
		(sheetfile "ADA4087.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 16 "Net-(U3B--)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 11 "Net-(C12-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 151.85 131.4 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R20"
			(at 0 -1.43 90)
			(layer "F.SilkS")
		)
		(property "Value" "2.2k"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/ADA4087/")
		(sheetfile "ADA4087.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 18 "Net-(C13-Pad2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 23 "Net-(J7-In)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 151.85 107.75 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C8"
			(at 0 -1.43 90)
			(layer "F.SilkS")
		)
		(property "Value" "2.7n"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/ADA4087/")
		(sheetfile "ADA4087.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "Net-(U3A--)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 9 "Net-(C7-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 128.35 124.05 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R16"
			(at 0 -1.43 0)
			(layer "F.SilkS")
		)
		(property "Value" "4.42k"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/ADA4087/")
		(sheetfile "ADA4087.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 15 "Net-(U3C--)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 14 "Net-(J6-In)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Loop_D1.80mm_Drill1.0mm_Beaded"
		(layer "F.Cu")
		(at 115.18 99.08)
		(descr "wire loop with bead as test point, loop diameter 1.8mm, hole diameter 1.0mm")
		(tags "test point wire loop bead")
		(property "Reference" "TP1"
			(at 0.7 2.5 0)
			(layer "F.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -2.8 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "LT3045_breakout.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.7 2.5 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "LDO+5")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/TestPoint.3dshapes/TestPoint_Loop_D1.80mm_Drill1.0mm_Beaded.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Loop_D1.80mm_Drill1.0mm_Beaded"
		(layer "F.Cu")
		(at 82.08 96.88)
		(descr "wire loop with bead as test point, loop diameter 1.8mm, hole diameter 1.0mm")
		(tags "test point wire loop bead")
		(property "Reference" "TP4"
			(at 3.15 1.38 0)
			(layer "F.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -2.8 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "LT3045_breakout.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.7 2.5 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "Net-(J9-In)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/TestPoint.3dshapes/TestPoint_Loop_D1.80mm_Drill1.0mm_Beaded.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 128.35 108.525 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R19"
			(at 0 -1.43 0)
			(layer "F.SilkS")
		)
		(property "Value" "4.42k"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/ADA4087/")
		(sheetfile "ADA4087.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 16 "Net-(U3B--)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 12 "Net-(J4-In)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_rect
		(start 75.375 84.3)
		(end 173.55 147.15)
		(fill no)
		(layer "Edge.Cuts")
	)
	(zone
		(net 2)
		(net_name "GND")
		(layers "F.Cu" "B.Cu" "In1.Cu" "In2.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 77.025 86.1) (xy 76.925 145.2) (xy 172.6 146.375) (xy 172.725 84.85)
			)
		)
	)
	(embedded_fonts no)
)
