(kicad_pcb (version 20171130) (host pcbnew 5.1.9)
  (general
    (thickness 1.6)
    (drawings 17)
    (tracks 70)
    (zones 0)
    (modules 8)
    (nets 13)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.3048)
    (trace_clearance 0.2)
    (zone_clearance 0.254)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (grid_origin 173.81 103.79)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerber"))
  )
  (net 0 "")
  (net 1 +5V)
  (net 2 "Net-(D1-Pad1)")
  (net 3 GND)
  (net 4 /IN-)
  (net 5 /IN+)
  (net 6 "Net-(J1-Pad4)")
  (net 7 VBUS)
  (net 8 /EN)
  (net 9 "Net-(U1-Pad7)")
  (net 10 "Net-(U1-Pad6)")
  (net 11 /OUT+)
  (net 12 /OUT-)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net /EN)
    (add_net /IN+)
    (add_net /IN-)
    (add_net /OUT+)
    (add_net /OUT-)
    (add_net GND)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(U1-Pad6)")
    (add_net "Net-(U1-Pad7)")
    (add_net VBUS)
  )
  (module adafruit:Amphenol-USB-A-UE27ACX4X0X (layer F.Cu) (tedit 5DD9E7F9)
    (at 119.2 112.79 90)
    (fp_text reference J3 (at 0 0.5 90) (layer F.SilkS) hide)
    (fp_text value USB_A (at 0 3 90) (layer F.Fab))
    (fp_text user EDGE (at 0 11 90) (layer Dwgs.User))
    (pad 1 thru_hole circle (at -3.5 -2.71 90) (size 1.3 1.3) (drill 0.92) (layers *.Cu *.Mask)
      (net 7 VBUS))
    (pad 4 thru_hole circle (at 3.5 -2.71 90) (size 1.3 1.3) (drill 0.92) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 3 thru_hole circle (at 1 -2.71 90) (size 1.3 1.3) (drill 0.92) (layers *.Cu *.Mask)
      (net 11 /OUT+))
    (pad 2 thru_hole circle (at -1 -2.72 90) (size 1.3 1.3) (drill 0.92) (layers *.Cu *.Mask)
      (net 12 /OUT-))
    (pad 5 thru_hole circle (at 6.57 0 90) (size 3 3) (drill 2.3) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 5 thru_hole circle (at -6.57 0 90) (size 3 3) (drill 2.3) (layers *.Cu *.Mask)
      (net 3 GND))
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x04_P2.54mm_Horizontal (layer F.Cu) (tedit 5A19A424)
    (at 114.12 105.06 270)
    (descr "Through hole angled socket strip, 1x04, 2.54mm pitch, 8.51mm socket length, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole angled socket strip THT 1x04 2.54mm single row")
    (fp_text reference J2 (at -4.38 -2.77 90) (layer F.SilkS))
    (fp_text value Conn_01x04_Female (at -4.38 10.39 90) (layer F.Fab))
    (fp_text user %R (at -5.775 3.81) (layer F.Fab))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 VBUS))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x04_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module chickadee:chickadee_3mm_fcu (layer F.Cu) (tedit 0)
    (at 110.31 116.59)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value "Chickadee 3mm" (at 0.75 0) (layer F.SilkS) hide)
  )
  (module Package_DFN_QFN:UQFN-10_1.6x2.1mm_P0.5mm (layer F.Cu) (tedit 5B5C1E86)
    (at 110.31 112.54 90)
    (descr "UQFN, 10 Pin (http://ww1.microchip.com/downloads/en/DeviceDoc/00001725D.pdf (Page 12)), generated with kicad-footprint-generator ipc_dfn_qfn_generator.py")
    (tags "UQFN DFN_QFN")
    (attr smd)
    (fp_text reference U1 (at 0 -2.35 90) (layer F.SilkS) hide)
    (fp_text value USB3740B-AI9 (at 0 2.35 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 10 smd roundrect (at -0.5 -1 90) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 /IN+))
    (pad 9 smd roundrect (at 0 -1 90) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 /IN-))
    (pad 8 smd roundrect (at 0.5 -1 90) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 7 smd roundrect (at 0.625 -0.25 90) (size 1.05 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 "Net-(U1-Pad7)"))
    (pad 6 smd roundrect (at 0.625 0.25 90) (size 1.05 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 "Net-(U1-Pad6)"))
    (pad 5 smd roundrect (at 0.5 1 90) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (pad 4 smd roundrect (at 0 1 90) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 3 smd roundrect (at -0.5 1 90) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 /EN))
    (pad 2 smd roundrect (at -0.625 0.25 90) (size 1.05 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 /OUT+))
    (pad 1 smd roundrect (at -0.625 -0.25 90) (size 1.05 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 /OUT-))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/UQFN-10_1.6x2.1mm_P0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_THT:SW_Slide_1P2T_CK_OS102011MS2Q (layer F.Cu) (tedit 5C5044D5)
    (at 108.34 121.79)
    (descr "CuK miniature slide switch, OS series, SPDT, https://www.ckswitches.com/media/1428/os.pdf")
    (tags "switch SPDT")
    (fp_text reference SW1 (at 3.99 -2.99) (layer F.SilkS) hide)
    (fp_text value SW_SPDT (at 2 3) (layer F.Fab))
    (fp_text user %R (at 3.99 -2.99) (layer F.Fab))
    (pad "" thru_hole oval (at 6.1 0) (size 2.2 3.5) (drill 1.5) (layers *.Cu *.Mask))
    (pad "" thru_hole oval (at -2.1 0) (size 2.2 3.5) (drill 1.5) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 4 0) (size 1.5 2.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 2 thru_hole oval (at 2 0) (size 1.5 2.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 /EN))
    (pad 1 thru_hole rect (at 0 0) (size 1.5 2.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Button_Switch_THT.3dshapes/SW_Slide_1P2T_CK_OS102011MS2Q.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 109.34 125.19 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 1k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 /EN))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module adafruit:4UCONN_20329_V2_USB (layer F.Cu) (tedit 5C85D8AC)
    (at 103.6425 113.2515 270)
    (fp_text reference J1 (at -2.778 5.852 90) (layer F.SilkS) hide)
    (fp_text value USB_B_Micro (at -2.778 6.41 90) (layer F.Fab))
    (fp_text user "PCB EDGE" (at 0 4 90) (layer F.Fab))
    (pad "" np_thru_hole circle (at -1.95 0 270) (size 0.7 0.7) (drill 0.7) (layers *.Mask B.Cu))
    (pad "" np_thru_hole circle (at 1.95 0 270) (size 0.7 0.7) (drill 0.7) (layers *.Mask B.Cu))
    (pad 6 thru_hole rect (at 3.6 1.9 90) (size 2.413 2.413) (drill oval 0.8 1.3) (layers *.Cu *.Mask)
      (net 3 GND) (solder_mask_margin 0.0508))
    (pad 6 thru_hole rect (at -3.6 1.9 90) (size 2.413 2.413) (drill oval 0.9 1.3) (layers *.Cu *.Mask)
      (net 3 GND) (solder_mask_margin 0.0508))
    (pad 6 thru_hole circle (at -3.3 -0.9 90) (size 1.143 1.143) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 GND) (solder_mask_margin 0.0508))
    (pad 6 thru_hole circle (at 3.3 -0.9 270) (size 1.143 1.143) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 GND) (solder_mask_margin 0.0508))
    (pad 1 smd rect (at -1.3 -0.775 270) (size 0.4 1.35) (layers F.Cu F.Mask)
      (net 1 +5V) (solder_mask_margin 0.0508))
    (pad 2 smd rect (at -0.65 -0.775 270) (size 0.4 1.35) (layers F.Cu F.Mask)
      (net 4 /IN-) (solder_mask_margin 0.0508))
    (pad 3 smd rect (at 0 -0.775 270) (size 0.4 1.35) (layers F.Cu F.Mask)
      (net 5 /IN+) (solder_mask_margin 0.0508))
    (pad 4 smd rect (at 0.65 -0.775 270) (size 0.4 1.35) (layers F.Cu F.Mask)
      (net 6 "Net-(J1-Pad4)") (solder_mask_margin 0.0508))
    (pad 5 smd rect (at 1.3 -0.775 270) (size 0.4 1.35) (layers F.Cu F.Mask)
      (net 3 GND) (solder_mask_margin 0.0508))
    (pad 6 smd rect (at -0.75 2) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 3 GND) (solder_mask_margin 0.0508))
    (pad 6 smd rect (at 0.75 2) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 3 GND) (solder_mask_margin 0.0508))
  )
  (module LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B4B45C9)
    (at 113.04 125.19)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (attr smd)
    (fp_text reference D1 (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text GND (at 106.5 106.33 90) (layer F.SilkS))
  (gr_text GND (at 114.12 106.33 90) (layer F.SilkS))
  (gr_text VOUT (at 111.58 106.33 90) (layer F.SilkS))
  (gr_text VIN (at 109.04 106.33 90) (layer F.SilkS))
  (gr_line (start 117.93 126.65) (end 103.79 126.65) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 121.74 107.6) (end 121.74 122.84) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 103.79 103.79) (end 117.93 103.79) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 117.93 107.6) (end 121.74 107.6) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 117.93 122.84) (end 117.93 126.65) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_text OUT (at 113.6755 113.6325) (layer F.SilkS))
  (gr_text ckd.tech/usbjoules/v2 (at 111.707 114.6485 -50) (layer B.SilkS))
  (gr_text IN (at 107.31 113.6325) (layer F.SilkS))
  (gr_text ON (at 102.74 124.11) (layer F.SilkS))
  (gr_text OFF (at 118.14 124.11) (layer F.SilkS))
  (gr_line (start 100 122.86) (end 100 107.58) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 103.79 122.86) (end 100 122.86) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 103.79 107.58) (end 103.79 103.79) (angle -90) (layer Edge.Cuts) (width 0.05))
  (zone (net 3) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 121.74 126.65) (xy 100.15 126.65) (xy 100.15 103.79) (xy 121.74 103.79)
      )
    )
  )
)
