<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.1.0">
<drawing>
<board>
<plain>
<text>I2C</text>
<text>I2C</text>
<text>TACOCAT v1</text>
<text>Left</text>
<text>Right</text>
<wire x1="135.52" y1="88.19" x2="135.47" y2="2.77" width="0" layer="20"/>
<wire x1="133.16" y1="0.01" x2="2.41" y2="-0.02" width="0" layer="20"/>
<wire x1="0" y1="3.32" x2="-0.05" y2="88.2" width="0" layer="20"/>
<text>VBAT</text>
<text>13</text>
<text>12</text>
<text>14</text>
<text>17</text>
<text>16</text>
<text>4</text>
<text>0</text>
<text>23</text>
<text>15</text>
<text>VBAT</text>
<text>I2C</text>
<text>+</text>
<text>+</text>
<text>I2C</text>
<text>Audio out</text>
<text>Audio out</text>
<text>Audio in</text>
<text>Audio in</text>
<text>27</text>
<text>26</text>
<text>25</text>
<text>35</text>
<text>34</text>
<text>33</text>
<text>32</text>
<text>39</text>
<text>38</text>
<text>37</text>
<text>36</text>
<text>RST</text>
<text>3.3V</text>
<text>VBAT</text>
<text>VUSB</text>
<text>2</text>
<text>5</text>
<text>18</text>
<text>19</text>
<text>SCL</text>
<text>RX</text>
<text>TX</text>
<text>21</text>
<text>GND</text>
<wire x1="1.7" y1="90.15" x2="1.75" y2="90.15" width="0" layer="20"/>
<text>4</text>
<wire x1="1.75" y1="90.15" x2="133.5" y2="90.15" width="0" layer="20"/>
<wire x1="133.5" y1="90.15" x2="133.51" y2="90.15" width="0" layer="20"/>
<wire x1="-0.05" y1="88.3" x2="-0.05" y2="88.2" width="0" layer="20"/>
<wire x1="-0.05" y1="88.2" x2="-0.05" y2="88.1" width="0" layer="20"/>
<wire x1="2.5" y1="0" x2="-0.05" y2="2.55" width="0" layer="20" curve="-90"/>
<wire x1="-0.05" y1="2.55" x2="-0.05" y2="3.3" width="0" layer="20"/>
<wire x1="133.1" y1="0" x2="135.45" y2="2.35" width="0" layer="20" curve="90"/>
<wire x1="135.45" y1="2.35" x2="135.45" y2="2.8" width="0" layer="20"/>
<wire x1="1.75" y1="90.15" x2="0" y2="88.4" width="0" layer="20" curve="90"/>
<wire x1="0" y1="88.4" x2="0" y2="88.25" width="0" layer="20"/>
<wire x1="133.5" y1="90.15" x2="135.5" y2="88.15" width="0" layer="20" curve="-90"/>
<wire x1="135.5" y1="88.15" x2="135.5" y2="88.1" width="0" layer="20"/>
<text>NOTE: the position of the TRRS ports will hit the alignment pins of the switches. 
There is no way around this since there isn't enough space between the switches; 
the workaround will be to trim off the excess pin stickout out of the PCB.</text>
<text>5</text>
<text>4</text>
<text>3</text>
<text>2</text>
<text>1</text>
<text>~</text>
<text>Tab</text>
<text>Q</text>
<text>W</text>
<text>E</text>
<text>R</text>
<text>T</text>
<text>G</text>
<text>F</text>
<text>D</text>
<text>S</text>
<text>A</text>
<text>Caps</text>
<text>Shift</text>
<text>Z</text>
<text>X</text>
<text>C</text>
<text>V</text>
<text>B</text>
<text>Extra</text>
<text>Space</text>
<text>Back</text>
<text>Extra</text>
<text>Alt</text>
<text>Win</text>
<text>Ctrl</text>
<text>Esc</text>
<text>6</text>
<text>7</text>
<text>8</text>
<text>9</text>
<text>0</text>
<text>+</text>
<text>Extra</text>
<text>[ ]</text>
<text>P</text>
<text>O</text>
<text>I</text>
<text>U</text>
<text>Y</text>
<text>H</text>
<text>J</text>
<text>K</text>
<text>L</text>
<text>;</text>
<text>"</text>
<text>/</text>
<text>Up</text>
<text>&lt;</text>
<text>&gt;</text>
<text>M</text>
<text>N</text>
<text>Extra</text>
<text>Enter</text>
<text>Del</text>
<text>Extra</text>
<text>Right</text>
<text>Down</text>
<text>Left</text>
<text>NOTE: the alignment pins for the springed male I2C connector 
will have to be drilled manually</text>
<text>M3</text>
<text>M3</text>
<text>M3</text>
<text>M3</text>
<text>M3</text>
<text>M3</text>
<text>M3</text>
<text>M3</text>
<text>NOTE: all switches, LEDs, diodes, resistor and capacitors go on one side 
of the board; all remaining IO (USB, pogopins and TRRS) go on the opposite side</text>
</plain>
<libraries>
<library name="adafruit">
<packages>
<package name="DO-1N4148">
</package>
<package name="1X15-CB">
</package>
<package name="0204/7">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0204, grid 7.5 mm</description>
</package>
<package name="C025-025X050">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 mm, outline 2.5 x 5 mm</description>
</package>
<package name="WS2812B-NARROW">
</package>
</packages>
</library>
<library name="cherrymx">
<description>Cherry MX Keyswitch PCB footprints</description>
<packages>
<package name="CHERRY-MX-SYMM-NOSILK">
<description>Cherry MX Keyswitch footprint</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AUDIO_JACK_3.5MM_TRRS_SMD_RA">
<description>&lt;h3&gt;TRRS 3.5MM Right Angle Stereo Jack - SMT&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 4&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”http://cdn.sparkfun.com/datasheets/Prototyping/20153.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;AUDIO_JACK_TRRS&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X20_NOSILK">
<description>&lt;h3&gt;Plated Through Hole -20 Pin No Silk&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:20&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_20&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X05_NO_SILK">
<description>&lt;h3&gt;Plated Through Hole - 5 Pin No Silk Outline&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:5&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_05&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X05_NO_SILK_SMALL">
<description>&lt;h3&gt;Plated Through Hole - 5 Pin No Silk Outline&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:5&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_05&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="USB-B-MICRO-SMD-HOLES">
<description>&lt;h3&gt;USB - microB SMD&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:5&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Micro-USB.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;USB_MICRO-B&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="JST-2-SMD">
<description>&lt;h3&gt;JST-Right Angle Male Header SMT&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch: 2mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”http://www.4uconnector.com/online/object/4udrawing/20404.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;li&gt;JST_2MM_MALE&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="D1" library="adafruit" package="DO-1N4148" value="">
<attribute name="VALUE"/>
</element>
<element name="D10" library="adafruit" package="DO-1N4148" value="">
<attribute name="VALUE"/>
</element>
<element name="D11" library="adafruit" package="DO-1N4148" value="">
<attribute name="VALUE"/>
</element>
<element name="D12" library="adafruit" package="DO-1N4148" value="">
<attribute name="VALUE"/>
</element>
<element name="D13" library="adafruit" package="DO-1N4148" value="">
<attribute name="VALUE"/>
</element>
<element name="D15" library="adafruit" package="DO-1N4148" value="">
<attribute name="VALUE"/>
</element>
<element name="D16" library="adafruit" package="DO-1N4148" value="">
<attribute name="VALUE"/>
</element>
<element name="D17" library="adafruit" package="DO-1N4148" value="">
<attribute name="VALUE"/>
</element>
<element name="D18" library="adafruit" package="DO-1N4148" value="">
<attribute name="VALUE"/>
</element>
<element name="D19" library="adafruit" package="DO-1N4148" value="">
<attribute name="VALUE"/>
</element>
<element name="D2" library="adafruit" package="DO-1N4148" value="">
<attribute name="VALUE"/>
</element>
<element name="D20" library="adafruit" package="DO-1N4148" value="">
<attribute name="VALUE"/>
</element>
<element name="D22" library="adafruit" package="DO-1N4148" value="">
<attribute name="VALUE"/>
</element>
<element name="D23" library="adafruit" package="DO-1N4148" value="">
<attribute name="VALUE"/>
</element>
<element name="D24" library="adafruit" package="DO-1N4148" value="">
<attribute name="VALUE"/>
</element>
<element name="D25" library="adafruit" package="DO-1N4148" value="">
<attribute name="VALUE"/>
</element>
<element name="D26" library="adafruit" package="DO-1N4148" value="">
<attribute name="VALUE"/>
</element>
<element name="D27" library="adafruit" package="DO-1N4148" value="">
<attribute name="VALUE"/>
</element>
<element name="D28" library="adafruit" package="DO-1N4148" value="">
<attribute name="VALUE"/>
</element>
<element name="D29" library="adafruit" package="DO-1N4148" value="">
<attribute name="VALUE"/>
</element>
<element name="D3" library="adafruit" package="DO-1N4148" value="">
<attribute name="VALUE"/>
</element>
<element name="D30" library="adafruit" package="DO-1N4148" value="">
<attribute name="VALUE"/>
</element>
<element name="D31" library="adafruit" package="DO-1N4148" value="">
<attribute name="VALUE"/>
</element>
<element name="D32" library="adafruit" package="DO-1N4148" value="">
<attribute name="VALUE"/>
</element>
<element name="D33" library="adafruit" package="DO-1N4148" value="">
<attribute name="VALUE"/>
</element>
<element name="D34" library="adafruit" package="DO-1N4148" value="">
<attribute name="VALUE"/>
</element>
<element name="D4" library="adafruit" package="DO-1N4148" value="">
<attribute name="VALUE"/>
</element>
<element name="D5" library="adafruit" package="DO-1N4148" value="">
<attribute name="VALUE"/>
</element>
<element name="D6" library="adafruit" package="DO-1N4148" value="">
<attribute name="VALUE"/>
</element>
<element name="D7" library="adafruit" package="DO-1N4148" value="">
<attribute name="VALUE"/>
</element>
<element name="D8" library="adafruit" package="DO-1N4148" value="">
<attribute name="VALUE"/>
</element>
<element name="D9" library="adafruit" package="DO-1N4148" value="">
<attribute name="VALUE"/>
</element>
<element name="U$1" library="cherrymx" package="CHERRY-MX-SYMM-NOSILK" value="CHERRY-MXSYMM-NOSILK"/>
<element name="U$10" library="cherrymx" package="CHERRY-MX-SYMM-NOSILK" value="CHERRY-MXSYMM-NOSILK"/>
<element name="U$11" library="cherrymx" package="CHERRY-MX-SYMM-NOSILK" value="CHERRY-MXSYMM-NOSILK"/>
<element name="U$13" library="cherrymx" package="CHERRY-MX-SYMM-NOSILK" value="CHERRY-MXSYMM-NOSILK"/>
<element name="U$14" library="cherrymx" package="CHERRY-MX-SYMM-NOSILK" value="CHERRY-MXSYMM-NOSILK"/>
<element name="U$15" library="cherrymx" package="CHERRY-MX-SYMM-NOSILK" value="CHERRY-MXSYMM-NOSILK"/>
<element name="U$16" library="cherrymx" package="CHERRY-MX-SYMM-NOSILK" value="CHERRY-MXSYMM-NOSILK"/>
<element name="U$17" library="cherrymx" package="CHERRY-MX-SYMM-NOSILK" value="CHERRY-MXSYMM-NOSILK"/>
<element name="U$18" library="cherrymx" package="CHERRY-MX-SYMM-NOSILK" value="CHERRY-MXSYMM-NOSILK"/>
<element name="U$2" library="cherrymx" package="CHERRY-MX-SYMM-NOSILK" value="CHERRY-MXSYMM-NOSILK"/>
<element name="U$20" library="cherrymx" package="CHERRY-MX-SYMM-NOSILK" value="CHERRY-MXSYMM-NOSILK"/>
<element name="U$21" library="cherrymx" package="CHERRY-MX-SYMM-NOSILK" value="CHERRY-MXSYMM-NOSILK"/>
<element name="U$22" library="cherrymx" package="CHERRY-MX-SYMM-NOSILK" value="CHERRY-MXSYMM-NOSILK"/>
<element name="U$23" library="cherrymx" package="CHERRY-MX-SYMM-NOSILK" value="CHERRY-MXSYMM-NOSILK"/>
<element name="U$24" library="cherrymx" package="CHERRY-MX-SYMM-NOSILK" value="CHERRY-MXSYMM-NOSILK"/>
<element name="U$25" library="cherrymx" package="CHERRY-MX-SYMM-NOSILK" value="CHERRY-MXSYMM-NOSILK"/>
<element name="U$26" library="cherrymx" package="CHERRY-MX-SYMM-NOSILK" value="CHERRY-MXSYMM-NOSILK"/>
<element name="U$28" library="cherrymx" package="CHERRY-MX-SYMM-NOSILK" value="CHERRY-MXSYMM-NOSILK"/>
<element name="U$29" library="cherrymx" package="CHERRY-MX-SYMM-NOSILK" value="CHERRY-MXSYMM-NOSILK"/>
<element name="U$3" library="cherrymx" package="CHERRY-MX-SYMM-NOSILK" value="CHERRY-MXSYMM-NOSILK"/>
<element name="U$30" library="cherrymx" package="CHERRY-MX-SYMM-NOSILK" value="CHERRY-MXSYMM-NOSILK"/>
<element name="U$31" library="cherrymx" package="CHERRY-MX-SYMM-NOSILK" value="CHERRY-MXSYMM-NOSILK"/>
<element name="U$32" library="cherrymx" package="CHERRY-MX-SYMM-NOSILK" value="CHERRY-MXSYMM-NOSILK"/>
<element name="U$33" library="cherrymx" package="CHERRY-MX-SYMM-NOSILK" value="CHERRY-MXSYMM-NOSILK"/>
<element name="U$34" library="cherrymx" package="CHERRY-MX-SYMM-NOSILK" value="CHERRY-MXSYMM-NOSILK"/>
<element name="U$4" library="cherrymx" package="CHERRY-MX-SYMM-NOSILK" value="CHERRY-MXSYMM-NOSILK"/>
<element name="U$5" library="cherrymx" package="CHERRY-MX-SYMM-NOSILK" value="CHERRY-MXSYMM-NOSILK"/>
<element name="U$6" library="cherrymx" package="CHERRY-MX-SYMM-NOSILK" value="CHERRY-MXSYMM-NOSILK"/>
<element name="U$7" library="cherrymx" package="CHERRY-MX-SYMM-NOSILK" value="CHERRY-MXSYMM-NOSILK"/>
<element name="U$8" library="cherrymx" package="CHERRY-MX-SYMM-NOSILK" value="CHERRY-MXSYMM-NOSILK"/>
<element name="U$9" library="cherrymx" package="CHERRY-MX-SYMM-NOSILK" value="CHERRY-MXSYMM-NOSILK"/>
<element name="JP3" library="adafruit" package="1X15-CB" value=""/>
<element name="R1" library="adafruit" package="0204/7" value="330"/>
<element name="J1" library="SparkFun-Connectors" package="1X20_NOSILK" value="">
<attribute name="VALUE"/>
</element>
<element name="U$12" library="cherrymx" package="CHERRY-MX-SYMM-NOSILK" value="CHERRY-MXSYMM-NOSILK"/>
<element name="C11" library="adafruit" package="C025-025X050" value=".1 uF"/>
<element name="LED1" library="adafruit" package="WS2812B-NARROW" value="WS2812B_5050N"/>
<element name="LED2" library="adafruit" package="WS2812B-NARROW" value="WS2812B_5050N"/>
<element name="C23" library="adafruit" package="C025-025X050" value=".1 uF"/>
<element name="LED3" library="adafruit" package="WS2812B-NARROW" value="WS2812B_5050N"/>
<element name="C24" library="adafruit" package="C025-025X050" value=".1 uF"/>
<element name="LED4" library="adafruit" package="WS2812B-NARROW" value="WS2812B_5050N"/>
<element name="C25" library="adafruit" package="C025-025X050" value=".1 uF"/>
<element name="LED5" library="adafruit" package="WS2812B-NARROW" value="WS2812B_5050N"/>
<element name="C26" library="adafruit" package="C025-025X050" value=".1 uF"/>
<element name="LED6" library="adafruit" package="WS2812B-NARROW" value="WS2812B_5050N"/>
<element name="C27" library="adafruit" package="C025-025X050" value=".1 uF"/>
<element name="LED7" library="adafruit" package="WS2812B-NARROW" value="WS2812B_5050N"/>
<element name="C28" library="adafruit" package="C025-025X050" value=".1 uF"/>
<element name="LED8" library="adafruit" package="WS2812B-NARROW" value="WS2812B_5050N"/>
<element name="C12" library="adafruit" package="C025-025X050" value=".1 uF"/>
<element name="LED9" library="adafruit" package="WS2812B-NARROW" value="WS2812B_5050N"/>
<element name="C13" library="adafruit" package="C025-025X050" value=".1 uF"/>
<element name="LED10" library="adafruit" package="WS2812B-NARROW" value="WS2812B_5050N"/>
<element name="C14" library="adafruit" package="C025-025X050" value=".1 uF"/>
<element name="LED11" library="adafruit" package="WS2812B-NARROW" value="WS2812B_5050N"/>
<element name="C15" library="adafruit" package="C025-025X050" value=".1 uF"/>
<element name="LED12" library="adafruit" package="WS2812B-NARROW" value="WS2812B_5050N"/>
<element name="C16" library="adafruit" package="C025-025X050" value=".1 uF"/>
<element name="LED13" library="adafruit" package="WS2812B-NARROW" value="WS2812B_5050N"/>
<element name="C6" library="adafruit" package="C025-025X050" value=".1 uF"/>
<element name="LED14" library="adafruit" package="WS2812B-NARROW" value="WS2812B_5050N"/>
<element name="C7" library="adafruit" package="C025-025X050" value=".1 uF"/>
<element name="LED15" library="adafruit" package="WS2812B-NARROW" value="WS2812B_5050N"/>
<element name="C8" library="adafruit" package="C025-025X050" value=".1 uF"/>
<element name="LED16" library="adafruit" package="WS2812B-NARROW" value="WS2812B_5050N"/>
<element name="C9" library="adafruit" package="C025-025X050" value=".1 uF"/>
<element name="LED17" library="adafruit" package="WS2812B-NARROW" value="WS2812B_5050N"/>
<element name="C10" library="adafruit" package="C025-025X050" value=".1 uF"/>
<element name="LED18" library="adafruit" package="WS2812B-NARROW" value="WS2812B_5050N"/>
<element name="C1" library="adafruit" package="C025-025X050" value=".1 uF"/>
<element name="LED19" library="adafruit" package="WS2812B-NARROW" value="WS2812B_5050N"/>
<element name="C2" library="adafruit" package="C025-025X050" value=".1 uF"/>
<element name="LED20" library="adafruit" package="WS2812B-NARROW" value="WS2812B_5050N"/>
<element name="C3" library="adafruit" package="C025-025X050" value=".1 uF"/>
<element name="LED21" library="adafruit" package="WS2812B-NARROW" value="WS2812B_5050N"/>
<element name="C4" library="adafruit" package="C025-025X050" value=".1 uF"/>
<element name="LED22" library="adafruit" package="WS2812B-NARROW" value="WS2812B_5050N"/>
<element name="C5" library="adafruit" package="C025-025X050" value=".1 uF"/>
<element name="J7" library="SparkFun-Connectors" package="AUDIO_JACK_3.5MM_TRRS_SMD_RA" value="AUDIO_JACK_TRRSSMD_RA">
<attribute name="PROD_ID" value="CONN-10676"/>
<attribute name="SF_ID" value="PRT-12639"/>
</element>
<element name="J8" library="SparkFun-Connectors" package="AUDIO_JACK_3.5MM_TRRS_SMD_RA" value="AUDIO_JACK_TRRSSMD_RA">
<attribute name="PROD_ID" value="CONN-10676"/>
<attribute name="SF_ID" value="PRT-12639"/>
</element>
<element name="J9" library="SparkFun-Connectors" package="AUDIO_JACK_3.5MM_TRRS_SMD_RA" value="AUDIO_JACK_TRRSSMD_RA">
<attribute name="PROD_ID" value="CONN-10676"/>
<attribute name="SF_ID" value="PRT-12639"/>
</element>
<element name="J10" library="SparkFun-Connectors" package="AUDIO_JACK_3.5MM_TRRS_SMD_RA" value="AUDIO_JACK_TRRSSMD_RA">
<attribute name="PROD_ID" value="CONN-10676"/>
<attribute name="SF_ID" value="PRT-12639"/>
</element>
<element name="J12" library="SparkFun-Connectors" package="1X05_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="1X05_NO_SILK_SMALL" value="">
<attribute name="VALUE"/>
</element>
<element name="J3" library="SparkFun-Connectors" package="USB-B-MICRO-SMD-HOLES" value="">
<attribute name="VALUE"/>
</element>
<element name="J5" library="SparkFun-Connectors" package="USB-B-MICRO-SMD-HOLES" value="">
<attribute name="VALUE"/>
</element>
<element name="R2" library="adafruit" package="0204/7" value="330"/>
<element name="LED23" library="adafruit" package="WS2812B-NARROW" value="WS2812B_5050N"/>
<element name="LED24" library="adafruit" package="WS2812B-NARROW" value="WS2812B_5050N"/>
<element name="LED25" library="adafruit" package="WS2812B-NARROW" value="WS2812B_5050N"/>
<element name="LED26" library="adafruit" package="WS2812B-NARROW" value="WS2812B_5050N"/>
<element name="LED27" library="adafruit" package="WS2812B-NARROW" value="WS2812B_5050N"/>
<element name="LED28" library="adafruit" package="WS2812B-NARROW" value="WS2812B_5050N"/>
<element name="LED29" library="adafruit" package="WS2812B-NARROW" value="WS2812B_5050N"/>
<element name="LED30" library="adafruit" package="WS2812B-NARROW" value="WS2812B_5050N"/>
<element name="LED31" library="adafruit" package="WS2812B-NARROW" value="WS2812B_5050N"/>
<element name="LED32" library="adafruit" package="WS2812B-NARROW" value="WS2812B_5050N"/>
<element name="LED33" library="adafruit" package="WS2812B-NARROW" value="WS2812B_5050N"/>
<element name="LED34" library="adafruit" package="WS2812B-NARROW" value="WS2812B_5050N"/>
<element name="LED35" library="adafruit" package="WS2812B-NARROW" value="WS2812B_5050N"/>
<element name="LED36" library="adafruit" package="WS2812B-NARROW" value="WS2812B_5050N"/>
<element name="LED37" library="adafruit" package="WS2812B-NARROW" value="WS2812B_5050N"/>
<element name="LED38" library="adafruit" package="WS2812B-NARROW" value="WS2812B_5050N"/>
<element name="LED39" library="adafruit" package="WS2812B-NARROW" value="WS2812B_5050N"/>
<element name="LED40" library="adafruit" package="WS2812B-NARROW" value="WS2812B_5050N"/>
<element name="LED41" library="adafruit" package="WS2812B-NARROW" value="WS2812B_5050N"/>
<element name="LED42" library="adafruit" package="WS2812B-NARROW" value="WS2812B_5050N"/>
<element name="LED43" library="adafruit" package="WS2812B-NARROW" value="WS2812B_5050N"/>
<element name="LED44" library="adafruit" package="WS2812B-NARROW" value="WS2812B_5050N"/>
<element name="J11" library="SparkFun-Connectors" package="JST-2-SMD" value="">
<attribute name="PROD_ID" value="CONN-11443"/>
<attribute name="SF_ID" value="PRT-08612"/>
<attribute name="VALUE"/>
</element>
<element name="J4" library="SparkFun-Connectors" package="JST-2-SMD" value="">
<attribute name="PROD_ID" value="CONN-11443"/>
<attribute name="SF_ID" value="PRT-08612"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="R4">
<contactref element="U$11" pad="SW1@0"/>
<contactref element="U$11" pad="SW1@1"/>
<contactref element="U$6" pad="SW1@0"/>
<contactref element="U$6" pad="SW1@1"/>
<contactref element="U$7" pad="SW1@0"/>
<contactref element="U$7" pad="SW1@1"/>
<contactref element="U$8" pad="SW1@0"/>
<contactref element="U$8" pad="SW1@1"/>
<contactref element="U$9" pad="SW1@0"/>
<contactref element="U$9" pad="SW1@1"/>
<contactref element="U$10" pad="SW1@0"/>
<contactref element="U$10" pad="SW1@1"/>
<contactref element="JP3" pad="5"/>
</signal>
<signal name="R5">
<contactref element="U$26" pad="SW1@0"/>
<contactref element="U$26" pad="SW1@1"/>
<contactref element="U$5" pad="SW1@0"/>
<contactref element="U$5" pad="SW1@1"/>
<contactref element="U$4" pad="SW1@0"/>
<contactref element="U$4" pad="SW1@1"/>
<contactref element="U$3" pad="SW1@0"/>
<contactref element="U$3" pad="SW1@1"/>
<contactref element="U$2" pad="SW1@0"/>
<contactref element="U$2" pad="SW1@1"/>
<contactref element="U$1" pad="SW1@0"/>
<contactref element="U$1" pad="SW1@1"/>
<contactref element="U$12" pad="SW1@0"/>
<contactref element="U$12" pad="SW1@1"/>
<contactref element="JP3" pad="1"/>
</signal>
<signal name="R3">
<contactref element="U$18" pad="SW1@0"/>
<contactref element="U$18" pad="SW1@1"/>
<contactref element="U$13" pad="SW1@0"/>
<contactref element="U$13" pad="SW1@1"/>
<contactref element="U$14" pad="SW1@0"/>
<contactref element="U$14" pad="SW1@1"/>
<contactref element="U$15" pad="SW1@0"/>
<contactref element="U$15" pad="SW1@1"/>
<contactref element="U$16" pad="SW1@0"/>
<contactref element="U$16" pad="SW1@1"/>
<contactref element="U$17" pad="SW1@0"/>
<contactref element="U$17" pad="SW1@1"/>
<contactref element="JP3" pad="8"/>
</signal>
<signal name="R1">
<contactref element="U$34" pad="SW1@0"/>
<contactref element="U$34" pad="SW1@1"/>
<contactref element="U$29" pad="SW1@0"/>
<contactref element="U$29" pad="SW1@1"/>
<contactref element="U$30" pad="SW1@0"/>
<contactref element="U$30" pad="SW1@1"/>
<contactref element="U$31" pad="SW1@0"/>
<contactref element="U$31" pad="SW1@1"/>
<contactref element="U$32" pad="SW1@0"/>
<contactref element="U$32" pad="SW1@1"/>
<contactref element="U$33" pad="SW1@0"/>
<contactref element="U$33" pad="SW1@1"/>
<contactref element="JP3" pad="10"/>
</signal>
<signal name="R2">
<contactref element="U$28" pad="SW1@0"/>
<contactref element="U$28" pad="SW1@1"/>
<contactref element="U$20" pad="SW1@0"/>
<contactref element="U$20" pad="SW1@1"/>
<contactref element="U$21" pad="SW1@0"/>
<contactref element="U$21" pad="SW1@1"/>
<contactref element="U$22" pad="SW1@0"/>
<contactref element="U$22" pad="SW1@1"/>
<contactref element="U$23" pad="SW1@0"/>
<contactref element="U$23" pad="SW1@1"/>
<contactref element="U$24" pad="SW1@0"/>
<contactref element="U$24" pad="SW1@1"/>
<contactref element="U$25" pad="SW1@0"/>
<contactref element="U$25" pad="SW1@1"/>
<contactref element="JP3" pad="9"/>
</signal>
<signal name="GND">
<contactref element="JP3" pad="15"/>
<contactref element="J1" pad="17"/>
<contactref element="J1" pad="20"/>
<contactref element="LED1" pad="3-GND"/>
<contactref element="C11" pad="2"/>
<contactref element="LED2" pad="3-GND"/>
<contactref element="C23" pad="2"/>
<contactref element="LED3" pad="3-GND"/>
<contactref element="C24" pad="2"/>
<contactref element="LED4" pad="3-GND"/>
<contactref element="C25" pad="2"/>
<contactref element="LED5" pad="3-GND"/>
<contactref element="C26" pad="2"/>
<contactref element="LED6" pad="3-GND"/>
<contactref element="C27" pad="2"/>
<contactref element="LED7" pad="3-GND"/>
<contactref element="C28" pad="2"/>
<contactref element="LED8" pad="3-GND"/>
<contactref element="LED9" pad="3-GND"/>
<contactref element="LED10" pad="3-GND"/>
<contactref element="LED11" pad="3-GND"/>
<contactref element="LED12" pad="3-GND"/>
<contactref element="C12" pad="2"/>
<contactref element="C13" pad="2"/>
<contactref element="C14" pad="2"/>
<contactref element="C15" pad="2"/>
<contactref element="C16" pad="2"/>
<contactref element="LED13" pad="3-GND"/>
<contactref element="LED14" pad="3-GND"/>
<contactref element="LED15" pad="3-GND"/>
<contactref element="LED16" pad="3-GND"/>
<contactref element="LED17" pad="3-GND"/>
<contactref element="C6" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="C9" pad="2"/>
<contactref element="C10" pad="2"/>
<contactref element="LED18" pad="3-GND"/>
<contactref element="LED19" pad="3-GND"/>
<contactref element="LED20" pad="3-GND"/>
<contactref element="LED21" pad="3-GND"/>
<contactref element="LED22" pad="3-GND"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="J12" pad="1"/>
<contactref element="J2" pad="1"/>
<contactref element="LED23" pad="3-GND"/>
<contactref element="LED24" pad="3-GND"/>
<contactref element="LED25" pad="3-GND"/>
<contactref element="LED26" pad="3-GND"/>
<contactref element="LED27" pad="3-GND"/>
<contactref element="LED28" pad="3-GND"/>
<contactref element="LED29" pad="3-GND"/>
<contactref element="LED30" pad="3-GND"/>
<contactref element="LED31" pad="3-GND"/>
<contactref element="LED32" pad="3-GND"/>
<contactref element="LED33" pad="3-GND"/>
<contactref element="LED34" pad="3-GND"/>
<contactref element="LED35" pad="3-GND"/>
<contactref element="LED36" pad="3-GND"/>
<contactref element="LED37" pad="3-GND"/>
<contactref element="LED38" pad="3-GND"/>
<contactref element="LED39" pad="3-GND"/>
<contactref element="LED40" pad="3-GND"/>
<contactref element="LED41" pad="3-GND"/>
<contactref element="LED42" pad="3-GND"/>
<contactref element="LED43" pad="3-GND"/>
<contactref element="LED44" pad="3-GND"/>
<contactref element="J11" pad="1"/>
<contactref element="J4" pad="1"/>
<contactref element="J3" pad="GND"/>
<contactref element="J5" pad="GND"/>
</signal>
<signal name="N$1">
<contactref element="U$1" pad="SW2@1"/>
<contactref element="U$1" pad="SW2@0"/>
<contactref element="D1" pad="A"/>
</signal>
<signal name="C1">
<contactref element="D1" pad="C"/>
<contactref element="D29" pad="C"/>
<contactref element="D22" pad="C"/>
<contactref element="D15" pad="C"/>
<contactref element="D8" pad="C"/>
<contactref element="J1" pad="13"/>
</signal>
<signal name="N$3">
<contactref element="U$6" pad="SW2@1"/>
<contactref element="U$6" pad="SW2@0"/>
<contactref element="D8" pad="A"/>
</signal>
<signal name="N$4">
<contactref element="U$13" pad="SW2@1"/>
<contactref element="U$13" pad="SW2@0"/>
<contactref element="D15" pad="A"/>
</signal>
<signal name="N$5">
<contactref element="U$20" pad="SW2@1"/>
<contactref element="U$20" pad="SW2@0"/>
<contactref element="D22" pad="A"/>
</signal>
<signal name="N$6">
<contactref element="U$29" pad="SW2@1"/>
<contactref element="U$29" pad="SW2@0"/>
<contactref element="D29" pad="A"/>
</signal>
<signal name="N$8">
<contactref element="U$2" pad="SW2@1"/>
<contactref element="U$2" pad="SW2@0"/>
<contactref element="D2" pad="A"/>
</signal>
<signal name="N$9">
<contactref element="U$7" pad="SW2@1"/>
<contactref element="U$7" pad="SW2@0"/>
<contactref element="D9" pad="A"/>
</signal>
<signal name="N$10">
<contactref element="U$14" pad="SW2@1"/>
<contactref element="U$14" pad="SW2@0"/>
<contactref element="D16" pad="A"/>
</signal>
<signal name="N$11">
<contactref element="U$30" pad="SW2@1"/>
<contactref element="U$30" pad="SW2@0"/>
<contactref element="D30" pad="A"/>
</signal>
<signal name="N$12">
<contactref element="U$31" pad="SW2@1"/>
<contactref element="U$31" pad="SW2@0"/>
<contactref element="D31" pad="A"/>
</signal>
<signal name="N$13">
<contactref element="U$22" pad="SW2@1"/>
<contactref element="U$22" pad="SW2@0"/>
<contactref element="D24" pad="A"/>
</signal>
<signal name="N$14">
<contactref element="U$15" pad="SW2@1"/>
<contactref element="U$15" pad="SW2@0"/>
<contactref element="D17" pad="A"/>
</signal>
<signal name="N$15">
<contactref element="U$8" pad="SW2@1"/>
<contactref element="U$8" pad="SW2@0"/>
<contactref element="D10" pad="A"/>
</signal>
<signal name="N$16">
<contactref element="U$3" pad="SW2@1"/>
<contactref element="U$3" pad="SW2@0"/>
<contactref element="D3" pad="A"/>
</signal>
<signal name="N$17">
<contactref element="U$4" pad="SW2@1"/>
<contactref element="U$4" pad="SW2@0"/>
<contactref element="D4" pad="A"/>
</signal>
<signal name="N$18">
<contactref element="U$9" pad="SW2@1"/>
<contactref element="U$9" pad="SW2@0"/>
<contactref element="D11" pad="A"/>
</signal>
<signal name="N$19">
<contactref element="U$16" pad="SW2@1"/>
<contactref element="U$16" pad="SW2@0"/>
<contactref element="D18" pad="A"/>
</signal>
<signal name="N$20">
<contactref element="U$23" pad="SW2@1"/>
<contactref element="U$23" pad="SW2@0"/>
<contactref element="D25" pad="A"/>
</signal>
<signal name="N$21">
<contactref element="U$32" pad="SW2@1"/>
<contactref element="U$32" pad="SW2@0"/>
<contactref element="D32" pad="A"/>
</signal>
<signal name="N$22">
<contactref element="U$33" pad="SW2@1"/>
<contactref element="U$33" pad="SW2@0"/>
<contactref element="D33" pad="A"/>
</signal>
<signal name="N$23">
<contactref element="U$24" pad="SW2@1"/>
<contactref element="U$24" pad="SW2@0"/>
<contactref element="D26" pad="A"/>
</signal>
<signal name="N$24">
<contactref element="U$17" pad="SW2@1"/>
<contactref element="U$17" pad="SW2@0"/>
<contactref element="D19" pad="A"/>
</signal>
<signal name="N$25">
<contactref element="U$10" pad="SW2@1"/>
<contactref element="U$10" pad="SW2@0"/>
<contactref element="D12" pad="A"/>
</signal>
<signal name="N$26">
<contactref element="U$5" pad="SW2@1"/>
<contactref element="U$5" pad="SW2@0"/>
<contactref element="D5" pad="A"/>
</signal>
<signal name="N$27">
<contactref element="U$26" pad="SW2@1"/>
<contactref element="U$26" pad="SW2@0"/>
<contactref element="D6" pad="A"/>
</signal>
<signal name="N$28">
<contactref element="U$11" pad="SW2@1"/>
<contactref element="U$11" pad="SW2@0"/>
<contactref element="D13" pad="A"/>
</signal>
<signal name="N$29">
<contactref element="D20" pad="A"/>
<contactref element="U$18" pad="SW2@1"/>
<contactref element="U$18" pad="SW2@0"/>
</signal>
<signal name="N$30">
<contactref element="U$25" pad="SW2@1"/>
<contactref element="U$25" pad="SW2@0"/>
<contactref element="D27" pad="A"/>
</signal>
<signal name="N$31">
<contactref element="U$34" pad="SW2@1"/>
<contactref element="U$34" pad="SW2@0"/>
<contactref element="D34" pad="A"/>
</signal>
<signal name="C2">
<contactref element="D2" pad="C"/>
<contactref element="D9" pad="C"/>
<contactref element="D23" pad="C"/>
<contactref element="D16" pad="C"/>
<contactref element="D30" pad="C"/>
<contactref element="J1" pad="6"/>
</signal>
<signal name="C3">
<contactref element="D3" pad="C"/>
<contactref element="D24" pad="C"/>
<contactref element="D17" pad="C"/>
<contactref element="D10" pad="C"/>
<contactref element="D31" pad="C"/>
<contactref element="J1" pad="9"/>
</signal>
<signal name="C4">
<contactref element="D4" pad="C"/>
<contactref element="D32" pad="C"/>
<contactref element="D25" pad="C"/>
<contactref element="D18" pad="C"/>
<contactref element="D11" pad="C"/>
<contactref element="J1" pad="10"/>
</signal>
<signal name="C5">
<contactref element="D5" pad="C"/>
<contactref element="D19" pad="C"/>
<contactref element="D26" pad="C"/>
<contactref element="D33" pad="C"/>
<contactref element="D12" pad="C"/>
<contactref element="J1" pad="11"/>
</signal>
<signal name="C6">
<contactref element="D6" pad="C"/>
<contactref element="D34" pad="C"/>
<contactref element="D27" pad="C"/>
<contactref element="D20" pad="C"/>
<contactref element="D13" pad="C"/>
<contactref element="J1" pad="12"/>
</signal>
<signal name="N$38">
<contactref element="U$21" pad="SW2@1"/>
<contactref element="U$21" pad="SW2@0"/>
<contactref element="D23" pad="A"/>
</signal>
<signal name="N$2">
<contactref element="U$28" pad="SW2@1"/>
<contactref element="U$28" pad="SW2@0"/>
<contactref element="D28" pad="A"/>
</signal>
<signal name="N$7">
<contactref element="D7" pad="A"/>
<contactref element="U$12" pad="SW2@0"/>
<contactref element="U$12" pad="SW2@1"/>
</signal>
<signal name="C7">
<contactref element="D7" pad="C"/>
<contactref element="D28" pad="C"/>
<contactref element="J1" pad="5"/>
</signal>
<signal name="+3V3">
<contactref element="J1" pad="16"/>
</signal>
<signal name="SDA">
<contactref element="JP3" pad="14"/>
<contactref element="J12" pad="5"/>
<contactref element="J2" pad="5"/>
<contactref element="J3" pad="D-"/>
<contactref element="J5" pad="D-"/>
</signal>
<signal name="TX">
<contactref element="JP3" pad="13"/>
</signal>
<signal name="RX">
<contactref element="JP3" pad="12"/>
</signal>
<signal name="0">
<contactref element="JP3" pad="4"/>
</signal>
<signal name="17">
<contactref element="JP3" pad="2"/>
</signal>
<signal name="SCL">
<contactref element="JP3" pad="11"/>
<contactref element="J12" pad="4"/>
<contactref element="J2" pad="4"/>
<contactref element="J3" pad="D+"/>
<contactref element="J5" pad="D+"/>
</signal>
<signal name="4">
<contactref element="JP3" pad="3"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="VBAT">
<contactref element="J1" pad="18"/>
<contactref element="LED1" pad="1-VDD"/>
<contactref element="C11" pad="1"/>
<contactref element="C23" pad="1"/>
<contactref element="LED2" pad="1-VDD"/>
<contactref element="C24" pad="1"/>
<contactref element="LED3" pad="1-VDD"/>
<contactref element="C25" pad="1"/>
<contactref element="LED4" pad="1-VDD"/>
<contactref element="C26" pad="1"/>
<contactref element="LED5" pad="1-VDD"/>
<contactref element="C27" pad="1"/>
<contactref element="LED6" pad="1-VDD"/>
<contactref element="C28" pad="1"/>
<contactref element="LED7" pad="1-VDD"/>
<contactref element="C12" pad="1"/>
<contactref element="LED8" pad="1-VDD"/>
<contactref element="C13" pad="1"/>
<contactref element="LED9" pad="1-VDD"/>
<contactref element="C14" pad="1"/>
<contactref element="LED10" pad="1-VDD"/>
<contactref element="C15" pad="1"/>
<contactref element="LED11" pad="1-VDD"/>
<contactref element="C16" pad="1"/>
<contactref element="LED12" pad="1-VDD"/>
<contactref element="C6" pad="1"/>
<contactref element="LED13" pad="1-VDD"/>
<contactref element="C7" pad="1"/>
<contactref element="LED14" pad="1-VDD"/>
<contactref element="C8" pad="1"/>
<contactref element="LED15" pad="1-VDD"/>
<contactref element="C9" pad="1"/>
<contactref element="LED16" pad="1-VDD"/>
<contactref element="C10" pad="1"/>
<contactref element="LED17" pad="1-VDD"/>
<contactref element="C1" pad="1"/>
<contactref element="LED18" pad="1-VDD"/>
<contactref element="C2" pad="1"/>
<contactref element="LED19" pad="1-VDD"/>
<contactref element="C3" pad="1"/>
<contactref element="LED20" pad="1-VDD"/>
<contactref element="C4" pad="1"/>
<contactref element="LED21" pad="1-VDD"/>
<contactref element="C5" pad="1"/>
<contactref element="LED22" pad="1-VDD"/>
<contactref element="LED23" pad="1-VDD"/>
<contactref element="LED24" pad="1-VDD"/>
<contactref element="LED25" pad="1-VDD"/>
<contactref element="LED26" pad="1-VDD"/>
<contactref element="LED27" pad="1-VDD"/>
<contactref element="LED28" pad="1-VDD"/>
<contactref element="LED29" pad="1-VDD"/>
<contactref element="LED30" pad="1-VDD"/>
<contactref element="LED31" pad="1-VDD"/>
<contactref element="LED32" pad="1-VDD"/>
<contactref element="LED33" pad="1-VDD"/>
<contactref element="LED34" pad="1-VDD"/>
<contactref element="LED35" pad="1-VDD"/>
<contactref element="LED36" pad="1-VDD"/>
<contactref element="LED37" pad="1-VDD"/>
<contactref element="LED38" pad="1-VDD"/>
<contactref element="LED39" pad="1-VDD"/>
<contactref element="LED40" pad="1-VDD"/>
<contactref element="LED41" pad="1-VDD"/>
<contactref element="LED42" pad="1-VDD"/>
<contactref element="LED43" pad="1-VDD"/>
<contactref element="LED44" pad="1-VDD"/>
<contactref element="J11" pad="2"/>
<contactref element="J4" pad="2"/>
<contactref element="J2" pad="2"/>
<contactref element="J12" pad="2"/>
<contactref element="J3" pad="ID"/>
<contactref element="J5" pad="ID"/>
</signal>
<signal name="RST">
<contactref element="J1" pad="15"/>
</signal>
<signal name="13">
<contactref element="J1" pad="14"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="VUSB">
<contactref element="J1" pad="19"/>
<contactref element="J12" pad="3"/>
<contactref element="J2" pad="3"/>
<contactref element="J3" pad="VBUS"/>
<contactref element="J5" pad="VBUS"/>
</signal>
<signal name="N$54">
<contactref element="LED8" pad="4-DIN"/>
<contactref element="LED17" pad="2-DOUT"/>
</signal>
<signal name="N$58">
<contactref element="LED2" pad="4-DIN"/>
<contactref element="LED12" pad="2-DOUT"/>
</signal>
<signal name="N$48">
<contactref element="R1" pad="2"/>
<contactref element="LED1" pad="4-DIN"/>
</signal>
<signal name="N$53">
<contactref element="LED2" pad="2-DOUT"/>
<contactref element="LED3" pad="4-DIN"/>
</signal>
<signal name="N$55">
<contactref element="LED4" pad="4-DIN"/>
<contactref element="LED3" pad="2-DOUT"/>
</signal>
<signal name="N$56">
<contactref element="LED4" pad="2-DOUT"/>
<contactref element="LED5" pad="4-DIN"/>
</signal>
<signal name="N$57">
<contactref element="LED5" pad="2-DOUT"/>
<contactref element="LED6" pad="4-DIN"/>
</signal>
<signal name="N$59">
<contactref element="LED6" pad="2-DOUT"/>
<contactref element="LED7" pad="4-DIN"/>
</signal>
<signal name="N$50">
<contactref element="LED9" pad="4-DIN"/>
<contactref element="LED8" pad="2-DOUT"/>
</signal>
<signal name="N$51">
<contactref element="LED9" pad="2-DOUT"/>
<contactref element="LED10" pad="4-DIN"/>
</signal>
<signal name="N$52">
<contactref element="LED10" pad="2-DOUT"/>
<contactref element="LED11" pad="4-DIN"/>
</signal>
<signal name="N$60">
<contactref element="LED11" pad="2-DOUT"/>
<contactref element="LED12" pad="4-DIN"/>
</signal>
<signal name="N$37">
<contactref element="LED13" pad="4-DIN"/>
<contactref element="LED22" pad="2-DOUT"/>
</signal>
<signal name="N$40">
<contactref element="LED14" pad="4-DIN"/>
<contactref element="LED13" pad="2-DOUT"/>
</signal>
<signal name="N$41">
<contactref element="LED14" pad="2-DOUT"/>
<contactref element="LED15" pad="4-DIN"/>
</signal>
<signal name="N$49">
<contactref element="LED15" pad="2-DOUT"/>
<contactref element="LED16" pad="4-DIN"/>
</signal>
<signal name="N$61">
<contactref element="LED16" pad="2-DOUT"/>
<contactref element="LED17" pad="4-DIN"/>
</signal>
<signal name="N$33">
<contactref element="LED18" pad="4-DIN"/>
<contactref element="LED1" pad="2-DOUT"/>
</signal>
<signal name="N$34">
<contactref element="LED19" pad="4-DIN"/>
<contactref element="LED18" pad="2-DOUT"/>
</signal>
<signal name="N$35">
<contactref element="LED19" pad="2-DOUT"/>
<contactref element="LED20" pad="4-DIN"/>
</signal>
<signal name="N$39">
<contactref element="LED20" pad="2-DOUT"/>
<contactref element="LED21" pad="4-DIN"/>
</signal>
<signal name="N$42">
<contactref element="LED21" pad="2-DOUT"/>
<contactref element="LED22" pad="4-DIN"/>
</signal>
<signal name="N$36">
<contactref element="J7" pad="RING1"/>
<contactref element="J8" pad="RING1"/>
<contactref element="J9" pad="RING1"/>
<contactref element="J10" pad="RING1"/>
</signal>
<signal name="N$43">
<contactref element="J7" pad="TIP"/>
<contactref element="J8" pad="TIP"/>
<contactref element="J9" pad="TIP"/>
<contactref element="J10" pad="TIP"/>
</signal>
<signal name="N$44">
<contactref element="J7" pad="RING2"/>
<contactref element="J8" pad="RING2"/>
<contactref element="J9" pad="RING2"/>
<contactref element="J10" pad="RING2"/>
</signal>
<signal name="6">
<contactref element="JP3" pad="6"/>
</signal>
<signal name="7">
<contactref element="JP3" pad="7"/>
</signal>
<signal name="N$32">
</signal>
<signal name="N$45">
<contactref element="J7" pad="EARTH"/>
<contactref element="J8" pad="EARTH"/>
<contactref element="J9" pad="EARTH"/>
<contactref element="J10" pad="EARTH"/>
</signal>
<signal name="39">
<contactref element="J1" pad="4"/>
</signal>
<signal name="38">
<contactref element="J1" pad="3"/>
</signal>
<signal name="37">
<contactref element="J1" pad="2"/>
</signal>
<signal name="36">
<contactref element="J1" pad="1"/>
</signal>
<signal name="N$46">
<contactref element="LED30" pad="4-DIN"/>
<contactref element="LED39" pad="2-DOUT"/>
</signal>
<signal name="N$47">
<contactref element="LED24" pad="4-DIN"/>
<contactref element="LED34" pad="2-DOUT"/>
</signal>
<signal name="N$62">
<contactref element="R2" pad="2"/>
<contactref element="LED23" pad="4-DIN"/>
</signal>
<signal name="N$63">
<contactref element="LED24" pad="2-DOUT"/>
<contactref element="LED25" pad="4-DIN"/>
</signal>
<signal name="N$64">
<contactref element="LED26" pad="4-DIN"/>
<contactref element="LED25" pad="2-DOUT"/>
</signal>
<signal name="N$65">
<contactref element="LED26" pad="2-DOUT"/>
<contactref element="LED27" pad="4-DIN"/>
</signal>
<signal name="N$66">
<contactref element="LED27" pad="2-DOUT"/>
<contactref element="LED28" pad="4-DIN"/>
</signal>
<signal name="N$67">
<contactref element="LED28" pad="2-DOUT"/>
<contactref element="LED29" pad="4-DIN"/>
</signal>
<signal name="N$68">
<contactref element="LED31" pad="4-DIN"/>
<contactref element="LED30" pad="2-DOUT"/>
</signal>
<signal name="N$69">
<contactref element="LED31" pad="2-DOUT"/>
<contactref element="LED32" pad="4-DIN"/>
</signal>
<signal name="N$70">
<contactref element="LED32" pad="2-DOUT"/>
<contactref element="LED33" pad="4-DIN"/>
</signal>
<signal name="N$71">
<contactref element="LED33" pad="2-DOUT"/>
<contactref element="LED34" pad="4-DIN"/>
</signal>
<signal name="N$72">
<contactref element="LED35" pad="4-DIN"/>
<contactref element="LED44" pad="2-DOUT"/>
</signal>
<signal name="N$73">
<contactref element="LED36" pad="4-DIN"/>
<contactref element="LED35" pad="2-DOUT"/>
</signal>
<signal name="N$74">
<contactref element="LED36" pad="2-DOUT"/>
<contactref element="LED37" pad="4-DIN"/>
</signal>
<signal name="N$75">
<contactref element="LED37" pad="2-DOUT"/>
<contactref element="LED38" pad="4-DIN"/>
</signal>
<signal name="N$76">
<contactref element="LED38" pad="2-DOUT"/>
<contactref element="LED39" pad="4-DIN"/>
</signal>
<signal name="N$77">
<contactref element="LED40" pad="4-DIN"/>
<contactref element="LED23" pad="2-DOUT"/>
</signal>
<signal name="N$78">
<contactref element="LED41" pad="4-DIN"/>
<contactref element="LED40" pad="2-DOUT"/>
</signal>
<signal name="N$79">
<contactref element="LED41" pad="2-DOUT"/>
<contactref element="LED42" pad="4-DIN"/>
</signal>
<signal name="N$80">
<contactref element="LED42" pad="2-DOUT"/>
<contactref element="LED43" pad="4-DIN"/>
</signal>
<signal name="N$81">
<contactref element="LED43" pad="2-DOUT"/>
<contactref element="LED44" pad="4-DIN"/>
</signal>
<signal name="34">
<contactref element="J1" pad="7"/>
</signal>
<signal name="35">
<contactref element="J1" pad="8"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
