(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 18)
    (no_connects 0)
    (area 118.515001 96.36 149.300001 112.744999)
    (thickness 1.6)
    (drawings 11)
    (tracks 38)
    (zones 0)
    (modules 7)
    (nets 6)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.5)
    (user_trace_width 0.5)
    (user_trace_width 0.75)
    (user_trace_width 1)
    (trace_clearance 0.2)
    (zone_clearance 0.3)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +5V)
  (net 2 GND)
  (net 3 +3V3)
  (net 4 "Net-(D1-Pad1)")
  (net 5 "Net-(D1-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.2)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +5V)
    (add_net GND)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
  )
  (module Connectors:USB_Micro-B_10103594-0001LF (layer F.Cu) (tedit 5AC0312D)
    (at 133.35 106.045 270)
    (descr "Micro USB Type B 10103594-0001LF")
    (tags "USB USB_B USB_micro USB_OTG")
    (attr smd)
    (fp_text reference J1 (at 0 0 360) (layer F.SilkS))
    (fp_text value USB_OTG (at 0 3.285 270) (layer F.Fab))
    (pad 1 smd rect (at -1.3 -1.5) (size 1.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D1-Pad2)"))
    (pad 2 smd rect (at -0.65 -1.5) (size 1.65 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at 0 -1.5) (size 1.65 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at 0.65 -1.5) (size 1.65 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 1.3 -1.5) (size 1.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 thru_hole oval (at -2.42 -1.62) (size 1.5 1.1) (drill 1.05) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 6 thru_hole oval (at 2.42 -1.62) (size 1.5 1.1) (drill 1.05) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 6 thru_hole oval (at -2.73 1.38) (size 1.7 1.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 6 thru_hole oval (at 2.73 1.38) (size 1.7 1.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 6 smd rect (at -0.96 1.62) (size 2.5 1.43) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at 0.96 1.62) (size 2.5 1.43) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module Diodes_SMD:D_SOD-323_HandSoldering (layer F.Cu) (tedit 58641869)
    (at 138.43 106.045 90)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D1 (at 0 0 180) (layer F.SilkS))
    (fp_text value D_Schottky (at 0.1 1.9 90) (layer F.Fab))
    (fp_text user %R (at -1.885 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 1.25 0 90) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_2010_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 141.605 106.07 270)
    (descr "Resistor SMD 2010, hand soldering")
    (tags "resistor 2010")
    (attr smd)
    (fp_text reference F1 (at 0 0 360) (layer F.SilkS))
    (fp_text value Polyfuse (at 0 -1.905 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -3.15 0 270) (size 2.4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 3.15 0 270) (size 2.4 2.5) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_2010.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 145.491681 108.585 180)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J3 (at 0.076681 -2.54 360) (layer F.SilkS))
    (fp_text value Conn_01x03 (at -1.905 2.54 270) (layer F.Fab))
    (fp_text user %R (at 0 2.54 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 142.24 103.505 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference C1 (at 0 0 540) (layer B.SilkS))
    (fp_text value 1u (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 142.24 108.585 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference C2 (at 0 0 360) (layer B.SilkS))
    (fp_text value 1u (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-5_HandSoldering (layer B.Cu) (tedit 58CE4E7E)
    (at 138.43 106.045 270)
    (descr "5-pin SOT23 package")
    (tags "SOT-23-5 hand-soldering")
    (attr smd)
    (fp_text reference U1 (at 0.635 0 270) (layer B.SilkS))
    (fp_text value MIC5504-3.3YM5 (at 0 -2.9 270) (layer B.Fab))
    (fp_text user %R (at 0 0 540) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0.95 270) (size 1.56 0.65) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at -1.35 0 270) (size 1.56 0.65) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -1.35 -0.95 270) (size 1.56 0.65) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 4 smd rect (at 1.35 -0.95 270) (size 1.56 0.65) (layers B.Cu B.Paste B.Mask))
    (pad 5 smd rect (at 1.35 0.95 270) (size 1.56 0.65) (layers B.Cu B.Paste B.Mask)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes\SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_arc (start 132.715 102.87) (end 130.175 102.87) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 132.715 109.22) (end 132.715 111.76) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 146.685 109.22) (end 149.225 109.22) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 146.685 102.87) (end 146.685 100.33) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text GND (at 147.955 106.045 90) (layer F.SilkS))
  (gr_text 5V (at 147.955 102.87 90) (layer F.SilkS))
  (gr_text 3V3 (at 147.955 109.22 90) (layer F.SilkS))
  (gr_line (start 130.175 109.22) (end 130.175 102.87) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 146.685 111.76) (end 132.715 111.76) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 149.225 102.87) (end 149.225 109.22) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 132.715 100.33) (end 146.685 100.33) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.3)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 130.81 100.33) (xy 149.225 100.33) (xy 149.225 111.76) (xy 130.81 111.76)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.3)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 149.225 100.33) (xy 130.81 100.33) (xy 130.81 111.76) (xy 149.225 111.76)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 132.715 104.14) (xy 133.985 104.14) (xy 133.985 107.95) (xy 132.715 107.95)
      )
    )
  )
)
