(kicad_pcb (version 20171130) (host pcbnew "(5.1.5-0)")
  (general
    (thickness 1.6)
    (drawings 8)
    (tracks 12)
    (zones 0)
    (modules 5)
    (nets 3)
  )
  (page A4)
  (title_block
    (date 2020-01-15)
    (rev 1.3)
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.4064)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (grid_origin 127.000001 96.520001)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(D1-Pad1)")
  (net 2 "Net-(D1-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
  )
  (module TestPoint:TestPoint_Pad_D1.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 131.7625 95.123)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference "IR Detector(Q1)" (at 1.143 0) (layer F.SilkS))
    (fp_text value TestPoint (at 0 1.55) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.45) (layer F.Fab) hide)
    (pad 1 smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask))
  )
  (module TestPoint:TestPoint_Pad_D1.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 131.7625 93.091)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference "IR Emitter(D1)" (at 1.143 0) (layer F.SilkS))
    (fp_text value TestPoint (at 0 1.55) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.45) (layer F.Fab) hide)
    (pad 1 smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask))
  )
  (module TestPoint:TestPoint_Pad_D1.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 131.7625 91.059)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference "White LED(D2)" (at 1.143 0) (layer F.SilkS))
    (fp_text value TestPoint (at 0 1.55) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.45) (layer F.Fab) hide)
    (pad 1 smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask))
  )
  (module asl_footprints:1206_reverse_smd (layer F.Cu) (tedit 5E87BE74)
    (at 126.198001 93.218001 180)
    (fp_text reference D1 (at -3.341999 0.000001 180) (layer F.SilkS) hide)
    (fp_text value LED (at 0.635 -1.905) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0 270) (size 2.3 2.3) (drill 2.3) (layers *.Cu *.Mask))
    (pad 2 smd rect (at 1.625 0 270) (size 1.7 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -1.625 0 270) (size 1.7 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (model ${KIPRJMOD}/libs/3d/reverse_LED.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module asl_footprints:board_to_board_joint (layer B.Cu) (tedit 5E1E2791)
    (at 146.823001 93.115 270)
    (fp_text reference J1 (at -1.675 3.948001 270) (layer B.SilkS) hide)
    (fp_text value Conn_01x02_Male (at 0 -2.54 270) (layer B.Fab) hide)
    (pad 2 smd rect (at 1.675 1.5 270) (size 2 3) (layers B.Cu B.Paste B.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (pad 1 smd rect (at -1.675 1.5 270) (size 2 3) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(D1-Pad2)"))
  )
  (gr_text "Side\nEmitter/Detector\nv1.4" (at 135.382 93.1545) (layer B.SilkS))
  (gr_arc (start 127.000001 93.218001) (end 127.000001 90.043001) (angle -180) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 146.823001 90.043) (end 127.000001 90.043001) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 146.823001 90.043) (end 146.823001 96.393) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 127 96.393) (end 146.823001 96.393) (layer Edge.Cuts) (width 0.05))
)
