<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.5.2">
<drawing>
<board>
<plain>
<circle x="8.5" y="8.5" radius="7.4" width="0.001" layer="46"/>
<text>gChart</text>
<text>Joule</text>
<text>Thief</text>
</plain>
<libraries>
<library name="testpad">
<description>&lt;b&gt;Test Pins/Pads&lt;/b&gt;&lt;p&gt;
Cream on SMD OFF.&lt;br&gt;
new: Attribute TP_SIGNAL_NAME&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TP18R">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="74xx-little-de">
<description>&lt;b&gt;Single and Dual Gates Family, US symbols&lt;/b&gt;&lt;p&gt;
Little logic devices from Texas Instruments&lt;br&gt;
TinyLogic(R) from FAIRCHILD Semiconductor TM
&lt;p&gt;
&lt;author&gt;Created by evgeni@eniks.com&lt;/author&gt;&lt;br&gt;
&lt;author&gt;Extended by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DBV_R-PDSO-G6">
<description>&lt;b&gt;DBV (R-PDSO-G6)&lt;/b&gt; PLASTIC SMALL-OUTLINE PACKAGE&lt;p&gt;
SOT (SOT-23) - DBV&lt;br&gt;
Source: http://focus.ti.com/lit/ds/symlink/sn74lvc1g3157.</description>
</package>
</packages>
</library>
<library name="ref-packages">
<description>&lt;b&gt;Reference Package&lt;/b&gt;&lt;p&gt;</description>
<packages>
<package name="C0805K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 0805 Reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 2012</description>
</package>
<package name="C1210K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 1210 Reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 3225</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="-" library="testpad" package="TP18R" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="+" library="testpad" package="TP18R" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC" library="74xx-little-de" package="DBV_R-PDSO-G6" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="ref-packages" package="C0805K" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="ref-packages" package="C0805K" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R" library="ref-packages" package="C0805K" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L" library="ref-packages" package="C1210K" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="S$3">
<contactref element="C2" pad="1"/>
</signal>
<signal name="GND">
<contactref element="IC" pad="2"/>
<contactref element="R" pad="1"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="S$2">
</signal>
<signal name="FB">
<contactref element="-" pad="TP"/>
<contactref element="R" pad="2"/>
<contactref element="IC" pad="4"/>
</signal>
<signal name="VBAT">
<contactref element="C1" pad="2"/>
<contactref element="L" pad="2"/>
<contactref element="IC" pad="6"/>
<contactref element="IC" pad="3"/>
</signal>
<signal name="SW">
<contactref element="IC" pad="1"/>
<contactref element="L" pad="1"/>
</signal>
<signal name="VOUT">
<contactref element="+" pad="TP"/>
<contactref element="IC" pad="5"/>
<contactref element="C2" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
