<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<board>
<plain>
<wire x1="5.08" y1="0" x2="96.52" y2="0" width="0" layer="20"/>
<wire x1="101.6" y1="5.08" x2="101.6" y2="63.5" width="0" layer="20"/>
<text>actuated pad</text>
<text>ground pad</text>
<text>ground pad</text>
<text>ground pad</text>
<text>ground pad</text>
<text>LEVER electrovibration board
v1.0 09.2015 nytlabs / AKA</text>
<wire x1="96.52" y1="68.58" x2="5.08" y2="68.58" width="0" layer="20"/>
<wire x1="0" y1="63.5" x2="0" y2="5.08" width="0" layer="20"/>
<wire x1="0" y1="63.5" x2="5.08" y2="68.58" width="0" layer="20" curve="-90"/>
<wire x1="5.08" y1="0" x2="0" y2="5.08" width="0" layer="20" curve="-90"/>
<wire x1="101.6" y1="5.08" x2="96.52" y2="0" width="0" layer="20" curve="-90"/>
<wire x1="96.52" y1="68.58" x2="101.6" y2="63.5" width="0" layer="20" curve="-90"/>
<text>HI-V</text>
<hole x="86.36" y="15.24" drill="3.2"/>
<hole x="86.36" y="53.34" drill="3.2"/>
<hole x="66.04" y="15.24" drill="3.2"/>
<hole x="66.04" y="53.34" drill="3.2"/>
</plain>
<libraries>
<library name="AKA_test">
<packages>
<package name="PA0367">
<description>&lt;b&gt;SMT Flyback Transformer&lt;/b&gt;
&lt;br/&gt;For PhotoFlash Capacitor Charger
&lt;br/&gt;&lt;em&gt;For Use with Linear Technology’s LT3420&lt;/em&gt;
&lt;br/&gt;by Pulse Electronics
&lt;hr&gt;
&lt;br/&gt;1:12 ratio
&lt;br/&gt;Low side: pins 2 and 3
&lt;br/&gt;High side: pins 1 and 4
&lt;br/&gt;Pins 2 and 4 are the dotted poles in transformer schematic
&lt;hr&gt;
&lt;br/&gt;Min 18 uH inductance at Irated (Irated is 1.5A DC)
&lt;br/&gt;Leakage Inductance (2-3 with 1-4 shorted): 0.75 uH MAX
&lt;br/&gt;Primary DCR: 180 milliohm MAX
&lt;br/&gt;Secondary DCR 18 ohm MAX
&lt;br/&gt;Primary Secondary isolation: 500Vrms</description>
</package>
<package name="TO263">
<description>&lt;b&gt;SMALL OUTLINE TRANSISTOR&lt;/b&gt;&lt;p&gt;
TS-005</description>
</package>
<package name="SO8">
<description>&lt;b&gt;SMALL OUTLINE INTEGRATED CIRCUIT&lt;/b&gt;</description>
</package>
<package name="DPAK">
<description>&lt;b&gt;DPAK&lt;/b&gt; CASE 369-07&lt;br&gt;
Source MOTOROLA / ON Semiconductor mjd32-d.pdf</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="TRIM-3386">
</package>
<package name="C1812">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete semiconductors- transistors, diodes, TRIACs, optoisolators, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TO-92">
<description>&lt;b&gt;TO 92&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="R2010">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="1206">
</package>
<package name="PAD.03X.05">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X08_LOCK">
</package>
<package name="JST-2-SMD">
<description>2mm SMD side-entry connector. tDocu layer indicates the actual physical plastic housing. +/- indicate SparkFun standard batteries and wiring.</description>
</package>
</packages>
</library>
<library name="wirepad">
<description>&lt;b&gt;Single Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="5-2,5">
<description>&lt;b&gt;THROUGH-HOLE PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="Teensy_3_Series_Board_v1.0">
<packages>
<package name="TEENSY_3.1_BASIC">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="1:12_TRNSFRMR" library="AKA_test" package="PA0367" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="AKA_test" package="TO263" value="RB751"/>
<element name="C1" library="adafruit" package="C1812" value="2.2uF"/>
<element name="Q3" library="SparkFun-DiscreteSemi" package="TO-92" value="MPSA42">
<attribute name="PROD_ID" value="TRANS-09536"/>
</element>
<element name="R1" library="SparkFun-Passives" package="R2010" value="100k"/>
<element name="R2" library="SparkFun-Passives" package="1206" value="1k"/>
<element name="R4" library="SparkFun-Passives" package="1206" value="1k"/>
<element name="128X64_SSD1306_OLED" library="SparkFun-Connectors" package="1X08_LOCK" value=""/>
<element name="R3" library="SparkFun-Passives" package="R2010" value="220k"/>
<element name="PAD1" library="wirepad" package="5-2,5" value="WIREPADSMD5-2,5">
<attribute name="VALUE"/>
</element>
<element name="PAD2" library="wirepad" package="5-2,5" value="WIREPADSMD5-2,5">
<attribute name="VALUE"/>
</element>
<element name="GND$1" library="wirepad" package="5-2,5" value="WIREPADSMD5-2,5">
<attribute name="VALUE"/>
</element>
<element name="PAD4" library="wirepad" package="5-2,5" value="WIREPADSMD5-2,5">
<attribute name="VALUE"/>
</element>
<element name="PAD5" library="wirepad" package="5-2,5" value="WIREPADSMD5-2,5">
<attribute name="VALUE"/>
</element>
<element name="JP1" library="SparkFun-Connectors" package="JST-2-SMD" value="M02-JST-2MM-SMT">
<attribute name="PROD_ID" value="CONN-08352"/>
</element>
<element name="TM1" library="adafruit" package="TRIM-3386" value=""/>
<element name="HI-V" library="SparkFun-Passives" package="PAD.03X.05" value="TEST-POINT3X5"/>
<element name="U$1" library="AKA_test" package="SO8" value="FDS6911">
<attribute name="VALUE"/>
</element>
<element name="U1" library="AKA_test" package="DPAK" value="L78M"/>
<element name="TEENSY3.1" library="Teensy_3_Series_Board_v1.0" package="TEENSY_3.1_BASIC" value="TEENSY_3.1_BASIC">
<attribute name="NAME"/>
</element>
<element name="R5" library="SparkFun-Passives" package="1206" value="33"/>
</elements>
<signals>
<signal name="GND">
<contactref element="C1" pad="2"/>
<contactref element="R2" pad="1"/>
<contactref element="1:12_TRNSFRMR" pad="4"/>
<contactref element="128X64_SSD1306_OLED" pad="1"/>
<contactref element="PAD2" pad="1"/>
<contactref element="GND$1" pad="1"/>
<contactref element="PAD4" pad="1"/>
<contactref element="PAD5" pad="1"/>
<contactref element="JP1" pad="1"/>
<contactref element="U$1" pad="1"/>
<contactref element="U1" pad="4"/>
<contactref element="TEENSY3.1" pad="GND1"/>
<contactref element="TEENSY3.1" pad="GND"/>
</signal>
<signal name="HI-V">
<contactref element="D1" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="R1" pad="2"/>
<contactref element="HI-V" pad="P$1"/>
</signal>
<signal name="PWM">
<contactref element="U$1" pad="2"/>
<contactref element="TEENSY3.1" pad="4"/>
</signal>
<signal name="N$13">
<contactref element="R1" pad="1"/>
<contactref element="Q3" pad="1"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="N$14">
<contactref element="Q3" pad="3"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$15">
<contactref element="R4" pad="1"/>
<contactref element="Q3" pad="2"/>
</signal>
<signal name="DAC">
<contactref element="R4" pad="2"/>
<contactref element="TEENSY3.1" pad="A14"/>
</signal>
<signal name="5V_REG">
<contactref element="TM1" pad="3"/>
<contactref element="U1" pad="3"/>
<contactref element="TEENSY3.1" pad="VIN"/>
<contactref element="128X64_SSD1306_OLED" pad="2"/>
</signal>
<signal name="FREQ_POT">
<contactref element="TM1" pad="2"/>
<contactref element="TEENSY3.1" pad="21/A7"/>
</signal>
<signal name="OLED_RESET">
<contactref element="128X64_SSD1306_OLED" pad="5"/>
<contactref element="TEENSY3.1" pad="20/A6"/>
</signal>
<signal name="SDA">
<contactref element="128X64_SSD1306_OLED" pad="8"/>
<contactref element="TEENSY3.1" pad="18/A4"/>
</signal>
<signal name="SCL">
<contactref element="128X64_SSD1306_OLED" pad="7"/>
<contactref element="TEENSY3.1" pad="19/A5"/>
</signal>
<signal name="N$1">
<contactref element="1:12_TRNSFRMR" pad="3"/>
<contactref element="U$1" pad="8"/>
<contactref element="U$1" pad="7"/>
</signal>
<signal name="N$3">
<contactref element="1:12_TRNSFRMR" pad="1"/>
<contactref element="D1" pad="2"/>
</signal>
<signal name="PAD">
<contactref element="R3" pad="1"/>
<contactref element="PAD1" pad="1"/>
</signal>
<signal name="V-BAT">
<contactref element="U1" pad="1"/>
<contactref element="1:12_TRNSFRMR" pad="2"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="VBAT">
<contactref element="TEENSY3.1" pad="VBAT"/>
</signal>
<signal name="AGND">
<contactref element="TEENSY3.1" pad="AGND"/>
<contactref element="TM1" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="TEENSY3.1" pad="3.3V"/>
<contactref element="TEENSY3.1" pad="3.3V1"/>
</signal>
<signal name="N$4">
<contactref element="JP1" pad="2"/>
<contactref element="R5" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
