(kicad_pcb (version 20171130) (host pcbnew "(5.1.4-0-10_14)")
  (general
    (thickness 1.6)
    (drawings 21)
    (tracks 324)
    (zones 0)
    (modules 115)
    (nets 21)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.5)
    (user_trace_width 0.2)
    (user_trace_width 0.35)
    (user_trace_width 0.5)
    (user_trace_width 0.75)
    (user_trace_width 1)
    (user_trace_width 1.5)
    (user_trace_width 2)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (user_via 0.4 0.3)
    (user_via 0.4 0.3)
    (user_via 0.5 0.3)
    (user_via 0.8 0.5)
    (user_via 1 0.7)
    (user_via 1.5 1)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.15)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 5.08 5.08)
    (pad_drill 2.032)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +5V)
  (net 2 "Net-(D1-Pad1)")
  (net 3 "Net-(D2-Pad1)")
  (net 4 GND)
  (net 5 -5V5)
  (net 6 "Net-(J3-Pad1)")
  (net 7 "Net-(J4-Pad1)")
  (net 8 "Net-(J5-Pad1)")
  (net 9 "Net-(C3-Pad1)")
  (net 10 "Net-(J1-Pad2)")
  (net 11 "Net-(J1-Pad3)")
  (net 12 "Net-(J1-Pad4)")
  (net 13 /Tx)
  (net 14 /Rx)
  (net 15 "Net-(R3-Pad2)")
  (net 16 "Net-(R4-Pad2)")
  (net 17 "Net-(R5-Pad2)")
  (net 18 "Net-(J6-Pad1)")
  (net 19 "Net-(R6-Pad2)")
  (net 20 "Net-(R7-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net -5V5)
    (add_net /Rx)
    (add_net /Tx)
    (add_net GND)
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(J4-Pad1)")
    (add_net "Net-(J5-Pad1)")
    (add_net "Net-(J6-Pad1)")
    (add_net "Net-(R3-Pad2)")
    (add_net "Net-(R4-Pad2)")
    (add_net "Net-(R5-Pad2)")
    (add_net "Net-(R6-Pad2)")
    (add_net "Net-(R7-Pad2)")
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 134.62 111.76)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 139.7 111.76)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 142.24 111.76)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 137.16 111.76)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 137.16 109.22)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 142.24 109.22)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 139.7 109.22)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 134.62 109.22)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 134.62 114.3)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 134.62 101.6)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 139.7 101.6)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 137.16 106.68)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 139.7 114.3)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 142.24 114.3)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 137.16 114.3)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 137.16 101.6)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 142.24 101.6)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 142.24 106.68)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 134.62 106.68)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 139.7 106.68)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 137.16 104.14)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 142.24 104.14)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 139.7 104.14)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 134.62 104.14)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 132.08 119.38)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 124.46 119.38)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 137.16 119.38)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 129.54 119.38)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 142.24 119.38)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 132.08 116.84)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 124.46 116.84)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 127 116.84)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 127 119.38)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 134.62 119.38)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 139.7 119.38)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 137.16 116.84)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 142.24 116.84)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 129.54 116.84)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 139.7 116.84)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 134.62 116.84)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 132.08 127)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 124.46 127)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 127 127)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 137.16 127)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 142.24 127)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 129.54 127)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 139.7 127)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 134.62 127)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 134.62 121.92)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 139.7 121.92)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 142.24 121.92)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 129.54 121.92)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 137.16 121.92)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 132.08 121.92)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 124.46 121.92)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 127 121.92)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 127 124.46)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 134.62 124.46)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 139.7 124.46)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 142.24 124.46)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 129.54 124.46)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 137.16 124.46)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 132.08 124.46)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 124.46 124.46)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 127 129.54)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 134.62 129.54)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 139.7 129.54)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 142.24 129.54)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 129.54 129.54)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 137.16 129.54)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 132.08 129.54)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 124.46 129.54)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 137.16 132.08)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 139.7 132.08)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 142.24 132.08)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 134.62 132.08)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 132.08 132.08)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 129.54 132.08)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 127 132.08)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:Hole (layer F.Cu) (tedit 5D2355F3)
    (at 124.46 132.08)
    (fp_text reference "" (at 0.508 4.064) (layer F.SilkS))
    (fp_text value Hole (at 0.254 2.286) (layer F.Fab))
    (pad "" thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module RF_Switch_Controller:PinSocket_1x03_P2.54mm (layer B.Cu) (tedit 5DB388B6)
    (at 158.115 126.492 270)
    (fp_text reference J2 (at 0 -8.001) (layer B.SilkS))
    (fp_text value Interboard_Conn (at 0 -7.85 270) (layer B.Fab))
    (fp_text user %R (at 0 -2.54 180) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /Tx))
    (pad 2 thru_hole oval (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /Rx))
    (pad 3 thru_hole oval (at 0 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RF_Switch_Controller:LED_0805_HandSolder (layer F.Cu) (tedit 5DB48FBE)
    (at 133.35 86.36 270)
    (attr smd)
    (fp_text reference D1 (at 2.54 0) (layer F.SilkS) hide)
    (fp_text value Amber (at 0 1.65 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 "Net-(D1-Pad1)"))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RF_Switch_Controller:MountingHole_80mil (layer F.Cu) (tedit 5DB48F90)
    (at 107.315 81.28)
    (attr virtual)
    (fp_text reference H1 (at 3.937 0) (layer F.SilkS) hide)
    (fp_text value Mounting_Hole (at 0 3.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.08 5.08) (drill 2.032) (layers *.Cu *.Mask)
      (net 4 GND))
  )
  (module RF_Switch_Controller:MountingHole_80mil (layer F.Cu) (tedit 5DB4951A)
    (at 107.315 132.08)
    (attr virtual)
    (fp_text reference H2 (at 3.937 0) (layer F.SilkS) hide)
    (fp_text value Mounting_Hole (at 0 3.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.08 5.08) (drill 2.032) (layers *.Cu *.Mask)
      (net 4 GND))
  )
  (module RF_Switch_Controller:MountingHole_80mil (layer F.Cu) (tedit 5DB49016)
    (at 189.865 81.28)
    (attr virtual)
    (fp_text reference H3 (at 4.191 0) (layer F.SilkS) hide)
    (fp_text value Mounting_Hole (at 0 3.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.08 5.08) (drill 2.032) (layers *.Cu *.Mask)
      (net 4 GND))
  )
  (module RF_Switch_Controller:MountingHole_80mil (layer F.Cu) (tedit 5DB4903F)
    (at 189.865 132.08)
    (attr virtual)
    (fp_text reference H4 (at 4.191 0) (layer F.SilkS) hide)
    (fp_text value Mounting_Hole (at 0 3.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.08 5.08) (drill 2.032) (layers *.Cu *.Mask)
      (net 4 GND))
  )
  (module RF_Switch_Controller:R_0805_HandSolder (layer F.Cu) (tedit 5D1E2DCA)
    (at 151.765 84.074 270)
    (attr smd)
    (fp_text reference R7 (at 2.667 0 180) (layer F.SilkS))
    (fp_text value 78.7k (at 0 1.65 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 5 -5V5))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 20 "Net-(R7-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RF_Switch_Controller:TestPoint_1mm (layer F.Cu) (tedit 5DB48F95)
    (at 127 81.28 270)
    (fp_text reference TP1 (at 0 2.5 90) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 -2.8 90) (layer F.Fab))
    (fp_text user %R (at 0.7 2.5 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 +5V))
  )
  (module RF_Switch_Controller:TestPoint_1mm (layer F.Cu) (tedit 5DB48F98)
    (at 120.65 81.28 270)
    (fp_text reference TP2 (at 0 2.5 90) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 -2.8 90) (layer F.Fab))
    (fp_text user %R (at 0.7 2.5 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 4 GND))
  )
  (module RF_Switch_Controller:C_0805_HandSolder (layer F.Cu) (tedit 5D1E325B)
    (at 145.415 84.074 90)
    (attr smd)
    (fp_text reference C3 (at -2.667 0 180) (layer F.SilkS))
    (fp_text value 2.2uF (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 4 GND))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 9 "Net-(C3-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RF_Switch_Controller:C_0805_HandSolder (layer F.Cu) (tedit 5D1E325B)
    (at 148.59 80.899 180)
    (attr smd)
    (fp_text reference C6 (at 0 1.651 180) (layer F.SilkS))
    (fp_text value 2.2uF (at 0 1.65 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 4 GND))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 5 -5V5))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RF_Switch_Controller:LED_0805_HandSolder (layer F.Cu) (tedit 5DB4900E)
    (at 165.1 86.36 270)
    (attr smd)
    (fp_text reference D2 (at 0 -1.65 270) (layer F.SilkS) hide)
    (fp_text value Amber (at 0 1.65 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 3 "Net-(D2-Pad1)"))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RF_Switch_Controller:R_0805_HandSolder (layer F.Cu) (tedit 5D1E2DCA)
    (at 154.305 84.074 270)
    (attr smd)
    (fp_text reference R8 (at 2.667 0) (layer F.SilkS))
    (fp_text value 21.5k (at 0 1.65 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 4 GND))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 20 "Net-(R7-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RF_Switch_Controller:R_0805_HandSolder (layer F.Cu) (tedit 5D1E2DCA)
    (at 133.35 81.915 90)
    (attr smd)
    (fp_text reference R9 (at 2.54 0 180) (layer F.SilkS))
    (fp_text value 1k (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 4 GND))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RF_Switch_Controller:R_0805_HandSolder (layer F.Cu) (tedit 5D1E2DCA)
    (at 165.1 81.915 90)
    (attr smd)
    (fp_text reference R10 (at 2.54 0 180) (layer F.SilkS))
    (fp_text value 1k (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 3 "Net-(D2-Pad1)"))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 5 -5V5))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RF_Switch_Controller:IE0509S (layer F.Cu) (tedit 5DB22AC2)
    (at 139.065 80.01 270)
    (fp_text reference U1 (at 10.795 -1.27) (layer F.SilkS))
    (fp_text value IE0509S (at 3.81 -1.905 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 -0.0762 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 2 thru_hole circle (at 2.5654 -0.0762 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 3 thru_hole circle (at 5.1054 -0.0762 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 9 "Net-(C3-Pad1)"))
    (pad 4 thru_hole circle (at 7.6454 -0.0762 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 4 GND))
  )
  (module RF_Switch_Controller:SOT-23-5 (layer F.Cu) (tedit 5DB22B38)
    (at 148.59 84.074)
    (attr smd)
    (fp_text reference U4 (at 0 2.667) (layer F.SilkS))
    (fp_text value TPS72301 (at 0 2.9) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 2 smd rect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C3-Pad1)"))
    (pad 3 smd rect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C3-Pad1)"))
    (pad 4 smd rect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(R7-Pad2)"))
    (pad 5 smd rect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 5 -5V5))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RF_Switch_Controller:TestPoint_1mm (layer F.Cu) (tedit 5DB49012)
    (at 158.75 81.28)
    (fp_text reference TP7 (at 0.7 2.5) (layer F.SilkS) hide)
    (fp_text value Test_Point (at 0 -2.8) (layer F.Fab))
    (fp_text user %R (at 0.7 2.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 5 -5V5))
  )
  (module RF_Switch_Controller:C_0805_HandSolder (layer B.Cu) (tedit 5D1E325B)
    (at 154.94 121.92 90)
    (attr smd)
    (fp_text reference C1 (at 0 1.905) (layer B.SilkS))
    (fp_text value 10nF (at 0 -1.65 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 1 +5V))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RF_Switch_Controller:C_0805_HandSolder (layer B.Cu) (tedit 5D1E325B)
    (at 162.56 132.715)
    (attr smd)
    (fp_text reference C2 (at 3.175 0) (layer B.SilkS))
    (fp_text value 10nF (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 1 +5V))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RF_Switch_Controller:C_0805_HandSolder (layer B.Cu) (tedit 5D1E325B)
    (at 166.37 123.19 270)
    (attr smd)
    (fp_text reference C4 (at 0 -1.905) (layer B.SilkS))
    (fp_text value 10nF (at 0 -1.65 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 5 -5V5))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RF_Switch_Controller:C_0805_HandSolder (layer B.Cu) (tedit 5D1E325B)
    (at 161.925 135.89 180)
    (attr smd)
    (fp_text reference C5 (at -3.175 0) (layer B.SilkS))
    (fp_text value 10nF (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 5 -5V5))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RF_Switch_Controller:PinHeader_1x05_P2.54mm (layer F.Cu) (tedit 5DF80A03)
    (at 127 101.6)
    (fp_text reference J1 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Micro_USB_Breakout (at 0 12.49) (layer F.Fab))
    (fp_text user %R (at 0 5.08 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J1-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RF_Switch_Controller:R_0805_HandSolder (layer B.Cu) (tedit 5D1E2DCA)
    (at 161.925 123.825)
    (attr smd)
    (fp_text reference R1 (at 0 -1.905) (layer B.SilkS))
    (fp_text value R (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 13 /Tx))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 4 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RF_Switch_Controller:R_0805_HandSolder (layer B.Cu) (tedit 5D1E2DCA)
    (at 157.48 129.54 180)
    (attr smd)
    (fp_text reference R2 (at -3.175 0) (layer B.SilkS))
    (fp_text value R (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 4 GND))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 14 /Rx))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RF_Switch_Controller:R_0805_HandSolder (layer F.Cu) (tedit 5D1E2DCA)
    (at 158.115 116.84 270)
    (attr smd)
    (fp_text reference R3 (at -2.54 0 180) (layer F.SilkS))
    (fp_text value 20R (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 15 "Net-(R3-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 8 "Net-(J5-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RF_Switch_Controller:R_0805_HandSolder (layer F.Cu) (tedit 5D1E2DCA)
    (at 163.195 116.84 270)
    (attr smd)
    (fp_text reference R4 (at -2.54 0 180) (layer F.SilkS))
    (fp_text value 20R (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 6 "Net-(J3-Pad1)"))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 16 "Net-(R4-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RF_Switch_Controller:R_0805_HandSolder (layer F.Cu) (tedit 5D1E2DCA)
    (at 167.64 129.54 180)
    (attr smd)
    (fp_text reference R5 (at -3.175 0) (layer F.SilkS))
    (fp_text value 20R (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 17 "Net-(R5-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 18 "Net-(J6-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RF_Switch_Controller:R_0805_HandSolder (layer F.Cu) (tedit 5D1E2DCA)
    (at 167.64 134.62 180)
    (attr smd)
    (fp_text reference R6 (at -3.175 0) (layer F.SilkS))
    (fp_text value 20R (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 7 "Net-(J4-Pad1)"))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 19 "Net-(R6-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RF_Switch_Controller:SOIC-8_3.9x4.9mm_P1.27mm (layer F.Cu) (tedit 5DF80A66)
    (at 160.655 121.92)
    (attr smd)
    (fp_text reference U2 (at -5.08 0) (layer F.SilkS))
    (fp_text value MADR-009269 (at 0 3.4) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 8 smd roundrect (at 2.475 -1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 "Net-(R4-Pad2)"))
    (pad 7 smd roundrect (at 2.475 -0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (pad 6 smd roundrect (at 2.475 0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (pad 5 smd roundrect (at 2.475 1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 -5V5))
    (pad 4 smd roundrect (at -2.475 1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 /Tx))
    (pad 3 smd roundrect (at -2.475 0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (pad 2 smd roundrect (at -2.475 -0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (pad 1 smd roundrect (at -2.475 -1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 "Net-(R3-Pad2)"))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RF_Switch_Controller:SOIC-8_3.9x4.9mm_P1.27mm (layer F.Cu) (tedit 5DF80A66)
    (at 162.56 132.08 270)
    (attr smd)
    (fp_text reference U3 (at 0 3.81 180) (layer F.SilkS))
    (fp_text value MADR-009269 (at 0 3.4 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -2.475 -1.905 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 "Net-(R5-Pad2)"))
    (pad 2 smd roundrect (at -2.475 -0.635 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (pad 3 smd roundrect (at -2.475 0.635 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (pad 4 smd roundrect (at -2.475 1.905 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 /Rx))
    (pad 5 smd roundrect (at 2.475 1.905 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 -5V5))
    (pad 6 smd roundrect (at 2.475 0.635 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (pad 7 smd roundrect (at 2.475 -0.635 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (pad 8 smd roundrect (at 2.475 -1.905 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 "Net-(R6-Pad2)"))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RF_Switch_Controller:SMA (layer F.Cu) (tedit 5DF80864)
    (at 198.12 99.695 180)
    (attr smd)
    (fp_text reference J3 (at -1.5 7) (layer F.SilkS) hide)
    (fp_text value Conn_Coaxial (at -1.72 -7.11) (layer F.Fab))
    (fp_text user %R (at -1.5 7) (layer F.Fab))
    (pad 1 smd rect (at -1.72 0 180) (size 5.08 2.29) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(J3-Pad1)"))
    (pad 2 smd rect (at -1.72 -4.38 180) (size 5.08 2.42) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 2 smd rect (at -1.72 4.38 180) (size 5.08 2.42) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 2 smd rect (at -1.72 -4.38 180) (size 5.08 2.42) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 2 smd rect (at -1.72 4.38 180) (size 5.08 2.42) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 2 thru_hole circle (at 1.72 -4.38 180) (size 0.97 0.97) (drill 0.46) (layers *.Cu)
      (net 4 GND))
    (pad 2 thru_hole circle (at 1.72 4.38 180) (size 0.97 0.97) (drill 0.46) (layers *.Cu)
      (net 4 GND))
    (pad 2 smd rect (at 1.27 -4.38 180) (size 0.95 0.46) (layers F.Cu)
      (net 4 GND))
    (pad 2 smd rect (at 1.27 4.38 180) (size 0.95 0.46) (layers F.Cu)
      (net 4 GND))
    (pad 2 smd rect (at 1.27 -4.38 180) (size 0.95 0.46) (layers B.Cu)
      (net 4 GND))
    (pad 2 smd rect (at 1.27 4.38 180) (size 0.95 0.46) (layers B.Cu)
      (net 4 GND))
    (model ${KISYS3DMOD}/Connector_Coaxial.3dshapes/SMA_Molex_73251-1153_EdgeMount_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RF_Switch_Controller:SMA (layer F.Cu) (tedit 5DF80864)
    (at 198.12 126.365 180)
    (attr smd)
    (fp_text reference J4 (at -1.5 7) (layer F.SilkS) hide)
    (fp_text value Conn_Coaxial (at -1.72 -7.11) (layer F.Fab))
    (fp_text user %R (at -1.5 7) (layer F.Fab))
    (pad 1 smd rect (at -1.72 0 180) (size 5.08 2.29) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(J4-Pad1)"))
    (pad 2 smd rect (at -1.72 -4.38 180) (size 5.08 2.42) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 2 smd rect (at -1.72 4.38 180) (size 5.08 2.42) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 2 smd rect (at -1.72 -4.38 180) (size 5.08 2.42) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 2 smd rect (at -1.72 4.38 180) (size 5.08 2.42) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 2 thru_hole circle (at 1.72 -4.38 180) (size 0.97 0.97) (drill 0.46) (layers *.Cu)
      (net 4 GND))
    (pad 2 thru_hole circle (at 1.72 4.38 180) (size 0.97 0.97) (drill 0.46) (layers *.Cu)
      (net 4 GND))
    (pad 2 smd rect (at 1.27 -4.38 180) (size 0.95 0.46) (layers F.Cu)
      (net 4 GND))
    (pad 2 smd rect (at 1.27 4.38 180) (size 0.95 0.46) (layers F.Cu)
      (net 4 GND))
    (pad 2 smd rect (at 1.27 -4.38 180) (size 0.95 0.46) (layers B.Cu)
      (net 4 GND))
    (pad 2 smd rect (at 1.27 4.38 180) (size 0.95 0.46) (layers B.Cu)
      (net 4 GND))
    (model ${KISYS3DMOD}/Connector_Coaxial.3dshapes/SMA_Molex_73251-1153_EdgeMount_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RF_Switch_Controller:SMA (layer F.Cu) (tedit 5DF80864)
    (at 198.12 86.36 180)
    (attr smd)
    (fp_text reference J5 (at -1.5 7) (layer F.SilkS) hide)
    (fp_text value Conn_Coaxial (at -1.72 -7.11) (layer F.Fab))
    (fp_text user %R (at -1.5 7) (layer F.Fab))
    (pad 2 smd rect (at 1.27 4.38 180) (size 0.95 0.46) (layers B.Cu)
      (net 4 GND))
    (pad 2 smd rect (at 1.27 -4.38 180) (size 0.95 0.46) (layers B.Cu)
      (net 4 GND))
    (pad 2 smd rect (at 1.27 4.38 180) (size 0.95 0.46) (layers F.Cu)
      (net 4 GND))
    (pad 2 smd rect (at 1.27 -4.38 180) (size 0.95 0.46) (layers F.Cu)
      (net 4 GND))
    (pad 2 thru_hole circle (at 1.72 4.38 180) (size 0.97 0.97) (drill 0.46) (layers *.Cu)
      (net 4 GND))
    (pad 2 thru_hole circle (at 1.72 -4.38 180) (size 0.97 0.97) (drill 0.46) (layers *.Cu)
      (net 4 GND))
    (pad 2 smd rect (at -1.72 4.38 180) (size 5.08 2.42) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 2 smd rect (at -1.72 -4.38 180) (size 5.08 2.42) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 2 smd rect (at -1.72 4.38 180) (size 5.08 2.42) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 2 smd rect (at -1.72 -4.38 180) (size 5.08 2.42) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 1 smd rect (at -1.72 0 180) (size 5.08 2.29) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(J5-Pad1)"))
    (model ${KISYS3DMOD}/Connector_Coaxial.3dshapes/SMA_Molex_73251-1153_EdgeMount_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RF_Switch_Controller:SMA (layer F.Cu) (tedit 5DF80864)
    (at 198.12 113.03 180)
    (attr smd)
    (fp_text reference J6 (at -1.5 7) (layer F.SilkS) hide)
    (fp_text value Conn_Coaxial (at -1.72 -7.11) (layer F.Fab))
    (fp_text user %R (at -1.5 7) (layer F.Fab))
    (pad 2 smd rect (at 1.27 4.38 180) (size 0.95 0.46) (layers B.Cu)
      (net 4 GND))
    (pad 2 smd rect (at 1.27 -4.38 180) (size 0.95 0.46) (layers B.Cu)
      (net 4 GND))
    (pad 2 smd rect (at 1.27 4.38 180) (size 0.95 0.46) (layers F.Cu)
      (net 4 GND))
    (pad 2 smd rect (at 1.27 -4.38 180) (size 0.95 0.46) (layers F.Cu)
      (net 4 GND))
    (pad 2 thru_hole circle (at 1.72 4.38 180) (size 0.97 0.97) (drill 0.46) (layers *.Cu)
      (net 4 GND))
    (pad 2 thru_hole circle (at 1.72 -4.38 180) (size 0.97 0.97) (drill 0.46) (layers *.Cu)
      (net 4 GND))
    (pad 2 smd rect (at -1.72 4.38 180) (size 5.08 2.42) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 2 smd rect (at -1.72 -4.38 180) (size 5.08 2.42) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 2 smd rect (at -1.72 4.38 180) (size 5.08 2.42) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 2 smd rect (at -1.72 -4.38 180) (size 5.08 2.42) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 1 smd rect (at -1.72 0 180) (size 5.08 2.29) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(J6-Pad1)"))
    (model ${KISYS3DMOD}/Connector_Coaxial.3dshapes/SMA_Molex_73251-1153_EdgeMount_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 118.745 125.73) (end 100.965 125.73) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 118.745 87.63) (end 118.745 125.73) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 118.745 87.63) (end 100.965 87.63) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 100.965 87.63) (end 100.965 74.93) (layer Edge.Cuts) (width 0.15))
  (gr_text "-5V5 OK" (at 165.1 88.9) (layer F.SilkS))
  (gr_text "Rx Control 2" (at 190.5 113.03) (layer F.SilkS))
  (gr_text "Rx Control 1" (at 190.5 126.365) (layer F.SilkS))
  (gr_text "Tx Control 2" (at 190.5 86.36) (layer F.SilkS))
  (gr_text "Tx Control 1" (at 190.5 99.695) (layer F.SilkS))
  (gr_text "+5V OK" (at 133.35 88.9) (layer F.SilkS))
  (gr_text GND (at 120.65 84.455) (layer F.SilkS))
  (gr_text +5V (at 127 84.455) (layer F.SilkS))
  (gr_text "RF Switch Controller\nrev B\nDecember 2019" (at 176.53 80.01) (layer F.SilkS))
  (gr_line (start 100.965 138.43) (end 100.965 125.73) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 202.565 138.43) (end 100.965 138.43) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 202.565 74.93) (end 202.565 138.43) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 100.965 74.93) (end 202.565 74.93) (layer Edge.Cuts) (width 0.15))
  (gr_text B (at 270.51 193.04) (layer Cmts.User))
  (gr_text "December 2019" (at 215.9 193.04) (layer Cmts.User))
  (gr_text "RF Switch Controller" (at 199.39 189.23) (layer Cmts.User))
  (gr_text "Vlad Smarandache\nRamshaw Group" (at 196.85 173.99) (layer Cmts.User))
  (zone (net 4) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 100.965 125.73) (xy 118.745 125.73) (xy 118.745 87.63) (xy 100.965 87.63) (xy 100.965 74.93)
        (xy 202.565 74.93) (xy 202.565 138.43) (xy 100.965 138.43)
      )
    )
  )
  (zone (net 4) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 100.965 125.73) (xy 118.745 125.73) (xy 118.745 87.63) (xy 100.965 87.63) (xy 100.965 74.93)
        (xy 202.565 74.93) (xy 202.565 138.43) (xy 100.965 138.43)
      )
    )
  )
)
