(kicad_pcb (version 20171130) (host pcbnew "(5.1.2-1)-1")
  (general
    (thickness 1.6)
    (drawings 14)
    (tracks 470)
    (zones 0)
    (modules 66)
    (nets 80)
  )
  (page A4)
  (title_block
    (title "Nixie Clock Bottom PCB")
    (date 2019-08-15)
    (rev 1)
    (company "Tony Zhang")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.254)
    (user_trace_width 0.762)
    (user_trace_width 1.27)
    (trace_clearance 0.254)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.762)
    (via_drill 0.381)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 6.4 6.4)
    (pad_drill 3.200001)
    (pad_to_mask_clearance 0.0508)
    (solder_mask_min_width 0.1016)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +BATT)
  (net 2 GND)
  (net 3 VCC)
  (net 4 +VDC)
  (net 5 "Net-(C6-Pad1)")
  (net 6 "/Power Supplies/HV")
  (net 7 +3V3)
  (net 8 /Atmega328P/XTAL1)
  (net 9 /Atmega328P/XTAL2)
  (net 10 "Net-(D1-Pad1)")
  (net 11 "Net-(D2-Pad1)")
  (net 12 "Net-(D2-Pad2)")
  (net 13 /disp_clk)
  (net 14 /RX)
  (net 15 /TX)
  (net 16 /AD0)
  (net 17 /AD1)
  (net 18 /AD2)
  (net 19 /pwm_red)
  (net 20 /pwm_grn)
  (net 21 /pwm_blu)
  (net 22 "/Qwiic Ports/LV_SDA")
  (net 23 "/Qwiic Ports/LV_SCL")
  (net 24 "Net-(L1-Pad1)")
  (net 25 /HV_SDA)
  (net 26 /HV_SCL)
  (net 27 /led_ctrl)
  (net 28 /clk_mode)
  (net 29 /clk_st_stp)
  (net 30 /clk_rst)
  (net 31 "Net-(U1-Pad1)")
  (net 32 "Net-(U1-Pad2)")
  (net 33 /19b_D)
  (net 34 /19b_B)
  (net 35 /19b_C)
  (net 36 /disp_latch)
  (net 37 /disp_data)
  (net 38 "Net-(C7-Pad1)")
  (net 39 "Net-(D1-Pad2)")
  (net 40 "/Tube Control Registers/h7")
  (net 41 "/Tube Control Registers/h6")
  (net 42 "/Tube Control Registers/h5")
  (net 43 "/Tube Control Registers/h4")
  (net 44 "/Tube Control Registers/h3")
  (net 45 "/Tube Control Registers/h2")
  (net 46 "/Tube Control Registers/h1")
  (net 47 "/Tube Control Registers/h0")
  (net 48 "/Tube Control Registers/m7")
  (net 49 "/Tube Control Registers/m6")
  (net 50 "/Tube Control Registers/m5")
  (net 51 "/Tube Control Registers/m4")
  (net 52 "/Tube Control Registers/m3")
  (net 53 "/Tube Control Registers/m2")
  (net 54 "/Tube Control Registers/m1")
  (net 55 "/Tube Control Registers/m0")
  (net 56 "/Tube Control Registers/s7")
  (net 57 "/Tube Control Registers/s6")
  (net 58 "/Tube Control Registers/s5")
  (net 59 "/Tube Control Registers/s4")
  (net 60 "/Tube Control Registers/s3")
  (net 61 "/Tube Control Registers/s2")
  (net 62 "/Tube Control Registers/s1")
  (net 63 "/Tube Control Registers/s0")
  (net 64 "/Tube Control Registers/d1")
  (net 65 "/Tube Control Registers/d2")
  (net 66 "/Tube Control Registers/d3")
  (net 67 "/Tube Control Registers/d4")
  (net 68 "/Tube Control Registers/d5")
  (net 69 "/Tube Control Registers/d6")
  (net 70 "Net-(U1-Pad7)")
  (net 71 "Net-(U6-Pad9)")
  (net 72 "Net-(U6-Pad14)")
  (net 73 "Net-(U7-Pad14)")
  (net 74 "Net-(U8-Pad14)")
  (net 75 "Net-(U9-Pad1)")
  (net 76 "Net-(U9-Pad15)")
  (net 77 /RESET)
  (net 78 "Net-(D3-Pad2)")
  (net 79 "Net-(R4-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.762)
    (via_drill 0.381)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +BATT)
    (add_net +VDC)
    (add_net /19b_B)
    (add_net /19b_C)
    (add_net /19b_D)
    (add_net /AD0)
    (add_net /AD1)
    (add_net /AD2)
    (add_net /Atmega328P/XTAL1)
    (add_net /Atmega328P/XTAL2)
    (add_net /HV_SCL)
    (add_net /HV_SDA)
    (add_net "/Power Supplies/HV")
    (add_net "/Qwiic Ports/LV_SCL")
    (add_net "/Qwiic Ports/LV_SDA")
    (add_net /RESET)
    (add_net /RX)
    (add_net /TX)
    (add_net "/Tube Control Registers/d1")
    (add_net "/Tube Control Registers/d2")
    (add_net "/Tube Control Registers/d3")
    (add_net "/Tube Control Registers/d4")
    (add_net "/Tube Control Registers/d5")
    (add_net "/Tube Control Registers/d6")
    (add_net "/Tube Control Registers/h0")
    (add_net "/Tube Control Registers/h1")
    (add_net "/Tube Control Registers/h2")
    (add_net "/Tube Control Registers/h3")
    (add_net "/Tube Control Registers/h4")
    (add_net "/Tube Control Registers/h5")
    (add_net "/Tube Control Registers/h6")
    (add_net "/Tube Control Registers/h7")
    (add_net "/Tube Control Registers/m0")
    (add_net "/Tube Control Registers/m1")
    (add_net "/Tube Control Registers/m2")
    (add_net "/Tube Control Registers/m3")
    (add_net "/Tube Control Registers/m4")
    (add_net "/Tube Control Registers/m5")
    (add_net "/Tube Control Registers/m6")
    (add_net "/Tube Control Registers/m7")
    (add_net "/Tube Control Registers/s0")
    (add_net "/Tube Control Registers/s1")
    (add_net "/Tube Control Registers/s2")
    (add_net "/Tube Control Registers/s3")
    (add_net "/Tube Control Registers/s4")
    (add_net "/Tube Control Registers/s5")
    (add_net "/Tube Control Registers/s6")
    (add_net "/Tube Control Registers/s7")
    (add_net /clk_mode)
    (add_net /clk_rst)
    (add_net /clk_st_stp)
    (add_net /disp_clk)
    (add_net /disp_data)
    (add_net /disp_latch)
    (add_net /led_ctrl)
    (add_net /pwm_blu)
    (add_net /pwm_grn)
    (add_net /pwm_red)
    (add_net GND)
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(L1-Pad1)")
    (add_net "Net-(R4-Pad2)")
    (add_net "Net-(U1-Pad1)")
    (add_net "Net-(U1-Pad2)")
    (add_net "Net-(U1-Pad7)")
    (add_net "Net-(U6-Pad14)")
    (add_net "Net-(U6-Pad9)")
    (add_net "Net-(U7-Pad14)")
    (add_net "Net-(U8-Pad14)")
    (add_net "Net-(U9-Pad1)")
    (add_net "Net-(U9-Pad15)")
    (add_net VCC)
  )
  (net_class HV ""
    (clearance 0.4064)
    (trace_width 0.254)
    (via_dia 0.762)
    (via_drill 0.381)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module logos:chinese-signature-5mm (layer F.Cu) (tedit 5D58F63A)
    (at 123.19 100.33)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 locked (layer F.Cu) (tedit 56D1B4CB)
    (at 55.88 114.3)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 208.28 81.28)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 locked (layer F.Cu) (tedit 56D1B4CB)
    (at 208.28 114.3)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 locked (layer F.Cu) (tedit 56D1B4CB)
    (at 55.88 81.28)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Potentiometers:Potentiometer_Bourns_PTV09A-2_Vertical (layer B.Cu) (tedit 58826B08)
    (at 199.39 114.3 270)
    (descr "Potentiometer, vertically mounted, Omeg PC16PU, Omeg PC16PU, Omeg PC16PU, Vishay/Spectrol 248GJ/249GJ Single, Vishay/Spectrol 248GJ/249GJ Single, Vishay/Spectrol 248GJ/249GJ Single, Vishay/Spectrol 248GH/249GH Single, Vishay/Spectrol 148/149 Single, Vishay/Spectrol 148/149 Single, Vishay/Spectrol 148/149 Single, Vishay/Spectrol 148A/149A Single with mounting plates, Vishay/Spectrol 148/149 Double, Vishay/Spectrol 148A/149A Double with mounting plates, Piher PC-16 Single, Piher PC-16 Single, Piher PC-16 Single, Piher PC-16SV Single, Piher PC-16 Double, Piher PC-16 Triple, Piher T16H Single, Piher T16L Single, Piher T16H Double, Alps RK163 Single, Alps RK163 Double, Alps RK097 Single, Alps RK097 Double, Bourns PTV09A-2 Single with mounting sleve Single, http://www.bourns.com/docs/Product-Datasheets/ptv09.pdf")
    (tags "Potentiometer vertical  Omeg PC16PU  Omeg PC16PU  Omeg PC16PU  Vishay/Spectrol 248GJ/249GJ Single  Vishay/Spectrol 248GJ/249GJ Single  Vishay/Spectrol 248GJ/249GJ Single  Vishay/Spectrol 248GH/249GH Single  Vishay/Spectrol 148/149 Single  Vishay/Spectrol 148/149 Single  Vishay/Spectrol 148/149 Single  Vishay/Spectrol 148A/149A Single with mounting plates  Vishay/Spectrol 148/149 Double  Vishay/Spectrol 148A/149A Double with mounting plates  Piher PC-16 Single  Piher PC-16 Single  Piher PC-16 Single  Piher PC-16SV Single  Piher PC-16 Double  Piher PC-16 Triple  Piher T16H Single  Piher T16L Single  Piher T16H Double  Alps RK163 Single  Alps RK163 Double  Alps RK097 Single  Alps RK097 Double  Bourns PTV09A-2 Single with mounting sleve Single")
    (fp_text reference RV1 (at 0 11.05 270) (layer B.SilkS))
    (fp_text value 10k (at 0 -6.05 270) (layer B.Fab))
    (pad 3 thru_hole circle (at 0 5 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 0 2.5 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 27 /led_ctrl))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 0 thru_hole circle (at -3.3 7.5 270) (size 4.6 4.6) (drill 2.3) (layers *.Cu *.Mask))
    (pad 0 thru_hole circle (at -3.3 -2.5 270) (size 4.6 4.6) (drill 2.3) (layers *.Cu *.Mask))
    (model Potentiometers.3dshapes/Potentiometer_Bourns_PTV09A-2_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_THT:SW_Tactile_SPST_Angled_PTS645Vx83-2LFS (layer B.Cu) (tedit 592CAFEF)
    (at 177.8 116.205)
    (descr "tactile switch SPST right angle, PTS645VL83-2 LFS")
    (tags "tactile switch SPST angled PTS645VL83-2 LFS C&K Button")
    (fp_text reference SW3 (at 2.25 -1.68) (layer B.SilkS))
    (fp_text value Reset (at 2.25 -5.38988) (layer B.Fab))
    (fp_text user %R (at 2.25 -1.68) (layer B.Fab))
    (pad "" thru_hole circle (at 5.76 -2.49) (size 2.1 2.1) (drill 1.3) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 4.5 0) (size 1.75 1.75) (drill 0.99) (layers *.Cu *.Mask)
      (net 30 /clk_rst))
    (pad 1 thru_hole circle (at 0 0) (size 1.75 1.75) (drill 0.99) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad "" thru_hole circle (at -1.25 -2.49) (size 2.1 2.1) (drill 1.3) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Buttons_Switches_THT.3dshapes/SW_Tactile_SPST_Angled_PTS645Vx83-2LFS.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_THT:SW_Tactile_SPST_Angled_PTS645Vx83-2LFS (layer B.Cu) (tedit 592CAFEF)
    (at 165.1 116.205)
    (descr "tactile switch SPST right angle, PTS645VL83-2 LFS")
    (tags "tactile switch SPST angled PTS645VL83-2 LFS C&K Button")
    (fp_text reference SW2 (at 2.25 -1.68) (layer B.SilkS))
    (fp_text value Start/stop (at 2.25 -5.38988) (layer B.Fab))
    (fp_text user %R (at 2.25 -1.68) (layer B.Fab))
    (pad "" thru_hole circle (at 5.76 -2.49) (size 2.1 2.1) (drill 1.3) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 4.5 0) (size 1.75 1.75) (drill 0.99) (layers *.Cu *.Mask)
      (net 29 /clk_st_stp))
    (pad 1 thru_hole circle (at 0 0) (size 1.75 1.75) (drill 0.99) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad "" thru_hole circle (at -1.25 -2.49) (size 2.1 2.1) (drill 1.3) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Buttons_Switches_THT.3dshapes/SW_Tactile_SPST_Angled_PTS645Vx83-2LFS.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_THT:SW_Tactile_SPST_Angled_PTS645Vx83-2LFS (layer B.Cu) (tedit 592CAFEF)
    (at 152.4 116.205)
    (descr "tactile switch SPST right angle, PTS645VL83-2 LFS")
    (tags "tactile switch SPST angled PTS645VL83-2 LFS C&K Button")
    (fp_text reference SW1 (at 2.25 -1.68) (layer B.SilkS))
    (fp_text value Mode (at 2.25 -5.38988) (layer B.Fab))
    (fp_text user %R (at 2.25 -1.68) (layer B.Fab))
    (pad "" thru_hole circle (at 5.76 -2.49) (size 2.1 2.1) (drill 1.3) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 4.5 0) (size 1.75 1.75) (drill 0.99) (layers *.Cu *.Mask)
      (net 28 /clk_mode))
    (pad 1 thru_hole circle (at 0 0) (size 1.75 1.75) (drill 0.99) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad "" thru_hole circle (at -1.25 -2.49) (size 2.1 2.1) (drill 1.3) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Buttons_Switches_THT.3dshapes/SW_Tactile_SPST_Angled_PTS645Vx83-2LFS.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-8_W7.62mm placed (layer F.Cu) (tedit 59C78D6B)
    (at 193.04 101.6 180)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U1 (at 3.81 -2.33) (layer F.SilkS))
    (fp_text value DS1307N+ (at 3.81 9.95) (layer F.Fab))
    (fp_text user %R (at 3.81 3.81) (layer F.Fab))
    (pad 8 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 7 thru_hole oval (at 7.62 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 70 "Net-(U1-Pad7)"))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +BATT))
    (pad 6 thru_hole oval (at 7.62 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 /HV_SCL))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 "Net-(U1-Pad2)"))
    (pad 5 thru_hole oval (at 7.62 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 /HV_SDA))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 "Net-(U1-Pad1)"))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-8_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58AA84A8)
    (at 187.96 100.33 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at 0 1.75 90) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 1.75 90) (layer B.Fab))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 3 VCC))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystals:Crystal_SMD_MicroCrystal_MS3V-T1R placed (layer B.Cu) (tedit 58CD2E9D)
    (at 190.5 105.41 90)
    (descr "SMD Watch Crystal MicroCrystal MS3V-T1R 5.2mm length 1.4mm diameter http://www.microcrystal.com/images/_Product-Documentation/03_TF_metal_Packages/01_Datasheet/MS3V-T1R.pdf")
    (tags ['MS3V-T1R'])
    (attr smd)
    (fp_text reference Y1 (at -2.07 0.704167 180) (layer B.SilkS))
    (fp_text value 32.768kHz/12.5pF (at 2.07 0.704167 180) (layer B.Fab))
    (fp_text user %R (at 0 -1.333333 90) (layer B.Fab))
    (pad 3 smd rect (at 0 -3.733333 90) (size 1.5 2.4) (layers B.Cu B.Paste B.Mask))
    (pad 2 smd rect (at 0.5 1.866667 90) (size 0.6 1.1) (layers B.Cu B.Paste B.Mask)
      (net 31 "Net-(U1-Pad1)"))
    (pad 1 smd rect (at -0.5 1.866667 90) (size 0.6 1.1) (layers B.Cu B.Paste B.Mask)
      (net 32 "Net-(U1-Pad2)"))
    (model ${KISYS3DMOD}/Crystals.3dshapes/Crystal_SMD_MicroCrystal_MS3V-T1R.wrl
      (offset (xyz 0 -0.9333333187027397 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-28_W7.62mm_Socket (layer F.Cu) (tedit 59C78D6B)
    (at 180.34 101.6 270)
    (descr "28-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket")
    (fp_text reference U5 (at 3.81 -2.33 90) (layer F.SilkS))
    (fp_text value ATmega328P-PU (at 3.81 35.35 90) (layer F.Fab))
    (fp_text user %R (at 3.81 16.51 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 77 /RESET))
    (pad 15 thru_hole oval (at 7.62 33.02 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 /pwm_red))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 /RX))
    (pad 16 thru_hole oval (at 7.62 30.48 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 /pwm_grn))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 /TX))
    (pad 17 thru_hole oval (at 7.62 27.94 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 /pwm_blu))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 /clk_rst))
    (pad 18 thru_hole oval (at 7.62 25.4 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 /disp_clk))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 /clk_st_stp))
    (pad 19 thru_hole oval (at 7.62 22.86 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 /disp_data))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 /clk_mode))
    (pad 20 thru_hole oval (at 7.62 20.32 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 21 thru_hole oval (at 7.62 17.78 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 8 thru_hole oval (at 0 17.78 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 22 thru_hole oval (at 7.62 15.24 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 9 thru_hole oval (at 0 20.32 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 /Atmega328P/XTAL1))
    (pad 23 thru_hole oval (at 7.62 12.7 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 /AD0))
    (pad 10 thru_hole oval (at 0 22.86 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 /Atmega328P/XTAL2))
    (pad 24 thru_hole oval (at 7.62 10.16 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 /AD1))
    (pad 11 thru_hole oval (at 0 25.4 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 /disp_latch))
    (pad 25 thru_hole oval (at 7.62 7.62 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 /AD2))
    (pad 12 thru_hole oval (at 0 27.94 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 /19b_B))
    (pad 26 thru_hole oval (at 7.62 5.08 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 /led_ctrl))
    (pad 13 thru_hole oval (at 0 30.48 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 /19b_C))
    (pad 27 thru_hole oval (at 7.62 2.54 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 /HV_SDA))
    (pad 14 thru_hole oval (at 0 33.02 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 /19b_D))
    (pad 28 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 /HV_SCL))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-28_W7.62mm_Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlocks_Phoenix:TerminalBlock_Phoenix_PT-3.5mm_2pol (layer F.Cu) (tedit 59FF0756)
    (at 99.06 114.3)
    (descr "2-way 3.5mm pitch terminal block, Phoenix PT series")
    (fp_text reference J5 (at 1.75 -4.3) (layer F.SilkS))
    (fp_text value Screw_Terminal_01x02 (at 1.75 6) (layer F.Fab))
    (fp_text user %R (at 1.75 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 3.5 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 10 "Net-(D1-Pad1)"))
    (pad 1 thru_hole rect (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 4 +VDC))
    (model ${KISYS3DMOD}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_PT-3.5mm_2pol.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlocks_Phoenix:TerminalBlock_Phoenix_PT-3.5mm_8pol (layer F.Cu) (tedit 59FF0756)
    (at 190.5 81.28 180)
    (descr "8-way 3.5mm pitch terminal block, Phoenix PT series")
    (fp_text reference J3 (at 27.94 0 90) (layer F.SilkS))
    (fp_text value Screw_Terminal_01x08 (at 12.25 6) (layer F.Fab))
    (fp_text user %R (at 12.25 0) (layer F.Fab))
    (pad 3 thru_hole circle (at 7 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 77 /RESET))
    (pad 2 thru_hole circle (at 3.5 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole circle (at 10.5 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 14 /RX))
    (pad 5 thru_hole circle (at 14 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 15 /TX))
    (pad 6 thru_hole circle (at 17.5 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 18 /AD2))
    (pad 7 thru_hole circle (at 21 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 17 /AD1))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 8 thru_hole circle (at 24.5 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 16 /AD0))
    (model ${KISYS3DMOD}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_PT-3.5mm_8pol.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:CP_Radial_D10.0mm_P5.00mm (layer B.Cu) (tedit 597BC7C2)
    (at 64.77 86.36 270)
    (descr "CP, Radial series, Radial, pin pitch=5.00mm, , diameter=10mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 5.00mm  diameter 10mm Electrolytic Capacitor")
    (fp_text reference C10 (at 2.5 6.31 270) (layer B.SilkS))
    (fp_text value 10uF/300V (at 2.5 -6.31 270) (layer B.Fab))
    (fp_text user %R (at 2.5 0 270) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 6 "/Power Supplies/HV"))
    (pad 2 thru_hole circle (at 5 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D10.0mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1210_HandSoldering (layer F.Cu) (tedit 58AA84FB)
    (at 62.23 80.55 90)
    (descr "Capacitor SMD 1210, hand soldering")
    (tags "capacitor 1210")
    (attr smd)
    (fp_text reference C1 (at 0 -2.25 270) (layer F.SilkS))
    (fp_text value 0.1uF/300V (at 0 2.5 270) (layer F.Fab))
    (fp_text user %R (at 0 -2.25 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 6 "/Power Supplies/HV"))
    (pad 2 smd rect (at 2 0 90) (size 2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:TO-252-2 placed (layer F.Cu) (tedit 590079C0)
    (at 199.39 82.55 90)
    (descr "TO-252 / DPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO252/PG-TO252-3-1/")
    (tags "DPAK TO-252 DPAK-3 TO-252-3 SOT-428")
    (attr smd)
    (fp_text reference U4 (at -6.35 0) (layer F.SilkS))
    (fp_text value LF33_TO252 (at 0 4.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -4.2 -2.28 90) (size 2.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 3 smd rect (at -4.2 2.28 90) (size 2.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 7 +3V3))
    (pad 2 smd rect (at 2.1 0 90) (size 6.4 5.8) (layers F.Cu F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 3.775 1.525 90) (size 3.05 2.75) (layers F.Cu F.Paste)
      (net 2 GND))
    (pad 2 smd rect (at 0.425 -1.525 90) (size 3.05 2.75) (layers F.Cu F.Paste)
      (net 2 GND))
    (pad 2 smd rect (at 3.775 -1.525 90) (size 3.05 2.75) (layers F.Cu F.Paste)
      (net 2 GND))
    (pad 2 smd rect (at 0.425 1.525 90) (size 3.05 2.75) (layers F.Cu F.Paste)
      (net 2 GND))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/TO-252-2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module clock-bottom-footprints:Keystone_3000_1x12mm-CoinCell (layer B.Cu) (tedit 5D54A50D)
    (at 205.74 97.79 270)
    (descr http://www.keyelco.com/product-pdf.cfm?p=777)
    (tags "Keystone type 3000 coin cell retainer")
    (attr smd)
    (fp_text reference BT1 (at 0 8 90) (layer B.SilkS))
    (fp_text value CR1225 (at 0 -7.5 90) (layer B.Fab))
    (pad 2 smd rect (at 0 0 270) (size 4 4) (layers B.Cu B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 7.9 0 270) (size 3.5 3.3) (layers B.Cu B.Paste B.Mask)
      (net 1 +BATT))
    (pad 1 smd rect (at -7.9 0 270) (size 3.5 3.3) (layers B.Cu B.Paste B.Mask)
      (net 1 +BATT))
    (model Battery_Holders.3dshapes/Keystone_3000_1x12mm-CoinCell.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-16_3.9x9.9mm_Pitch1.27mm (layer F.Cu) (tedit 58CC8F64)
    (at 132.08 87.63 270)
    (descr "16-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U8 (at 5.08 3.81 180) (layer F.SilkS))
    (fp_text value 74HC595 (at 0 6 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -4.445 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 62 "/Tube Control Registers/s1"))
    (pad 2 smd rect (at -2.7 -3.175 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 61 "/Tube Control Registers/s2"))
    (pad 3 smd rect (at -2.7 -1.905 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 60 "/Tube Control Registers/s3"))
    (pad 4 smd rect (at -2.7 -0.635 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 59 "/Tube Control Registers/s4"))
    (pad 5 smd rect (at -2.7 0.635 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 58 "/Tube Control Registers/s5"))
    (pad 6 smd rect (at -2.7 1.905 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 57 "/Tube Control Registers/s6"))
    (pad 7 smd rect (at -2.7 3.175 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 56 "/Tube Control Registers/s7"))
    (pad 8 smd rect (at -2.7 4.445 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 9 smd rect (at 2.7 4.445 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 73 "Net-(U7-Pad14)"))
    (pad 10 smd rect (at 2.7 3.175 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 11 smd rect (at 2.7 1.905 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 /disp_clk))
    (pad 12 smd rect (at 2.7 0.635 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 36 /disp_latch))
    (pad 13 smd rect (at 2.7 -0.635 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 14 smd rect (at 2.7 -1.905 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 74 "Net-(U8-Pad14)"))
    (pad 15 smd rect (at 2.7 -3.175 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 63 "/Tube Control Registers/s0"))
    (pad 16 smd rect (at 2.7 -4.445 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-16_3.9x9.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-16_3.9x9.9mm_Pitch1.27mm (layer F.Cu) (tedit 58CC8F64)
    (at 120.65 87.63 270)
    (descr "16-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U7 (at 5.08 3.81 180) (layer F.SilkS))
    (fp_text value 74HC595 (at 0 6 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -4.445 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 54 "/Tube Control Registers/m1"))
    (pad 2 smd rect (at -2.7 -3.175 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 53 "/Tube Control Registers/m2"))
    (pad 3 smd rect (at -2.7 -1.905 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 52 "/Tube Control Registers/m3"))
    (pad 4 smd rect (at -2.7 -0.635 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 51 "/Tube Control Registers/m4"))
    (pad 5 smd rect (at -2.7 0.635 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 50 "/Tube Control Registers/m5"))
    (pad 6 smd rect (at -2.7 1.905 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 49 "/Tube Control Registers/m6"))
    (pad 7 smd rect (at -2.7 3.175 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 48 "/Tube Control Registers/m7"))
    (pad 8 smd rect (at -2.7 4.445 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 9 smd rect (at 2.7 4.445 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 72 "Net-(U6-Pad14)"))
    (pad 10 smd rect (at 2.7 3.175 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 11 smd rect (at 2.7 1.905 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 /disp_clk))
    (pad 12 smd rect (at 2.7 0.635 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 36 /disp_latch))
    (pad 13 smd rect (at 2.7 -0.635 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 14 smd rect (at 2.7 -1.905 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 73 "Net-(U7-Pad14)"))
    (pad 15 smd rect (at 2.7 -3.175 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 55 "/Tube Control Registers/m0"))
    (pad 16 smd rect (at 2.7 -4.445 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-16_3.9x9.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 58CE4E7E)
    (at 196.85 92.71 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q3 (at 0 -2.5) (layer F.SilkS))
    (fp_text value BSS138 (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 7 +3V3))
    (pad 2 smd rect (at -1 0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 22 "/Qwiic Ports/LV_SDA"))
    (pad 3 smd rect (at 1 0 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 25 /HV_SDA))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58AA84A8)
    (at 150.475 88.265)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C19 (at 0 -1.905 180) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.75 180) (layer B.Fab))
    (fp_text user %R (at 0 1.75 180) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_THT:D_DO-41_SOD81_P10.16mm_Horizontal (layer F.Cu) (tedit 5921392F)
    (at 72.39 92.71)
    (descr "D, DO-41_SOD81 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "D DO-41_SOD81 series Axial Horizontal pin pitch 10.16mm  length 5.2mm diameter 2.7mm")
    (fp_text reference D2 (at 5.08 -2.41) (layer F.SilkS))
    (fp_text value SB140 (at 5.08 2.41) (layer F.Fab))
    (fp_text user %R (at 5.08 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 11 "Net-(D2-Pad1)"))
    (pad 2 thru_hole oval (at 10.16 0) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 12 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/Diodes_THT.3dshapes/D_DO-41_SOD81_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:CP_Radial_D10.0mm_P5.00mm (layer B.Cu) (tedit 597BC7C2)
    (at 97.79 104.14 90)
    (descr "CP, Radial series, Radial, pin pitch=5.00mm, , diameter=10mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 5.00mm  diameter 10mm Electrolytic Capacitor")
    (fp_text reference C4 (at -2.54 5.08 180) (layer B.SilkS))
    (fp_text value 470uF (at 2.5 -6.31 270) (layer B.Fab))
    (fp_text user %R (at 2.5 0 270) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 4 +VDC))
    (pad 2 thru_hole circle (at 5 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D10.0mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:CP_Radial_D6.3mm_P2.50mm placed (layer B.Cu) (tedit 597BC7C2)
    (at 110.49 105.41 180)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=6.3mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 6.3mm Electrolytic Capacitor")
    (fp_text reference C8 (at 5.715 0 270) (layer B.SilkS))
    (fp_text value 47uF (at 1.25 -4.46) (layer B.Fab))
    (fp_text user %R (at 1.25 0) (layer B.Fab))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 +VDC))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D6.3mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystals:Crystal_HC49-U_Vertical (layer F.Cu) (tedit 58CD2E9C)
    (at 158.75 96.52)
    (descr "Crystal THT HC-49/U http://5hertz.com/pdfs/04404_D.pdf")
    (tags "THT crystalHC-49/U")
    (fp_text reference Y2 (at 2.44 -3.525) (layer F.SilkS))
    (fp_text value "16 MHz" (at 2.44 3.525) (layer F.Fab))
    (fp_text user %R (at 2.44 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 /Atmega328P/XTAL2))
    (pad 2 thru_hole circle (at 4.88 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 /Atmega328P/XTAL1))
    (model ${KISYS3DMOD}/Crystals.3dshapes/Crystal_HC49-U_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58AA84A8)
    (at 165.08 93.98 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C13 (at 0 1.75) (layer B.SilkS))
    (fp_text value 22pF (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 1.75) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 8 /Atmega328P/XTAL1))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58AA84A8)
    (at 160.02 93.98 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C14 (at 0 1.75 180) (layer B.SilkS))
    (fp_text value 22pF (at 0 -1.75 180) (layer B.Fab))
    (fp_text user %R (at 0 1.75 180) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 9 /Atmega328P/XTAL2))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 181.61 93.98 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R6 (at 3.81 0 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 77 /RESET))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58AA84A8)
    (at 163.83 106.68)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C12 (at 0 -2.032) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 1.75) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 205.74 86.36)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C11 (at 0 -1.75) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 7 +3V3))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58AA84A8)
    (at 138.43 115.57 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at 0 1.75 270) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 1.75 270) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58AA84A8)
    (at 144.78 86.34 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C16 (at 0 -1.905 90) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 1.75 270) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x03_Pitch2.54mm locked (layer F.Cu) (tedit 59650532)
    (at 147.32 114.3 270)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (fp_text reference J2 (at 1.27 7.62 90) (layer F.SilkS))
    (fp_text value Conn_02x03_Odd_Even (at 1.27 7.41 90) (layer F.Fab))
    (fp_text user %R (at 1.27 2.54) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /pwm_blu))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 /pwm_grn))
    (pad 4 thru_hole oval (at 2.54 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 5 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /pwm_red))
    (pad 6 thru_hole oval (at 2.54 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 VCC))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58AA84A8)
    (at 86.36 100.33)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C7 (at 0 -1.905) (layer B.SilkS))
    (fp_text value 1nF (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 1.75) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 38 "Net-(C7-Pad1)"))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 80.01 101.6 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C5 (at 0 -1.75 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +VDC))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58AA84A8)
    (at 87.63 104.14 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C6 (at 0 1.75 270) (layer B.SilkS))
    (fp_text value 1nF (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 1.75 270) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(C6-Pad1)"))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-16_3.9x9.9mm_Pitch1.27mm (layer F.Cu) (tedit 58CC8F64)
    (at 152.4 87.63 270)
    (descr "16-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U9 (at 5.08 3.81 180) (layer F.SilkS))
    (fp_text value 74HC595 (at 0 6 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -4.445 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 75 "Net-(U9-Pad1)"))
    (pad 2 smd rect (at -2.7 -3.175 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 69 "/Tube Control Registers/d6"))
    (pad 3 smd rect (at -2.7 -1.905 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 68 "/Tube Control Registers/d5"))
    (pad 4 smd rect (at -2.7 -0.635 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 67 "/Tube Control Registers/d4"))
    (pad 5 smd rect (at -2.7 0.635 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 66 "/Tube Control Registers/d3"))
    (pad 6 smd rect (at -2.7 1.905 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 65 "/Tube Control Registers/d2"))
    (pad 7 smd rect (at -2.7 3.175 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 64 "/Tube Control Registers/d1"))
    (pad 8 smd rect (at -2.7 4.445 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 9 smd rect (at 2.7 4.445 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 74 "Net-(U8-Pad14)"))
    (pad 10 smd rect (at 2.7 3.175 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 11 smd rect (at 2.7 1.905 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 /disp_clk))
    (pad 12 smd rect (at 2.7 0.635 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 36 /disp_latch))
    (pad 13 smd rect (at 2.7 -0.635 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 14 smd rect (at 2.7 -1.905 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 37 /disp_data))
    (pad 15 smd rect (at 2.7 -3.175 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 76 "Net-(U9-Pad15)"))
    (pad 16 smd rect (at 2.7 -4.445 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-16_3.9x9.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x06_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 66.04 78.74 90)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (fp_text reference J1 (at 0 15.24 90) (layer F.SilkS))
    (fp_text value Conn_01x06_Female (at 0 15.03 90) (layer F.Fab))
    (fp_text user %R (at 0 6.35) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "/Power Supplies/HV"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "/Power Supplies/HV"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "/Power Supplies/HV"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x06_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58AA84A8)
    (at 130.155 88.265)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C18 (at 0 1.75) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 1.75) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58AA84A8)
    (at 118.745 88.265)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C17 (at 0 1.75) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 1.75) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58AA84A8)
    (at 107.315 88.265)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C15 (at 0 1.75) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 1.75) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Potentiometers:Potentiometer_Trimmer_Bourns_3339P_Horizontal (layer F.Cu) (tedit 58826FD6)
    (at 86.36 83.82)
    (descr "Potentiometer, horizontally mounted, Omeg PC16PU, Omeg PC16PU, Omeg PC16PU, Vishay/Spectrol 248GJ/249GJ Single, Vishay/Spectrol 248GJ/249GJ Single, Vishay/Spectrol 248GJ/249GJ Single, Vishay/Spectrol 248GH/249GH Single, Vishay/Spectrol 148/149 Single, Vishay/Spectrol 148/149 Single, Vishay/Spectrol 148/149 Single, Vishay/Spectrol 148A/149A Single with mounting plates, Vishay/Spectrol 148/149 Double, Vishay/Spectrol 148A/149A Double with mounting plates, Piher PC-16 Single, Piher PC-16 Single, Piher PC-16 Single, Piher PC-16SV Single, Piher PC-16 Double, Piher PC-16 Triple, Piher T16H Single, Piher T16L Single, Piher T16H Double, Alps RK163 Single, Alps RK163 Double, Alps RK097 Single, Alps RK097 Double, Bourns PTV09A-2 Single with mounting sleve Single, Bourns PTV09A-1 with mounting sleve Single, Bourns PRS11S Single, Alps RK09K Single with mounting sleve Single, Alps RK09K with mounting sleve Single, Alps RK09L Single, Alps RK09L Single, Alps RK09L Double, Alps RK09L Double, Alps RK09Y Single, Bourns 3339S Single, Bourns 3339S Single, Bourns 3339P Single, http://www.alps.com/prod/info/E/HTML/Potentiometer/RotaryPotentiometers/RK09Y11/RK09Y11L0001.html")
    (tags "Potentiometer horizontal  Omeg PC16PU  Omeg PC16PU  Omeg PC16PU  Vishay/Spectrol 248GJ/249GJ Single  Vishay/Spectrol 248GJ/249GJ Single  Vishay/Spectrol 248GJ/249GJ Single  Vishay/Spectrol 248GH/249GH Single  Vishay/Spectrol 148/149 Single  Vishay/Spectrol 148/149 Single  Vishay/Spectrol 148/149 Single  Vishay/Spectrol 148A/149A Single with mounting plates  Vishay/Spectrol 148/149 Double  Vishay/Spectrol 148A/149A Double with mounting plates  Piher PC-16 Single  Piher PC-16 Single  Piher PC-16 Single  Piher PC-16SV Single  Piher PC-16 Double  Piher PC-16 Triple  Piher T16H Single  Piher T16L Single  Piher T16H Double  Alps RK163 Single  Alps RK163 Double  Alps RK097 Single  Alps RK097 Double  Bourns PTV09A-2 Single with mounting sleve Single  Bourns PTV09A-1 with mounting sleve Single  Bourns PRS11S Single  Alps RK09K Single with mounting sleve Single  Alps RK09K with mounting sleve Single  Alps RK09L Single  Alps RK09L Single  Alps RK09L Double  Alps RK09L Double  Alps RK09Y Single  Bourns 3339S Single  Bourns 3339S Single  Bourns 3339P Single")
    (fp_text reference R5 (at 0 -2.54) (layer F.SilkS))
    (fp_text value 2k (at 0 2.52) (layer F.Fab))
    (pad 3 thru_hole circle (at 0 -5.08) (size 1.26 1.26) (drill 0.7) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at -2.54 -2.54) (size 1.26 1.26) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at 0 0) (size 1.26 1.26) (drill 0.7) (layers *.Cu *.Mask)
      (net 79 "Net-(R4-Pad2)"))
    (model Potentiometers.3dshapes/Potentiometer_Trimmer_Bourns_3339P_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Housings_SOIC:SOIC-16_3.9x9.9mm_Pitch1.27mm (layer F.Cu) (tedit 58CC8F64)
    (at 109.22 87.63 270)
    (descr "16-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U6 (at 5.08 3.81 180) (layer F.SilkS))
    (fp_text value 74HC595 (at 0 6 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -4.445 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 46 "/Tube Control Registers/h1"))
    (pad 2 smd rect (at -2.7 -3.175 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 45 "/Tube Control Registers/h2"))
    (pad 3 smd rect (at -2.7 -1.905 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 44 "/Tube Control Registers/h3"))
    (pad 4 smd rect (at -2.7 -0.635 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 43 "/Tube Control Registers/h4"))
    (pad 5 smd rect (at -2.7 0.635 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 42 "/Tube Control Registers/h5"))
    (pad 6 smd rect (at -2.7 1.905 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 41 "/Tube Control Registers/h6"))
    (pad 7 smd rect (at -2.7 3.175 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 40 "/Tube Control Registers/h7"))
    (pad 8 smd rect (at -2.7 4.445 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 9 smd rect (at 2.7 4.445 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 71 "Net-(U6-Pad9)"))
    (pad 10 smd rect (at 2.7 3.175 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 11 smd rect (at 2.7 1.905 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 /disp_clk))
    (pad 12 smd rect (at 2.7 0.635 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 36 /disp_latch))
    (pad 13 smd rect (at 2.7 -0.635 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 14 smd rect (at 2.7 -1.905 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 72 "Net-(U6-Pad14)"))
    (pad 15 smd rect (at 2.7 -3.175 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 47 "/Tube Control Registers/h0"))
    (pad 16 smd rect (at 2.7 -4.445 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-16_3.9x9.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x20_Pitch2.54mm locked (layer F.Cu) (tedit 59650533)
    (at 106.68 81.28 90)
    (descr "Through hole straight pin header, 2x20, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x20 2.54mm double row")
    (fp_text reference J8 (at 1.27 -2.33 90) (layer F.SilkS))
    (fp_text value Conn_02x20_Odd_Even (at 1.27 50.59 90) (layer F.Fab))
    (fp_text user %R (at 1.27 24.13) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 "/Tube Control Registers/h7"))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 "/Tube Control Registers/h6"))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 "/Tube Control Registers/h5"))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 "/Tube Control Registers/h4"))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 "/Tube Control Registers/h3"))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 "/Tube Control Registers/h2"))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 "/Tube Control Registers/h1"))
    (pad 8 thru_hole oval (at 2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 "/Tube Control Registers/h0"))
    (pad 9 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 48 "/Tube Control Registers/m7"))
    (pad 10 thru_hole oval (at 2.54 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 "/Tube Control Registers/m6"))
    (pad 11 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 50 "/Tube Control Registers/m5"))
    (pad 12 thru_hole oval (at 2.54 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 51 "/Tube Control Registers/m4"))
    (pad 13 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 52 "/Tube Control Registers/m3"))
    (pad 14 thru_hole oval (at 2.54 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 53 "/Tube Control Registers/m2"))
    (pad 15 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 54 "/Tube Control Registers/m1"))
    (pad 16 thru_hole oval (at 2.54 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 55 "/Tube Control Registers/m0"))
    (pad 17 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 18 thru_hole oval (at 2.54 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 19 thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 56 "/Tube Control Registers/s7"))
    (pad 20 thru_hole oval (at 2.54 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 57 "/Tube Control Registers/s6"))
    (pad 21 thru_hole oval (at 0 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 58 "/Tube Control Registers/s5"))
    (pad 22 thru_hole oval (at 2.54 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 59 "/Tube Control Registers/s4"))
    (pad 23 thru_hole oval (at 0 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 60 "/Tube Control Registers/s3"))
    (pad 24 thru_hole oval (at 2.54 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 61 "/Tube Control Registers/s2"))
    (pad 25 thru_hole oval (at 0 30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 62 "/Tube Control Registers/s1"))
    (pad 26 thru_hole oval (at 2.54 30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 63 "/Tube Control Registers/s0"))
    (pad 27 thru_hole oval (at 0 33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 /19b_D))
    (pad 28 thru_hole oval (at 2.54 33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 /19b_C))
    (pad 29 thru_hole oval (at 0 35.56 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 /19b_B))
    (pad 30 thru_hole oval (at 2.54 35.56 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 31 thru_hole oval (at 0 38.1 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 32 thru_hole oval (at 2.54 38.1 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 33 thru_hole oval (at 0 40.64 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 34 thru_hole oval (at 2.54 40.64 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 35 thru_hole oval (at 0 43.18 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 64 "/Tube Control Registers/d1"))
    (pad 36 thru_hole oval (at 2.54 43.18 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 65 "/Tube Control Registers/d2"))
    (pad 37 thru_hole oval (at 0 45.72 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 66 "/Tube Control Registers/d3"))
    (pad 38 thru_hole oval (at 2.54 45.72 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 67 "/Tube Control Registers/d4"))
    (pad 39 thru_hole oval (at 0 48.26 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 68 "/Tube Control Registers/d5"))
    (pad 40 thru_hole oval (at 2.54 48.26 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 69 "/Tube Control Registers/d6"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x20_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering placed (layer F.Cu) (tedit 58E0A804)
    (at 201.93 102.95 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R10 (at 0 -1.7 90) (layer F.SilkS))
    (fp_text value 10k (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 7 +3V3))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 23 "/Qwiic Ports/LV_SCL"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering placed (layer F.Cu) (tedit 58E0A804)
    (at 201.93 92.71 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R9 (at -0.08 -1.7 90) (layer F.SilkS))
    (fp_text value 10k (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 7 +3V3))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 22 "/Qwiic Ports/LV_SDA"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering placed (layer F.Cu) (tedit 58E0A804)
    (at 184.785 109.22 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R8 (at 0 1.905 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 26 /HV_SCL))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering placed (layer F.Cu) (tedit 58E0A804)
    (at 184.15 91.36)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R7 (at -3.81 0.08 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 25 /HV_SDA))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-220-3_Horizontal (layer B.Cu) (tedit 58CE52AD)
    (at 115.57 102.87 90)
    (descr "TO-220-3, Horizontal, RM 2.54mm")
    (tags "TO-220-3 Horizontal RM 2.54mm")
    (fp_text reference U3 (at 2.54 20.58 270) (layer B.SilkS))
    (fp_text value L7805 (at 2.54 -1.9 270) (layer B.Fab))
    (fp_text user %R (at 2.54 20.58 270) (layer B.Fab))
    (pad 0 np_thru_hole oval (at 2.54 16.66 90) (size 3.5 3.5) (drill 3.5) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 4 +VDC))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole oval (at 5.08 0 90) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 3 VCC))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-220-3_Horizontal.wrl
      (offset (xyz 2.539999961853027 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-8_W7.62mm (layer F.Cu) (tedit 59C78D6B)
    (at 90.17 107.95 180)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U2 (at 3.81 -2.33) (layer F.SilkS))
    (fp_text value MC34063AP (at 3.81 9.95) (layer F.Fab))
    (fp_text user %R (at 3.81 3.81) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(L1-Pad1)"))
    (pad 5 thru_hole oval (at 7.62 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 "Net-(C7-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(D2-Pad2)"))
    (pad 6 thru_hole oval (at 7.62 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 +VDC))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(C6-Pad1)"))
    (pad 7 thru_hole oval (at 7.62 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(L1-Pad1)"))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 8 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(L1-Pad1)"))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-8_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 82.55 88.9)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R4 (at 3.81 -2.31) (layer F.SilkS))
    (fp_text value 3k3 (at 3.81 2.31) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 "Net-(C7-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 79 "Net-(R4-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 72.39 85.09)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R3 (at 3.81 2.54) (layer F.SilkS))
    (fp_text value 560k (at 3.81 2.31) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "/Power Supplies/HV"))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 "Net-(C7-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 93.98 113.03 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R2 (at 3.81 0) (layer F.SilkS))
    (fp_text value 1k (at 3.81 2.31) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(D2-Pad2)"))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 72.39 116.84)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (fp_text reference R1 (at 6.35 0) (layer F.SilkS))
    (fp_text value 0R1/0.5W (at 6.35 2.66) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(L1-Pad1)"))
    (pad 2 thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 +VDC))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 placed (layer F.Cu) (tedit 58CE4E7E)
    (at 198.12 100.33 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q4 (at 0 2.54) (layer F.SilkS))
    (fp_text value BSS138 (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 7 +3V3))
    (pad 2 smd rect (at -1 0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 23 "/Qwiic Ports/LV_SCL"))
    (pad 3 smd rect (at 1 0 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 26 /HV_SCL))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-220-3_Horizontal (layer F.Cu) (tedit 58CE52AD)
    (at 68.58 97.79 180)
    (descr "TO-220-3, Horizontal, RM 2.54mm")
    (tags "TO-220-3 Horizontal RM 2.54mm")
    (fp_text reference Q2 (at 2.54 -20.58) (layer F.SilkS))
    (fp_text value IRF640N (at 2.54 1.9) (layer F.Fab))
    (fp_text user %R (at 2.54 -20.58) (layer F.Fab))
    (pad 3 thru_hole oval (at 5.08 0 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(D2-Pad1)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 78 "Net-(D3-Pad2)"))
    (pad 0 np_thru_hole oval (at 2.54 -16.66 180) (size 3.5 3.5) (drill 3.5) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-220-3_Horizontal.wrl
      (offset (xyz 2.539999961853027 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-92_Inline_Wide (layer F.Cu) (tedit 58CE52AF)
    (at 74.93 101.6 90)
    (descr "TO-92 leads in-line, wide, drill 0.8mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q1 (at 2.54 -3.56 270) (layer F.SilkS))
    (fp_text value BC516 (at 2.54 2.79 90) (layer F.Fab))
    (fp_text user %R (at 2.54 -3.56 270) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.52 1.52) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(D2-Pad2)"))
    (pad 3 thru_hole circle (at 5.08 0 180) (size 1.52 1.52) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(D2-Pad1)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.52 1.52) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-92_Inline_Wide.wrl
      (offset (xyz 2.539999961853027 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Inductors_THT:L_Radial_D8.7mm_P5.00mm_Fastron_07HCP (layer B.Cu) (tedit 587E3FCE)
    (at 78.74 109.22 180)
    (descr "L, Radial series, Radial, pin pitch=5.00mm, , diameter=8.7mm, Fastron, 07HCP, http://cdn-reichelt.de/documents/datenblatt/B400/DS_07HCP.pdf")
    (tags "L Radial series Radial pin pitch 5.00mm  diameter 8.7mm Fastron 07HCP")
    (fp_text reference L1 (at 2.54 2.54) (layer B.SilkS))
    (fp_text value 150uH (at 2.5 -5.41) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 24 "Net-(L1-Pad1)"))
    (pad 2 thru_hole circle (at 5 0 180) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 78 "Net-(D3-Pad2)"))
    (model Inductors_THT.3dshapes/L_Radial_D8.7mm_P5.00mm_Fastron_07HCP.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST:JST_SH_SM04B-SRSS-TB_04x1.00mm_Angled placed (layer F.Cu) (tedit 56B07436)
    (at 210.185 102.87 90)
    (descr http://www.jst-mfg.com/product/pdf/eng/eSH.pdf)
    (tags "connector jst sh")
    (attr smd)
    (fp_text reference J7 (at -1.5 -4 90) (layer F.SilkS))
    (fp_text value "Qwiic right angle" (at 0 4.5 90) (layer F.Fab))
    (pad 1 smd rect (at -1.5 -1.9375 90) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -0.5 -1.9375 90) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 7 +3V3))
    (pad 3 smd rect (at 0.5 -1.9375 90) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 22 "/Qwiic Ports/LV_SDA"))
    (pad 4 smd rect (at 1.5 -1.9375 90) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 23 "/Qwiic Ports/LV_SCL"))
    (pad "" smd rect (at -2.8 1.9375 90) (size 1.2 1.8) (layers F.Cu F.Paste F.Mask))
    (pad "" smd rect (at 2.8 1.9375 90) (size 1.2 1.8) (layers F.Cu F.Paste F.Mask))
  )
  (module Connectors_JST:JST_SH_SM04B-SRSS-TB_04x1.00mm_Angled placed (layer F.Cu) (tedit 56B07436)
    (at 210.185 92.71 90)
    (descr http://www.jst-mfg.com/product/pdf/eng/eSH.pdf)
    (tags "connector jst sh")
    (attr smd)
    (fp_text reference J6 (at -1.5 -4 90) (layer F.SilkS))
    (fp_text value "Qwiic right angle" (at 0 4.5 90) (layer F.Fab))
    (pad 1 smd rect (at -1.5 -1.9375 90) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -0.5 -1.9375 90) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 7 +3V3))
    (pad 3 smd rect (at 0.5 -1.9375 90) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 22 "/Qwiic Ports/LV_SDA"))
    (pad 4 smd rect (at 1.5 -1.9375 90) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 23 "/Qwiic Ports/LV_SCL"))
    (pad "" smd rect (at -2.8 1.9375 90) (size 1.2 1.8) (layers F.Cu F.Paste F.Mask))
    (pad "" smd rect (at 2.8 1.9375 90) (size 1.2 1.8) (layers F.Cu F.Paste F.Mask))
  )
  (module Connectors:BARREL_JACK locked placed (layer F.Cu) (tedit 5861378E)
    (at 98.68 86.995 270)
    (descr "DC Barrel Jack")
    (tags "Power Jack")
    (fp_text reference J4 (at -8.45 5.75 270) (layer F.SilkS))
    (fp_text value Barrel_Jack_Switch (at -6.2 -5.5 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 3.5 3.5) (drill oval 1 3) (layers *.Cu *.Mask)
      (net 39 "Net-(D1-Pad2)"))
    (pad 2 thru_hole rect (at -6 0 270) (size 3.5 3.5) (drill oval 1 3) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole rect (at -3 4.7 270) (size 3.5 3.5) (drill oval 3 1) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module Diodes_THT:D_DO-201AD_P15.24mm_Horizontal (layer F.Cu) (tedit 5921392E)
    (at 55.88 88.9 270)
    (descr "D, DO-201AD series, Axial, Horizontal, pin pitch=15.24mm, , length*diameter=9.5*5.2mm^2, , http://www.diodes.com/_files/packages/DO-201AD.pdf")
    (tags "D DO-201AD series Axial Horizontal pin pitch 15.24mm  length 9.5mm diameter 5.2mm")
    (fp_text reference D3 (at 7.62 -3.66 90) (layer F.SilkS))
    (fp_text value "UF5408 (or UF4007)" (at 7.62 3.66 90) (layer F.Fab))
    (fp_text user %R (at 7.62 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 3.2 3.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 6 "/Power Supplies/HV"))
    (pad 2 thru_hole oval (at 15.24 0 270) (size 3.2 3.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 78 "Net-(D3-Pad2)"))
    (model ${KISYS3DMOD}/Diodes_THT.3dshapes/D_DO-201AD_P15.24mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_THT:D_DO-41_SOD81_P10.16mm_Horizontal placed (layer F.Cu) (tedit 5921392F)
    (at 101.6 92.71 180)
    (descr "D, DO-41_SOD81 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "D DO-41_SOD81 series Axial Horizontal pin pitch 10.16mm  length 5.2mm diameter 2.7mm")
    (fp_text reference D1 (at 5.08 -2.41) (layer F.SilkS))
    (fp_text value 1N4001 (at 5.08 2.41) (layer F.Fab))
    (fp_text user %R (at 5.08 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 10 "Net-(D1-Pad1)"))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 39 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Diodes_THT.3dshapes/D_DO-41_SOD81_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:CP_Radial_D6.3mm_P2.50mm (layer B.Cu) (tedit 597BC7C2)
    (at 110.49 97.79 180)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=6.3mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 6.3mm Electrolytic Capacitor")
    (fp_text reference C9 (at 5.715 0 90) (layer B.SilkS))
    (fp_text value 47uF (at 1.25 -4.46) (layer B.Fab))
    (fp_text user %R (at 1.25 0) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D6.3mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "DANGER!\nHigh voltages (<250Vdc)" (at 114.3 114.3) (layer F.SilkS))
  (gr_text A0 (at 166 85.09 90) (layer F.SilkS))
  (gr_text A1 (at 169.5 85.09 90) (layer F.SilkS))
  (gr_text A2 (at 173 85.09 90) (layer F.SilkS))
  (gr_text TX (at 176.5 85.09 90) (layer F.SilkS))
  (gr_text RX (at 180 85.09 90) (layer F.SilkS))
  (gr_text RESET (at 183.5 85.09 90) (layer F.SilkS))
  (gr_text GND (at 187 85.09 90) (layer F.SilkS))
  (gr_text 5V (at 190.5 85.09 90) (layer F.SilkS))
  (gr_text "Nixie Clock Bottom PCB, rev. 1\nTony Zhang, 2019 08 17" (at 114.3 109.22) (layer F.SilkS))
  (gr_line (start 213.36 119.38) (end 213.36 76.2) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 50.8 119.38) (end 213.36 119.38) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 50.8 76.2) (end 50.8 119.38) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 213.36 76.2) (end 50.8 76.2) (layer Edge.Cuts) (width 0.05))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 213.36 76.2) (xy 50.8 76.2) (xy 50.8 119.38) (xy 213.36 119.38)
      )
    )
  )
  (zone (net 3) (net_name VCC) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 213.36 109.22) (xy 213.36 119.38) (xy 193.04 119.38) (xy 193.04 109.22)
      )
    )
  )
  (zone (net 7) (net_name +3V3) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 213.36 76.2) (xy 194.31 76.2) (xy 194.31 107.95) (xy 213.36 107.95)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 101.6 76.2) (xy 50.8 76.2) (xy 50.8 119.38) (xy 101.6 119.38)
      )
    )
  )
  (zone (net 3) (net_name VCC) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 193.04 76.2) (xy 193.04 119.38) (xy 106.68 119.38) (xy 104.14 119.38) (xy 104.14 76.2)
      )
    )
  )
)
