(kicad_pcb (version 20171130) (host pcbnew "(5.0.0)")
  (general
    (thickness 1.6)
    (drawings 38)
    (tracks 243)
    (zones 0)
    (modules 19)
    (nets 24)
  )
  (page A4)
  (title_block
    (title "DMX Demonstrator - Control-Pro Clock (DMX-CPCB)")
    (date 2023-12-04)
    (rev 1.3)
    (company "Crazy Giraffe Software")
    (comment 2 "Designed by: SparkyBobo")
    (comment 3 https://creativecommons.org/licenses/by-sa/4.0/)
    (comment 4 "Released under the Creative Commons Attribution Share-Alike 4.0m License")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.1)
    (edge_width 0.1524)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 3.302 2)
    (pad_drill 2.159)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "grb"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 +5V)
  (net 3 "Net-(SW2-Pad1)")
  (net 4 "Net-(D7-Pad1)")
  (net 5 "Net-(D6-Pad1)")
  (net 6 "Net-(R10-Pad2)")
  (net 7 "Net-(D8-Pad1)")
  (net 8 "Net-(R9-Pad2)")
  (net 9 "Net-(SW1-Pad1)")
  (net 10 "Net-(SW1-Pad6)")
  (net 11 /DIM1)
  (net 12 /DIM2)
  (net 13 /DIM3)
  (net 14 /DIM4)
  (net 15 /~CLK_STEP)
  (net 16 /SPD_LO)
  (net 17 /SPD_WIPER)
  (net 18 /SPD_HI)
  (net 19 /~CLK_FST)
  (net 20 /~CLK_SLO)
  (net 21 /~HWD_DT)
  (net 22 /~CLOCK)
  (net 23 /~DATA)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net /DIM1)
    (add_net /DIM2)
    (add_net /DIM3)
    (add_net /DIM4)
    (add_net /SPD_HI)
    (add_net /SPD_LO)
    (add_net /SPD_WIPER)
    (add_net /~CLK_FST)
    (add_net /~CLK_SLO)
    (add_net /~CLK_STEP)
    (add_net /~CLOCK)
    (add_net /~DATA)
    (add_net /~HWD_DT)
    (add_net GND)
    (add_net "Net-(D6-Pad1)")
    (add_net "Net-(D7-Pad1)")
    (add_net "Net-(D8-Pad1)")
    (add_net "Net-(R10-Pad2)")
    (add_net "Net-(R9-Pad2)")
    (add_net "Net-(SW1-Pad1)")
    (add_net "Net-(SW1-Pad6)")
    (add_net "Net-(SW2-Pad1)")
  )
  (module footprints:BOURNS_PTV09A_1 (layer F.Cu) (tedit 5F62B2B8)
    (at 137.242 116.516)
    (fp_text reference R5 (at 6.3 4.9) (layer F.SilkS))
    (fp_text value 10k (at 0 -0.5) (layer F.Fab))
    (pad 1 thru_hole circle (at -2.5 7) (size 2.2 2.2) (drill 1) (layers *.Cu *.Mask)
      (net 16 /SPD_LO))
    (pad 2 thru_hole circle (at 0 7) (size 2.2 2.2) (drill 1) (layers *.Cu *.Mask)
      (net 17 /SPD_WIPER))
    (pad 3 thru_hole circle (at 2.5 7) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 18 /SPD_HI))
    (pad 4 thru_hole roundrect (at -4.4 0) (size 3 3) (drill oval 2 2.2) (layers *.Cu *.Mask) (roundrect_rratio 0.25))
    (pad 5 thru_hole roundrect (at 4.4 0) (size 3 3) (drill oval 2 2.4) (layers *.Cu *.Mask) (roundrect_rratio 0.25))
  )
  (module Connector_IDC:IDC-Header_2x08_P2.54mm_Horizontal (layer F.Cu) (tedit 59DE20FF)
    (at 172.974 91.192)
    (descr "Through hole angled IDC box header, 2x08, 2.54mm pitch, double rows")
    (tags "Through hole IDC box header THT 2x08 2.54mm double row")
    (fp_text reference J1 (at 6.105 -6.35) (layer F.SilkS))
    (fp_text value OUTPUT (at 6.105 24.384) (layer F.Fab))
    (fp_text user %R (at 8.805 8.89 90) (layer F.Fab))
    (pad 16 thru_hole oval (at 2.54 17.78) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 15 thru_hole oval (at 0 17.78) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 14 thru_hole oval (at 2.54 15.24) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 19 /~CLK_FST))
    (pad 13 thru_hole oval (at 0 15.24) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 14 /DIM4))
    (pad 12 thru_hole oval (at 2.54 12.7) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 20 /~CLK_SLO))
    (pad 11 thru_hole oval (at 0 12.7) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 13 /DIM3))
    (pad 10 thru_hole oval (at 2.54 10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 15 /~CLK_STEP))
    (pad 9 thru_hole oval (at 0 10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 12 /DIM2))
    (pad 8 thru_hole oval (at 2.54 7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 16 /SPD_LO))
    (pad 7 thru_hole oval (at 0 7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 11 /DIM1))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 17 /SPD_WIPER))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 /~DATA))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 18 /SPD_HI))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 22 /~CLOCK))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 21 /~HWD_DT))
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/Connector_IDC.3dshapes/IDC-Header_2x08_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 132.334 76.454 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R7 (at 5.08 -2.286 90) (layer F.SilkS))
    (fp_text value 330 (at 5.08 2.37 90) (layer F.Fab))
    (fp_text user %R (at 5.08 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 /~CLOCK))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(D7-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_IDC:IDC-Header_2x08_P2.54mm_Horizontal (layer F.Cu) (tedit 59DE20FF)
    (at 101.092 108.966 180)
    (descr "Through hole angled IDC box header, 2x08, 2.54mm pitch, double rows")
    (tags "Through hole IDC box header THT 2x08 2.54mm double row")
    (fp_text reference J2 (at 6.105 -6.35 180) (layer F.SilkS))
    (fp_text value INPUT (at 6.105 24.384 180) (layer F.Fab))
    (fp_text user %R (at 8.805 8.89 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 21 /~HWD_DT))
    (pad 3 thru_hole oval (at 0 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 22 /~CLOCK))
    (pad 4 thru_hole oval (at 2.54 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 18 /SPD_HI))
    (pad 5 thru_hole oval (at 0 5.08 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 /~DATA))
    (pad 6 thru_hole oval (at 2.54 5.08 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 17 /SPD_WIPER))
    (pad 7 thru_hole oval (at 0 7.62 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 11 /DIM1))
    (pad 8 thru_hole oval (at 2.54 7.62 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 16 /SPD_LO))
    (pad 9 thru_hole oval (at 0 10.16 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 12 /DIM2))
    (pad 10 thru_hole oval (at 2.54 10.16 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 15 /~CLK_STEP))
    (pad 11 thru_hole oval (at 0 12.7 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 13 /DIM3))
    (pad 12 thru_hole oval (at 2.54 12.7 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 20 /~CLK_SLO))
    (pad 13 thru_hole oval (at 0 15.24 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 14 /DIM4))
    (pad 14 thru_hole oval (at 2.54 15.24 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 19 /~CLK_FST))
    (pad 15 thru_hole oval (at 0 17.78 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 16 thru_hole oval (at 2.54 17.78 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_IDC.3dshapes/IDC-Header_2x08_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 156.21 105.41 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R9 (at 8.128 -2.286 90) (layer F.SilkS))
    (fp_text value 330 (at 5.08 2.37 90) (layer F.Fab))
    (fp_text user %R (at 5.08 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 /~CLK_SLO))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(R9-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:ESWITCH_100_DPDT_M1 (layer F.Cu) (tedit 5F6FA4A7)
    (at 147.038 86.692 180)
    (fp_text reference SW1 (at 7.75 -0.05 180) (layer F.SilkS))
    (fp_text value CLOCK_SPEED (at 0 -0.5 180) (layer F.Fab))
    (pad 1 thru_hole oval (at -2.413 -4.699 180) (size 3.302 2) (drill oval 2.159 0.9) (layers *.Cu *.Mask)
      (net 9 "Net-(SW1-Pad1)"))
    (pad 2 thru_hole oval (at -2.413 0 180) (size 3.302 2) (drill oval 2.159 0.9) (layers *.Cu *.Mask)
      (net 8 "Net-(R9-Pad2)"))
    (pad 3 thru_hole oval (at -2.413 4.699 180) (size 3.302 2) (drill oval 2.159 0.9) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole oval (at 2.413 -4.699 180) (size 3.302 2) (drill oval 2.159 0.9) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole oval (at 2.413 0 180) (size 3.302 2) (drill oval 2.159 0.9) (layers *.Cu *.Mask)
      (net 6 "Net-(R10-Pad2)"))
    (pad 6 thru_hole oval (at 2.413 4.699 180) (size 3.302 2) (drill oval 2.159 0.9) (layers *.Cu *.Mask)
      (net 10 "Net-(SW1-Pad6)"))
  )
  (module footprints:ESWITCH_100_SPDT_M1 (layer F.Cu) (tedit 5F6FA4D5)
    (at 127.038 86.692 180)
    (fp_text reference SW2 (at 5.5 -0.05 180) (layer F.SilkS))
    (fp_text value CLOCK_STEP (at 0 -0.5 180) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 -4.699 180) (size 3.302 2) (drill oval 2.159 0.9) (layers *.Cu *.Mask)
      (net 3 "Net-(SW2-Pad1)"))
    (pad 2 thru_hole oval (at 0 0 180) (size 3.302 2) (drill oval 2.159 0.9) (layers *.Cu *.Mask)
      (net 15 /~CLK_STEP))
    (pad 3 thru_hole oval (at 0 4.699 180) (size 3.302 2) (drill oval 2.159 0.9) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module LED_THT:LED_D5.0mm (layer F.Cu) (tedit 5995936A)
    (at 175.814 76.242)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (fp_text reference D8 (at 1.27 -3.96) (layer F.SilkS))
    (fp_text value ACTIVE (at 1.27 3.96) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 7 "Net-(D8-Pad1)"))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D5.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 172.212 83.312 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R8 (at 3.048 2.54 90) (layer F.SilkS))
    (fp_text value 330 (at 5.08 2.37 90) (layer F.Fab))
    (fp_text user %R (at 5.08 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(D8-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 /~HWD_DT))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 127.508 76.454 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R6 (at 5.08 -2.37 90) (layer F.SilkS))
    (fp_text value 330 (at 5.08 2.37 90) (layer F.Fab))
    (fp_text user %R (at 5.08 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(D6-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 /~DATA))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 161.29 105.41 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R10 (at 8.382 -2.286 90) (layer F.SilkS))
    (fp_text value 330 (at 5.08 2.37 90) (layer F.Fab))
    (fp_text user %R (at 5.08 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 /~CLK_FST))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(R10-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_THT:LED_D5.0mm (layer F.Cu) (tedit 5995936A)
    (at 135.838 70.866)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (fp_text reference D6 (at 1.27 -3.96) (layer F.SilkS))
    (fp_text value DATA (at 1.27 3.96) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 5 "Net-(D6-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D5.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_THT:LED_D5.0mm (layer F.Cu) (tedit 5995936A)
    (at 135.838 58.692)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (fp_text reference D7 (at 1.27 -3.96) (layer F.SilkS))
    (fp_text value CLOCK (at 1.27 3.96) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 "Net-(D7-Pad1)"))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D5.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5F6FABBC)
    (at 179.088 130.566)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference MH4 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5F6FABA9)
    (at 179.088 56.856)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference MH3 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 6317EC5E)
    (at 95.118 130.566)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference MH2 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 6317EC3C)
    (at 95.218 56.856)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference MH1 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module footprints:OSHW-LOGO-S (layer B.Cu) (tedit 200000)
    (at 171.664 135.832 180)
    (descr "OPEN-SOURCE HARDWARE (OSHW) LOGO - SMALL - SILKSCREEN")
    (tags "OPEN-SOURCE HARDWARE (OSHW) LOGO - SMALL - SILKSCREEN")
    (attr virtual)
    (fp_text reference "" (at 0 0 180) (layer B.SilkS))
    (fp_text value "" (at 0 0 180) (layer B.SilkS))
  )
  (module footprints:logo_cr_5x5 (layer B.Cu) (tedit 0)
    (at 149.664 134.852 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (gr_line (start 187.104 133.692) (end 187.104 53.692) (layer Edge.Cuts) (width 0.1524))
  (gr_line (start 92.104 138.692) (end 182.104 138.692) (layer Edge.Cuts) (width 0.1524))
  (gr_line (start 87.104 53.692) (end 87.104 133.692) (layer Edge.Cuts) (width 0.1524))
  (gr_line (start 182.104 48.692) (end 92.104 48.692) (layer Edge.Cuts) (width 0.1524))
  (gr_arc (start 92.104 133.692) (end 87.104 133.692) (angle -90) (layer Edge.Cuts) (width 0.1524))
  (gr_arc (start 92.104 53.692) (end 92.104 48.692) (angle -90) (layer Edge.Cuts) (width 0.1524))
  (gr_arc (start 182.104 53.692) (end 187.104 53.692) (angle -90) (layer Edge.Cuts) (width 0.1524))
  (gr_arc (start 182.104 133.692) (end 182.104 138.692) (angle -90) (layer Edge.Cuts) (width 0.1524))
  (gr_text Detected (at 177.104 70.242) (layer F.SilkS))
  (gr_text Data (at 143.764 71.246) (layer F.SilkS))
  (gr_text Clock (at 144 58.746) (layer F.SilkS))
  (gr_text "Clock\nSpeed" (at 137.292 107.416) (layer F.SilkS))
  (gr_text "DMX-CPCB, Rev 1.3\nCrazy Giraffe Software" (at 160.414 136.102) (layer B.SilkS))
  (gr_text Fast (at 147.038 78.486) (layer F.SilkS))
  (gr_text Slow (at 147.038 94.892) (layer F.SilkS))
  (gr_text "Clock\nStep" (at 127.038 96.492) (layer F.SilkS))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 87.122 48.768) (xy 187.004 48.792) (xy 187.004 138.592) (xy 87.122 138.684)
      )
    )
  )
  (zone (net 2) (net_name +5V) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 87.122 48.768) (xy 187.004 48.792) (xy 187.004 138.592) (xy 87.122 138.684)
      )
    )
  )
)
