(kicad_pcb (version 4) (host pcbnew 4.0.5)
  (general
    (links 58)
    (no_connects 0)
    (area 99.924999 100.424999 165.075001 130.575001)
    (thickness 1.6002)
    (drawings 10)
    (tracks 200)
    (zones 0)
    (modules 18)
    (nets 37)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (44 Edge.Cuts user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.1524)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.762)
    (uvia_drill 0.508)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 6)
    (pad_drill 0)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (grid_origin 100 100.5)
    (visible_elements FFFEFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(AE0-Pad1)")
  (net 2 /3V3)
  (net 3 GND)
  (net 4 /5V)
  (net 5 "Net-(P1-Pad1)")
  (net 6 /ID_SC)
  (net 7 /ID_SD)
  (net 8 "Net-(U1-Pad1)")
  (net 9 "Net-(U1-Pad3)")
  (net 10 "Net-(U1-Pad4)")
  (net 11 "Net-(U1-Pad5)")
  (net 12 "Net-(U1-Pad7)")
  (net 13 "Net-(U1-Pad8)")
  (net 14 "Net-(U1-Pad10)")
  (net 15 "Net-(U1-Pad11)")
  (net 16 "Net-(U1-Pad12)")
  (net 17 "Net-(U1-Pad13)")
  (net 18 "Net-(U1-Pad15)")
  (net 19 "Net-(U1-Pad16)")
  (net 20 "Net-(U1-Pad17)")
  (net 21 "Net-(U1-Pad18)")
  (net 22 /MOSI)
  (net 23 /MISO)
  (net 24 "Net-(U1-Pad22)")
  (net 25 /SCLK)
  (net 26 /CS)
  (net 27 "Net-(U1-Pad26)")
  (net 28 /DIO0)
  (net 29 /DIO1)
  (net 30 /RESET)
  (net 31 /DIO2)
  (net 32 /DIO3)
  (net 33 "Net-(U1-Pad36)")
  (net 34 /DIO4)
  (net 35 /DIO5)
  (net 36 "Net-(U1-Pad40)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net /CS)
    (add_net /DIO0)
    (add_net /DIO1)
    (add_net /DIO2)
    (add_net /DIO3)
    (add_net /DIO4)
    (add_net /DIO5)
    (add_net /ID_SC)
    (add_net /ID_SD)
    (add_net /MISO)
    (add_net /MOSI)
    (add_net /RESET)
    (add_net /SCLK)
    (add_net "Net-(P1-Pad1)")
    (add_net "Net-(U1-Pad1)")
    (add_net "Net-(U1-Pad10)")
    (add_net "Net-(U1-Pad11)")
    (add_net "Net-(U1-Pad12)")
    (add_net "Net-(U1-Pad13)")
    (add_net "Net-(U1-Pad15)")
    (add_net "Net-(U1-Pad16)")
    (add_net "Net-(U1-Pad17)")
    (add_net "Net-(U1-Pad18)")
    (add_net "Net-(U1-Pad22)")
    (add_net "Net-(U1-Pad26)")
    (add_net "Net-(U1-Pad3)")
    (add_net "Net-(U1-Pad36)")
    (add_net "Net-(U1-Pad4)")
    (add_net "Net-(U1-Pad40)")
    (add_net "Net-(U1-Pad5)")
    (add_net "Net-(U1-Pad7)")
    (add_net "Net-(U1-Pad8)")
  )
  (net_class GND ""
    (clearance 0.1524)
    (trace_width 0.3)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net GND)
  )
  (net_class PWR ""
    (clearance 0.25)
    (trace_width 0.5)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net /3V3)
    (add_net /5V)
  )
  (net_class RF ""
    (clearance 0.25)
    (trace_width 0.7)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net "Net-(AE0-Pad1)")
  )
  (module Mounting_Holes:MountingHole_2.7mm_M2.5 locked (layer F.Cu) (tedit 59E638A3)
    (at 161.5 127)
    (descr "Mounting Hole 2.7mm, no annular, M2.5")
    (tags "mounting hole 2.7mm no annular m2.5")
    (clearance 1.625)
    (attr virtual)
    (fp_text reference REF** (at 0 5) (layer F.Fab) hide)
    (fp_text value MountingHole_2.7mm_M2.5 (at 0.5 10) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.7mm_M2.5 locked (layer F.Cu) (tedit 59E63883)
    (at 103.5 127)
    (descr "Mounting Hole 2.7mm, no annular, M2.5")
    (tags "mounting hole 2.7mm no annular m2.5")
    (clearance 1.625)
    (attr virtual)
    (fp_text reference REF** (at 3.5 6) (layer F.Fab) hide)
    (fp_text value MountingHole_2.7mm_M2.5 (at 0.5 10) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.7mm_M2.5 locked (layer F.Cu) (tedit 59E63896)
    (at 161.5 104)
    (descr "Mounting Hole 2.7mm, no annular, M2.5")
    (tags "mounting hole 2.7mm no annular m2.5")
    (clearance 1.625)
    (attr virtual)
    (fp_text reference REF** (at 0 -6.5) (layer F.Fab) hide)
    (fp_text value MountingHole_2.7mm_M2.5 (at 0 3.7) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.7mm_M2.5 locked (layer F.Cu) (tedit 59E63874)
    (at 103.5 104)
    (descr "Mounting Hole 2.7mm, no annular, M2.5")
    (tags "mounting hole 2.7mm no annular m2.5")
    (clearance 1.625)
    (zone_connect 0)
    (attr virtual)
    (fp_text reference REF** (at 4 -7.5) (layer F.Fab) hide)
    (fp_text value MountingHole_2.7mm_M2.5 (at 0 3.7) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask)
      (zone_connect 0))
  )
  (module RFModules:Amphenol132432 (layer F.Cu) (tedit 59E89C48)
    (at 107 115 270)
    (fp_text reference AE0 (at -6.25 1.25 360) (layer F.SilkS))
    (fp_text value Antenna (at 0 -2 270) (layer F.Fab))
    (pad "" smd rect (at 4.25 3 270) (size 1.5 6) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad "" smd rect (at -4.25 3 270) (size 1.5 6) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad "" smd rect (at 4.25 3 270) (size 1.5 6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad "" smd rect (at -4.25 3 270) (size 1.5 6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 1 smd rect (at 0 3.5 270) (size 1.5 7) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(AE0-Pad1)"))
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 59E89C29)
    (at 127.5 128)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C1 (at -4.25 0) (layer F.SilkS))
    (fp_text value 10uF (at 0 2) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 /3V3))
    (pad 2 smd rect (at 2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 59E89C31)
    (at 134.5 128)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C2 (at 4.25 0) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 2) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 /3V3))
    (pad 2 smd rect (at 2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 59E89BFD)
    (at 157 114.75)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C3 (at -4.5 0) (layer F.SilkS))
    (fp_text value 100nF (at 0 2) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 /3V3))
    (pad 2 smd rect (at 2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 59E89C39)
    (at 121 114.75 270)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C4 (at -4 0 360) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 2 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 4 /5V))
    (pad 2 smd rect (at 2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 59E89C42)
    (at 111 114.75 270)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C5 (at -4 0 360) (layer F.SilkS))
    (fp_text value 22uF (at 0 2 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 /3V3))
    (pad 2 smd rect (at 2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x01_Pitch2.54mm (layer F.Cu) (tedit 59E89CC7)
    (at 162.75 119 90)
    (descr "Through hole straight pin header, 2x01, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x01 2.54mm double row")
    (fp_text reference P1 (at -2.25 0 180) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 1.27 2.33 90) (layer F.Fab))
    (fp_text user %R (at 1.27 0 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(P1-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 59E89C14)
    (at 157 122)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R1 (at -4.5 0) (layer F.SilkS))
    (fp_text value 1K (at 0 1.9) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 /3V3))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(P1-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 59E89C0C)
    (at 157 119.5)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R2 (at -4.5 0) (layer F.SilkS))
    (fp_text value 3.9K (at 0 1.9) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 /3V3))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 6 /ID_SC))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 59E89C05)
    (at 157 117)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R3 (at -4.5 0) (layer F.SilkS))
    (fp_text value 3.9K (at 0 1.9) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 /3V3))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 7 /ID_SD))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RFModules:RFM69HW-S2 (layer F.Cu) (tedit 59E89C21)
    (at 126.5 109.75)
    (fp_text reference U2 (at 1 -1) (layer F.SilkS))
    (fp_text value RFM69HW (at 8 7) (layer F.Fab))
    (pad 9 smd rect (at 16 15) (size 4 1.2) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 8 smd rect (at 0 15) (size 4 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 /3V3))
    (pad 10 smd rect (at 16 13) (size 4 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(AE0-Pad1)"))
    (pad 11 smd rect (at 16 11) (size 4 1.2) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 12 smd rect (at 16 9) (size 4 1.2) (layers F.Cu F.Paste F.Mask)
      (net 25 /SCLK))
    (pad 13 smd rect (at 16 7) (size 4 1.2) (layers F.Cu F.Paste F.Mask)
      (net 23 /MISO))
    (pad 14 smd rect (at 16 5) (size 4 1.2) (layers F.Cu F.Paste F.Mask)
      (net 22 /MOSI))
    (pad 15 smd rect (at 16 3) (size 4 1.2) (layers F.Cu F.Paste F.Mask)
      (net 26 /CS))
    (pad 16 smd rect (at 16 1) (size 4 1.2) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 7 smd rect (at 0 13) (size 4 1.2) (layers F.Cu F.Paste F.Mask)
      (net 35 /DIO5))
    (pad 6 smd rect (at 0 11) (size 4 1.2) (layers F.Cu F.Paste F.Mask)
      (net 34 /DIO4))
    (pad 5 smd rect (at 0 9) (size 4 1.2) (layers F.Cu F.Paste F.Mask)
      (net 32 /DIO3))
    (pad 3 smd rect (at 0 5) (size 4 1.2) (layers F.Cu F.Paste F.Mask)
      (net 29 /DIO1))
    (pad 4 smd rect (at 0 7) (size 4 1.2) (layers F.Cu F.Paste F.Mask)
      (net 31 /DIO2))
    (pad 2 smd rect (at 0 3) (size 4 1.2) (layers F.Cu F.Paste F.Mask)
      (net 28 /DIO0))
    (pad 1 smd rect (at 0 1) (size 4 1.2) (layers F.Cu F.Paste F.Mask)
      (net 30 /RESET))
  )
  (module SMD_Packages:SOIC-8-N (layer F.Cu) (tedit 59E89CC4)
    (at 157.75 110.75 90)
    (descr "Module Narrow CMS SOJ 8 pins large")
    (tags "CMS SOJ")
    (attr smd)
    (fp_text reference U3 (at -1.75 5 180) (layer F.SilkS))
    (fp_text value CAT24C32 (at 0 1.27 90) (layer F.Fab))
    (pad 8 smd rect (at -1.905 -3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 2 /3V3))
    (pad 7 smd rect (at -0.635 -3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(P1-Pad1)"))
    (pad 6 smd rect (at 0.635 -3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 6 /ID_SC))
    (pad 5 smd rect (at 1.905 -3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 7 /ID_SD))
    (pad 4 smd rect (at 1.905 3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 3 smd rect (at 0.635 3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 2 smd rect (at -0.635 3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 1 smd rect (at -1.905 3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model SMD_Packages.3dshapes/SOIC-8-N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.38 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:TO-252-2 (layer F.Cu) (tedit 59E89CD5)
    (at 116 116.5 270)
    (descr "TO-252 / DPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO252/PG-TO252-3-1/")
    (tags "DPAK TO-252 DPAK-3 TO-252-3 SOT-428")
    (attr smd)
    (fp_text reference U4 (at -6.25 -2.25 360) (layer F.SilkS))
    (fp_text value TLV2217-33 (at 0 4.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -4.2 -2.28 270) (size 2.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 4 /5V))
    (pad 3 smd rect (at -4.2 2.28 270) (size 2.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 /3V3))
    (pad 2 smd rect (at 2.1 0 270) (size 6.4 5.8) (layers F.Cu F.Mask)
      (net 3 GND))
    (pad 2 smd rect (at 3.775 1.525 270) (size 3.05 2.75) (layers F.Cu F.Paste)
      (net 3 GND))
    (pad 2 smd rect (at 0.425 -1.525 270) (size 3.05 2.75) (layers F.Cu F.Paste)
      (net 3 GND))
    (pad 2 smd rect (at 3.775 -1.525 270) (size 3.05 2.75) (layers F.Cu F.Paste)
      (net 3 GND))
    (pad 2 smd rect (at 0.425 1.525 270) (size 3.05 2.75) (layers F.Cu F.Paste)
      (net 3 GND))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/TO-252-2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_2x20_Pitch2.54mm (layer B.Cu) (tedit 59E89CAE)
    (at 108.5 105.25 270)
    (descr "Through hole straight socket strip, 2x20, 2.54mm pitch, double rows")
    (tags "Through hole socket strip THT 2x20 2.54mm double row")
    (fp_text reference U1 (at 2.25 0 360) (layer B.SilkS))
    (fp_text value Raspberry_Pi_2_3 (at -1.27 -50.59 270) (layer B.Fab))
    (fp_text user %R (at -1.27 2.33 270) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(U1-Pad1)"))
    (pad 2 thru_hole oval (at -2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /5V))
    (pad 3 thru_hole oval (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(U1-Pad3)"))
    (pad 4 thru_hole oval (at -2.54 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(U1-Pad4)"))
    (pad 5 thru_hole oval (at 0 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(U1-Pad5)"))
    (pad 6 thru_hole oval (at -2.54 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 7 thru_hole oval (at 0 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(U1-Pad7)"))
    (pad 8 thru_hole oval (at -2.54 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(U1-Pad8)"))
    (pad 9 thru_hole oval (at 0 -10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 10 thru_hole oval (at -2.54 -10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(U1-Pad10)"))
    (pad 11 thru_hole oval (at 0 -12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(U1-Pad11)"))
    (pad 12 thru_hole oval (at -2.54 -12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(U1-Pad12)"))
    (pad 13 thru_hole oval (at 0 -15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(U1-Pad13)"))
    (pad 14 thru_hole oval (at -2.54 -15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 15 thru_hole oval (at 0 -17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(U1-Pad15)"))
    (pad 16 thru_hole oval (at -2.54 -17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(U1-Pad16)"))
    (pad 17 thru_hole oval (at 0 -20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(U1-Pad17)"))
    (pad 18 thru_hole oval (at -2.54 -20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(U1-Pad18)"))
    (pad 19 thru_hole oval (at 0 -22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 /MOSI))
    (pad 20 thru_hole oval (at -2.54 -22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 21 thru_hole oval (at 0 -25.4 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 /MISO))
    (pad 22 thru_hole oval (at -2.54 -25.4 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(U1-Pad22)"))
    (pad 23 thru_hole oval (at 0 -27.94 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 /SCLK))
    (pad 24 thru_hole oval (at -2.54 -27.94 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 /CS))
    (pad 25 thru_hole oval (at 0 -30.48 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 26 thru_hole oval (at -2.54 -30.48 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(U1-Pad26)"))
    (pad 27 thru_hole oval (at 0 -33.02 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /ID_SD))
    (pad 28 thru_hole oval (at -2.54 -33.02 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /ID_SC))
    (pad 29 thru_hole oval (at 0 -35.56 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 /DIO0))
    (pad 30 thru_hole oval (at -2.54 -35.56 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 31 thru_hole oval (at 0 -38.1 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 /DIO1))
    (pad 32 thru_hole oval (at -2.54 -38.1 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 /RESET))
    (pad 33 thru_hole oval (at 0 -40.64 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 /DIO2))
    (pad 34 thru_hole oval (at -2.54 -40.64 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 35 thru_hole oval (at 0 -43.18 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 /DIO3))
    (pad 36 thru_hole oval (at -2.54 -43.18 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 "Net-(U1-Pad36)"))
    (pad 37 thru_hole oval (at 0 -45.72 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 /DIO4))
    (pad 38 thru_hole oval (at -2.54 -45.72 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 /DIO5))
    (pad 39 thru_hole oval (at 0 -48.26 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 40 thru_hole oval (at -2.54 -48.26 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 "Net-(U1-Pad40)"))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_2x20_Pitch2.54mm.wrl
      (at (xyz -0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (gr_line (start 100 103.5) (end 100 127.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 165 103.5) (end 165 127.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (dimension 58 (width 0.3) (layer F.Fab)
    (gr_text "58.000 mm" (at 132.5 91.15) (layer F.Fab))
    (feature1 (pts (xy 161.5 104) (xy 161.5 89.8)))
    (feature2 (pts (xy 103.5 104) (xy 103.5 89.8)))
    (crossbar (pts (xy 103.5 92.5) (xy 161.5 92.5)))
    (arrow1a (pts (xy 161.5 92.5) (xy 160.373496 93.086421)))
    (arrow1b (pts (xy 161.5 92.5) (xy 160.373496 91.913579)))
    (arrow2a (pts (xy 103.5 92.5) (xy 104.626504 93.086421)))
    (arrow2b (pts (xy 103.5 92.5) (xy 104.626504 91.913579)))
  )
  (dimension 23 (width 0.3) (layer F.Fab)
    (gr_text "23.000 mm" (at 178.35 115.5 270) (layer F.Fab))
    (feature1 (pts (xy 161.5 127) (xy 179.7 127)))
    (feature2 (pts (xy 161.5 104) (xy 179.7 104)))
    (crossbar (pts (xy 177 104) (xy 177 127)))
    (arrow1a (pts (xy 177 127) (xy 176.413579 125.873496)))
    (arrow1b (pts (xy 177 127) (xy 177.586421 125.873496)))
    (arrow2a (pts (xy 177 104) (xy 176.413579 105.126504)))
    (arrow2b (pts (xy 177 104) (xy 177.586421 105.126504)))
  )
  (gr_line (start 103 130.5) (end 162 130.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 103 127.5) (end 103 130.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 162 127.5) (end 165 127.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 103 103.5) (end 100 103.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 162 103.5) (end 162 100.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 103 100.5) (end 162 100.5) (angle 90) (layer Edge.Cuts) (width 0.15))
)
