<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.4.2">
<drawing>
<board>
<plain>
<wire x1="2.032" y1="112.268" x2="74.93" y2="112.268" width="0" layer="20"/>
<wire x1="77.216" y1="109.982" x2="77.216" y2="2.286" width="0" layer="20"/>
<text>BTN_DOWN</text>
<text>BTN_SEL</text>
<text>BTN_UP</text>
<text>BTN_NEXT</text>
<wire x1="74.93" y1="0" x2="2.032" y2="0" width="0" layer="20"/>
<wire x1="-0.254" y1="2.286" x2="-0.254" y2="109.982" width="0" layer="20"/>
<text>SAM D51 MICROCONTROLLER</text>
<text>EXTRA PORTS (JST-PH)</text>
<text>The center port provides an I²C interface. The other 
two ports provide access to pins A8 and A9 (PB03 &amp;
PB02, respectively) via current limiting resistors R15 
&amp; R16. D5 &amp; D6 are 3.6V zener diodes to protect pins
from overvoltage: they shunt excess power to ground 
when the voltage exceeds their breakdown point.</text>
<text>32KB SRAM CHIP</text>
<text>Optional 23K256 SRAM chip U7
provides a buffer for the display. 
It uses the e-paper screen's SPI 
interface on SERCOM4.
Chip select SRCS is D53/PB14.</text>
<text>THE OPEN BOOK</text>
<text>BTN_PREV</text>
<text>Bits:
0: Left
1: Down
2: Up
3: Right
4: Select
5: Previous
6: Next
7: SD</text>
<text>BTN_RIGHT</text>
<text>BTN_LEFT</text>
<text>BTN_RESET</text>
<text>OSO-BOOK-A1-02</text>
<text>A8</text>
<text>3V</text>
<text>GND</text>
<text>A9</text>
<text>3V</text>
<text>GND</text>
<text>SDA</text>
<text>3V</text>
<text>GND</text>
<text>SCL</text>
<text>SERIAL PORT</text>
<text></text>
<text>Pins: ECS=D44/PB07 EDC
=D45/PB05 ERST=D46
/PA00 EBSY=D47/PA01</text>
<text>THE OPEN BOOK IS
OPEN SOURCE HARDWARE! 
CC-BY-SA 4.0</text>
<text>GND</text>
<text>RX</text>
<text>TX</text>
<text>GND</text>
<text>RX</text>
<text>TX</text>
<text>3V</text>
<text>3V</text>
<text>BTN_LOCK</text>
<wire x1="74.93" y1="112.268" x2="77.216" y2="109.982" width="0" layer="20" curve="-90"/>
<wire x1="2.032" y1="112.268" x2="-0.254" y2="109.982" width="0" layer="20" curve="90"/>
<wire x1="-0.254" y1="2.286" x2="2.032" y2="0" width="0" layer="20" curve="90"/>
<wire x1="74.93" y1="0" x2="77.216" y2="2.286" width="0" layer="20" curve="90"/>
<text>POWER SUPPLY</text>
<text>BATTERY AND 
CHARGING</text>
<text>D1&amp;Q1 conspire to let 
only the higher of VBAT &amp; VBUS 
reach 3.3V regulator U1. C1 
filters regulator input; C2 &amp; C3 
filter output. R1 pulls EN high 
to keep the regulator on. 
BATTERY: U2 is a LiPo charging 
controller. Powered by VBUS, it 
charges the battery at a rate 
determined by R3. C4=filter for 
VBAT, R4 limits current to CHG 
     LED. R8 &amp; R9 are a voltage 
     divider for VBAT to make a 
     battery gauge on A6/PB01.</text>
<text>VBAT</text>
<text>RESET</text>
<text>AREF
PA03</text>
<text>3V</text>
<text>GND</text>
<text>A0
PA02</text>
<text>A1
PA05</text>
<text>A2
PB08</text>
<text>A3
PB09</text>
<text>A4
PA04</text>
<text>A5
PA06</text>
<text>SCK
PA17</text>
<text>MOSI
PB23</text>
<text>MISO
PB22</text>
<text>RX
PB17</text>
<text>TX
PB16</text>
<text>GND</text>
<text>EN</text>
<text>VBUS</text>
<text>LED
D13
PA23</text>
<text>D12
PA22</text>
<text>D11
PA21</text>
<text>D10
PA20</text>
<text>D9
PA19</text>
<text>D6
PA18</text>
<text>D5
PA16</text>
<text>SCL
PA13</text>
<text>SDA
PA12</text>
<text>*Notes on this bit
           can be
           found
           at end 
           of the
           POWER 
           SUPPLY
           block.</text>
<text>RESET BUTTON</text>
<text>R6 pulls !RESET high. 
Btn pulls it 
low. C13 is a 
filter cap. R7 
discharges 
C13. Double 
tap for UF2 
bootloader.</text>
<text>R3 Values</text>
<text>10K = 100mA &lt;- RECOMMEND!!!
5K = 200mA  2K = 500mA</text>
<text>WARNING: OVER 100mA, BE ABSOLUTELY CERTAIN
THAT YOUR BATTERY SUPPORTS THE DESIRED 
RATE OF CHARGE!! PLEASE DON'T CATCH FIRE.</text>
<text>AUDIO COMBO JACK</text>
<text>A0/PA02: R audio out
A1/PA05: L audio out
A7/PB04: Raw mic in
</text>
<text>ENABLE SWITCH</text>
<text>R1 up top pulls EN high. 
Switching SW1 pulls EN 
     low, disabling pwr 
     supply U1 along with 
     most of the board.</text>
<text>E-PAPER DISPLAY</text>
<text>BUTTON REGISTER</text>
<text>U5 is a 74165 8-bit
shift register. It takes 
the state of 7 of the 
board's buttons (L/D/U/R
/Sel/Prev/Next) and fits 
them in a single byte.</text>
<text>DEBUG PORT</text>
<text>An SWD connector
(and test points)
  allow access to 
  the serial wire 
  debug interface.
  R5=SWCLK pullup</text>
<text>The Open Book by Joey Castillo
@josecastillo. Based in large 
part on @Adafruit's awesome 
open source designs! OSO logo 
&amp; lazer bear by Joseph Devens, 
@DoctorDevens. Thanks to Tom F, 
Josh L, Brent R, OSHPark &amp; many 
others. Made with . in BK &amp; TX.</text>
<text>Pins: 
BUTTON_LATCH: D48/PB31
BUTTON_OUT:  D49/PB30
BUTTON_CLOCK: D50/PB00</text>
<text>THE OPEN</text>
<text>2MB QSPI FLASH</text>
<text>U4 is another GD25Q16C Flash
chip. It's the CIRCUITPY drive 
that shows up when you plug 
it in! It's on a dedicated QSPI 
bus (PB10, PB11, PA08-PA11). 
CircuitPy uses this internally;
Arduino can use it with SCK 35, 
CS 36 and data lines 37-40.</text>
<text>BABEL FLASH CHIP</text>
<text>U6 is a GD25Q16C Flash 
memory chip on the main SPI 
bus (BCS: D52/PB06). Stores 
Unicode character data and 
Unifont glyphs for every code 
point in the Basic Multliingual 
Plane. Contents covered by GPL
with font embedding exception.</text>
<text>MICROSD</text>
<text>Uses the main SPI 
bus (MISO, MOSI, SCK). 
SDCS is D4/PA14.</text>
<text>Lots to unpack here. For starters, the Feather 
pinout is mostly identical to the Adafruit SAMD51 
boards you're familiar with, PWM &amp; analog pins 
where you expect them (minus "extra" pin D4). 
SERCOM0: Serial (RX/TX = D0/D1 = PB17/PB16)
SERCOM1: SPI (MOSI/MISO/SCK = D27/D26/D28 = PB23/PB22/PA17)
SERCOM2: I²C (SDA/SCL = D24/D25 = PA12/PA13)
SERCOM4: SPI for the display:
MOSI1/MISO1/SCK1 = D41/D43/D42
=PB15/PB12/PB13.
For CircuitPython, use pin names 
(i.e. SCK, D8, A4). Arduino: number 
after D is digital pin number (D4=4),
&amp; for analog pins, use number with `A' prefix
(A0). Most folks can ignore pad names (PA12), 
but they're useful for firmware development.</text>
<text>BOOK</text>
<text>BTN_NEXT</text>
<text>BTN_PREV</text>
<text>RESET</text>
<text>SWCLK</text>
<text>3V3</text>
<text>GND</text>
<text>SWDIO</text>
<text>STATUS LED</text>
<text>plz don't steal the bear tho.</text>
<text>NEOPIXEL=D8=
  PA15</text>
<text>COLOPHON</text>
<text>C5, C6, C7, C8: filtering 
caps on each power pin.</text>
<text>C9&amp;C10: filter</text>
<text>caps on VDDCORE,
output from the
chip's voltage
regulator.</text>
<text>C11 &amp; C12 filter AVCC/
AREF, isolated by FB1</text>
<text>+MIC PREAMP</text>
<text>U8 is a MAX4466 amp for 
an inline electret mic. </text>
<text>Amplified mic
 signal on
A10/PA07</text>
<text>R11-R12 are resistor arrays to 
keep inputs from floating. C25 
(&amp; many small capacitors you see 
near devices) are bypass caps; 
they filter current spikes &amp; dips.</text>
<text>card
detect</text>
<text>LOCK_BUTTON=D51=PA27</text>
<text>BUILDING YOUR BOOK</text>
<text>    NOTE: This project requires some surface mount soldering. You may be 
    able to make do with a soldering iron, flux and wick, but a reflow oven is 
ideal. The only really fine-pitched parts are the SAMD51 and the flex cable
connector; other than that, most chips are wide-pitch SOIC, and all resistors 
and capacitors are 0805 or larger so you can place them by eye with fine 
tweezers. All surface mount  parts are on one side (the back). 

           The board is arranged in `blocks' surrounded by dotted lines. All 
           parts within a block are related to that block's function. Example:
           in the `Button Register' block, U5 is the shift register, C26 is a 
           decoupling capacitor for the shift register, and R13 and R14 are 
           pull-up and pull-down resistors for the shift register inputs. If 
           you were to omit everything in this block, the device would still 
           function, just without the buttons.

           At bare minimum, you need to populate the `Power Supply' and
           `SAM D51 Microcontroller' blocks, and probably `Reset Button'. 
You almost certainly also want `Battery and Charging' to take book on the go. 
Note that the Feather headers are `inside' this block, but you can choose to 
add those or not separately. A 400mAh battery fits nicely in the gap between
the headers, atop the lazer bear.

From here, baseline functionality comes from the `E-Paper Display', `MicroSD' 
and `Button Register' blocks. This is probably the minimum viable book. 

From here, populate:
* The `2MB QSPI Flash' &amp; `Status LED' blocks if you plan to use CircuitPython.
* The `Babel Flash Chip' block for universal language support with Babel.
* The `32KB SRAM Chip' block to add a display buffer (can save some RAM).
* The `Extra Ports' block to add STEMMA-compatible I²C and analog connectors.
* The `Audio Combo Jack' block to add stereo audio output, and raw mic input 
   from the inline mic on A7. If you do this, you can also populate:
* The `+Mic Preamp' block for amplified microphone input on A10.

There's also a `Lock Button' and a `Serial Port' at the top; the lock button is 
connected directly to an interrupt pin on the SAMD51, and you can solder 
some socket header onto the serial port for access to the UART pins.

Populate your board. If you are using a reflow oven, reflow BEFORE attaching 
the e-ink screen or soldering any thru-hole components. Once that's done, use 
Atmel Studio + a J-Link (connected to either the debug port or the test pads) 
to flash the UF2 bootloader onto the SAMD51. You should now be able to 
         double-tap the reset button and see the red LED pulse. 

Unplug your device. Now you can solder on the thru-hole buttons and the 
`Enable Switch', if you want it.

Finally: using the Arduino IDE, upload the Open Book screen test sketch, and 
then unplug your device. Thread the screen's flex cable through the hole up 
top, and secure it in the flex connector. Power up the device. If you see the 
screen refresh, you're done! Secure the screen to this area with double sided 
    tape; you don't need this documentation anymore.</text>
<text>oddlyspecific.org/book</text>
<text>Project info:</text>
</plain>
<libraries>
<library name="My Stuff">
<description>Generated from &lt;b&gt;Hiking Log FeatherWing.brd&lt;/b&gt;&lt;p&gt;
by exp-lbrs.ulp</description>
<packages>
<package name="EINK_DISPLAY_4_2IN">
</package>
<package name="A10767">
</package>
<package name="TL3330AF130QG">
</package>
<package name="OSO_GRAPHIC">
</package>
<package name="OSO_BEAR_750MIL">
</package>
<package name="OSO_TEXT_435MIL">
</package>
<package name="OSO_ONELINE_125MIL">
</package>
<package name="MJTP1250-TRY2">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="MICROSD">
</package>
</packages>
</library>
<library name="microbuilder">
<packages>
<package name="0805">
<description>0805 (2012 Metric)</description>
</package>
<package name="0805-NO">
</package>
<package name="JSTPH4">
<description>4 Pin JST PH Series Female Connector&lt;br/&gt;
Righ-Angle SMT</description>
</package>
<package name="JSTPH3">
</package>
<package name="_0805MP">
<description>&lt;b&gt;0805 MicroPitch&lt;/b&gt;</description>
</package>
<package name="SOD-123">
<description>&lt;b&gt;SOD-123&lt;/b&gt;
&lt;p&gt;Source: http://www.diodes.com/datasheets/ds30139.pdf&lt;/p&gt;</description>
</package>
<package name="INDUCTOR_4X4MM_NR401">
</package>
<package name="0805_10MGAP">
</package>
<package name="MOUNTINGHOLE_2.5_PLATED">
</package>
<package name="FIDUCIAL_1MM">
</package>
<package name="TESTPOINT_ROUND_2MM_NO">
</package>
<package name="2X05_1.27MM_BOX_POSTS">
<description>&lt;p&gt;4UCon: 20317&lt;/p&gt;</description>
</package>
<package name="SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt; - 5 Pin</description>
</package>
<package name="JSTPH2">
<description>2-Pin JST PH Series Right-Angle Connector (+/- for batteries)</description>
</package>
<package name="SOT23-R">
<description>&lt;b&gt;SOT23&lt;/b&gt; - Reflow soldering</description>
</package>
<package name="SO16">
<description>&lt;b&gt;Small Outline package&lt;/b&gt; 150 mil</description>
</package>
<package name="SOIC8_150MIL">
<description>&lt;b&gt;Small Outline IC - 150mil Wide&lt;/b&gt;</description>
</package>
<package name="SC70-5">
</package>
</packages>
</library>
<library name="Parts">
<packages>
<package name="SOT23-3">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="1X03">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X01">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="CHIP-LED0805">
<description>&lt;b&gt;Hyper CHIPLED Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
LB R99A&lt;br&gt;
Source: http://www.osram.convergy.de/ ... lb_r99a.pdf</description>
</package>
<package name="LED3535">
</package>
</packages>
</library>
<library name="oshw">
<description>&lt;p&gt;&lt;strong&gt;Open Source Hardware PCB Logos&lt;/strong&gt;
&lt;p&gt;A simple polygon based version of the OSHWA logos for use on Eagle PCB's
&lt;p&gt;For use please refer to the OSHWA definition at &lt;a href="http://www.oshwa.org/definition/"&gt;http://www.oshwa.org/definition/&lt;/a&gt;
&lt;p&gt;Based on the NBitWonder version (&lt;a href="http://nbitwonder.com"&gt;http://nbitwonder.com&lt;/a&gt;)
&lt;p&gt;&lt;strong&gt;Andrew Cooper&lt;/strong&gt;&lt;br&gt;28Nov2016&lt;br&gt;&lt;a href="http://www.darkerview.com"&gt;www.DarkerView.com&lt;/a&gt;</description>
<packages>
<package name="OSHW_5MM">
</package>
</packages>
</library>
<library name="Open Book Library">
<packages>
<package name="TQFP64-10X10">
<description>&lt;b&gt;Thin Quad Flat Pack&lt;/b&gt;&lt;p&gt;
package type TQ</description>
</package>
</packages>
</library>
<library name="10118193-0001LF">
<packages>
<package name="FCI_10118193-0001LF">
</package>
</packages>
</library>
<library name="resistor">
<description>&lt;b&gt;Resistors, Capacitors, Inductors&lt;/b&gt;&lt;p&gt;
Based on the previous libraries:
&lt;ul&gt;
&lt;li&gt;r.lbr
&lt;li&gt;cap.lbr 
&lt;li&gt;cap-fe.lbr
&lt;li&gt;captant.lbr
&lt;li&gt;polcap.lbr
&lt;li&gt;ipc-smd.lbr
&lt;/ul&gt;
All SMD packages are defined according to the IPC specifications and  CECC&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;p&gt;
&lt;p&gt;
for Electrolyt Capacitors see also :&lt;p&gt;
www.bccomponents.com &lt;p&gt;
www.panasonic.com&lt;p&gt;
www.kemet.com&lt;p&gt;
&lt;p&gt;
for trimmer refence see : &lt;u&gt;www.electrospec-inc.com/cross_references/trimpotcrossref.asp&lt;/u&gt;&lt;p&gt;

&lt;map name="nav_main"&gt;
&lt;area shape="rect" coords="0,1,140,23" href="../military_specs.asp" title=""&gt;
&lt;area shape="rect" coords="0,24,140,51" href="../about.asp" title=""&gt;
&lt;area shape="rect" coords="1,52,140,77" href="../rfq.asp" title=""&gt;
&lt;area shape="rect" coords="0,78,139,103" href="../products.asp" title=""&gt;
&lt;area shape="rect" coords="1,102,138,128" href="../excess_inventory.asp" title=""&gt;
&lt;area shape="rect" coords="1,129,138,150" href="../edge.asp" title=""&gt;
&lt;area shape="rect" coords="1,151,139,178" href="../industry_links.asp" title=""&gt;
&lt;area shape="rect" coords="0,179,139,201" href="../comments.asp" title=""&gt;
&lt;area shape="rect" coords="1,203,138,231" href="../directory.asp" title=""&gt;
&lt;area shape="default" nohref&gt;
&lt;/map&gt;

&lt;html&gt;

&lt;title&gt;&lt;/title&gt;

 &lt;LINK REL="StyleSheet" TYPE="text/css" HREF="style-sheet.css"&gt;

&lt;body bgcolor="#ffffff" text="#000000" marginwidth="0" marginheight="0" topmargin="0" leftmargin="0"&gt;
&lt;table border=0 cellspacing=0 cellpadding=0 width="100%" cellpaddding=0 height="55%"&gt;
&lt;tr valign="top"&gt;

&lt;/td&gt;
&lt;! &lt;td width="10"&gt;&amp;nbsp;&lt;/td&gt;
&lt;td width="90%"&gt;

&lt;b&gt;&lt;font color="#0000FF" size="4"&gt;TRIM-POT CROSS REFERENCE&lt;/font&gt;&lt;/b&gt;
&lt;P&gt;
&lt;TABLE BORDER=0 CELLSPACING=1 CELLPADDING=2&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;RECTANGULAR MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;BOURNS&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;BI&amp;nbsp;TECH&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;DALE-VISHAY&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;PHILIPS/MEPCO&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;MURATA&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;PANASONIC&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;SPECTROL&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;MILSPEC&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;&lt;TD&gt;&amp;nbsp;&lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3 &gt;
      3005P&lt;BR&gt;
      3006P&lt;BR&gt;
      3006W&lt;BR&gt;
      3006Y&lt;BR&gt;
      3009P&lt;BR&gt;
      3009W&lt;BR&gt;
      3009Y&lt;BR&gt;
      3057J&lt;BR&gt;
      3057L&lt;BR&gt;
      3057P&lt;BR&gt;
      3057Y&lt;BR&gt;
      3059J&lt;BR&gt;
      3059L&lt;BR&gt;
      3059P&lt;BR&gt;
      3059Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      89P&lt;BR&gt;
      89W&lt;BR&gt;
      89X&lt;BR&gt;
      89PH&lt;BR&gt;
      76P&lt;BR&gt;
      89XH&lt;BR&gt;
      78SLT&lt;BR&gt;
      78L&amp;nbsp;ALT&lt;BR&gt;
      56P&amp;nbsp;ALT&lt;BR&gt;
      78P&amp;nbsp;ALT&lt;BR&gt;
      T8S&lt;BR&gt;
      78L&lt;BR&gt;
      56P&lt;BR&gt;
      78P&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      T18/784&lt;BR&gt;
      783&lt;BR&gt;
      781&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      2199&lt;BR&gt;
      1697/1897&lt;BR&gt;
      1680/1880&lt;BR&gt;
      2187&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      8035EKP/CT20/RJ-20P&lt;BR&gt;
      -&lt;BR&gt;
      RJ-20X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      1211L&lt;BR&gt;
      8012EKQ&amp;nbsp;ALT&lt;BR&gt;
      8012EKR&amp;nbsp;ALT&lt;BR&gt;
      1211P&lt;BR&gt;
      8012EKJ&lt;BR&gt;
      8012EKL&lt;BR&gt;
      8012EKQ&lt;BR&gt;
      8012EKR&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      2101P&lt;BR&gt;
      2101W&lt;BR&gt;
      2101Y&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      2102L&lt;BR&gt;
      2102S&lt;BR&gt;
      2102Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      EVMCOG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      43P&lt;BR&gt;
      43W&lt;BR&gt;
      43Y&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      40L&lt;BR&gt;
      40P&lt;BR&gt;
      40Y&lt;BR&gt;
      70Y-T602&lt;BR&gt;
      70L&lt;BR&gt;
      70P&lt;BR&gt;
      70Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      -&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SQUARE MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
   &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MURATA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;SPECTROL&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MILSPEC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3250L&lt;BR&gt;
      3250P&lt;BR&gt;
      3250W&lt;BR&gt;
      3250X&lt;BR&gt;
      3252P&lt;BR&gt;
      3252W&lt;BR&gt;
      3252X&lt;BR&gt;
      3260P&lt;BR&gt;
      3260W&lt;BR&gt;
      3260X&lt;BR&gt;
      3262P&lt;BR&gt;
      3262W&lt;BR&gt;
      3262X&lt;BR&gt;
      3266P&lt;BR&gt;
      3266W&lt;BR&gt;
      3266X&lt;BR&gt;
      3290H&lt;BR&gt;
      3290P&lt;BR&gt;
      3290W&lt;BR&gt;
      3292P&lt;BR&gt;
      3292W&lt;BR&gt;
      3292X&lt;BR&gt;
      3296P&lt;BR&gt;
      3296W&lt;BR&gt;
      3296X&lt;BR&gt;
      3296Y&lt;BR&gt;
      3296Z&lt;BR&gt;
      3299P&lt;BR&gt;
      3299W&lt;BR&gt;
      3299X&lt;BR&gt;
      3299Y&lt;BR&gt;
      3299Z&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      -&lt;BR&gt;
      64W&amp;nbsp;ALT&lt;BR&gt;
      -&lt;BR&gt;
      64P&amp;nbsp;ALT&lt;BR&gt;
      64W&amp;nbsp;ALT&lt;BR&gt;
      64X&amp;nbsp;ALT&lt;BR&gt;
      64P&lt;BR&gt;
      64W&lt;BR&gt;
      64X&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66P&lt;BR&gt;
      66W&lt;BR&gt;
      66X&lt;BR&gt;
      67P&lt;BR&gt;
      67W&lt;BR&gt;
      67X&lt;BR&gt;
      67Y&lt;BR&gt;
      67Z&lt;BR&gt;
      68P&lt;BR&gt;
      68W&lt;BR&gt;
      68X&lt;BR&gt;
      67Y&amp;nbsp;ALT&lt;BR&gt;
      67Z&amp;nbsp;ALT&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      5050&lt;BR&gt;
      5091&lt;BR&gt;
      5080&lt;BR&gt;
      5087&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T63YB&lt;BR&gt;
      T63XB&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      5887&lt;BR&gt;
      5891&lt;BR&gt;
      5880&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T93Z&lt;BR&gt;
      T93YA&lt;BR&gt;
      T93XA&lt;BR&gt;
      T93YB&lt;BR&gt;
      T93XB&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8026EKP&lt;BR&gt;
      8026EKW&lt;BR&gt;
      8026EKM&lt;BR&gt;
      8026EKP&lt;BR&gt;
      8026EKB&lt;BR&gt;
      8026EKM&lt;BR&gt;
      1309X&lt;BR&gt;
      1309P&lt;BR&gt;
      1309W&lt;BR&gt;
      8024EKP&lt;BR&gt;
      8024EKW&lt;BR&gt;
      8024EKN&lt;BR&gt;
      RJ-9P/CT9P&lt;BR&gt;
      RJ-9W&lt;BR&gt;
      RJ-9X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3103P&lt;BR&gt;
      3103Y&lt;BR&gt;
      3103Z&lt;BR&gt;
      3103P&lt;BR&gt;
      3103Y&lt;BR&gt;
      3103Z&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3105P/3106P&lt;BR&gt;
      3105W/3106W&lt;BR&gt;
      3105X/3106X&lt;BR&gt;
      3105Y/3106Y&lt;BR&gt;
      3105Z/3105Z&lt;BR&gt;
      3102P&lt;BR&gt;
      3102W&lt;BR&gt;
      3102X&lt;BR&gt;
      3102Y&lt;BR&gt;
      3102Z&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMCBG&lt;BR&gt;
      EVMCCG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      55-1-X&lt;BR&gt;
      55-4-X&lt;BR&gt;
      55-3-X&lt;BR&gt;
      55-2-X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      50-2-X&lt;BR&gt;
      50-4-X&lt;BR&gt;
      50-3-X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      64P&lt;BR&gt;
      64W&lt;BR&gt;
      64X&lt;BR&gt;
      64Y&lt;BR&gt;
      64Z&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SINGLE TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MURATA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;SPECTROL&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MILSPEC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3323P&lt;BR&gt;
      3323S&lt;BR&gt;
      3323W&lt;BR&gt;
      3329H&lt;BR&gt;
      3329P&lt;BR&gt;
      3329W&lt;BR&gt;
      3339H&lt;BR&gt;
      3339P&lt;BR&gt;
      3339W&lt;BR&gt;
      3352E&lt;BR&gt;
      3352H&lt;BR&gt;
      3352K&lt;BR&gt;
      3352P&lt;BR&gt;
      3352T&lt;BR&gt;
      3352V&lt;BR&gt;
      3352W&lt;BR&gt;
      3362H&lt;BR&gt;
      3362M&lt;BR&gt;
      3362P&lt;BR&gt;
      3362R&lt;BR&gt;
      3362S&lt;BR&gt;
      3362U&lt;BR&gt;
      3362W&lt;BR&gt;
      3362X&lt;BR&gt;
      3386B&lt;BR&gt;
      3386C&lt;BR&gt;
      3386F&lt;BR&gt;
      3386H&lt;BR&gt;
      3386K&lt;BR&gt;
      3386M&lt;BR&gt;
      3386P&lt;BR&gt;
      3386S&lt;BR&gt;
      3386W&lt;BR&gt;
      3386X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      25P&lt;BR&gt;
      25S&lt;BR&gt;
      25RX&lt;BR&gt;
      82P&lt;BR&gt;
      82M&lt;BR&gt;
      82PA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      91E&lt;BR&gt;
      91X&lt;BR&gt;
      91T&lt;BR&gt;
      91B&lt;BR&gt;
      91A&lt;BR&gt;
      91V&lt;BR&gt;
      91W&lt;BR&gt;
      25W&lt;BR&gt;
      25V&lt;BR&gt;
      25P&lt;BR&gt;
      -&lt;BR&gt;
      25S&lt;BR&gt;
      25U&lt;BR&gt;
      25RX&lt;BR&gt;
      25X&lt;BR&gt;
      72XW&lt;BR&gt;
      72XL&lt;BR&gt;
      72PM&lt;BR&gt;
      72RX&lt;BR&gt;
      -&lt;BR&gt;
      72PX&lt;BR&gt;
      72P&lt;BR&gt;
      72RXW&lt;BR&gt;
      72RXL&lt;BR&gt;
      72X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T7YB&lt;BR&gt;
      T7YA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      TXD&lt;BR&gt;
      TYA&lt;BR&gt;
      TYP&lt;BR&gt;
      -&lt;BR&gt;
      TYD&lt;BR&gt;
      TX&lt;BR&gt;
      -&lt;BR&gt;
      150SX&lt;BR&gt;
      100SX&lt;BR&gt;
      102T&lt;BR&gt;
      101S&lt;BR&gt;
      190T&lt;BR&gt;
      150TX&lt;BR&gt;
      101&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      101SX&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ET6P&lt;BR&gt;
      ET6S&lt;BR&gt;
      ET6X&lt;BR&gt;
      RJ-6W/8014EMW&lt;BR&gt;
      RJ-6P/8014EMP&lt;BR&gt;
      RJ-6X/8014EMX&lt;BR&gt;
      TM7W&lt;BR&gt;
      TM7P&lt;BR&gt;
      TM7X&lt;BR&gt;
      -&lt;BR&gt;
      8017SMS&lt;BR&gt;
      -&lt;BR&gt;
      8017SMB&lt;BR&gt;
      8017SMA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      CT-6W&lt;BR&gt;
      CT-6H&lt;BR&gt;
      CT-6P&lt;BR&gt;
      CT-6R&lt;BR&gt;
      -&lt;BR&gt;
      CT-6V&lt;BR&gt;
      CT-6X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8038EKV&lt;BR&gt;
      -&lt;BR&gt;
      8038EKX&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8038EKP&lt;BR&gt;
      8038EKZ&lt;BR&gt;
      8038EKW&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3321H&lt;BR&gt;
      3321P&lt;BR&gt;
      3321N&lt;BR&gt;
      1102H&lt;BR&gt;
      1102P&lt;BR&gt;
      1102T&lt;BR&gt;
      RVA0911V304A&lt;BR&gt;
      -&lt;BR&gt;
      RVA0911H413A&lt;BR&gt;
      RVG0707V100A&lt;BR&gt;
      RVA0607V(H)306A&lt;BR&gt;
      RVA1214H213A&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3104B&lt;BR&gt;
      3104C&lt;BR&gt;
      3104F&lt;BR&gt;
      3104H&lt;BR&gt;
      -&lt;BR&gt;
      3104M&lt;BR&gt;
      3104P&lt;BR&gt;
      3104S&lt;BR&gt;
      3104W&lt;BR&gt;
      3104X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      EVMQ0G&lt;BR&gt;
      EVMQIG&lt;BR&gt;
      EVMQ3G&lt;BR&gt;
      EVMS0G&lt;BR&gt;
      EVMQ0G&lt;BR&gt;
      EVMG0G&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMK4GA00B&lt;BR&gt;
      EVM30GA00B&lt;BR&gt;
      EVMK0GA00B&lt;BR&gt;
      EVM38GA00B&lt;BR&gt;
      EVMB6&lt;BR&gt;
      EVLQ0&lt;BR&gt;
      -&lt;BR&gt;
      EVMMSG&lt;BR&gt;
      EVMMBG&lt;BR&gt;
      EVMMAG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMMCS&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM1&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM0&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM3&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      62-3-1&lt;BR&gt;
      62-1-2&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      67R&lt;BR&gt;
      -&lt;BR&gt;
      67P&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      67X&lt;BR&gt;
      63V&lt;BR&gt;
      63S&lt;BR&gt;
      63M&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      63H&lt;BR&gt;
      63P&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      63X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;
&lt;P&gt;&amp;nbsp;&lt;P&gt;
&lt;TABLE BORDER=0 CELLSPACING=1 CELLPADDING=3&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;
      &lt;FONT color="#0000FF" SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SMD TRIM-POT CROSS REFERENCE&lt;/B&gt;&lt;/FONT&gt;
      &lt;P&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURNS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;TOCOS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AUX/KYOCERA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3224G&lt;BR&gt;
      3224J&lt;BR&gt;
      3224W&lt;BR&gt;
      3269P&lt;BR&gt;
      3269W&lt;BR&gt;
      3269X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      44G&lt;BR&gt;
      44J&lt;BR&gt;
      44W&lt;BR&gt;
      84P&lt;BR&gt;
      84W&lt;BR&gt;
      84X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST63Z&lt;BR&gt;
      ST63Y&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST5P&lt;BR&gt;
      ST5W&lt;BR&gt;
      ST5X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SINGLE TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURNS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;TOCOS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AUX/KYOCERA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3314G&lt;BR&gt;
      3314J&lt;BR&gt;
      3364A/B&lt;BR&gt;
      3364C/D&lt;BR&gt;
      3364W/X&lt;BR&gt;
      3313G&lt;BR&gt;
      3313J&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      23B&lt;BR&gt;
      23A&lt;BR&gt;
      21X&lt;BR&gt;
      21W&lt;BR&gt;
      -&lt;BR&gt;
      22B&lt;BR&gt;
      22A&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ST5YL/ST53YL&lt;BR&gt;
      ST5YJ/5T53YJ&lt;BR&gt;
      ST-23A&lt;BR&gt;
      ST-22B&lt;BR&gt;
      ST-22&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ST-4B&lt;BR&gt;
      ST-4A&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST-3B&lt;BR&gt;
      ST-3A&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      EVM-6YS&lt;BR&gt;
      EVM-1E&lt;BR&gt;
      EVM-1G&lt;BR&gt;
      EVM-1D&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      G4B&lt;BR&gt;
      G4A&lt;BR&gt;
      TR04-3S1&lt;BR&gt;
      TRG04-2S1&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      DVR-43A&lt;BR&gt;
      CVR-42C&lt;BR&gt;
      CVR-42A/C&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;
&lt;P&gt;
&lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;ALT =&amp;nbsp;ALTERNATE&lt;/B&gt;&lt;/FONT&gt;
&lt;P&gt;

&amp;nbsp;
&lt;P&gt;
&lt;/td&gt;
&lt;/tr&gt;
&lt;/table&gt;
&lt;/BODY&gt;&lt;/HTML&gt;</description>
<packages>
<package name="C1210">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SJ-43514-SMT">
<packages>
<package name="CUI_SJ-43514-SMT">
</package>
</packages>
</library>
<library name="Adafruit Feather M0 Express">
<description>Generated from &lt;b&gt;Adafruit Feather M0 Express.sch&lt;/b&gt;&lt;p&gt;
by exp-lbrs.ulp</description>
<packages>
<package name="MICROBUILDER_SOIC8_150MIL">
<description>&lt;b&gt;Small Outline IC - 150mil Wide&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="pygamer-microbuilder">
<packages>
<package name="FEATHERWING_SMT2">
</package>
</packages>
</library>
<library name="resistor array">
<packages>
<package name="EXBV8V">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$2" library="My Stuff" package="EINK_DISPLAY_4_2IN" value="WAVESHARE_4_2_INCH_EINK_DISPLAY"/>
<element name="MICROSD" library="adafruit" package="MICROSD" value="MICROSD"/>
<element name="C20" library="microbuilder" package="0805-NO" value="1uF/25V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C19" library="microbuilder" package="0805-NO" value="1uF/25V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C21" library="microbuilder" package="0805-NO" value="1uF/25V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C18" library="microbuilder" package="0805-NO" value="1uF/25V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C17" library="microbuilder" package="0805-NO" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C16" library="microbuilder" package="0805-NO" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C15" library="microbuilder" package="0805-NO" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PORT_I2C" library="microbuilder" package="JSTPH4" value="JST PH 4">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C27" library="microbuilder" package="0805-NO" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PORT_A8" library="microbuilder" package="JSTPH3" value="JST PH 3">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R15" library="microbuilder" package="_0805MP" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D5" library="microbuilder" package="SOD-123" value="3.6V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C23" library="microbuilder" package="0805-NO" value="1uF/25V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C22" library="microbuilder" package="0805-NO" value="1uF/25V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D2" library="microbuilder" package="SOD-123" value="MBR0530">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D3" library="microbuilder" package="SOD-123" value="MBR0530">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C24" library="microbuilder" package="0805-NO" value="4.7uF/25V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D4" library="microbuilder" package="SOD-123" value="MBR0530">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L1" library="microbuilder" package="INDUCTOR_4X4MM_NR401" value="10uH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R12" library="microbuilder" package="0805_10MGAP" value="0.47ohm">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q2" library="Parts" package="SOT23-3" value="IRLML0100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SW1" library="My Stuff" package="A10767" value="SPDT_SWITCH">
<attribute name="NAME"/>
</element>
<element name="BTN_PREV_ALT" library="My Stuff" package="TL3330AF130QG" value="SPST_TACTILE_SWITCHRA">
<attribute name="NAME"/>
</element>
<element name="BTN_RESET" library="My Stuff" package="TL3330AF130QG" value="SPST_TACTILE_SWITCHRA">
<attribute name="NAME"/>
</element>
<element name="PORT_A9" library="microbuilder" package="JSTPH3" value="JST PH 3">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R16" library="microbuilder" package="_0805MP" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D6" library="microbuilder" package="SOD-123" value="3.6V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C25" library="microbuilder" package="0805_10MGAP" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C26" library="microbuilder" package="0805_10MGAP" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C14" library="microbuilder" package="0805-NO" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="BTN_NEXT_ALT" library="My Stuff" package="TL3330AF130QG" value="SPST_TACTILE_SWITCHRA">
<attribute name="NAME"/>
</element>
<element name="JP1" library="adafruit" package="1X03" value="">
<attribute name="VALUE"/>
</element>
<element name="GOLD_ORB_SM1" library="oshw" package="OSHW_5MM" value="OSHWLOGOLOGO5MM"/>
<element name="U$1" library="microbuilder" package="MOUNTINGHOLE_2.5_PLATED" value="MOUNTINGHOLE2.5">
<attribute name="BOM" value="EXCLUDE"/>
</element>
<element name="U$4" library="microbuilder" package="MOUNTINGHOLE_2.5_PLATED" value="MOUNTINGHOLE2.5">
<attribute name="BOM" value="EXCLUDE"/>
</element>
<element name="FID1" library="microbuilder" package="FIDUCIAL_1MM" value="FIDUCIAL_1MM">
<attribute name="BOM" value="EXCLUDE"/>
</element>
<element name="FID2" library="microbuilder" package="FIDUCIAL_1MM" value="FIDUCIAL_1MM">
<attribute name="BOM" value="EXCLUDE"/>
</element>
<element name="FID3" library="microbuilder" package="FIDUCIAL_1MM" value="FIDUCIAL_1MM">
<attribute name="BOM" value="EXCLUDE"/>
</element>
<element name="FID4" library="microbuilder" package="FIDUCIAL_1MM" value="FIDUCIAL_1MM">
<attribute name="BOM" value="EXCLUDE"/>
</element>
<element name="U$5" library="microbuilder" package="MOUNTINGHOLE_2.5_PLATED" value="MOUNTINGHOLE2.5">
<attribute name="BOM" value="EXCLUDE"/>
</element>
<element name="U$7" library="microbuilder" package="MOUNTINGHOLE_2.5_PLATED" value="MOUNTINGHOLE2.5">
<attribute name="BOM" value="EXCLUDE"/>
</element>
<element name="JP2" library="adafruit" package="1X01" value="">
<attribute name="VALUE"/>
</element>
<element name="BTN_LOCK" library="My Stuff" package="TL3330AF130QG" value="SPST_TACTILE_SWITCHRA"/>
<element name="TP6" library="microbuilder" package="TESTPOINT_ROUND_2MM_NO" value=""/>
<element name="TP7" library="microbuilder" package="TESTPOINT_ROUND_2MM_NO" value=""/>
<element name="TP8" library="microbuilder" package="TESTPOINT_ROUND_2MM_NO" value=""/>
<element name="X2" library="microbuilder" package="2X05_1.27MM_BOX_POSTS" value="2x5 0.05&quot; SWD">
<attribute name="VALUE"/>
</element>
<element name="R5" library="microbuilder" package="0805_10MGAP" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="microbuilder" package="0805_10MGAP" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="microbuilder" package="0805_10MGAP" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U3" library="Open Book Library" package="TQFP64-10X10" value="ATSAMD51J64-TQFP(10X10)">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="10118193-0001LF" package="FCI_10118193-0001LF" value="10118193-0001LF">
<attribute name="DESCRIPTION" value=" Single Port 5 Contact Shielded SMT MICRO USB B-Type Receptacle "/>
<attribute name="DIGI-KEY_PART_NUMBER" value="609-4616-1-ND"/>
<attribute name="DIGI-KEY_PURCHASE_URL" value="https://www.digikey.com/product-detail/en/amphenol-icc-fci/10118193-0001LF/609-4616-1-ND/2785380?utm_source=snapeda&amp;utm_medium=aggregator&amp;utm_campaign=symbol"/>
<attribute name="MF" value="Amphenol ICC"/>
<attribute name="MP" value="10118193-0001LF"/>
<attribute name="PACKAGE" value="None"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="microbuilder" package="0805-NO" value="10µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="microbuilder" package="0805-NO" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="microbuilder" package="0805-NO" value="10µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="microbuilder" package="SOT23-5" value="AP2112-3.3">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X1" library="microbuilder" package="JSTPH2" value="JSTPH">
<attribute name="VALUE"/>
</element>
<element name="C5" library="microbuilder" package="0805_10MGAP" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="microbuilder" package="0805_10MGAP" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="microbuilder" package="0805-NO" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="microbuilder" package="SOD-123" value="MBR120">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q1" library="microbuilder" package="SOT23-R" value="DMG341">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="microbuilder" package="0805-NO" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U2" library="microbuilder" package="SOT23-5" value="MCP73831T-2ACI/OT">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="microbuilder" package="0805-NO" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="microbuilder" package="0805-NO" value="10µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="microbuilder" package="0805-NO" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="microbuilder" package="0805-NO" value="100K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="microbuilder" package="0805-NO" value="100K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="microbuilder" package="0805-NO" value="100K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U4" library="microbuilder" package="SOIC8_150MIL" value="GD25Q16C (or GD25Q32C)">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="microbuilder" package="0805-NO" value="100K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="microbuilder" package="0805-NO" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="FB2" library="microbuilder" package="0805" value="Ferrite">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C30" library="resistor" package="C1210" value="100uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C31" library="resistor" package="C1210" value="100uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R20" library="microbuilder" package="0805-NO" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R19" library="microbuilder" package="0805-NO" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R17" library="microbuilder" package="0805-NO" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R18" library="microbuilder" package="0805-NO" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U5" library="microbuilder" package="SO16" value="74AC165D">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="SJ-43514-SMT" package="CUI_SJ-43514-SMT" value="SJ-43514-SMT">
<attribute name="CUI_PURCHASE_URL" value="https://www.cui.com/product/interconnect/connectors/audio-connectors/jacks/sj-4351x-smt-series?utm_source=snapeda.com&amp;utm_medium=referral&amp;utm_campaign=snapedaBOM"/>
<attribute name="DESCRIPTION" value="3.5 mm, 4 Conductors, Right Angle, Surface Mount _SMT_, Audio Jack Connector"/>
<attribute name="DIGI-KEY_PART_NUMBER" value="CP-43514SJCT-ND"/>
<attribute name="DIGI-KEY_PURCHASE_URL" value="https://www.digikey.com/product-detail/en/cui-inc/SJ-43514-SMT-TR/CP-43514SJCT-ND/669734?utm_source=snapeda&amp;utm_medium=aggregator&amp;utm_campaign=symbol"/>
<attribute name="MF" value="CUI Inc."/>
<attribute name="MP" value="SJ-43514-SMT-TR"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="None"/>
<attribute name="VALUE"/>
</element>
<element name="FID5" library="microbuilder" package="FIDUCIAL_1MM" value="FIDUCIAL_1MM">
<attribute name="BOM" value="EXCLUDE"/>
</element>
<element name="FID6" library="microbuilder" package="FIDUCIAL_1MM" value="FIDUCIAL_1MM">
<attribute name="BOM" value="EXCLUDE"/>
</element>
<element name="FB1" library="microbuilder" package="0805" value="Ferrite">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C12" library="microbuilder" package="0805-NO" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C11" library="microbuilder" package="0805-NO" value="10µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U6" library="Adafruit Feather M0 Express" package="MICROBUILDER_SOIC8_150MIL" value="GD25Q16C (or GD25Q32C)">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C28" library="microbuilder" package="0805_10MGAP" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U7" library="microbuilder" package="SOIC8_150MIL" value="23K256-I/SN">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C29" library="microbuilder" package="0805_10MGAP" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP1" library="microbuilder" package="TESTPOINT_ROUND_2MM_NO" value=""/>
<element name="TP2" library="microbuilder" package="TESTPOINT_ROUND_2MM_NO" value=""/>
<element name="C8" library="microbuilder" package="0805_10MGAP" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$44" library="My Stuff" package="OSO_GRAPHIC" value="OSO_GRAPHIC"/>
<element name="U$45" library="My Stuff" package="OSO_BEAR_750MIL" value="OSO_BEAR"/>
<element name="U$47" library="My Stuff" package="OSO_TEXT_435MIL" value="OSO_TEXT"/>
<element name="U$48" library="My Stuff" package="OSO_ONELINE_125MIL" value="OSO_TEXTOSO_TEXT_ONELINE_125MIL"/>
<element name="LED" library="adafruit" package="CHIP-LED0805" value="RED">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CHG" library="adafruit" package="CHIP-LED0805" value="AMBER">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="STATUS" library="adafruit" package="LED3535" value="WS2812B3535"/>
<element name="MS1" library="pygamer-microbuilder" package="FEATHERWING_SMT2" value="FEATHERWING_SMTDUAL"/>
<element name="U$23" library="My Stuff" package="MJTP1250-TRY2" value="SPST_TACTILE_SWITCHTHRU-SECONDTRY"/>
<element name="U$46" library="My Stuff" package="MJTP1250-TRY2" value="SPST_TACTILE_SWITCHTHRU-SECONDTRY"/>
<element name="U$49" library="My Stuff" package="MJTP1250-TRY2" value="SPST_TACTILE_SWITCHTHRU-SECONDTRY"/>
<element name="U$50" library="My Stuff" package="MJTP1250-TRY2" value="SPST_TACTILE_SWITCHTHRU-SECONDTRY"/>
<element name="U$51" library="My Stuff" package="MJTP1250-TRY2" value="SPST_TACTILE_SWITCHTHRU-SECONDTRY"/>
<element name="U$52" library="My Stuff" package="MJTP1250-TRY2" value="SPST_TACTILE_SWITCHTHRU-SECONDTRY"/>
<element name="U$53" library="My Stuff" package="MJTP1250-TRY2" value="SPST_TACTILE_SWITCHTHRU-SECONDTRY"/>
<element name="U8" library="microbuilder" package="SC70-5" value="MAX4466EXK+T">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C32" library="microbuilder" package="0805-NO" value="0.1µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C33" library="microbuilder" package="0805-NO" value="0.01uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R23" library="microbuilder" package="0805-NO" value="1M">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R24" library="microbuilder" package="0805-NO" value="1M">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C34" library="microbuilder" package="0805-NO" value="100pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R26" library="microbuilder" package="0805-NO" value="100K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C35" library="microbuilder" package="0805-NO" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R21" library="microbuilder" package="0805-NO" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R22" library="microbuilder" package="0805-NO" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R25" library="microbuilder" package="0805-NO" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R13" library="resistor array" package="EXBV8V" value="100K">
<attribute name="MANUFACTURER_PART_NUMBER" value="EXBV8V103JV"/>
<attribute name="NAME"/>
<attribute name="VENDOR" value="Panasonic"/>
</element>
<element name="R14" library="resistor array" package="EXBV8V" value="100K">
<attribute name="MANUFACTURER_PART_NUMBER" value="EXBV8V103JV"/>
<attribute name="NAME"/>
<attribute name="VENDOR" value="Panasonic"/>
</element>
<element name="R6" library="microbuilder" package="0805_10MGAP" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C13" library="microbuilder" package="0805_10MGAP" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="microbuilder" package="0805_10MGAP" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="MICROSD" pad="6"/>
<contactref element="MICROSD" pad="MT1"/>
<contactref element="MICROSD" pad="MT2"/>
<contactref element="C17" pad="1"/>
<contactref element="C18" pad="1"/>
<contactref element="U$2" pad="17"/>
<contactref element="C19" pad="1"/>
<contactref element="C20" pad="1"/>
<contactref element="C21" pad="1"/>
<contactref element="U$2" pad="8"/>
<contactref element="C15" pad="1"/>
<contactref element="C16" pad="1"/>
<contactref element="PORT_I2C" pad="1"/>
<contactref element="PORT_A8" pad="1"/>
<contactref element="D5" pad="A"/>
<contactref element="D2" pad="C"/>
<contactref element="C22" pad="2"/>
<contactref element="R12" pad="2"/>
<contactref element="C23" pad="2"/>
<contactref element="SW1" pad="P$3"/>
<contactref element="PORT_A9" pad="1"/>
<contactref element="D6" pad="A"/>
<contactref element="C25" pad="2"/>
<contactref element="C27" pad="2"/>
<contactref element="C26" pad="2"/>
<contactref element="JP1" pad="2"/>
<contactref element="X2" pad="3"/>
<contactref element="X2" pad="5"/>
<contactref element="C9" pad="2"/>
<contactref element="C10" pad="2"/>
<contactref element="U3" pad="7"/>
<contactref element="U3" pad="22"/>
<contactref element="U3" pad="33"/>
<contactref element="U3" pad="47"/>
<contactref element="U3" pad="54"/>
<contactref element="J2" pad="S2"/>
<contactref element="J2" pad="S5"/>
<contactref element="J2" pad="S4"/>
<contactref element="J2" pad="S3"/>
<contactref element="J2" pad="S1"/>
<contactref element="J2" pad="S6"/>
<contactref element="U1" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="X1" pad="1"/>
<contactref element="C5" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="U2" pad="2"/>
<contactref element="R9" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="U4" pad="4"/>
<contactref element="C14" pad="2"/>
<contactref element="FB2" pad="2"/>
<contactref element="U5" pad="8"/>
<contactref element="U5" pad="10"/>
<contactref element="U5" pad="15"/>
<contactref element="C12" pad="2"/>
<contactref element="C11" pad="2"/>
<contactref element="U6" pad="4"/>
<contactref element="C28" pad="2"/>
<contactref element="U7" pad="4"/>
<contactref element="C29" pad="2"/>
<contactref element="J2" pad="5"/>
<contactref element="TP1" pad="P$1"/>
<contactref element="C8" pad="2"/>
<contactref element="LED" pad="C"/>
<contactref element="STATUS" pad="4"/>
<contactref element="MS1" pad="4"/>
<contactref element="MS1" pad="4'"/>
<contactref element="MS1" pad="16"/>
<contactref element="MS1" pad="16'"/>
<contactref element="BTN_LOCK" pad="P$2"/>
<contactref element="R13" pad="6"/>
<contactref element="R14" pad="8"/>
<contactref element="R13" pad="7"/>
<contactref element="R13" pad="8"/>
<contactref element="R14" pad="5"/>
<contactref element="R14" pad="6"/>
<contactref element="R14" pad="7"/>
<contactref element="BTN_RESET" pad="P$1"/>
<contactref element="C13" pad="1"/>
</signal>
<signal name="EINK_CS">
<contactref element="U$2" pad="12"/>
<contactref element="U3" pad="10"/>
</signal>
<signal name="EINK_DC">
<contactref element="U$2" pad="11"/>
<contactref element="U3" pad="6"/>
</signal>
<signal name="EINK_BUSY">
<contactref element="U$2" pad="9"/>
<contactref element="U3" pad="2"/>
</signal>
<signal name="A1">
<contactref element="U3" pad="14"/>
<contactref element="R19" pad="2"/>
<contactref element="MS1" pad="6'"/>
<contactref element="MS1" pad="6"/>
</signal>
<signal name="A0">
<contactref element="U3" pad="3"/>
<contactref element="R17" pad="2"/>
<contactref element="MS1" pad="5"/>
<contactref element="MS1" pad="5'"/>
</signal>
<signal name="SCK">
<contactref element="MICROSD" pad="5"/>
<contactref element="U3" pad="36"/>
<contactref element="U6" pad="6"/>
<contactref element="MS1" pad="11"/>
<contactref element="MS1" pad="11'"/>
</signal>
<signal name="MOSI">
<contactref element="MICROSD" pad="3"/>
<contactref element="U3" pad="50"/>
<contactref element="U6" pad="5"/>
<contactref element="MS1" pad="12"/>
<contactref element="MS1" pad="12'"/>
</signal>
<signal name="MISO">
<contactref element="MICROSD" pad="7"/>
<contactref element="U3" pad="49"/>
<contactref element="U6" pad="2"/>
<contactref element="MS1" pad="13'"/>
<contactref element="MS1" pad="13"/>
</signal>
<signal name="RX">
<contactref element="JP1" pad="3"/>
<contactref element="U3" pad="40"/>
<contactref element="MS1" pad="14"/>
<contactref element="MS1" pad="14'"/>
</signal>
<signal name="TX">
<contactref element="JP1" pad="1"/>
<contactref element="U3" pad="39"/>
<contactref element="MS1" pad="15"/>
<contactref element="MS1" pad="15'"/>
</signal>
<signal name="SCL">
<contactref element="PORT_I2C" pad="4"/>
<contactref element="U3" pad="30"/>
<contactref element="MS1" pad="18'"/>
<contactref element="MS1" pad="18"/>
</signal>
<signal name="SDA">
<contactref element="PORT_I2C" pad="3"/>
<contactref element="U3" pad="29"/>
<contactref element="MS1" pad="17"/>
<contactref element="MS1" pad="17'"/>
</signal>
<signal name="EN">
<contactref element="SW1" pad="P$2"/>
<contactref element="U1" pad="3"/>
<contactref element="R1" pad="1"/>
<contactref element="MS1" pad="27'"/>
<contactref element="MS1" pad="27"/>
</signal>
<signal name="+3V3">
<contactref element="L1" pad="P$2"/>
<contactref element="U$2" pad="15"/>
<contactref element="C17" pad="2"/>
<contactref element="U$2" pad="16"/>
<contactref element="MICROSD" pad="4"/>
<contactref element="C25" pad="1"/>
<contactref element="C26" pad="1"/>
<contactref element="C27" pad="1"/>
<contactref element="PORT_I2C" pad="2"/>
<contactref element="PORT_A8" pad="2"/>
<contactref element="PORT_A9" pad="2"/>
<contactref element="JP2" pad="1"/>
<contactref element="R5" pad="1"/>
<contactref element="X2" pad="1"/>
<contactref element="U3" pad="21"/>
<contactref element="U3" pad="34"/>
<contactref element="U3" pad="48"/>
<contactref element="U3" pad="56"/>
<contactref element="C3" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="U1" pad="5"/>
<contactref element="C5" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="C7" pad="1"/>
<contactref element="R11" pad="1"/>
<contactref element="U4" pad="8"/>
<contactref element="C14" pad="1"/>
<contactref element="U5" pad="16"/>
<contactref element="FB1" pad="1"/>
<contactref element="U6" pad="7"/>
<contactref element="U6" pad="3"/>
<contactref element="U6" pad="8"/>
<contactref element="C28" pad="1"/>
<contactref element="U7" pad="7"/>
<contactref element="U7" pad="8"/>
<contactref element="C29" pad="1"/>
<contactref element="TP2" pad="P$1"/>
<contactref element="C8" pad="1"/>
<contactref element="MS1" pad="2"/>
<contactref element="MS1" pad="2'"/>
<contactref element="STATUS" pad="2"/>
<contactref element="BTN_PREV_ALT" pad="P$2"/>
<contactref element="BTN_NEXT_ALT" pad="P$2"/>
<contactref element="U$49" pad="P$2"/>
<contactref element="U$51" pad="P$2"/>
<contactref element="U$23" pad="P$2"/>
<contactref element="U$46" pad="P$2"/>
<contactref element="U$50" pad="P$2"/>
<contactref element="U$52" pad="P$2"/>
<contactref element="U$53" pad="P$2"/>
<contactref element="R13" pad="5"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="GDR">
<contactref element="U$2" pad="2"/>
<contactref element="Q2" pad="1"/>
</signal>
<signal name="RESE">
<contactref element="U$2" pad="3"/>
<contactref element="R12" pad="1"/>
<contactref element="Q2" pad="2"/>
</signal>
<signal name="VCOM">
<contactref element="C21" pad="2"/>
<contactref element="U$2" pad="24"/>
</signal>
<signal name="PREVGL">
<contactref element="U$2" pad="23"/>
<contactref element="C22" pad="1"/>
<contactref element="D3" pad="A"/>
</signal>
<signal name="VSL">
<contactref element="U$2" pad="22"/>
<contactref element="C20" pad="2"/>
</signal>
<signal name="PREVGH">
<contactref element="U$2" pad="21"/>
<contactref element="C23" pad="1"/>
<contactref element="D4" pad="C"/>
</signal>
<signal name="VSH">
<contactref element="U$2" pad="20"/>
<contactref element="C19" pad="2"/>
</signal>
<signal name="VDD">
<contactref element="C18" pad="2"/>
<contactref element="U$2" pad="18"/>
</signal>
<signal name="A8_">
<contactref element="PORT_A8" pad="3"/>
<contactref element="R15" pad="1"/>
</signal>
<signal name="AVCC">
<contactref element="U3" pad="4"/>
<contactref element="U3" pad="8"/>
<contactref element="C12" pad="1"/>
<contactref element="C11" pad="1"/>
<contactref element="FB1" pad="2"/>
<contactref element="MS1" pad="3"/>
<contactref element="MS1" pad="3'"/>
<contactref element="U8" pad="5"/>
<contactref element="R22" pad="2"/>
<contactref element="R24" pad="2"/>
</signal>
<signal name="VGH">
<contactref element="U$2" pad="5"/>
<contactref element="C16" pad="2"/>
</signal>
<signal name="VGL">
<contactref element="U$2" pad="4"/>
<contactref element="C15" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="D3" pad="C"/>
<contactref element="D2" pad="A"/>
<contactref element="C24" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="D4" pad="A"/>
<contactref element="L1" pad="P$1"/>
<contactref element="Q2" pad="3"/>
<contactref element="C24" pad="1"/>
</signal>
<signal name="A9_">
<contactref element="PORT_A9" pad="3"/>
<contactref element="R16" pad="1"/>
</signal>
<signal name="A2">
<contactref element="U3" pad="11"/>
<contactref element="MS1" pad="7"/>
<contactref element="MS1" pad="7'"/>
</signal>
<signal name="+3V1">
</signal>
<signal name="USB_P">
<contactref element="U3" pad="46"/>
<contactref element="J2" pad="3"/>
</signal>
<signal name="USB_N">
<contactref element="U3" pad="45"/>
<contactref element="J2" pad="2"/>
</signal>
<signal name="D13">
<contactref element="U3" pad="44"/>
<contactref element="R10" pad="1"/>
<contactref element="MS1" pad="25'"/>
<contactref element="MS1" pad="25"/>
</signal>
<signal name="VBAT">
<contactref element="X1" pad="2"/>
<contactref element="Q1" pad="3"/>
<contactref element="U2" pad="3"/>
<contactref element="C4" pad="1"/>
<contactref element="R8" pad="1"/>
<contactref element="MS1" pad="28"/>
<contactref element="MS1" pad="28'"/>
</signal>
<signal name="A5">
<contactref element="U3" pad="15"/>
<contactref element="MS1" pad="10"/>
<contactref element="MS1" pad="10'"/>
</signal>
<signal name="A4">
<contactref element="U3" pad="13"/>
<contactref element="MS1" pad="9"/>
<contactref element="MS1" pad="9'"/>
</signal>
<signal name="A3">
<contactref element="U3" pad="12"/>
<contactref element="MS1" pad="8'"/>
<contactref element="MS1" pad="8"/>
</signal>
<signal name="D11">
<contactref element="U3" pad="42"/>
<contactref element="MS1" pad="23'"/>
<contactref element="MS1" pad="23"/>
</signal>
<signal name="D12">
<contactref element="U3" pad="43"/>
<contactref element="MS1" pad="24"/>
<contactref element="MS1" pad="24'"/>
</signal>
<signal name="D9">
<contactref element="U3" pad="38"/>
<contactref element="MS1" pad="21'"/>
<contactref element="MS1" pad="21"/>
</signal>
<signal name="D6">
<contactref element="U3" pad="37"/>
<contactref element="MS1" pad="20"/>
<contactref element="MS1" pad="20'"/>
</signal>
<signal name="D5">
<contactref element="U3" pad="35"/>
<contactref element="MS1" pad="19"/>
<contactref element="MS1" pad="19'"/>
</signal>
<signal name="D10">
<contactref element="U3" pad="41"/>
<contactref element="MS1" pad="22"/>
<contactref element="MS1" pad="22'"/>
</signal>
<signal name="!RESET">
<contactref element="X2" pad="10"/>
<contactref element="TP8" pad="P$1"/>
<contactref element="MS1" pad="1'"/>
<contactref element="MS1" pad="1"/>
<contactref element="C13" pad="2"/>
<contactref element="R6" pad="2"/>
<contactref element="R7" pad="2"/>
<contactref element="U3" pad="52"/>
</signal>
<signal name="SDCS">
<contactref element="U3" pad="31"/>
<contactref element="MICROSD" pad="2"/>
</signal>
<signal name="SWCLK">
<contactref element="X2" pad="4"/>
<contactref element="R5" pad="2"/>
<contactref element="U3" pad="57"/>
<contactref element="TP6" pad="P$1"/>
</signal>
<signal name="SWDIO">
<contactref element="X2" pad="2"/>
<contactref element="U3" pad="58"/>
<contactref element="TP7" pad="P$1"/>
</signal>
<signal name="VDDCORE2">
<contactref element="C9" pad="1"/>
<contactref element="C10" pad="1"/>
<contactref element="U3" pad="53"/>
</signal>
<signal name="D8_NEOPIX">
<contactref element="U3" pad="32"/>
<contactref element="STATUS" pad="1"/>
</signal>
<signal name="QSPI_DATA[0]">
<contactref element="U3" pad="17"/>
<contactref element="U4" pad="5"/>
</signal>
<signal name="QSPI_DATA[1]">
<contactref element="U3" pad="18"/>
<contactref element="U4" pad="2"/>
</signal>
<signal name="QSPI_DATA[2]">
<contactref element="U3" pad="19"/>
<contactref element="U4" pad="3"/>
</signal>
<signal name="QSPI_DATA[3]">
<contactref element="U3" pad="20"/>
<contactref element="U4" pad="7"/>
</signal>
<signal name="EINK_RST">
<contactref element="U3" pad="1"/>
<contactref element="U$2" pad="10"/>
</signal>
<signal name="D3_A9">
<contactref element="U3" pad="63"/>
<contactref element="R16" pad="2"/>
<contactref element="D6" pad="C"/>
</signal>
<signal name="QSPI_SCK">
<contactref element="U3" pad="23"/>
<contactref element="U4" pad="6"/>
</signal>
<signal name="QSPI_CS">
<contactref element="U3" pad="24"/>
<contactref element="U4" pad="1"/>
<contactref element="R11" pad="2"/>
</signal>
<signal name="D2_A8">
<contactref element="U3" pad="64"/>
<contactref element="R15" pad="2"/>
<contactref element="D5" pad="C"/>
</signal>
<signal name="EINK_SCK">
<contactref element="U3" pad="26"/>
<contactref element="U$2" pad="13"/>
<contactref element="U7" pad="6"/>
</signal>
<signal name="EINK_MOSI">
<contactref element="U3" pad="28"/>
<contactref element="U$2" pad="14"/>
<contactref element="U7" pad="5"/>
</signal>
<signal name="BUTTON_OUT">
<contactref element="U3" pad="59"/>
<contactref element="U5" pad="9"/>
</signal>
<signal name="BUTTON_CLK">
<contactref element="U3" pad="60"/>
<contactref element="U5" pad="2"/>
</signal>
<signal name="BUTTON_LATCH">
<contactref element="U3" pad="61"/>
<contactref element="U5" pad="1"/>
</signal>
<signal name="A6_VMEAS">
<contactref element="U3" pad="62"/>
<contactref element="R8" pad="2"/>
<contactref element="R9" pad="1"/>
</signal>
<signal name="VBUS">
<contactref element="J2" pad="1"/>
<contactref element="D1" pad="A"/>
<contactref element="Q1" pad="1"/>
<contactref element="U2" pad="4"/>
<contactref element="R2" pad="1"/>
<contactref element="CHG" pad="A"/>
<contactref element="MS1" pad="26"/>
<contactref element="MS1" pad="26'"/>
</signal>
<signal name="N$4">
<contactref element="R4" pad="1"/>
<contactref element="CHG" pad="C"/>
</signal>
<signal name="N$5">
<contactref element="R4" pad="2"/>
<contactref element="U2" pad="1"/>
</signal>
<signal name="PROG">
<contactref element="U2" pad="5"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="R10" pad="2"/>
<contactref element="LED" pad="A"/>
</signal>
<signal name="AUDIO_LEFT">
<contactref element="C31" pad="2"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="AUDIO_RIGHT">
<contactref element="C30" pad="2"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="N$15">
<contactref element="C31" pad="1"/>
<contactref element="R20" pad="2"/>
<contactref element="R19" pad="1"/>
</signal>
<signal name="N$70">
<contactref element="C30" pad="1"/>
<contactref element="R17" pad="1"/>
<contactref element="R18" pad="2"/>
</signal>
<signal name="BUTTON0">
<contactref element="U5" pad="11"/>
<contactref element="U$46" pad="P$1"/>
<contactref element="R14" pad="1"/>
</signal>
<signal name="BUTTON1">
<contactref element="U5" pad="12"/>
<contactref element="R14" pad="2"/>
<contactref element="U$23" pad="P$1"/>
</signal>
<signal name="BUTTON2">
<contactref element="U5" pad="13"/>
<contactref element="R14" pad="3"/>
<contactref element="U$49" pad="P$1"/>
</signal>
<signal name="BUTTON3">
<contactref element="U5" pad="14"/>
<contactref element="U$50" pad="P$1"/>
<contactref element="R14" pad="4"/>
</signal>
<signal name="BUTTON4">
<contactref element="U5" pad="3"/>
<contactref element="U$51" pad="P$1"/>
<contactref element="R13" pad="3"/>
</signal>
<signal name="BUTTON5">
<contactref element="U5" pad="4"/>
<contactref element="R13" pad="2"/>
<contactref element="BTN_PREV_ALT" pad="P$1"/>
<contactref element="U$53" pad="P$1"/>
</signal>
<signal name="BUTTON6">
<contactref element="U5" pad="5"/>
<contactref element="BTN_NEXT_ALT" pad="P$1"/>
<contactref element="U$52" pad="P$1"/>
<contactref element="R13" pad="1"/>
</signal>
<signal name="BUTTON7">
<contactref element="U5" pad="6"/>
<contactref element="R13" pad="4"/>
<contactref element="MICROSD" pad="CD2"/>
</signal>
<signal name="A7_MIC">
<contactref element="U3" pad="5"/>
<contactref element="J1" pad="1"/>
<contactref element="C33" pad="1"/>
<contactref element="R21" pad="1"/>
</signal>
<signal name="AGND">
<contactref element="R20" pad="1"/>
<contactref element="R18" pad="1"/>
<contactref element="FB2" pad="1"/>
<contactref element="J1" pad="4"/>
<contactref element="C32" pad="2"/>
<contactref element="U8" pad="2"/>
<contactref element="R23" pad="1"/>
<contactref element="C35" pad="2"/>
</signal>
<signal name="UNIFONT_CS">
<contactref element="U6" pad="1"/>
<contactref element="U3" pad="9"/>
</signal>
<signal name="EINK_MISO">
<contactref element="U3" pad="25"/>
<contactref element="U7" pad="2"/>
</signal>
<signal name="SRAM_CS">
<contactref element="U7" pad="1"/>
<contactref element="U3" pad="27"/>
</signal>
<signal name="V+">
<contactref element="D1" pad="C"/>
<contactref element="Q1" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="U1" pad="1"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="A10_MICAMP">
<contactref element="U3" pad="16"/>
<contactref element="U8" pad="4"/>
<contactref element="C34" pad="1"/>
<contactref element="R26" pad="2"/>
</signal>
<signal name="N$65">
<contactref element="C32" pad="1"/>
<contactref element="R21" pad="2"/>
<contactref element="R22" pad="1"/>
</signal>
<signal name="N$67">
<contactref element="U8" pad="1"/>
<contactref element="C33" pad="2"/>
<contactref element="R23" pad="2"/>
<contactref element="R24" pad="1"/>
</signal>
<signal name="N$68">
<contactref element="U8" pad="3"/>
<contactref element="R26" pad="1"/>
<contactref element="C34" pad="2"/>
<contactref element="R25" pad="1"/>
</signal>
<signal name="N$69">
<contactref element="C35" pad="1"/>
<contactref element="R25" pad="2"/>
</signal>
<signal name="BUTTONLOCK">
<contactref element="BTN_LOCK" pad="P$1"/>
<contactref element="U3" pad="51"/>
</signal>
<signal name="N$1">
<contactref element="BTN_RESET" pad="P$2"/>
<contactref element="R7" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
