(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (title_block
    (title "Split-stage HEMT amplifier 4K board")
    (date "2022-09-07")
    (rev "1.0")
  )
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "GND")
  (net 2 "1")
  (net 3 "14")
  (net 4 "21")
  (net 5 "20")
  (net 6 "17")
  (net 7 "GNDF")
  (net 8 "SOURCE")
  (net 9 "DRAIN")
  (net 10 "GATE")
  (net 11 "7")
  (net 12 "8")
  (net 13 "c")
  (net 14 "d")
  (net 15 "2")
  (net 16 "3")
  (net 17 "4m")
  (net 18 "e")
  (net 19 "g")
  (footprint "Capacitor_SMD:C_1812_4532Metric_Pad1.57x3.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 71.12 87.376 180)
    (descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference "Сfilt4" (at 3.8 0 90) (layer "F.SilkS"))
    (fp_text value "С" (at 0 2.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "2" smd roundrect (at 2.1375 0 180) (size 1.575 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1587301587)
      (net 13 "c"))
    (pad "8" smd roundrect (at -2.1375 0 180) (size 1.575 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1587301587)
      (net 1 "GND"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MyFootprintLibrary:SOT-23-Handsolder" (layer "F.Cu")
    (tedit 619D1D91)
    (at 58.92 107.726)
    (descr "SOT-23, Standard")
    (tags "SOT-23")
    (attr smd)
    (fp_text reference "Q2" (at -0.254 -2.54) (layer "F.SilkS"))
    (fp_text value "Q_NJFET_GDS" (at 0 2.5) (layer "F.Fab"))
    (fp_text user "G" (at -3.175 -1.27) (layer "F.SilkS"))
    (fp_text user "D" (at -3.175 1.27) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.35 -0.95) (size 1.65 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "GATE"))
    (pad "2" smd rect locked (at -1.35 0.95) (size 1.65 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "DRAIN"))
    (pad "3" smd rect locked (at 1.36 0) (size 1.65 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "SOURCE"))
    (model "${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 29.892 129.520401)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "1" thru_hole circle (at 0 -1.519401) (size 3.81 3.81) (drill 2.54) (layers *.Cu *.Mask)
      (net 7 "GNDF") (solder_mask_margin 1.27))
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 70.858 106.2385 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference "Rsrc2" (at -4.7895 0.254 270) (layer "F.SilkS"))
    (fp_text value "R" (at 0 1.82 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.4875 0 90) (size 1.425 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1754385965)
      (net 8 "SOURCE"))
    (pad "2" smd roundrect locked (at 1.4875 0 90) (size 1.425 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1754385965)
      (net 13 "c"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 68.186856 96.901599 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference "Rfollow" (at 3.175 0) (layer "F.SilkS"))
    (fp_text value "R" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.4875 0 90) (size 1.425 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1754385965)
      (net 14 "d"))
    (pad "2" smd roundrect locked (at 1.4875 0 90) (size 1.425 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1754385965)
      (net 1 "GND"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MyFootprintLibrary:0p1 inch mounting hole" (layer "F.Cu")
    (tedit 61958984)
    (at 29.362144 61.340401)
    (attr through_hole)
    (fp_text reference "J2" (at 0 3.175) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x01" (at 0 -3.175) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0.529856 -0.089401) (size 3.81 3.81) (drill 2.54) (layers *.Cu *.Mask)
      (net 7 "GNDF") (solder_mask_margin 1.27))
  )
  (footprint "Capacitor_SMD:C_1812_4532Metric_Pad1.57x3.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 81.018 87.406 180)
    (descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference "Сfilt5" (at 3.8 0 90) (layer "F.SilkS"))
    (fp_text value "С" (at 0 2.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.1375 0 180) (size 1.575 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1587301587))
    (pad "2" smd roundrect (at 2.1375 0 180) (size 1.575 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1587301587)
      (net 1 "GND"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1812_4532Metric_Pad1.57x3.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 63.786856 88.701599 90)
    (descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference "Сfilt3" (at 3.8 0) (layer "F.SilkS"))
    (fp_text value "С" (at 0 2.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.1375 0 90) (size 1.575 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1587301587)
      (net 19 "g"))
    (pad "2" smd roundrect (at 2.1375 0 90) (size 1.575 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1587301587)
      (net 18 "e"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 34.586856 96.901599 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference "GROUND JUMPERS" (at -4.728401 5.283144) (layer "F.SilkS"))
    (fp_text value "R" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.4875 0 90) (size 1.425 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1754385965)
      (net 1 "GND"))
    (pad "2" smd roundrect locked (at 1.4875 0 90) (size 1.425 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1754385965)
      (net 17 "4m"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "KiCad:380025213L001" (layer "F.Cu")
    (tedit 0)
    (at 58.586856 70.201599 180)
    (descr "380-025-213L001-1")
    (tags "Connector")
    (attr through_hole)
    (fp_text reference "D3" (at 0.420856 2.383599) (layer "F.SilkS"))
    (fp_text value "380025213L001" (at 0 -0.338) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 -0.338) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 7.62 -0.65 180) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask)
      (net 2 "1"))
    (pad "2" thru_hole circle (at 6.35 -0.65 180) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask)
      (net 15 "2"))
    (pad "3" thru_hole circle (at 5.08 -0.65 180) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask)
      (net 16 "3"))
    (pad "4" thru_hole circle (at 3.81 -0.65 180) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask))
    (pad "5" thru_hole circle (at 2.54 -0.65 180) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask))
    (pad "6" thru_hole circle (at 1.27 -0.65 180) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask))
    (pad "7" thru_hole circle (at 0 -0.65 180) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask)
      (net 11 "7"))
    (pad "8" thru_hole circle (at -1.27 -0.65 180) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask)
      (net 12 "8"))
    (pad "9" thru_hole circle (at -2.54 -0.65 180) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask)
      (net 1 "GND"))
    (pad "10" thru_hole circle (at -3.81 -0.65 180) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask)
      (net 1 "GND"))
    (pad "11" thru_hole circle (at -5.08 -0.65 180) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask)
      (net 1 "GND"))
    (pad "12" thru_hole circle (at -6.35 -0.65 180) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask)
      (net 1 "GND"))
    (pad "13" thru_hole circle (at -7.62 -0.65 180) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask)
      (net 1 "GND"))
    (pad "14" thru_hole circle (at 6.99 0.45 180) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask)
      (net 3 "14"))
    (pad "15" thru_hole circle (at 5.72 0.45 180) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask)
      (net 1 "GND"))
    (pad "16" thru_hole circle (at 4.45 0.45 180) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask)
      (net 1 "GND"))
    (pad "17" thru_hole circle (at 3.18 0.45 180) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask)
      (net 1 "GND"))
    (pad "18" thru_hole circle (at 1.91 0.45 180) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask)
      (net 1 "GND"))
    (pad "19" thru_hole circle (at 0.64 0.45 180) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask)
      (net 1 "GND"))
    (pad "20" thru_hole circle (at -0.64 0.45 180) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask)
      (net 5 "20"))
    (pad "21" thru_hole circle (at -1.91 0.45 180) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask)
      (net 4 "21"))
    (pad "22" thru_hole circle (at -3.18 0.45 180) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask)
      (net 1 "GND"))
    (pad "23" thru_hole circle (at -4.45 0.45 180) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask)
      (net 1 "GND"))
    (pad "24" thru_hole circle (at -5.72 0.45 180) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask)
      (net 1 "GND"))
    (pad "25" thru_hole circle (at -6.99 0.45 180) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask)
      (net 1 "GND"))
    (pad "MH1" thru_hole circle (at -12.275 -0.1 180) (size 4.305 4.305) (drill 2.87) (layers *.Cu *.Mask))
    (pad "MH2" thru_hole circle (at 12.275 -0.1 180) (size 4.305 4.305) (drill 2.87) (layers *.Cu *.Mask))
    (model "380-025-213L001.stp"
      (offset (xyz 7.62 0.65 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 44.186856 96.901599 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference "J4" (at 3.175 0) (layer "F.SilkS"))
    (fp_text value "R" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.4875 0 90) (size 1.425 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1754385965))
    (pad "2" smd roundrect locked (at 1.4875 0 90) (size 1.425 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1754385965))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 48.986856 96.901599 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference "J5" (at 3.175 0) (layer "F.SilkS"))
    (fp_text value "R" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.4875 0 90) (size 1.425 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1754385965)
      (net 1 "GND"))
    (pad "2" smd roundrect locked (at 1.4875 0 90) (size 1.425 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1754385965))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Dsub:mdm25-male-footprint" (layer "F.Cu")
    (tedit 0)
    (at 58.42 119.38)
    (descr "380-025-213L001-1")
    (tags "Connector")
    (attr through_hole)
    (fp_text reference "D2" (at 0.420856 2.383599) (layer "F.SilkS"))
    (fp_text value "Conn_01x25_Male" (at 0 -0.338) (layer "F.SilkS") hide)
    (fp_text user "13" (at 8.255 -2.54) (layer "F.SilkS"))
    (fp_text user "25" (at 8.255 2.54) (layer "F.SilkS"))
    (fp_text user "14" (at -8.89 2.54) (layer "F.SilkS"))
    (fp_text user "1" (at -8.255 -2.54) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 -0.338) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -7.62 -0.65) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask))
    (pad "2" thru_hole circle (at -6.35 -0.65) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask))
    (pad "3" thru_hole circle (at -5.08 -0.65) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask))
    (pad "4" thru_hole circle (at -3.81 -0.65) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask)
      (net 14 "d"))
    (pad "5" thru_hole circle (at -2.54 -0.65) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask)
      (net 19 "g"))
    (pad "6" thru_hole circle (at -1.27 -0.65) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask))
    (pad "7" thru_hole circle (at 0 -0.65) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask))
    (pad "8" thru_hole circle (at 1.27 -0.65) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask))
    (pad "9" thru_hole circle (at 2.54 -0.65) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask))
    (pad "10" thru_hole circle (at 3.81 -0.65) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask))
    (pad "11" thru_hole circle (at 5.08 -0.65) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask))
    (pad "12" thru_hole circle (at 6.35 -0.65) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask))
    (pad "13" thru_hole circle (at 7.62 -0.65) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask))
    (pad "14" thru_hole circle (at -6.99 0.45) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask)
      (net 17 "4m"))
    (pad "15" thru_hole circle (at -5.72 0.45) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask)
      (net 17 "4m"))
    (pad "16" thru_hole circle (at -4.45 0.45) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask))
    (pad "17" thru_hole circle (at -3.18 0.45) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask)
      (net 6 "17"))
    (pad "18" thru_hole circle (at -1.91 0.45) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask))
    (pad "19" thru_hole circle (at -0.64 0.45) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask))
    (pad "20" thru_hole circle (at 0.64 0.45) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask))
    (pad "21" thru_hole circle (at 1.91 0.45) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask))
    (pad "22" thru_hole circle (at 3.18 0.45) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask))
    (pad "23" thru_hole circle (at 4.45 0.45) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask))
    (pad "24" thru_hole circle (at 5.72 0.45) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask))
    (pad "25" thru_hole circle (at 6.99 0.45) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask))
    (pad "MH1" thru_hole circle (at -12.275 -0.1) (size 4.305 4.305) (drill 2.87) (layers *.Cu *.Mask))
    (pad "MH2" thru_hole circle (at 12.275 -0.1) (size 4.305 4.305) (drill 2.87) (layers *.Cu *.Mask))
    (model "380-025-213L001.stp"
      (offset (xyz 7.62 0.65 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1812_4532Metric_Pad1.57x3.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 57.386856 88.739099 90)
    (descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference "Сfilt2" (at 3.8 0) (layer "F.SilkS"))
    (fp_text value "С" (at 0 2.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.1375 0 90) (size 1.575 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1587301587)
      (net 19 "g"))
    (pad "2" smd roundrect (at 2.1375 0 90) (size 1.575 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1587301587)
      (net 19 "g"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 58.586856 80.514099 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference "Rfilt6" (at -0.033901 1.857144 90) (layer "F.SilkS"))
    (fp_text value "R" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.4875 0 90) (size 1.425 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1754385965)
      (net 19 "g"))
    (pad "2" smd roundrect locked (at 1.4875 0 90) (size 1.425 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1754385965))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1812_4532Metric_Pad1.57x3.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 36.986856 87.401599)
    (descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference "Сfilt1" (at 3.8 0 90) (layer "F.SilkS"))
    (fp_text value "С" (at 0 2.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.1375 0) (size 1.575 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1587301587)
      (net 17 "4m"))
    (pad "2" smd roundrect (at 2.1375 0) (size 1.575 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1587301587))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 72.986856 96.901599 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference "Rgate" (at -0.380401 -1.866856 90) (layer "F.SilkS"))
    (fp_text value "R" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.4875 0 90) (size 1.425 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1754385965)
      (net 10 "GATE"))
    (pad "2" smd roundrect locked (at 1.4875 0 90) (size 1.425 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1754385965)
      (net 18 "e"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 77.2165 97.03 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference "J9" (at 3.175 0) (layer "F.SilkS"))
    (fp_text value "R" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.4875 0 90) (size 1.425 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1754385965)
      (net 1 "GND"))
    (pad "2" smd roundrect locked (at 1.4875 0 90) (size 1.425 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1754385965)
      (net 13 "c"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1812_4532Metric_Pad1.57x3.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 74.93 105.5885 90)
    (descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference "Сsrc2" (at -5.4395 0 90) (layer "F.SilkS"))
    (fp_text value "С" (at 1.4875 3.15 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.1375 0 90) (size 1.575 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1587301587)
      (net 8 "SOURCE"))
    (pad "2" smd roundrect (at 2.1375 0 90) (size 1.575 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1587301587)
      (net 13 "c"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 95.242 133.126)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "1" thru_hole circle (at -7 -5.125) (size 3.81 3.81) (drill 2.54) (layers *.Cu *.Mask)
      (net 7 "GNDF") (solder_mask_margin 1.27))
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 73.144 80.8385 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference "Rfilt9" (at 0.0365 2.032 270) (layer "F.SilkS"))
    (fp_text value "R" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.4875 0 90) (size 1.425 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1754385965)
      (net 1 "GND"))
    (pad "2" smd roundrect locked (at 1.4875 0 90) (size 1.425 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1754385965)
      (net 12 "8"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 68.064 106.2385 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference "Rsrc1" (at 4.5355 0 90) (layer "F.SilkS"))
    (fp_text value "R" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.4875 0 270) (size 1.425 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1754385965)
      (net 1 "GND"))
    (pad "2" smd roundrect locked (at 1.4875 0 270) (size 1.425 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1754385965)
      (net 8 "SOURCE"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 68.6065 80.5185 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference "Rfilt8" (at -0.0295 1.9975 90) (layer "F.SilkS"))
    (fp_text value "R" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.4875 0 90) (size 1.425 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1754385965)
      (net 13 "c"))
    (pad "2" smd roundrect locked (at 1.4875 0 90) (size 1.425 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1754385965)
      (net 11 "7"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 39.386856 96.901599 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference "J3" (at 3.175 0) (layer "F.SilkS"))
    (fp_text value "R" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.4875 0 90) (size 1.425 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1754385965)
      (net 1 "GND"))
    (pad "2" smd roundrect locked (at 1.4875 0 90) (size 1.425 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1754385965))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 54.186856 80.514099 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference "Rfilt5" (at -0.033901 1.939144 90) (layer "F.SilkS"))
    (fp_text value "R" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.4875 0 90) (size 1.425 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1754385965))
    (pad "2" smd roundrect locked (at 1.4875 0 90) (size 1.425 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1754385965))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MyFootprintLibrary:0p1 inch mounting hole" (layer "F.Cu")
    (tedit 61958984)
    (at 89.092 60.301)
    (attr through_hole)
    (fp_text reference "J2" (at 0 3.175) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x01" (at 0 -3.175) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at -0.85 0.95) (size 3.81 3.81) (drill 2.54) (layers *.Cu *.Mask)
      (net 7 "GNDF") (solder_mask_margin 1.27))
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 81.272 80.5845 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference "Rfilt11" (at 0.0365 2.032 90) (layer "F.SilkS"))
    (fp_text value "R" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.4875 0 90) (size 1.425 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1754385965))
    (pad "2" smd roundrect locked (at 1.4875 0 90) (size 1.425 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1754385965)
      (net 5 "20"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 48.986856 80.514099 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference "Rfilt4" (at -0.033901 1.805144 90) (layer "F.SilkS"))
    (fp_text value "R" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.4875 0 90) (size 1.425 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1754385965))
    (pad "2" smd roundrect locked (at 1.4875 0 90) (size 1.425 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1754385965)
      (net 16 "3"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 63.386856 80.514099 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference "Rfilt7" (at -0.033901 1.883144 90) (layer "F.SilkS"))
    (fp_text value "R" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.4875 0 90) (size 1.425 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1754385965)
      (net 18 "e"))
    (pad "2" smd roundrect locked (at 1.4875 0 90) (size 1.425 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1754385965))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 58.586856 96.901599 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference "J7" (at 3.175 0) (layer "F.SilkS"))
    (fp_text value "R" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.4875 0 90) (size 1.425 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1754385965)
      (net 1 "GND"))
    (pad "2" smd roundrect locked (at 1.4875 0 90) (size 1.425 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1754385965))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 76.954 80.5845 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference "Rfilt10" (at 0.0365 1.778 90) (layer "F.SilkS"))
    (fp_text value "R" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.4875 0 90) (size 1.425 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1754385965)
      (net 9 "DRAIN"))
    (pad "2" smd roundrect locked (at 1.4875 0 90) (size 1.425 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1754385965)
      (net 4 "21"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1812_4532Metric_Pad1.57x3.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 51.499356 105.151599 180)
    (descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference "Сc2" (at 3.8 0 90) (layer "F.SilkS"))
    (fp_text value "С" (at 0 2.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.1375 0 180) (size 1.575 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1587301587)
      (net 10 "GATE"))
    (pad "2" smd roundrect (at 2.1375 0 180) (size 1.575 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1587301587)
      (net 14 "d"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 39.386856 80.501599 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference "Rfilt2" (at -0.046401 2.007144 90) (layer "F.SilkS"))
    (fp_text value "R" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.4875 0 90) (size 1.425 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1754385965))
    (pad "2" smd roundrect locked (at 1.4875 0 90) (size 1.425 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1754385965)
      (net 2 "1"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1812_4532Metric_Pad1.57x3.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 63.746 105.5885 -90)
    (descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference "Сsrc1" (at 5.4395 0.254 90) (layer "F.SilkS"))
    (fp_text value "С" (at 1.078 3.15 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.1375 0 270) (size 1.575 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1587301587)
      (net 1 "GND"))
    (pad "2" smd roundrect (at 2.1375 0 270) (size 1.575 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1587301587)
      (net 8 "SOURCE"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 54.186856 96.901599 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference "J6" (at 3.175 0) (layer "F.SilkS"))
    (fp_text value "R" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.4875 0 90) (size 1.425 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1754385965))
    (pad "2" smd roundrect locked (at 1.4875 0 90) (size 1.425 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1754385965))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 63.386856 96.901599 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference "J8" (at 3.175 0) (layer "F.SilkS"))
    (fp_text value "R" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.4875 0 90) (size 1.425 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1754385965)
      (net 17 "4m"))
    (pad "2" smd roundrect locked (at 1.4875 0 90) (size 1.425 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1754385965))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 81.526 97.0945 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference "Rgain" (at 3.175 0) (layer "F.SilkS"))
    (fp_text value "R" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.4875 0 90) (size 1.425 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1754385965)
      (net 9 "DRAIN"))
    (pad "2" smd roundrect locked (at 1.4875 0 90) (size 1.425 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1754385965))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 44.186856 80.514099 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference "Rfilt3" (at -0.033901 2.033144 90) (layer "F.SilkS"))
    (fp_text value "R" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.4875 0 90) (size 1.425 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1754385965))
    (pad "2" smd roundrect locked (at 1.4875 0 90) (size 1.425 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1754385965)
      (net 15 "2"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 34.586856 80.501599 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference "Rfilt1" (at -0.046401 1.981144 90) (layer "F.SilkS"))
    (fp_text value "R" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.4875 0 90) (size 1.425 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1754385965)
      (net 17 "4m"))
    (pad "2" smd roundrect locked (at 1.4875 0 90) (size 1.425 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1754385965)
      (net 3 "14"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_rect (start 26.162 57.15) (end 92.202 132.08) (layer "Edge.Cuts") (width 0.05) (fill none))
  (gr_text "FILTER BANK" (at 37.838 91.216) (layer "F.SilkS"))
  (gr_text "S" (at 61.206 108.996) (layer "F.SilkS"))
  (gr_text "SPLENDOR\nSplit-Stage Amp 4K (V0.1)\nMD 2023-01-10 \nKURINSKY GROUP " (at 80.764 114.33 90) (layer "F.SilkS"))
  (zone (net 1) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 1))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 85.344 76.708)
        (xy 32.610814 76.211578)
        (xy 32.512 71.882)
        (xy 85.344 72.136)
      )
    )
  )
  (zone (net 1) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 1))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 43.319003 76.906621)
        (xy 32.547312 76.3633)
        (xy 32.527427 64.002787)
        (xy 43.564397 64.016376)
      )
    )
  )
  (zone (net 1) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 1))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 85.344 76.708)
        (xy 73.048677 76.145344)
        (xy 73.152 64.008)
        (xy 85.344 64.008)
      )
    )
  )
  (zone (net 1) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 1))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 84.575776 69.021584)
        (xy 32.60459 68.603781)
        (xy 32.512 64.008)
        (xy 85.09 64.008)
      )
    )
  )
  (zone (net 1) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 1))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 85.09 124.968)
        (xy 32.512 124.714)
        (xy 32.512 76.2)
        (xy 85.344 76.2)
      )
    )
  )
)
