(kicad_pcb (version 20190331) (host pcbnew "(5.1.0-373-ge808c7f95)")
  (general
    (thickness 1.6)
    (drawings 32)
    (tracks 87)
    (modules 19)
    (nets 1)
  )
  (page "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user)
    (33 "F.Adhes" user)
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user)
    (37 "F.SilkS" user)
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user)
    (41 "Cmts.User" user)
    (42 "Eco1.User" user hide)
    (43 "Eco2.User" user hide)
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user hide)
    (47 "F.CrtYd" user hide)
    (48 "B.Fab" user hide)
    (49 "F.Fab" user hide)
  )
  (setup
    (last_trace_width 0.6)
    (user_trace_width 0.6)
    (user_trace_width 2)
    (user_trace_width 2.54)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.15)
    (via_size 0.6)
    (via_drill 0.33)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.15)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.7 1.7)
    (pad_drill 1)
    (pad_to_mask_clearance 0.2)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_80000001)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "output/"))
  )
  (net 0 "")
  (net_class "Default" "This is the default net class."
    (clearance 0.2)
    (trace_width 0.15)
    (via_dia 0.6)
    (via_drill 0.33)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module "mrmeeseeks:badgelife-shitty-label-gnd" (layer "F.Cu") (tedit 0)
    (at 78.74 38.8112 90)
    (fp_text reference "G***" (at 0 0 90) (layer "F.SilkS") hide)
    (fp_text value "LOGO" (at 0.75 0 90) (layer "F.SilkS") hide)
  )
  (module "badgelife_sao_v169bis:Badgelife-SAOv169-SAO-2x3" (layer "F.Cu") (tedit 5D36323F)
    (at 53.7464 63.1952)
    (descr "Through hole straight IDC box header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole IDC box header THT 2x03 2.54mm double row")
    (fp_text reference "#SAO" (at 0 -5.842) (layer "B.SilkS") hide)
    (fp_text value "Badgelife-SAOv169-SAO-2x3" (at 0 -7.7) (layer "F.Fab"))
    (fp_text user "GPIO2" (at 3.937 3.048) (layer "F.SilkS"))
    (fp_text user "SCL" (at 0 3.048) (layer "F.SilkS"))
    (fp_text user "GND" (at -2.54 3.048 unlocked) (layer "F.SilkS"))
    (fp_text user "GPIO1" (at 3.937 -2.794 unlocked) (layer "B.SilkS"))
    (fp_text user "SDA" (at 0 -2.794 unlocked) (layer "F.SilkS"))
    (fp_text user "VCC" (at -2.54 -2.794 unlocked) (layer "F.SilkS"))
    (fp_text user "%R" (at 0.06 0.02 270) (layer "F.Fab"))
    (fp_text user "VCC" (at -2.54 -2.794 unlocked) (layer "B.SilkS"))
    (fp_text user "SDA" (at 0 -2.794 unlocked) (layer "B.SilkS"))
    (fp_text user "GPIO1" (at 3.937 -2.794 unlocked) (layer "F.SilkS"))
    (fp_text user "GND" (at -2.54 3.048 unlocked) (layer "B.SilkS"))
    (fp_text user "SCL" (at 0 3.048) (layer "B.SilkS"))
    (fp_text user "GPIO2" (at 3.937 3.048) (layer "B.SilkS"))
    (pad "5" thru_hole circle (at 2.6 -1.25 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad "6" thru_hole circle (at 2.6 1.29 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad "3" thru_hole oval (at 0.06 -1.25 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad "4" thru_hole oval (at 0.06 1.29 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad "1" thru_hole oval (at -2.48 -1.25 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad "2" thru_hole rect (at -2.48 1.29 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (model "${KISYS3DMOD}/Connector_IDC.3dshapes/IDC-Header_2x03_P2.54mm_Vertical.wrl"
      (offset (xyz -2.5 1.2 -1.6))
      (scale (xyz 1 1 1))
      (rotate (xyz 180 0 90))
    )
  )
  (module "mrmeeseeks:Power_Rail-01x09" (layer "F.Cu") (tedit 5AC7D21B)
    (at 31.02864 50.37074 180)
    (descr "Through hole straight pin header, 1x07, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x07 2.54mm single row")
    (fp_text reference "J3" (at 0 -2.33 180) (layer "F.Fab") hide)
    (fp_text value "Conn_01x09" (at 0 17.57 180) (layer "F.Fab"))
    (fp_text user "%R" (at 0 7.62 270) (layer "F.Fab"))
    (pad "9" thru_hole rect (at 0 20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
    (pad "8" thru_hole rect (at 0 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
    (pad "7" thru_hole rect (at 0 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
    (pad "6" thru_hole rect (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
    (pad "5" thru_hole rect (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
    (pad "4" thru_hole rect (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
    (pad "3" thru_hole rect (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
    (pad "2" thru_hole rect (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
  )
  (module "mrmeeseeks:Power_Rail-01x08" (layer "F.Cu") (tedit 5AC7D1EA)
    (at 33.99536 53.05044 90)
    (descr "Through hole straight pin header, 1x07, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x07 2.54mm single row")
    (fp_text reference "J2" (at 0 -2.33 90) (layer "F.Fab") hide)
    (fp_text value "Conn_01x08" (at 0 17.57 90) (layer "F.Fab"))
    (fp_text user "%R" (at 0 7.62 180) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
    (pad "2" thru_hole rect (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
    (pad "3" thru_hole rect (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
    (pad "4" thru_hole rect (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
    (pad "5" thru_hole rect (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
    (pad "6" thru_hole rect (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
    (pad "7" thru_hole rect (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
    (pad "8" thru_hole rect (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
  )
  (module "mrmeeseeks:Power_Rail-01x08" (layer "F.Cu") (tedit 5AC7D1EA)
    (at 55.62092 26.9875 90)
    (descr "Through hole straight pin header, 1x07, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x07 2.54mm single row")
    (fp_text reference "J2" (at 0 -2.33 90) (layer "F.Fab") hide)
    (fp_text value "Conn_01x08" (at 0 17.57 90) (layer "F.Fab"))
    (fp_text user "%R" (at 0 7.62 180) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
    (pad "2" thru_hole rect (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
    (pad "3" thru_hole rect (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
    (pad "4" thru_hole rect (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
    (pad "5" thru_hole rect (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
    (pad "6" thru_hole rect (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
    (pad "7" thru_hole rect (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
    (pad "8" thru_hole rect (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
  )
  (module "mrmeeseeks:Pin_Header_Straight_2x09_Pitch2.54mm-NoSilk" (layer "F.Cu") (tedit 5AA33E7A)
    (at 58.13298 49.94402 180)
    (descr "Through hole straight pin header, 2x09, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x09 2.54mm double row")
    (fp_text reference "REF**" (at 1.27 -2.33 180) (layer "F.Fab") hide)
    (fp_text value "Pin_Header_Straight_2x09_Pitch2.54mm" (at 1.27 22.65 180) (layer "F.Fab"))
    (fp_text user "%R" (at 1.27 10.16 270) (layer "F.Fab"))
    (pad "18" thru_hole oval (at 2.54 20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "17" thru_hole oval (at 0 20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "16" thru_hole oval (at 2.54 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "15" thru_hole oval (at 0 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "14" thru_hole oval (at 2.54 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "13" thru_hole oval (at 0 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "12" thru_hole oval (at 2.54 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "11" thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "10" thru_hole oval (at 2.54 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "9" thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "8" thru_hole oval (at 2.54 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "7" thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "6" thru_hole oval (at 2.54 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "5" thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "4" thru_hole oval (at 2.54 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "3" thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "2" thru_hole oval (at 2.54 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module "mrmeeseeks:Pin_Header_Straight_2x09_Pitch2.54mm-NoSilk" (layer "F.Cu") (tedit 5D36193E)
    (at 36.42868 50.09134 180)
    (descr "Through hole straight pin header, 2x09, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x09 2.54mm double row")
    (fp_text reference "REF**" (at 1.27 -2.33 180) (layer "F.Fab") hide)
    (fp_text value "Pin_Header_Straight_2x09_Pitch2.54mm" (at 1.27 22.65 180) (layer "F.Fab"))
    (fp_text user "%R" (at 1.27 10.16 270) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "2" thru_hole oval (at 2.54 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "3" thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "4" thru_hole oval (at 2.54 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "5" thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "6" thru_hole oval (at 2.54 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "7" thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "8" thru_hole oval (at 2.54 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "9" thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "10" thru_hole oval (at 2.54 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "11" thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "12" thru_hole oval (at 2.54 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "13" thru_hole oval (at 0 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "14" thru_hole oval (at 2.54 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "15" thru_hole oval (at 0 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "16" thru_hole oval (at 2.54 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "17" thru_hole oval (at 0 20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "18" thru_hole oval (at 2.54 20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module "mrmeeseeks:Pin_Header_Straight_2x09_Pitch2.54mm-NoSilk" (layer "F.Cu") (tedit 5AA33E7A)
    (at 51.67268 50.09134 180)
    (descr "Through hole straight pin header, 2x09, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x09 2.54mm double row")
    (fp_text reference "REF**" (at 1.27 -2.33 180) (layer "F.Fab") hide)
    (fp_text value "Pin_Header_Straight_2x09_Pitch2.54mm" (at 1.27 22.65 180) (layer "F.Fab"))
    (fp_text user "%R" (at 1.27 10.16 270) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "2" thru_hole oval (at 2.54 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "3" thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "4" thru_hole oval (at 2.54 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "5" thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "6" thru_hole oval (at 2.54 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "7" thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "8" thru_hole oval (at 2.54 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "9" thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "10" thru_hole oval (at 2.54 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "11" thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "12" thru_hole oval (at 2.54 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "13" thru_hole oval (at 0 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "14" thru_hole oval (at 2.54 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "15" thru_hole oval (at 0 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "16" thru_hole oval (at 2.54 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "17" thru_hole oval (at 0 20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "18" thru_hole oval (at 2.54 20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module "mrmeeseeks:Pin_Header_Straight_2x09_Pitch2.54mm-NoSilk" (layer "F.Cu") (tedit 5AA33E7A)
    (at 46.57268 50.09134 180)
    (descr "Through hole straight pin header, 2x09, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x09 2.54mm double row")
    (fp_text reference "REF**" (at 1.27 -2.33 180) (layer "F.Fab") hide)
    (fp_text value "Pin_Header_Straight_2x09_Pitch2.54mm" (at 1.27 22.65 180) (layer "F.Fab"))
    (fp_text user "%R" (at 1.27 10.16 270) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "2" thru_hole oval (at 2.54 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "3" thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "4" thru_hole oval (at 2.54 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "5" thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "6" thru_hole oval (at 2.54 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "7" thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "8" thru_hole oval (at 2.54 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "9" thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "10" thru_hole oval (at 2.54 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "11" thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "12" thru_hole oval (at 2.54 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "13" thru_hole oval (at 0 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "14" thru_hole oval (at 2.54 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "15" thru_hole oval (at 0 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "16" thru_hole oval (at 2.54 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "17" thru_hole oval (at 0 20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "18" thru_hole oval (at 2.54 20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module "mrmeeseeks:Pin_Header_Straight_2x09_Pitch2.54mm-NoSilk" (layer "F.Cu") (tedit 5AA33E7A)
    (at 41.50868 50.09134 180)
    (descr "Through hole straight pin header, 2x09, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x09 2.54mm double row")
    (fp_text reference "REF**" (at 1.27 -2.33 180) (layer "F.Fab") hide)
    (fp_text value "Pin_Header_Straight_2x09_Pitch2.54mm" (at 1.27 22.65 180) (layer "F.Fab"))
    (fp_text user "%R" (at 1.27 10.16 270) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "2" thru_hole oval (at 2.54 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "3" thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "4" thru_hole oval (at 2.54 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "5" thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "6" thru_hole oval (at 2.54 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "7" thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "8" thru_hole oval (at 2.54 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "9" thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "10" thru_hole oval (at 2.54 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "11" thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "12" thru_hole oval (at 2.54 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "13" thru_hole oval (at 0 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "14" thru_hole oval (at 2.54 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "15" thru_hole oval (at 0 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "16" thru_hole oval (at 2.54 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "17" thru_hole oval (at 0 20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "18" thru_hole oval (at 2.54 20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module "mrmeeseeks:Power_Rail-01x08" (layer "F.Cu") (tedit 5AC7D1EA)
    (at 55.55996 52.9082 90)
    (descr "Through hole straight pin header, 1x07, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x07 2.54mm single row")
    (fp_text reference "J2" (at 0 -2.33 90) (layer "F.Fab") hide)
    (fp_text value "Conn_01x08" (at 0 17.57 90) (layer "F.Fab"))
    (fp_text user "%R" (at 0 7.62 180) (layer "F.Fab"))
    (pad "8" thru_hole rect (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
    (pad "7" thru_hole rect (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
    (pad "6" thru_hole rect (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
    (pad "5" thru_hole rect (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
    (pad "4" thru_hole rect (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
    (pad "3" thru_hole rect (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
    (pad "2" thru_hole rect (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
  )
  (module "mrmeeseeks:Power_Rail-01x08" (layer "F.Cu") (tedit 5AC7D1EA)
    (at 33.86836 27.15006 90)
    (descr "Through hole straight pin header, 1x07, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x07 2.54mm single row")
    (fp_text reference "J2" (at 0 -2.33 90) (layer "F.Fab") hide)
    (fp_text value "Conn_01x08" (at 0 17.57 90) (layer "F.Fab"))
    (fp_text user "%R" (at 0 7.62 180) (layer "F.Fab"))
    (pad "8" thru_hole rect (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
    (pad "7" thru_hole rect (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
    (pad "6" thru_hole rect (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
    (pad "5" thru_hole rect (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
    (pad "4" thru_hole rect (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
    (pad "3" thru_hole rect (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
    (pad "2" thru_hole rect (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
  )
  (module "mrmeeseeks:Power_Rail-01x09" (layer "F.Cu") (tedit 5AC7D21B)
    (at 76.073 49.96688 180)
    (descr "Through hole straight pin header, 1x07, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x07 2.54mm single row")
    (fp_text reference "J3" (at 0 -2.33 180) (layer "F.Fab") hide)
    (fp_text value "Conn_01x09" (at 0 17.57 180) (layer "F.Fab"))
    (fp_text user "%R" (at 0 7.62 270) (layer "F.Fab"))
    (pad "9" thru_hole rect (at 0 20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
    (pad "8" thru_hole rect (at 0 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
    (pad "7" thru_hole rect (at 0 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
    (pad "6" thru_hole rect (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
    (pad "5" thru_hole rect (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
    (pad "4" thru_hole rect (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
    (pad "3" thru_hole rect (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
    (pad "2" thru_hole rect (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1))
  )
  (module "mrmeeseeks:Pin_Header_Straight_2x09_Pitch2.54mm-NoSilk" (layer "F.Cu") (tedit 5AA33E7A)
    (at 63.21298 49.94402 180)
    (descr "Through hole straight pin header, 2x09, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x09 2.54mm double row")
    (fp_text reference "REF**" (at 1.27 -2.33 180) (layer "F.Fab") hide)
    (fp_text value "Pin_Header_Straight_2x09_Pitch2.54mm" (at 1.27 22.65 180) (layer "F.Fab"))
    (fp_text user "%R" (at 1.27 10.16 270) (layer "F.Fab"))
    (pad "18" thru_hole oval (at 2.54 20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "17" thru_hole oval (at 0 20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "16" thru_hole oval (at 2.54 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "15" thru_hole oval (at 0 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "14" thru_hole oval (at 2.54 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "13" thru_hole oval (at 0 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "12" thru_hole oval (at 2.54 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "11" thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "10" thru_hole oval (at 2.54 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "9" thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "8" thru_hole oval (at 2.54 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "7" thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "6" thru_hole oval (at 2.54 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "5" thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "4" thru_hole oval (at 2.54 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "3" thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "2" thru_hole oval (at 2.54 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module "mrmeeseeks:Pin_Header_Straight_2x09_Pitch2.54mm-NoSilk" (layer "F.Cu") (tedit 5AA33E7A)
    (at 68.27698 49.94402 180)
    (descr "Through hole straight pin header, 2x09, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x09 2.54mm double row")
    (fp_text reference "REF**" (at 1.27 -2.33 180) (layer "F.Fab") hide)
    (fp_text value "Pin_Header_Straight_2x09_Pitch2.54mm" (at 1.27 22.65 180) (layer "F.Fab"))
    (fp_text user "%R" (at 1.27 10.16 270) (layer "F.Fab"))
    (pad "18" thru_hole oval (at 2.54 20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "17" thru_hole oval (at 0 20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "16" thru_hole oval (at 2.54 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "15" thru_hole oval (at 0 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "14" thru_hole oval (at 2.54 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "13" thru_hole oval (at 0 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "12" thru_hole oval (at 2.54 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "11" thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "10" thru_hole oval (at 2.54 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "9" thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "8" thru_hole oval (at 2.54 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "7" thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "6" thru_hole oval (at 2.54 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "5" thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "4" thru_hole oval (at 2.54 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "3" thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "2" thru_hole oval (at 2.54 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module "mrmeeseeks:Pin_Header_Straight_2x09_Pitch2.54mm-NoSilk" (layer "F.Cu") (tedit 5AA33E7A)
    (at 73.37698 49.94402 180)
    (descr "Through hole straight pin header, 2x09, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x09 2.54mm double row")
    (fp_text reference "REF**" (at 1.27 -2.33 180) (layer "F.Fab") hide)
    (fp_text value "Pin_Header_Straight_2x09_Pitch2.54mm" (at 1.27 22.65 180) (layer "F.Fab"))
    (fp_text user "%R" (at 1.27 10.16 270) (layer "F.Fab"))
    (pad "18" thru_hole oval (at 2.54 20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "17" thru_hole oval (at 0 20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "16" thru_hole oval (at 2.54 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "15" thru_hole oval (at 0 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "14" thru_hole oval (at 2.54 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "13" thru_hole oval (at 0 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "12" thru_hole oval (at 2.54 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "11" thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "10" thru_hole oval (at 2.54 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "9" thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "8" thru_hole oval (at 2.54 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "7" thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "6" thru_hole oval (at 2.54 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "5" thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "4" thru_hole oval (at 2.54 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "3" thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "2" thru_hole oval (at 2.54 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module "mrmeeseeks:badgelife-shitty-label-3.3v" (layer "F.Cu") (tedit 0)
    (at 28.2448 39.0144 90)
    (fp_text reference "G***" (at 0 0 90) (layer "F.SilkS") hide)
    (fp_text value "LOGO" (at 0.75 0 90) (layer "F.SilkS") hide)
  )
  (module "mrmeeseeks:badgelife-shitty-label-sda" (layer "F.Cu") (tedit 0)
    (at 64.516 55.5244)
    (fp_text reference "G***" (at 0 0 180) (layer "F.SilkS") hide)
    (fp_text value "LOGO" (at 0.75 0 180) (layer "F.SilkS") hide)
  )
  (module "mrmeeseeks:badgelife-shitty-label-scl" (layer "F.Cu") (tedit 0)
    (at 42.7736 55.372)
    (fp_text reference "G***" (at 0 0) (layer "F.SilkS") hide)
    (fp_text value "LOGO" (at 0.75 0) (layer "F.SilkS") hide)
  )
  (gr_text "github.com/OSHPark/badgelife_dev_board" (at 53.848 22.225) (layer "B.SilkS"))
  (gr_line (start 82.042 56.642) (end 82.042 54.864) (layer "Edge.Cuts") (width 0.15))
  (gr_line (start 78.74 59.944) (end 82.042 56.642) (layer "Edge.Cuts") (width 0.15))
  (gr_line (start 80.10652 19.93392) (end 80.899 19.939) (layer "Edge.Cuts") (width 0.15))
  (gr_line (start 62.611 65.786) (end 62.611 69.08292) (layer "Edge.Cuts") (width 0.15))
  (gr_line (start 64.897 62.103) (end 62.611 65.786) (layer "Edge.Cuts") (width 0.15))
  (gr_line (start 68.834 62.103) (end 64.897 62.103) (layer "Edge.Cuts") (width 0.15))
  (gr_line (start 76.581 62.103) (end 68.834 62.103) (layer "Edge.Cuts") (width 0.15))
  (gr_line (start 78.74 59.944) (end 76.581 62.103) (layer "Edge.Cuts") (width 0.15))
  (gr_line (start 81.820063 20.86361) (end 82.042 54.864) (layer "Edge.Cuts") (width 0.15))
  (gr_arc (start 80.910744 20.848371) (end 81.820063 20.86361) (angle -91.7) (layer "Edge.Cuts") (width 0.15))
  (gr_line (start 27.53868 20.06092) (end 80.10652 19.93392) (layer "Edge.Cuts") (width 0.15))
  (gr_line (start 26.60904 20.98548) (end 26.62936 21.57476) (layer "Edge.Cuts") (width 0.15))
  (gr_arc (start 27.513281 20.960079) (end 27.52852 20.05076) (angle -91.7) (layer "Edge.Cuts") (width 0.15))
  (gr_line (start 26.74112 53.90388) (end 26.62936 21.5392) (layer "Edge.Cuts") (width 0.15))
  (gr_line (start 27.98064 55.42788) (end 26.74112 53.90388) (layer "Edge.Cuts") (width 0.15))
  (gr_line (start 28.52928 55.96636) (end 27.98064 55.42788) (layer "Edge.Cuts") (width 0.15))
  (gr_line (start 30.32252 57.7596) (end 28.52928 55.96636) (layer "Edge.Cuts") (width 0.15))
  (gr_line (start 34.57448 62.11316) (end 30.32252 57.7596) (layer "Edge.Cuts") (width 0.15))
  (gr_line (start 42.0624 62.12332) (end 34.57448 62.11316) (layer "Edge.Cuts") (width 0.15))
  (gr_line (start 43.37812 63.95212) (end 42.0624 62.12332) (layer "Edge.Cuts") (width 0.15))
  (gr_line (start 45.18152 65.89776) (end 43.37812 63.95212) (layer "Edge.Cuts") (width 0.15))
  (gr_line (start 45.1866 69.12864) (end 45.18152 65.89776) (layer "Edge.Cuts") (width 0.15))
  (gr_arc (start 46.085759 69.072759) (end 45.17644 69.05752) (angle -91.7) (layer "Edge.Cuts") (width 0.15))
  (gr_arc (start 61.701631 69.094782) (end 61.686392 70.004101) (angle -91.70746844) (layer "Edge.Cuts") (width 0.15))
  (gr_line (start 60.91936 70.00748) (end 61.76264 70.0024) (layer "Edge.Cuts") (width 0.15))
  (gr_line (start 46.101 69.98208) (end 60.91936 70.00748) (layer "Edge.Cuts") (width 0.15))
  (gr_text "v1.69bis" (at 53.7464 56.7944) (layer "B.SilkS"))
  (gr_text "#badgelife" (at 53.848 21.844) (layer "F.Mask"))
  (gr_text "#badgelife" (at 53.848 21.844) (layer "F.Cu"))
  (gr_text "GPIO1" (at 43.0276 24.8412) (layer "F.SilkS"))
  (gr_text "GPIO2" (at 64.4144 24.638) (layer "F.SilkS"))
)
