(kicad_pcb (version 20171130) (host pcbnew "(5.1.6)-1")
  (general
    (thickness 1.6)
    (drawings 8)
    (tracks 247)
    (zones 0)
    (modules 17)
    (nets 67)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (grid_origin -57.15 127)
    (visible_elements 7FFFEFFF)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "New folder/"))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad12)")
  (net 2 "Net-(J1-Pad11)")
  (net 3 "Net-(J1-Pad10)")
  (net 4 "Net-(J1-Pad9)")
  (net 5 "Net-(J1-Pad8)")
  (net 6 +5V)
  (net 7 5V_CHG)
  (net 8 PP_SS_C)
  (net 9 SEP_SW)
  (net 10 PP_SW)
  (net 11 GND)
  (net 12 EPS_Batt_Bus)
  (net 13 ADCS_UART1_TX)
  (net 14 ADCS_UART1_RX)
  (net 15 TMP_GND)
  (net 16 "Net-(J3-Pad4)")
  (net 17 "Net-(J3-Pad9)")
  (net 18 "Net-(J3-Pad10)")
  (net 19 "Net-(J3-Pad11)")
  (net 20 "Net-(J3-Pad12)")
  (net 21 "Net-(J6-Pad3)")
  (net 22 "Net-(J6-Pad4)")
  (net 23 5V_CUR_REG)
  (net 24 5V_IN_CUR_REG)
  (net 25 "Net-(J2-Pad3)")
  (net 26 "Net-(J2-Pad4)")
  (net 27 "Net-(J3-Pad7)")
  (net 28 "Net-(J3-Pad6)")
  (net 29 "Net-(J3-Pad3)")
  (net 30 "Net-(J3-Pad2)")
  (net 31 "Net-(J5-Pad4)")
  (net 32 "Net-(J5-Pad9)")
  (net 33 "Net-(J5-Pad10)")
  (net 34 "Net-(J5-Pad11)")
  (net 35 "Net-(J5-Pad12)")
  (net 36 "Net-(J6-Pad6)")
  (net 37 "Net-(J6-Pad8)")
  (net 38 "Net-(J6-Pad9)")
  (net 39 "Net-(J6-Pad10)")
  (net 40 "Net-(J6-Pad11)")
  (net 41 "Net-(J6-Pad12)")
  (net 42 "Net-(R_CUR_LIM1-Pad1)")
  (net 43 "Net-(U1-Pad4)")
  (net 44 CDH_CTS)
  (net 45 CDH_TXD)
  (net 46 CDH_RXD)
  (net 47 CDH_RTS)
  (net 48 "Net-(J4-Pad16)")
  (net 49 "Net-(J4-Pad17)")
  (net 50 "Net-(J4-Pad18)")
  (net 51 "Net-(J4-Pad19)")
  (net 52 "Net-(J4-Pad20)")
  (net 53 TMP_1+)
  (net 54 TMP_1-)
  (net 55 TMP_2+)
  (net 56 TMP_2-)
  (net 57 TMP_3+)
  (net 58 TMP_3-)
  (net 59 TMP_4+)
  (net 60 TMP_4-)
  (net 61 TMP_5+)
  (net 62 TMP_5-)
  (net 63 "Net-(J8-Pad11)")
  (net 64 "Net-(J8-Pad12)")
  (net 65 "Net-(J9-Pad12)")
  (net 66 "Net-(J9-Pad11)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net 5V_CHG)
    (add_net 5V_CUR_REG)
    (add_net 5V_IN_CUR_REG)
    (add_net ADCS_UART1_RX)
    (add_net ADCS_UART1_TX)
    (add_net CDH_CTS)
    (add_net CDH_RTS)
    (add_net CDH_RXD)
    (add_net CDH_TXD)
    (add_net EPS_Batt_Bus)
    (add_net GND)
    (add_net "Net-(J1-Pad10)")
    (add_net "Net-(J1-Pad11)")
    (add_net "Net-(J1-Pad12)")
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(J1-Pad9)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J2-Pad4)")
    (add_net "Net-(J3-Pad10)")
    (add_net "Net-(J3-Pad11)")
    (add_net "Net-(J3-Pad12)")
    (add_net "Net-(J3-Pad2)")
    (add_net "Net-(J3-Pad3)")
    (add_net "Net-(J3-Pad4)")
    (add_net "Net-(J3-Pad6)")
    (add_net "Net-(J3-Pad7)")
    (add_net "Net-(J3-Pad9)")
    (add_net "Net-(J4-Pad16)")
    (add_net "Net-(J4-Pad17)")
    (add_net "Net-(J4-Pad18)")
    (add_net "Net-(J4-Pad19)")
    (add_net "Net-(J4-Pad20)")
    (add_net "Net-(J5-Pad10)")
    (add_net "Net-(J5-Pad11)")
    (add_net "Net-(J5-Pad12)")
    (add_net "Net-(J5-Pad4)")
    (add_net "Net-(J5-Pad9)")
    (add_net "Net-(J6-Pad10)")
    (add_net "Net-(J6-Pad11)")
    (add_net "Net-(J6-Pad12)")
    (add_net "Net-(J6-Pad3)")
    (add_net "Net-(J6-Pad4)")
    (add_net "Net-(J6-Pad6)")
    (add_net "Net-(J6-Pad8)")
    (add_net "Net-(J6-Pad9)")
    (add_net "Net-(J8-Pad11)")
    (add_net "Net-(J8-Pad12)")
    (add_net "Net-(J9-Pad11)")
    (add_net "Net-(J9-Pad12)")
    (add_net "Net-(R_CUR_LIM1-Pad1)")
    (add_net "Net-(U1-Pad4)")
    (add_net PP_SS_C)
    (add_net PP_SW)
    (add_net SEP_SW)
    (add_net TMP_1+)
    (add_net TMP_1-)
    (add_net TMP_2+)
    (add_net TMP_2-)
    (add_net TMP_3+)
    (add_net TMP_3-)
    (add_net TMP_4+)
    (add_net TMP_4-)
    (add_net TMP_5+)
    (add_net TMP_5-)
    (add_net TMP_GND)
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 136.1 133)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference H4 (at 0 -4.2) (layer F.SilkS))
    (fp_text value MountingHole (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 136.1 70.5)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference H3 (at 0 -4.2) (layer F.SilkS))
    (fp_text value MountingHole (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 66.6 133.45)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference H2 (at 0 -4.2) (layer F.SilkS))
    (fp_text value MountingHole (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 65.35 69.75)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference H1 (at 0 -4.2) (layer F.SilkS))
    (fp_text value MountingHole (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module footprints:TPS2553QDBVRQ1 (layer F.Cu) (tedit 0)
    (at 83.82 99.06)
    (fp_text reference U1 (at 3.78 1.19) (layer F.SilkS))
    (fp_text value TPS2553QDBVRQ1 (at 0.28 -2.81) (layer F.SilkS))
    (fp_text user .Designator (at -3.81 0 90) (layer Dwgs.User))
    (fp_text user .Designator (at 2.54 0 270) (layer F.Fab))
    (fp_text user * (at 0 0) (layer F.Fab))
    (fp_text user * (at 0 0) (layer F.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
    (pad 6 smd rect (at 1.374999 -0.950001 90) (size 0.599999 1.000001) (layers F.Cu F.Paste F.Mask)
      (net 23 5V_CUR_REG))
    (pad 5 smd rect (at 1.374999 0 90) (size 0.599999 1.000001) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(R_CUR_LIM1-Pad1)"))
    (pad 4 smd rect (at 1.374999 0.949998 90) (size 0.599999 1.000001) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(U1-Pad4)"))
    (pad 3 smd rect (at -1.375001 0.949998 90) (size 0.599999 1.000001) (layers F.Cu F.Paste F.Mask)
      (net 24 5V_IN_CUR_REG))
    (pad 2 smd rect (at -1.375001 0 90) (size 0.599999 1.000001) (layers F.Cu F.Paste F.Mask)
      (net 11 GND))
    (pad 1 smd rect (at -1.375001 -0.950001 90) (size 0.599999 1.000001) (layers F.Cu F.Paste F.Mask)
      (net 24 5V_IN_CUR_REG))
  )
  (module "Power Resistor Library:SQP10AJB-33R" (layer F.Cu) (tedit 0)
    (at 74.93 127)
    (fp_text reference R1 (at 45.72 -7.62) (layer F.SilkS))
    (fp_text value 33 (at 45.72 -6.35) (layer F.SilkS))
    (fp_text user * (at 0 0) (layer F.Fab))
    (fp_text user * (at 0 0) (layer F.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
    (pad 2 thru_hole circle (at 56.388 0) (size 1.6256 1.6256) (drill 1.1176) (layers *.Cu *.Mask)
      (net 11 GND))
    (pad 1 thru_hole rect (at 0 0) (size 1.6256 1.6256) (drill 1.1176) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad8)"))
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 86.36 91.44)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C2 (at 0 -3.81) (layer F.SilkS))
    (fp_text value 150uF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 5V_CUR_REG))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0201_0603Metric (layer F.Cu) (tedit 5B301BBD)
    (at 88.9 96.52 90)
    (descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R_CUR_LIM1 (at 0 1.27 90) (layer F.SilkS))
    (fp_text value 59k (at 0 1.05 90) (layer F.Fab))
    (fp_text user %R (at 0 2.54 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.32 0 90) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 11 GND))
    (pad 1 smd roundrect (at -0.32 0 90) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 42 "Net-(R_CUR_LIM1-Pad1)"))
    (pad "" smd roundrect (at 0.345 0 90) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.345 0 90) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 78.74 91.44 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C1 (at 0 3.81) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 5V_IN_CUR_REG))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SAMAC:SHDR12W60P200_2X6_1400X500X690P (layer F.Cu) (tedit 0)
    (at 72.39 76.2 90)
    (descr "DF11-12DP-2DSA(24)")
    (tags Connector)
    (fp_text reference J1 (at 3.81 -1.27 180) (layer F.SilkS))
    (fp_text value "DF11-12DP-2DSA(24)-SamacSys_Parts" (at -8.89 -17.78 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 12 thru_hole circle (at -10 -2 90) (size 1.575 1.575) (drill 1.05) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad12)"))
    (pad 11 thru_hole circle (at -10 0 90) (size 1.575 1.575) (drill 1.05) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad11)"))
    (pad 10 thru_hole circle (at -8 -2 90) (size 1.575 1.575) (drill 1.05) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad10)"))
    (pad 9 thru_hole circle (at -8 0 90) (size 1.575 1.575) (drill 1.05) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad9)"))
    (pad 8 thru_hole circle (at -6 -2 90) (size 1.575 1.575) (drill 1.05) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad8)"))
    (pad 7 thru_hole circle (at -6 0 90) (size 1.575 1.575) (drill 1.05) (layers *.Cu *.Mask)
      (net 6 +5V))
    (pad 6 thru_hole circle (at -4 -2 90) (size 1.575 1.575) (drill 1.05) (layers *.Cu *.Mask)
      (net 7 5V_CHG))
    (pad 5 thru_hole circle (at -4 0 90) (size 1.575 1.575) (drill 1.05) (layers *.Cu *.Mask)
      (net 23 5V_CUR_REG))
    (pad 4 thru_hole circle (at -2 -2 90) (size 1.575 1.575) (drill 1.05) (layers *.Cu *.Mask)
      (net 8 PP_SS_C))
    (pad 3 thru_hole circle (at -2 0 90) (size 1.575 1.575) (drill 1.05) (layers *.Cu *.Mask)
      (net 9 SEP_SW))
    (pad 2 thru_hole circle (at 0 -2 90) (size 1.575 1.575) (drill 1.05) (layers *.Cu *.Mask)
      (net 8 PP_SS_C))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.575 1.575) (drill 1.05) (layers *.Cu *.Mask)
      (net 10 PP_SW))
  )
  (module SAMAC:SHDR4W70P200_2X2_600X1000X675P (layer F.Cu) (tedit 0)
    (at 93.98 76.2 90)
    (descr "DF11-4DP-2DS(24)")
    (tags Connector)
    (fp_text reference J2 (at 3.81 -2.54 180) (layer F.SilkS))
    (fp_text value "DF11-4DP-2DS(24)-TSL_Footprint_Library" (at 6.35 -2.54 180) (layer F.SilkS) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.35 1.35) (drill 0.9) (layers *.Cu *.Mask)
      (net 24 5V_IN_CUR_REG))
    (pad 2 thru_hole circle (at 0 -2 90) (size 1.35 1.35) (drill 0.9) (layers *.Cu *.Mask)
      (net 11 GND))
    (pad 3 thru_hole circle (at -2 0 90) (size 1.35 1.35) (drill 0.9) (layers *.Cu *.Mask)
      (net 25 "Net-(J2-Pad3)"))
    (pad 4 thru_hole circle (at -2 -2 90) (size 1.35 1.35) (drill 0.9) (layers *.Cu *.Mask)
      (net 26 "Net-(J2-Pad4)"))
  )
  (module SAMAC:SHDR12W60P200_2X6_1400X500X690P (layer F.Cu) (tedit 0)
    (at 111.76 74.93 90)
    (descr "DF11-12DP-2DSA(24)")
    (tags Connector)
    (fp_text reference J3 (at 3.81 -2.54 180) (layer F.SilkS))
    (fp_text value "DF11-12DP-2DSA(24)-SamacSys_Parts" (at 0 0 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 12 thru_hole circle (at -10 -2 90) (size 1.575 1.575) (drill 1.05) (layers *.Cu *.Mask)
      (net 20 "Net-(J3-Pad12)"))
    (pad 11 thru_hole circle (at -10 0 90) (size 1.575 1.575) (drill 1.05) (layers *.Cu *.Mask)
      (net 19 "Net-(J3-Pad11)"))
    (pad 10 thru_hole circle (at -8 -2 90) (size 1.575 1.575) (drill 1.05) (layers *.Cu *.Mask)
      (net 18 "Net-(J3-Pad10)"))
    (pad 9 thru_hole circle (at -8 0 90) (size 1.575 1.575) (drill 1.05) (layers *.Cu *.Mask)
      (net 17 "Net-(J3-Pad9)"))
    (pad 8 thru_hole circle (at -6 -2 90) (size 1.575 1.575) (drill 1.05) (layers *.Cu *.Mask)
      (net 11 GND))
    (pad 7 thru_hole circle (at -6 0 90) (size 1.575 1.575) (drill 1.05) (layers *.Cu *.Mask)
      (net 27 "Net-(J3-Pad7)"))
    (pad 6 thru_hole circle (at -4 -2 90) (size 1.575 1.575) (drill 1.05) (layers *.Cu *.Mask)
      (net 28 "Net-(J3-Pad6)"))
    (pad 5 thru_hole circle (at -4 0 90) (size 1.575 1.575) (drill 1.05) (layers *.Cu *.Mask)
      (net 11 GND))
    (pad 4 thru_hole circle (at -2 -2 90) (size 1.575 1.575) (drill 1.05) (layers *.Cu *.Mask)
      (net 16 "Net-(J3-Pad4)"))
    (pad 3 thru_hole circle (at -2 0 90) (size 1.575 1.575) (drill 1.05) (layers *.Cu *.Mask)
      (net 29 "Net-(J3-Pad3)"))
    (pad 2 thru_hole circle (at 0 -2 90) (size 1.575 1.575) (drill 1.05) (layers *.Cu *.Mask)
      (net 30 "Net-(J3-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.575 1.575) (drill 1.05) (layers *.Cu *.Mask)
      (net 12 EPS_Batt_Bus))
  )
  (module SAMAC:SHDR20W70P200_2X10_2200X1000X530P (layer F.Cu) (tedit 0)
    (at 111.76 97.79 90)
    (descr "DF11-20DP-2DS(24)")
    (tags Connector)
    (fp_text reference J4 (at -8.89 -11.43 180) (layer F.SilkS))
    (fp_text value "DF11-20DP-2DS(24)-TSL_Footprint_Library" (at 0 0 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.35 1.35) (drill 0.9) (layers *.Cu *.Mask)
      (net 44 CDH_CTS))
    (pad 2 thru_hole circle (at 0 -2 90) (size 1.35 1.35) (drill 0.9) (layers *.Cu *.Mask)
      (net 45 CDH_TXD))
    (pad 3 thru_hole circle (at -2 0 90) (size 1.35 1.35) (drill 0.9) (layers *.Cu *.Mask)
      (net 46 CDH_RXD))
    (pad 4 thru_hole circle (at -2 -2 90) (size 1.35 1.35) (drill 0.9) (layers *.Cu *.Mask)
      (net 7 5V_CHG))
    (pad 5 thru_hole circle (at -4 0 90) (size 1.35 1.35) (drill 0.9) (layers *.Cu *.Mask)
      (net 11 GND))
    (pad 6 thru_hole circle (at -4 -2 90) (size 1.35 1.35) (drill 0.9) (layers *.Cu *.Mask)
      (net 47 CDH_RTS))
    (pad 7 thru_hole circle (at -6 0 90) (size 1.35 1.35) (drill 0.9) (layers *.Cu *.Mask)
      (net 6 +5V))
    (pad 8 thru_hole circle (at -6 -2 90) (size 1.35 1.35) (drill 0.9) (layers *.Cu *.Mask)
      (net 11 GND))
    (pad 9 thru_hole circle (at -8 0 90) (size 1.35 1.35) (drill 0.9) (layers *.Cu *.Mask)
      (net 9 SEP_SW))
    (pad 10 thru_hole circle (at -8 -2 90) (size 1.35 1.35) (drill 0.9) (layers *.Cu *.Mask)
      (net 10 PP_SW))
    (pad 11 thru_hole circle (at -10 0 90) (size 1.35 1.35) (drill 0.9) (layers *.Cu *.Mask)
      (net 8 PP_SS_C))
    (pad 12 thru_hole circle (at -10 -2 90) (size 1.35 1.35) (drill 0.9) (layers *.Cu *.Mask)
      (net 12 EPS_Batt_Bus))
    (pad 13 thru_hole circle (at -12 0 90) (size 1.35 1.35) (drill 0.9) (layers *.Cu *.Mask)
      (net 13 ADCS_UART1_TX))
    (pad 14 thru_hole circle (at -12 -2 90) (size 1.35 1.35) (drill 0.9) (layers *.Cu *.Mask)
      (net 14 ADCS_UART1_RX))
    (pad 15 thru_hole circle (at -14 0 90) (size 1.35 1.35) (drill 0.9) (layers *.Cu *.Mask)
      (net 15 TMP_GND))
    (pad 16 thru_hole circle (at -14 -2 90) (size 1.35 1.35) (drill 0.9) (layers *.Cu *.Mask)
      (net 48 "Net-(J4-Pad16)"))
    (pad 17 thru_hole circle (at -16 0 90) (size 1.35 1.35) (drill 0.9) (layers *.Cu *.Mask)
      (net 49 "Net-(J4-Pad17)"))
    (pad 18 thru_hole circle (at -16 -2 90) (size 1.35 1.35) (drill 0.9) (layers *.Cu *.Mask)
      (net 50 "Net-(J4-Pad18)"))
    (pad 19 thru_hole circle (at -18 0 90) (size 1.35 1.35) (drill 0.9) (layers *.Cu *.Mask)
      (net 51 "Net-(J4-Pad19)"))
    (pad 20 thru_hole circle (at -18 -2 90) (size 1.35 1.35) (drill 0.9) (layers *.Cu *.Mask)
      (net 52 "Net-(J4-Pad20)"))
  )
  (module SAMAC:SHDR12W60P200_2X6_1400X500X690P (layer F.Cu) (tedit 0)
    (at 130.81 101.6 90)
    (descr "DF11-12DP-2DSA(24)")
    (tags Connector)
    (fp_text reference J5 (at 3.81 -1.27 180) (layer F.SilkS))
    (fp_text value "DF11-12DP-2DSA(24)-SamacSys_Parts" (at 0 0 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.575 1.575) (drill 1.05) (layers *.Cu *.Mask)
      (net 44 CDH_CTS))
    (pad 2 thru_hole circle (at 0 -2 90) (size 1.575 1.575) (drill 1.05) (layers *.Cu *.Mask)
      (net 45 CDH_TXD))
    (pad 3 thru_hole circle (at -2 0 90) (size 1.575 1.575) (drill 1.05) (layers *.Cu *.Mask)
      (net 46 CDH_RXD))
    (pad 4 thru_hole circle (at -2 -2 90) (size 1.575 1.575) (drill 1.05) (layers *.Cu *.Mask)
      (net 31 "Net-(J5-Pad4)"))
    (pad 5 thru_hole circle (at -4 0 90) (size 1.575 1.575) (drill 1.05) (layers *.Cu *.Mask)
      (net 11 GND))
    (pad 6 thru_hole circle (at -4 -2 90) (size 1.575 1.575) (drill 1.05) (layers *.Cu *.Mask)
      (net 47 CDH_RTS))
    (pad 7 thru_hole circle (at -6 0 90) (size 1.575 1.575) (drill 1.05) (layers *.Cu *.Mask)
      (net 6 +5V))
    (pad 8 thru_hole circle (at -6 -2 90) (size 1.575 1.575) (drill 1.05) (layers *.Cu *.Mask)
      (net 11 GND))
    (pad 9 thru_hole circle (at -8 0 90) (size 1.575 1.575) (drill 1.05) (layers *.Cu *.Mask)
      (net 32 "Net-(J5-Pad9)"))
    (pad 10 thru_hole circle (at -8 -2 90) (size 1.575 1.575) (drill 1.05) (layers *.Cu *.Mask)
      (net 33 "Net-(J5-Pad10)"))
    (pad 11 thru_hole circle (at -10 0 90) (size 1.575 1.575) (drill 1.05) (layers *.Cu *.Mask)
      (net 34 "Net-(J5-Pad11)"))
    (pad 12 thru_hole circle (at -10 -2 90) (size 1.575 1.575) (drill 1.05) (layers *.Cu *.Mask)
      (net 35 "Net-(J5-Pad12)"))
  )
  (module SAMAC:SHDR12W60P200_2X6_1400X500X690P (layer F.Cu) (tedit 0)
    (at 130.81 76.2 90)
    (descr "DF11-12DP-2DSA(24)")
    (tags Connector)
    (fp_text reference J6 (at 3.81 -2.54 180) (layer F.SilkS))
    (fp_text value "DF11-12DP-2DSA(24)-SamacSys_Parts" (at 0 0 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.575 1.575) (drill 1.05) (layers *.Cu *.Mask)
      (net 13 ADCS_UART1_TX))
    (pad 2 thru_hole circle (at 0 -2 90) (size 1.575 1.575) (drill 1.05) (layers *.Cu *.Mask)
      (net 14 ADCS_UART1_RX))
    (pad 3 thru_hole circle (at -2 0 90) (size 1.575 1.575) (drill 1.05) (layers *.Cu *.Mask)
      (net 21 "Net-(J6-Pad3)"))
    (pad 4 thru_hole circle (at -2 -2 90) (size 1.575 1.575) (drill 1.05) (layers *.Cu *.Mask)
      (net 22 "Net-(J6-Pad4)"))
    (pad 5 thru_hole circle (at -4 0 90) (size 1.575 1.575) (drill 1.05) (layers *.Cu *.Mask)
      (net 11 GND))
    (pad 6 thru_hole circle (at -4 -2 90) (size 1.575 1.575) (drill 1.05) (layers *.Cu *.Mask)
      (net 36 "Net-(J6-Pad6)"))
    (pad 7 thru_hole circle (at -6 0 90) (size 1.575 1.575) (drill 1.05) (layers *.Cu *.Mask)
      (net 6 +5V))
    (pad 8 thru_hole circle (at -6 -2 90) (size 1.575 1.575) (drill 1.05) (layers *.Cu *.Mask)
      (net 37 "Net-(J6-Pad8)"))
    (pad 9 thru_hole circle (at -8 0 90) (size 1.575 1.575) (drill 1.05) (layers *.Cu *.Mask)
      (net 38 "Net-(J6-Pad9)"))
    (pad 10 thru_hole circle (at -8 -2 90) (size 1.575 1.575) (drill 1.05) (layers *.Cu *.Mask)
      (net 39 "Net-(J6-Pad10)"))
    (pad 11 thru_hole circle (at -10 0 90) (size 1.575 1.575) (drill 1.05) (layers *.Cu *.Mask)
      (net 40 "Net-(J6-Pad11)"))
    (pad 12 thru_hole circle (at -10 -2 90) (size 1.575 1.575) (drill 1.05) (layers *.Cu *.Mask)
      (net 41 "Net-(J6-Pad12)"))
  )
  (module SAMAC:SHDR12W60P200_2X6_1400X500X690P (layer F.Cu) (tedit 0)
    (at 93.1 105.75 90)
    (descr "DF11-12DP-2DSA(24)")
    (tags Connector)
    (fp_text reference J8 (at 3.474999 -1.325001 180) (layer F.SilkS))
    (fp_text value "DF11-12DP-2DSA(24)-SamacSys_Parts-B4_V2-rescue" (at 0 0 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.575 1.575) (drill 1.05) (layers *.Cu *.Mask)
      (net 53 TMP_1+))
    (pad 2 thru_hole circle (at 0 -2 90) (size 1.575 1.575) (drill 1.05) (layers *.Cu *.Mask)
      (net 54 TMP_1-))
    (pad 3 thru_hole circle (at -2 0 90) (size 1.575 1.575) (drill 1.05) (layers *.Cu *.Mask)
      (net 55 TMP_2+))
    (pad 4 thru_hole circle (at -2 -2 90) (size 1.575 1.575) (drill 1.05) (layers *.Cu *.Mask)
      (net 56 TMP_2-))
    (pad 5 thru_hole circle (at -4 0 90) (size 1.575 1.575) (drill 1.05) (layers *.Cu *.Mask)
      (net 57 TMP_3+))
    (pad 6 thru_hole circle (at -4 -2 90) (size 1.575 1.575) (drill 1.05) (layers *.Cu *.Mask)
      (net 58 TMP_3-))
    (pad 7 thru_hole circle (at -6 0 90) (size 1.575 1.575) (drill 1.05) (layers *.Cu *.Mask)
      (net 59 TMP_4+))
    (pad 8 thru_hole circle (at -6 -2 90) (size 1.575 1.575) (drill 1.05) (layers *.Cu *.Mask)
      (net 60 TMP_4-))
    (pad 9 thru_hole circle (at -8 0 90) (size 1.575 1.575) (drill 1.05) (layers *.Cu *.Mask)
      (net 61 TMP_5+))
    (pad 10 thru_hole circle (at -8 -2 90) (size 1.575 1.575) (drill 1.05) (layers *.Cu *.Mask)
      (net 62 TMP_5-))
    (pad 11 thru_hole circle (at -10 0 90) (size 1.575 1.575) (drill 1.05) (layers *.Cu *.Mask)
      (net 63 "Net-(J8-Pad11)"))
    (pad 12 thru_hole circle (at -10 -2 90) (size 1.575 1.575) (drill 1.05) (layers *.Cu *.Mask)
      (net 64 "Net-(J8-Pad12)"))
  )
  (module SAMAC:SHDR12W60P200_2X6_1400X500X690P (layer F.Cu) (tedit 0)
    (at 82.1 105.75 90)
    (descr "DF11-12DP-2DSA(24)")
    (tags Connector)
    (fp_text reference J9 (at 3.25 -1.25 180) (layer F.SilkS))
    (fp_text value "DF11-12DP-2DSA(24)-SamacSys_Parts-B4_V2-rescue" (at 0 0 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 12 thru_hole circle (at -10 -2 90) (size 1.575 1.575) (drill 1.05) (layers *.Cu *.Mask)
      (net 65 "Net-(J9-Pad12)"))
    (pad 11 thru_hole circle (at -10 0 90) (size 1.575 1.575) (drill 1.05) (layers *.Cu *.Mask)
      (net 66 "Net-(J9-Pad11)"))
    (pad 10 thru_hole circle (at -8 -2 90) (size 1.575 1.575) (drill 1.05) (layers *.Cu *.Mask)
      (net 62 TMP_5-))
    (pad 9 thru_hole circle (at -8 0 90) (size 1.575 1.575) (drill 1.05) (layers *.Cu *.Mask)
      (net 61 TMP_5+))
    (pad 8 thru_hole circle (at -6 -2 90) (size 1.575 1.575) (drill 1.05) (layers *.Cu *.Mask)
      (net 60 TMP_4-))
    (pad 7 thru_hole circle (at -6 0 90) (size 1.575 1.575) (drill 1.05) (layers *.Cu *.Mask)
      (net 59 TMP_4+))
    (pad 6 thru_hole circle (at -4 -2 90) (size 1.575 1.575) (drill 1.05) (layers *.Cu *.Mask)
      (net 58 TMP_3-))
    (pad 5 thru_hole circle (at -4 0 90) (size 1.575 1.575) (drill 1.05) (layers *.Cu *.Mask)
      (net 57 TMP_3+))
    (pad 4 thru_hole circle (at -2 -2 90) (size 1.575 1.575) (drill 1.05) (layers *.Cu *.Mask)
      (net 56 TMP_2-))
    (pad 3 thru_hole circle (at -2 0 90) (size 1.575 1.575) (drill 1.05) (layers *.Cu *.Mask)
      (net 55 TMP_2+))
    (pad 2 thru_hole circle (at 0 -2 90) (size 1.575 1.575) (drill 1.05) (layers *.Cu *.Mask)
      (net 54 TMP_1-))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.575 1.575) (drill 1.05) (layers *.Cu *.Mask)
      (net 53 TMP_1+))
  )
  (gr_text "SERPENT EGSE PCB. Designed by Dhiren Wijesinghe :)" (at 103.35 66.75) (layer F.SilkS))
  (dimension 73.66 (width 0.15) (layer Dwgs.User)
    (gr_text "2.9000 in" (at 171.48 101.6 90) (layer Dwgs.User))
    (feature1 (pts (xy 142.24 64.77) (xy 170.766421 64.77)))
    (feature2 (pts (xy 142.24 138.43) (xy 170.766421 138.43)))
    (crossbar (pts (xy 170.18 138.43) (xy 170.18 64.77)))
    (arrow1a (pts (xy 170.18 64.77) (xy 170.766421 65.896504)))
    (arrow1b (pts (xy 170.18 64.77) (xy 169.593579 65.896504)))
    (arrow2a (pts (xy 170.18 138.43) (xy 170.766421 137.303496)))
    (arrow2b (pts (xy 170.18 138.43) (xy 169.593579 137.303496)))
  )
  (dimension 81.28 (width 0.15) (layer Dwgs.User)
    (gr_text "3.2000 in" (at 101.6 153.699999) (layer Dwgs.User))
    (feature1 (pts (xy 142.24 138.43) (xy 142.24 152.98642)))
    (feature2 (pts (xy 60.96 138.43) (xy 60.96 152.98642)))
    (crossbar (pts (xy 60.96 152.399999) (xy 142.24 152.399999)))
    (arrow1a (pts (xy 142.24 152.399999) (xy 141.113496 152.98642)))
    (arrow1b (pts (xy 142.24 152.399999) (xy 141.113496 151.813578)))
    (arrow2a (pts (xy 60.96 152.399999) (xy 62.086504 152.98642)))
    (arrow2b (pts (xy 60.96 152.399999) (xy 62.086504 151.813578)))
  )
  (gr_line (start 60.96 64.77) (end 60.96 138.43) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 142.24 64.77) (end 60.96 64.77) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 142.24 138.43) (end 142.24 64.77) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 60.96 138.43) (end 142.24 138.43) (layer Edge.Cuts) (width 0.05))
  (dimension 10.16 (width 0.15) (layer Dwgs.User)
    (gr_text "0.4000 in" (at 96.52 102.84) (layer Dwgs.User))
    (feature1 (pts (xy 101.6 107.95) (xy 101.6 103.553579)))
    (feature2 (pts (xy 91.44 107.95) (xy 91.44 103.553579)))
    (crossbar (pts (xy 91.44 104.14) (xy 101.6 104.14)))
    (arrow1a (pts (xy 101.6 104.14) (xy 100.473496 104.726421)))
    (arrow1b (pts (xy 101.6 104.14) (xy 100.473496 103.553579)))
    (arrow2a (pts (xy 91.44 104.14) (xy 92.566504 104.726421)))
    (arrow2b (pts (xy 91.44 104.14) (xy 92.566504 103.553579)))
  )
)
