(kicad_pcb (version 20171130) (host pcbnew "(5.1.0)-1")
  (general
    (thickness 1.6)
    (drawings 71)
    (tracks 205)
    (zones 0)
    (modules 14)
    (nets 28)
  )
  (page A4)
  (layers
    (0 Top signal)
    (31 Bottom signal)
    (33 F.Adhes user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 VCC)
  (net 3 +5V)
  (net 4 N$2)
  (net 5 N$6)
  (net 6 N$7)
  (net 7 N$8)
  (net 8 RTS)
  (net 9 N$4)
  (net 10 N$5)
  (net 11 N$9)
  (net 12 N$10)
  (net 13 N$11)
  (net 14 N$12)
  (net 15 N$14)
  (net 16 N$15)
  (net 17 N$16)
  (net 18 N$17)
  (net 19 N$18)
  (net 20 N$19)
  (net 21 N$20)
  (net 22 N$1)
  (net 23 N$21)
  (net 24 TX)
  (net 25 N$13)
  (net 26 RESET)
  (net 27 N$3)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net GND)
    (add_net N$1)
    (add_net N$10)
    (add_net N$11)
    (add_net N$12)
    (add_net N$13)
    (add_net N$14)
    (add_net N$15)
    (add_net N$16)
    (add_net N$17)
    (add_net N$18)
    (add_net N$19)
    (add_net N$2)
    (add_net N$20)
    (add_net N$21)
    (add_net N$3)
    (add_net N$4)
    (add_net N$5)
    (add_net N$6)
    (add_net N$7)
    (add_net N$8)
    (add_net N$9)
    (add_net RESET)
    (add_net RTS)
    (add_net TX)
    (add_net VCC)
  )
  (module xbee:XBEE (layer Top) (tedit 0)
    (at 148.3791 98.7806)
    (fp_text reference XBEE (at -3 16) (layer F.SilkS))
    (fp_text value XBEE (at 0 0) (layer F.SilkS) hide)
    (pad 20 thru_hole circle (at 11 -5.5) (size 1.4224 1.4224) (drill 0.7) (layers *.Cu *.Mask)
      (net 15 N$14) (solder_mask_margin 0.1016))
    (pad 19 thru_hole circle (at 11 -3.5) (size 1.4224 1.4224) (drill 0.7) (layers *.Cu *.Mask)
      (net 16 N$15) (solder_mask_margin 0.1016))
    (pad 18 thru_hole circle (at 11 -1.5) (size 1.4224 1.4224) (drill 0.7) (layers *.Cu *.Mask)
      (net 17 N$16) (solder_mask_margin 0.1016))
    (pad 17 thru_hole circle (at 11 0.5) (size 1.4224 1.4224) (drill 0.7) (layers *.Cu *.Mask)
      (net 18 N$17) (solder_mask_margin 0.1016))
    (pad 16 thru_hole circle (at 11 2.5) (size 1.4224 1.4224) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 RTS) (solder_mask_margin 0.1016))
    (pad 15 thru_hole circle (at 11 4.5) (size 1.4224 1.4224) (drill 0.7) (layers *.Cu *.Mask)
      (net 11 N$9) (solder_mask_margin 0.1016))
    (pad 14 thru_hole circle (at 11 6.5) (size 1.4224 1.4224) (drill 0.7) (layers *.Cu *.Mask)
      (net 19 N$18) (solder_mask_margin 0.1016))
    (pad 13 thru_hole circle (at 11 8.5) (size 1.4224 1.4224) (drill 0.7) (layers *.Cu *.Mask)
      (net 20 N$19) (solder_mask_margin 0.1016))
    (pad 12 thru_hole circle (at 11 10.5) (size 1.4224 1.4224) (drill 0.7) (layers *.Cu *.Mask)
      (net 9 N$4) (solder_mask_margin 0.1016))
    (pad 11 thru_hole circle (at 11 12.5) (size 1.4224 1.4224) (drill 0.7) (layers *.Cu *.Mask)
      (net 21 N$20) (solder_mask_margin 0.1016))
    (pad 1 thru_hole rect (at -11 -5.5) (size 1.4224 1.4224) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 VCC) (solder_mask_margin 0.1016))
    (pad 2 thru_hole circle (at -11 -3.5) (size 1.4224 1.4224) (drill 0.7) (layers *.Cu *.Mask)
      (net 24 TX) (solder_mask_margin 0.1016))
    (pad 3 thru_hole circle (at -11 -1.5) (size 1.4224 1.4224) (drill 0.7) (layers *.Cu *.Mask)
      (net 4 N$2) (solder_mask_margin 0.1016))
    (pad 4 thru_hole circle (at -11 0.5) (size 1.4224 1.4224) (drill 0.7) (layers *.Cu *.Mask)
      (net 5 N$6) (solder_mask_margin 0.1016))
    (pad 5 thru_hole circle (at -11 2.5) (size 1.4224 1.4224) (drill 0.7) (layers *.Cu *.Mask)
      (net 25 N$13) (solder_mask_margin 0.1016))
    (pad 6 thru_hole circle (at -11 4.5) (size 1.4224 1.4224) (drill 0.7) (layers *.Cu *.Mask)
      (net 6 N$7) (solder_mask_margin 0.1016))
    (pad 7 thru_hole circle (at -11 6.5) (size 1.4224 1.4224) (drill 0.7) (layers *.Cu *.Mask)
      (net 14 N$12) (solder_mask_margin 0.1016))
    (pad 8 thru_hole circle (at -11 8.5) (size 1.4224 1.4224) (drill 0.7) (layers *.Cu *.Mask)
      (net 13 N$11) (solder_mask_margin 0.1016))
    (pad 9 thru_hole circle (at -11 10.5) (size 1.4224 1.4224) (drill 0.7) (layers *.Cu *.Mask)
      (net 12 N$10) (solder_mask_margin 0.1016))
    (pad 10 thru_hole circle (at -11 12.5) (size 1.4224 1.4224) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
  )
  (module xbee:LED3MM (layer Top) (tedit 0)
    (at 137.9651 87.3506)
    (descr "<B>LED</B><p>\n3 mm, round")
    (fp_text reference D1 (at 1.905 -0.381) (layer F.SilkS) hide)
    (fp_text value "" (at 1.905 1.651) (layer F.Fab))
    (pad K thru_hole circle (at 1.27 0) (size 1.6764 1.6764) (drill 0.8128) (layers *.Cu *.Mask)
      (net 7 N$8) (solder_mask_margin 0.1016))
    (pad A thru_hole circle (at -1.27 0) (size 1.6764 1.6764) (drill 0.8128) (layers *.Cu *.Mask)
      (net 6 N$7) (solder_mask_margin 0.1016))
  )
  (module xbee:0207_10 (layer Top) (tedit 0)
    (at 148.3791 86.8426 180)
    (descr "<b>RESISTOR</b><p>\ntype 0207, grid 10 mm")
    (fp_text reference R1 (at -3.048 -1.524) (layer F.SilkS))
    (fp_text value 200 (at -2.2606 0.635) (layer F.Fab))
    (pad 2 thru_hole circle (at 5.08 0 180) (size 1.6764 1.6764) (drill 0.8128) (layers *.Cu *.Mask)
      (net 7 N$8) (solder_mask_margin 0.1016))
    (pad 1 thru_hole circle (at -5.08 0 180) (size 1.6764 1.6764) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
  )
  (module xbee:C025-025X050 (layer Top) (tedit 0)
    (at 148.3791 115.7986)
    (descr "<b>CAPACITOR</b><p>\ngrid 2.5 mm, outline 2.5 x 5 mm")
    (fp_text reference C1 (at -2.286 -1.524 90) (layer F.SilkS))
    (fp_text value "" (at -2.286 2.794) (layer F.Fab))
    (pad 2 thru_hole circle (at 1.27 0) (size 1.6764 1.6764) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad 1 thru_hole circle (at -1.27 0) (size 1.6764 1.6764) (drill 0.8128) (layers *.Cu *.Mask)
      (net 2 VCC) (solder_mask_margin 0.1016))
  )
  (module xbee:TO92 (layer Top) (tedit 0)
    (at 137.7111 117.5766 90)
    (descr "<b>VOLTAGE REGULATOR</b>")
    (fp_text reference IC1 (at 3.175 -0.635) (layer F.SilkS))
    (fp_text value "" (at 3.175 1.27 90) (layer F.Fab))
    (pad 3 thru_hole circle (at 2.159 0 90) (size 1.6764 1.6764) (drill 0.8128) (layers *.Cu *.Mask)
      (net 2 VCC) (solder_mask_margin 0.1016))
    (pad 2 thru_hole circle (at 0 0 90) (size 1.6764 1.6764) (drill 0.8128) (layers *.Cu *.Mask)
      (net 3 +5V) (solder_mask_margin 0.1016))
    (pad 1 thru_hole circle (at -2.159 0 90) (size 1.6764 1.6764) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
  )
  (module xbee:E2,5-5 (layer Top) (tedit 0)
    (at 159.3011 118.0846 270)
    (descr "<b>ELECTROLYTIC CAPACITOR</b><p>\ngrid 2.54 mm, diameter 5 mm")
    (fp_text reference C2 (at 2.413 -1.27) (layer F.SilkS))
    (fp_text value "" (at 2.413 2.413 90) (layer F.Fab))
    (pad + thru_hole circle (at -1.27 0 270) (size 1.6002 1.6002) (drill 0.8128) (layers *.Cu *.Mask)
      (net 2 VCC) (solder_mask_margin 0.1016))
    (pad - thru_hole circle (at 1.27 0 270) (size 1.6002 1.6002) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
  )
  (module xbee:DIL14 (layer Top) (tedit 0)
    (at 148.3791 104.1146 270)
    (descr "<b>Dual In Line Package</b>")
    (fp_text reference IC2 (at -8.636 3.048) (layer F.SilkS))
    (fp_text value 74LS125N (at -6.731 0.635 90) (layer F.Fab))
    (pad 14 thru_hole oval (at -7.62 -3.81) (size 2.6416 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 2 VCC) (solder_mask_margin 0.1016))
    (pad 13 thru_hole oval (at -5.08 -3.81) (size 2.6416 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad 12 thru_hole oval (at -2.54 -3.81) (size 2.6416 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 22 N$1) (solder_mask_margin 0.1016))
    (pad 11 thru_hole oval (at 0 -3.81) (size 2.6416 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 4 N$2) (solder_mask_margin 0.1016))
    (pad 10 thru_hole oval (at 2.54 -3.81) (size 2.6416 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad 9 thru_hole oval (at 5.08 -3.81) (size 2.6416 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 23 N$21) (solder_mask_margin 0.1016))
    (pad 5 thru_hole oval (at 2.54 3.81) (size 2.6416 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 27 N$3) (solder_mask_margin 0.1016))
    (pad 6 thru_hole oval (at 5.08 3.81) (size 2.6416 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 12 N$10) (solder_mask_margin 0.1016))
    (pad 4 thru_hole oval (at 0 3.81) (size 2.6416 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad 3 thru_hole oval (at -2.54 3.81) (size 2.6416 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 25 N$13) (solder_mask_margin 0.1016))
    (pad 8 thru_hole oval (at 7.62 -3.81) (size 2.6416 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 9 N$4) (solder_mask_margin 0.1016))
    (pad 7 thru_hole oval (at 7.62 3.81) (size 2.6416 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad 2 thru_hole oval (at -5.08 3.81) (size 2.6416 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 26 RESET) (solder_mask_margin 0.1016))
    (pad 1 thru_hole oval (at -7.62 3.81) (size 2.6416 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 26 RESET) (solder_mask_margin 0.1016))
  )
  (module xbee:LED3MM (layer Top) (tedit 0)
    (at 158.7931 87.3506 180)
    (descr "<B>LED</B><p>\n3 mm, round")
    (fp_text reference D2 (at 1.905 -0.381 180) (layer F.SilkS) hide)
    (fp_text value "" (at 1.905 1.651) (layer F.Fab))
    (pad K thru_hole circle (at 1.27 0 180) (size 1.6764 1.6764) (drill 0.8128) (layers *.Cu *.Mask)
      (net 10 N$5) (solder_mask_margin 0.1016))
    (pad A thru_hole circle (at -1.27 0 180) (size 1.6764 1.6764) (drill 0.8128) (layers *.Cu *.Mask)
      (net 11 N$9) (solder_mask_margin 0.1016))
  )
  (module xbee:0207_10 (layer Top) (tedit 0)
    (at 148.3791 89.8906)
    (descr "<b>RESISTOR</b><p>\ntype 0207, grid 10 mm")
    (fp_text reference R2 (at -3.048 -1.524) (layer F.SilkS))
    (fp_text value 200 (at -2.2606 0.635) (layer F.Fab))
    (pad 2 thru_hole circle (at 5.08 0) (size 1.6764 1.6764) (drill 0.8128) (layers *.Cu *.Mask)
      (net 10 N$5) (solder_mask_margin 0.1016))
    (pad 1 thru_hole circle (at -5.08 0) (size 1.6764 1.6764) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
  )
  (module xbee:1X10-BIG (layer Top) (tedit 0)
    (at 155.9991 101.5746 270)
    (fp_text reference U$3 (at -11.5062 -1.8288 270) (layer F.SilkS) hide)
    (fp_text value PINHD-1X10 (at -11.43 3.175 90) (layer F.Fab))
    (pad 10 thru_hole circle (at 11.43 0) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 21 N$20) (solder_mask_margin 0.1016))
    (pad 9 thru_hole circle (at 8.89 0) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 N$4) (solder_mask_margin 0.1016))
    (pad 8 thru_hole circle (at 6.35 0) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 20 N$19) (solder_mask_margin 0.1016))
    (pad 7 thru_hole circle (at 3.81 0) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 19 N$18) (solder_mask_margin 0.1016))
    (pad 6 thru_hole circle (at 1.27 0) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 11 N$9) (solder_mask_margin 0.1016))
    (pad 5 thru_hole circle (at -1.27 0) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 8 RTS) (solder_mask_margin 0.1016))
    (pad 4 thru_hole circle (at -3.81 0) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 18 N$17) (solder_mask_margin 0.1016))
    (pad 3 thru_hole circle (at -6.35 0) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 17 N$16) (solder_mask_margin 0.1016))
    (pad 2 thru_hole circle (at -8.89 0) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 16 N$15) (solder_mask_margin 0.1016))
    (pad 1 thru_hole circle (at -11.43 0) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 15 N$14) (solder_mask_margin 0.1016))
  )
  (module xbee:1X10-BIG (layer Top) (tedit 0)
    (at 140.7591 101.5746 90)
    (fp_text reference U$4 (at -11.5062 -1.8288 90) (layer F.SilkS) hide)
    (fp_text value PINHD-1X10 (at -11.43 3.175 90) (layer F.Fab))
    (pad 10 thru_hole circle (at 11.43 0 180) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 VCC) (solder_mask_margin 0.1016))
    (pad 9 thru_hole circle (at 8.89 0 180) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 24 TX) (solder_mask_margin 0.1016))
    (pad 8 thru_hole circle (at 6.35 0 180) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 N$2) (solder_mask_margin 0.1016))
    (pad 7 thru_hole circle (at 3.81 0 180) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 N$6) (solder_mask_margin 0.1016))
    (pad 6 thru_hole circle (at 1.27 0 180) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 25 N$13) (solder_mask_margin 0.1016))
    (pad 5 thru_hole circle (at -1.27 0 180) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 6 N$7) (solder_mask_margin 0.1016))
    (pad 4 thru_hole circle (at -3.81 0 180) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 14 N$12) (solder_mask_margin 0.1016))
    (pad 3 thru_hole circle (at -6.35 0 180) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 13 N$11) (solder_mask_margin 0.1016))
    (pad 2 thru_hole circle (at -8.89 0 180) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 12 N$10) (solder_mask_margin 0.1016))
    (pad 1 thru_hole circle (at -11.43 0 180) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
  )
  (module xbee:1X01 (layer Top) (tedit 0)
    (at 155.9991 115.5446)
    (descr "<b>PIN HEADER</b>")
    (fp_text reference JP3 (at -1.3462 -1.8288) (layer F.SilkS) hide)
    (fp_text value "" (at -1.27 3.175) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 +5V) (solder_mask_margin 0.1016))
  )
  (module xbee:0207_10 (layer Top) (tedit 0)
    (at 148.3791 93.1926 180)
    (descr "<b>RESISTOR</b><p>\ntype 0207, grid 10 mm")
    (fp_text reference R3 (at -3.048 -1.524) (layer F.SilkS))
    (fp_text value 10K (at -2.2606 0.635) (layer F.Fab))
    (pad 2 thru_hole circle (at 5.08 0 180) (size 1.6764 1.6764) (drill 0.8128) (layers *.Cu *.Mask)
      (net 26 RESET) (solder_mask_margin 0.1016))
    (pad 1 thru_hole circle (at -5.08 0 180) (size 1.6764 1.6764) (drill 0.8128) (layers *.Cu *.Mask)
      (net 2 VCC) (solder_mask_margin 0.1016))
  )
  (module xbee:1X10-BIG (layer Top) (tedit 0)
    (at 148.3791 122.1486 180)
    (fp_text reference U$1 (at -11.5062 -1.8288 180) (layer F.SilkS) hide)
    (fp_text value PINHD-1X10 (at -11.43 3.175) (layer F.Fab))
    (pad 10 thru_hole circle (at 11.43 0 270) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 VCC) (solder_mask_margin 0.1016))
    (pad 9 thru_hole circle (at 8.89 0 270) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 27 N$3) (solder_mask_margin 0.1016))
    (pad 8 thru_hole circle (at 6.35 0 270) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 26 RESET) (solder_mask_margin 0.1016))
    (pad 7 thru_hole circle (at 3.81 0 270) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad 6 thru_hole circle (at 1.27 0 270) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 8 RTS) (solder_mask_margin 0.1016))
    (pad 5 thru_hole circle (at -1.27 0 270) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 +5V) (solder_mask_margin 0.1016))
    (pad 4 thru_hole circle (at -3.81 0 270) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 22 N$1) (solder_mask_margin 0.1016))
    (pad 3 thru_hole circle (at -6.35 0 270) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 24 TX) (solder_mask_margin 0.1016))
    (pad 2 thru_hole circle (at -8.89 0 270) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 N$21) (solder_mask_margin 0.1016))
    (pad 1 thru_hole circle (at -11.43 0 270) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 VCC) (solder_mask_margin 0.1016))
  )
  (gr_line (start 135.3031 124.9046) (end 161.6991 124.9046) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 161.6991 124.9046) (end 161.6991 88.1247) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 158.677 88.1247) (end 161.6991 88.1247) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 158.677 85.1026) (end 138.0254 85.1026) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 138.025599 87.8251) (end 138.0254 85.1026) (angle -89.991582) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 135.3031 87.8249) (end 135.3031 124.9046) (layer Edge.Cuts) (width 0.15))
  (gr_text GND (at 145.0771 120.6246 90) (layer F.SilkS))
  (gr_text +5V (at 150.1571 120.3706 90) (layer F.SilkS))
  (gr_text TX (at 154.7291 120.6246 90) (layer F.SilkS))
  (gr_text RX (at 152.6971 120.6246 90) (layer F.SilkS))
  (gr_text RST (at 143.5531 123.6726) (layer F.SilkS))
  (gr_text CTS (at 156.7611 120.6246 90) (layer F.SilkS))
  (gr_text RTS (at 147.6171 120.6246 90) (layer F.SilkS))
  (gr_text 3V (at 159.3011 124.6886) (layer F.SilkS))
  (gr_text 5v (at 152.4431 116.3066) (layer F.SilkS))
  (gr_text AD4 (at 151.9351 114.0206) (layer F.SilkS))
  (gr_text CTS (at 158.5391 111.7346 90) (layer F.SilkS))
  (gr_text ON (at 154.4751 108.9406 90) (layer F.SilkS))
  (gr_text VREF (at 158.5391 106.9086 90) (layer F.SilkS))
  (gr_text ASC (at 154.4751 104.1146 90) (layer F.SilkS))
  (gr_text RTS (at 158.5391 101.5746 90) (layer F.SilkS))
  (gr_text AD3 (at 154.4751 99.0346 90) (layer F.SilkS))
  (gr_text AD2 (at 158.5391 96.7486 90) (layer F.SilkS))
  (gr_text AD1 (at 154.6021 90.9066) (layer F.SilkS))
  (gr_text AD0 (at 158.2851 91.9226 90) (layer F.SilkS))
  (gr_text ASC (at 157.2691 85.3186) (layer F.SilkS))
  (gr_text RSS (at 139.7431 86.3346) (layer F.SilkS))
  (gr_text GND (at 139.2351 113.1316) (layer F.SilkS))
  (gr_text DTR (at 143.0451 111.7346 90) (layer F.SilkS))
  (gr_text PWM1 (at 143.0451 106.9086 90) (layer F.SilkS))
  (gr_text RSS (at 139.2351 104.1146 90) (layer F.SilkS))
  (gr_text RES (at 139.2351 109.1946 90) (layer F.SilkS))
  (gr_text RST (at 143.0451 101.3206 90) (layer F.SilkS))
  (gr_text DO8 (at 139.2351 99.0346 90) (layer F.SilkS))
  (gr_text RX (at 144.0611 94.5896) (layer F.SilkS))
  (gr_text TX (at 139.2351 93.4466 90) (layer F.SilkS))
  (gr_text VCC (at 140.7591 88.6206) (layer F.SilkS))
  (gr_text + (at 160.0631 90.5256) (layer F.SilkS))
  (gr_text + (at 135.5521 90.6526) (layer F.SilkS))
  (gr_text RX (at 153.2051 123.6726) (layer F.SilkS))
  (gr_text TX (at 153.9671 124.6886) (layer F.SilkS))
  (gr_text - (at 144.3151 124.4346) (layer F.SilkS))
  (gr_text +5 (at 148.8871 124.6886) (layer F.SilkS))
  (gr_text DTR (at 139.7431 117.8306 90) (layer F.SilkS))
  (gr_text RST (at 142.5371 120.6246 90) (layer F.SilkS))
  (gr_text 3V (at 135.9331 124.6886) (layer F.SilkS))
  (gr_text 5v (at 154.4751 116.1796) (layer B.SilkS))
  (gr_text AD4 (at 157.1421 112.7506) (layer B.SilkS))
  (gr_text CTS (at 153.8401 111.6076 -90) (layer B.SilkS))
  (gr_text ON (at 157.2691 108.6866 -90) (layer B.SilkS))
  (gr_text VREF (at 153.8401 107.2896 -90) (layer B.SilkS))
  (gr_text ASC (at 157.2691 104.2416 -90) (layer B.SilkS))
  (gr_text RTS (at 153.7131 101.5746 -90) (layer B.SilkS))
  (gr_text AD3 (at 157.2691 98.9076 -90) (layer B.SilkS))
  (gr_text AD2 (at 153.8401 96.6216 -90) (layer B.SilkS))
  (gr_text AD1 (at 157.2691 93.7006 -90) (layer B.SilkS))
  (gr_text AD0 (at 159.9361 90.5256) (layer B.SilkS))
  (gr_text GND (at 142.0291 114.2746 -90) (layer B.SilkS))
  (gr_text DTR (at 138.4731 111.7346 -90) (layer B.SilkS))
  (gr_text PWM1 (at 138.4731 106.9086 -90) (layer B.SilkS))
  (gr_text RSS (at 141.9021 104.1146 -90) (layer B.SilkS))
  (gr_text RES (at 142.0291 109.1946 -90) (layer B.SilkS))
  (gr_text RST (at 138.6001 101.4476 -90) (layer B.SilkS))
  (gr_text DO8 (at 142.0291 98.9076 -90) (layer B.SilkS))
  (gr_text RX (at 138.6001 95.9866 -90) (layer B.SilkS))
  (gr_text TX (at 139.6161 91.6686 -90) (layer B.SilkS))
  (gr_text VCC (at 136.6951 89.6366) (layer B.SilkS))
  (gr_text www.ladyada.net/ (at 157.1421 118.2116) (layer B.SilkS))
  (gr_text make/xbee (at 154.7291 120.2436) (layer B.SilkS))
  (gr_text "XBee Adapter" (at 149.0141 92.3036 -90) (layer B.SilkS))
  (gr_text v1.0 (at 150.2841 109.7026) (layer B.SilkS))
  (zone (net 1) (net_name GND) (layer Bottom) (hatch edge 0.508)
    (priority 6)
    (connect_pads (clearance 0.4064))
    (min_thickness 0.4064)
    (fill yes (arc_segments 32) (thermal_gap 0.4564) (thermal_bridge_width 0.4564))
    (polygon
      (pts
        (xy 135.4251 124.9426) (xy 161.8411 124.9426) (xy 161.8411 85.0646) (xy 135.4251 85.0646)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer Top) (hatch edge 0.508)
    (priority 6)
    (connect_pads (clearance 0.4064))
    (min_thickness 0.4064)
    (fill yes (arc_segments 32) (thermal_gap 0.4564) (thermal_bridge_width 0.4564))
    (polygon
      (pts
        (xy 135.4251 124.6886) (xy 161.8411 124.6886) (xy 161.8411 85.0646) (xy 135.4251 85.0646)
      )
    )
  )
)
