(kicad_pcb (version 4) (host pcbnew 4.0.5)
  (general
    (links 49)
    (no_connects 0)
    (area 157.612014 86.919999 182.447001 116.661001)
    (thickness 1.6)
    (drawings 13)
    (tracks 161)
    (zones 0)
    (modules 24)
    (nets 9)
  )
  (page A4)
  (title_block
    (title "ATTiny 20 LEDs Ring")
    (date 2017-03-31)
    (rev 1.0)
    (company "Jens Hauke")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.19888 1.19888)
    (pad_drill 0)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010e0_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerber/))
  )
  (net 0 "")
  (net 1 "Net-(D1-Pad1)")
  (net 2 "Net-(IC1-Pad1)")
  (net 3 "Net-(D0-Pad2)")
  (net 4 "Net-(D0-Pad1)")
  (net 5 "Net-(D10-Pad1)")
  (net 6 "Net-(D12-Pad1)")
  (net 7 GND)
  (net 8 +3V3)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net GND)
    (add_net "Net-(D0-Pad1)")
    (add_net "Net-(D0-Pad2)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D10-Pad1)")
    (add_net "Net-(D12-Pad1)")
    (add_net "Net-(IC1-Pad1)")
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 58DE3698)
    (at 171.486 90.617 171)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D0 (at 0 -1.75 171) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.75 171) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 351) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D0-Pad2)"))
    (pad 1 smd rect (at -1.04902 0 351) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D0-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 58DE369E)
    (at 174.313 91.5354 153)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D1 (at 0 -1.75 153) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.75 153) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 333) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D0-Pad1)"))
    (pad 1 smd rect (at -1.04902 0 333) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 58DE36A2)
    (at 176.718 93.2825 135)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D2 (at 0 -1.75 135) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.75 135) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 315) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (pad 1 smd rect (at -1.04902 0 315) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D10-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 58DE36A5)
    (at 178.465 95.6871 117)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D3 (at 0 -1.75 117) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.75 117) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 297) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D10-Pad1)"))
    (pad 1 smd rect (at -1.04902 0 297) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D12-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 58DE36A8)
    (at 179.383 98.5139 99)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D4 (at 0 -1.75 99) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.75 99) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 279) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D12-Pad1)"))
    (pad 1 smd rect (at -1.04902 0 279) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D0-Pad2)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 58DE36AB)
    (at 179.383 101.486 81)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D5 (at 0 -1.75 81) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.75 81) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 261) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D0-Pad2)"))
    (pad 1 smd rect (at -1.04902 0 261) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 58DE36AE)
    (at 178.465 104.313 63)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D6 (at 0 -1.75 63) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.75 63) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 243) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (pad 1 smd rect (at -1.04902 0 243) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D12-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 58DE36B3)
    (at 176.718 106.718 45)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D7 (at 0 -1.75 45) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.75 45) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 225) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D12-Pad1)"))
    (pad 1 smd rect (at -1.04902 0 225) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D0-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 58DE36BF)
    (at 174.313 108.465 27)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D8 (at 0 -1.75 27) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.75 27) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 207) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D0-Pad1)"))
    (pad 1 smd rect (at -1.04902 0 207) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D10-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 58DE36C3)
    (at 171.486 109.383 9)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D9 (at 0 -1.75 9) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.75 9) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 189) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D10-Pad1)"))
    (pad 1 smd rect (at -1.04902 0 189) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D0-Pad2)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 58DE36C8)
    (at 168.514 109.383 351)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D10 (at 0 -1.75 351) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.75 351) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 171) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D0-Pad2)"))
    (pad 1 smd rect (at -1.04902 0 171) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D10-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 58DE36CB)
    (at 165.687 108.465 333)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D11 (at 0 -1.75 333) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.75 333) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 153) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D10-Pad1)"))
    (pad 1 smd rect (at -1.04902 0 153) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D0-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 58DE36CF)
    (at 163.282 106.718 315)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D12 (at 0 -1.75 315) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.75 315) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 135) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D0-Pad1)"))
    (pad 1 smd rect (at -1.04902 0 135) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D12-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 58DE36D3)
    (at 161.535 104.313 297)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D13 (at 0 -1.75 297) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.75 297) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 117) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D12-Pad1)"))
    (pad 1 smd rect (at -1.04902 0 117) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 58DE36D7)
    (at 160.617 101.486 279)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D14 (at 0 -1.75 279) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.75 279) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 99) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (pad 1 smd rect (at -1.04902 0 99) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D0-Pad2)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 58DE36DB)
    (at 160.617 98.5139 261)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D15 (at 0 -1.75 261) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.75 261) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 81) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D0-Pad2)"))
    (pad 1 smd rect (at -1.04902 0 81) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D12-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 58DE36DF)
    (at 161.535 95.6871 243)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D16 (at 0 -1.75 243) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.75 243) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 63) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D12-Pad1)"))
    (pad 1 smd rect (at -1.04902 0 63) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D10-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 58DE36E3)
    (at 163.282 93.2825 225)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D17 (at 0 -1.75 225) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.75 225) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 45) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D10-Pad1)"))
    (pad 1 smd rect (at -1.04902 0 45) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 58DE36E7)
    (at 165.687 91.5354 207)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D18 (at 0 -1.75 207) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.75 207) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 27) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (pad 1 smd rect (at -1.04902 0 27) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D0-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 58DE36EB)
    (at 168.514 90.617 189)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D19 (at 0 -1.75 189) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.75 189) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 9) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D0-Pad1)"))
    (pad 1 smd rect (at -1.04902 0 9) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D0-Pad2)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SMD-1206_Pol (layer B.Cu) (tedit 0)
    (at 179.324 112.903 270)
    (attr smd)
    (fp_text reference C1 (at 0 0 270) (layer B.SilkS))
    (fp_text value 10µ (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1.651 0 270) (size 1.524 2.032) (layers B.Cu B.Paste B.Mask)
      (net 8 +3V3))
    (pad 2 smd rect (at 1.651 0 270) (size 1.524 2.032) (layers B.Cu B.Paste B.Mask)
      (net 7 GND))
    (model SMD_Packages.3dshapes/SMD-1206_Pol.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.17 0.16 0.16))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIJ-8_5.3x5.3mm_Pitch1.27mm (layer F.Cu) (tedit 58DE3686)
    (at 170.053 99.949 90)
    (descr "8-Lead Plastic Small Outline (SM) - Medium, 5.28 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference IC1 (at 0 -3.68 90) (layer F.SilkS) hide)
    (fp_text value ATTINY45-P (at 0 3.68 90) (layer F.Fab))
    (pad 1 smd rect (at -3.65 -1.905 90) (size 1.7 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(IC1-Pad1)"))
    (pad 2 smd rect (at -3.65 -0.635 90) (size 1.7 0.65) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D0-Pad2)"))
    (pad 3 smd rect (at -3.65 0.635 90) (size 1.7 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (pad 4 smd rect (at -3.65 1.905 90) (size 1.7 0.65) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 5 smd rect (at 3.65 1.905 90) (size 1.7 0.65) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D0-Pad1)"))
    (pad 6 smd rect (at 3.65 0.635 90) (size 1.7 0.65) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D10-Pad1)"))
    (pad 7 smd rect (at 3.65 -0.635 90) (size 1.7 0.65) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D12-Pad1)"))
    (pad 8 smd rect (at 3.65 -1.905 90) (size 1.7 0.65) (layers F.Cu F.Paste F.Mask)
      (net 8 +3V3))
    (model Housings_SOIC.3dshapes/SOIJ-8_5.3x5.3mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_SMD:SW_SPST_KMR2 (layer F.Cu) (tedit 58DE366C)
    (at 161.163 112.395 90)
    (descr "CK components KMR2 tactile switch http://www.ck-components.com/kmr-2/tactile,10572,en.html")
    (tags "tactile switch kmr2")
    (attr smd)
    (fp_text reference SW1 (at 0 -2.45 90) (layer F.SilkS) hide)
    (fp_text value SW_Push (at 0 2.55 90) (layer F.Fab))
    (pad 1 smd rect (at -2.05 -0.8 180) (size 0.9 1) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(IC1-Pad1)"))
    (pad 2 smd rect (at -2.05 0.8 180) (size 0.9 1) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 1 smd rect (at 2.05 -0.8 180) (size 0.9 1) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(IC1-Pad1)"))
    (pad 2 smd rect (at 2.05 0.8 180) (size 0.9 1) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
  )
  (module Connectors:CR2032V (layer B.Cu) (tedit 58DE452A)
    (at 170.053 113.03)
    (fp_text reference BT1 (at -2.667 0) (layer B.SilkS))
    (fp_text value Battery_Cell (at 0 -5.08) (layer B.Fab))
    (pad 1 thru_hole circle (at -5.08 -1.778) (size 2.286 2.286) (drill 1.27) (layers *.Cu *.Mask)
      (net 8 +3V3))
    (pad 1 thru_hole circle (at 5.08 -1.778) (size 2.286 2.286) (drill 1.27) (layers *.Cu *.Mask)
      (net 8 +3V3))
    (pad 2 thru_hole circle (at 0 1.524) (size 2.286 2.286) (drill 1.27) (layers *.Cu *.Mask)
      (net 7 GND))
  )
  (gr_line (start 157.734 115.697) (end 157.734 87.884) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 158.623 116.586) (end 157.734 115.697) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 181.483 116.586) (end 158.623 116.586) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 182.372 115.697) (end 181.483 116.586) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 182.372 87.884) (end 182.372 115.697) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 181.483 86.995) (end 182.372 87.884) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 158.623 86.995) (end 181.483 86.995) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 157.734 87.884) (end 158.623 86.995) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text jens@4k2.de (at 170.053 89.9414) (layer B.Cu))
  (gr_text jens@4k2.de (at 181.102 115.062) (layer F.SilkS))
  (gr_text ©2017 (at 181.102 113.538) (layer F.SilkS))
  (zone (net 7) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 158.623 87.376) (xy 181.483 87.376) (xy 181.991 87.884) (xy 181.991 115.697) (xy 181.483 116.205)
        (xy 158.623 116.205) (xy 158.115 115.697) (xy 158.115 99.568) (xy 158.115 87.884)
      )
    )
    (polygon
      (pts        (xy 162.56 106.426) (xy 169.291 109.601) (xy 175.768 107.95) (xy 179.197 103.124) (xy 178.689 96.139)
        (xy 175.641 91.567) (xy 168.275 90.551) (xy 162.433 93.98) (xy 160.274 99.568) (xy 159.385 99.568)
        (xy 160.274 100.203)
      )
    )
  )
  (zone (net 8) (net_name +3V3) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 158.623 87.376) (xy 158.115 87.884) (xy 158.115 99.949) (xy 181.991 99.949) (xy 181.991 87.884)
        (xy 181.483 87.376)
      )
    )
  )
  (zone (net 7) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 158.115 100.457) (xy 158.115 115.697) (xy 158.623 116.205) (xy 181.483 116.205) (xy 181.991 115.697)
        (xy 181.991 100.457)
      )
    )
  )
)
