(kicad_pcb (version 20171130) (host pcbnew "(5.1.10-1-10_14)")
  (general
    (thickness 1.6)
    (drawings 25)
    (tracks 68)
    (zones 0)
    (modules 15)
    (nets 9)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.5)
    (user_trace_width 0.5)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (user_via 1 0.5)
    (user_via 5 3.2)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /VDD)
  (net 2 GND)
  (net 3 /AOMIN)
  (net 4 /MODIN)
  (net 5 /AOMOUT1)
  (net 6 /AOMOUT2)
  (net 7 /LVTTL)
  (net 8 "Net-(C4-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /AOMIN)
    (add_net /AOMOUT1)
    (add_net /AOMOUT2)
    (add_net /LVTTL)
    (add_net /MODIN)
    (add_net /VDD)
    (add_net GND)
    (add_net "Net-(C4-Pad1)")
  )
  (module Joshs_KiCAD_Footprints:03155391010 (layer F.Cu) (tedit 6179B636)
    (at 111.25 113 90)
    (descr 031-5539-1010-2)
    (tags Connector)
    (fp_text reference RF2 (at 2.2 -3.05 180) (layer F.SilkS))
    (fp_text value "Mod Gate" (at 2.54 0 270) (layer F.SilkS) hide)
    (fp_text user %R (at 2.54 0 270) (layer F.Fab))
    (pad MH2 thru_hole circle (at 7.62 -5.08 90) (size 3 3) (drill 2) (layers *.Cu *.Mask))
    (pad MH1 thru_hole circle (at -2.54 5.08 90) (size 3 3) (drill 2) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 2.54 0 90) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 /MODIN))
    (pad 2 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 GND))
    (model "/Users/joshrogers/OneDrive - The University of Manchester/Electronics/JoshsKiCADLibraries/SamacSys_Parts.3dshapes/031-5539-1010.stp"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Molex:Molex_KK-254_AE-6410-02A_1x02_P2.54mm_Vertical (layer B.Cu) (tedit 5EA53D3B)
    (at 124.25 85.25 90)
    (descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-02A example for new part number: 22-27-2021, 2 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex KK-254 vertical")
    (fp_text reference DC1 (at 1.27 4.12 270) (layer B.SilkS))
    (fp_text value VDD (at 1.27 -4.08 270) (layer B.Fab))
    (fp_text user %R (at 1.27 2.22 270) (layer B.Fab))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.74 2.19) (drill 1.19) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole roundrect (at 0 0 90) (size 1.74 2.19) (drill 1.19) (layers *.Cu *.Mask) (roundrect_rratio 0.143678)
      (net 8 "Net-(C4-Pad1)"))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_KK-254_AE-6410-02A_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder (layer F.Cu) (tedit 5F68FEEE)
    (at 124.25 112 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R2 (at 0 1.8) (layer F.SilkS))
    (fp_text value 2.2k (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.55 0 180) (size 1.3 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.192308)
      (net 2 GND))
    (pad 1 smd roundrect (at -1.55 0 180) (size 1.3 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.192308)
      (net 7 /LVTTL))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder (layer F.Cu) (tedit 5F68FEEE)
    (at 124.25 107.5)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at 0 -1.82) (layer F.SilkS))
    (fp_text value 1k (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.55 0) (size 1.3 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.192308)
      (net 7 /LVTTL))
    (pad 1 smd roundrect (at -1.55 0) (size 1.3 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.192308)
      (net 4 /MODIN))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:MSOP-8_3x3mm_P0.65mm (layer F.Cu) (tedit 5E509FDD)
    (at 124.25 101)
    (descr "MSOP, 8 Pin (https://www.jedec.org/system/files/docs/mo-187F.pdf variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "MSOP SO")
    (attr smd)
    (fp_text reference ADG919 (at 0 -2.45) (layer F.SilkS))
    (fp_text value ADG919BRMZ (at 0 2.45) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 8 smd roundrect (at 2.1125 -0.975) (size 1.625 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 /AOMOUT1))
    (pad 7 smd roundrect (at 2.1125 -0.325) (size 1.625 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 6 smd roundrect (at 2.1125 0.325) (size 1.625 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 5 smd roundrect (at 2.1125 0.975) (size 1.625 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 /AOMOUT2))
    (pad 4 smd roundrect (at -2.1125 0.975) (size 1.625 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 /AOMIN))
    (pad 3 smd roundrect (at -2.1125 0.325) (size 1.625 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 2 smd roundrect (at -2.1125 -0.325) (size 1.625 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 /LVTTL))
    (pad 1 smd roundrect (at -2.1125 -0.975) (size 1.625 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 /VDD))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/MSOP-8_3x3mm_P0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Joshs_KiCAD_Footprints:03155391010 (layer F.Cu) (tedit 6179B636)
    (at 111.25 88.25 270)
    (descr 031-5539-1010-2)
    (tags Connector)
    (fp_text reference RF1 (at 1.95 -2.75) (layer F.SilkS))
    (fp_text value "AOM IN" (at 2.54 0 90) (layer F.SilkS) hide)
    (fp_text user %R (at 2.54 0 90) (layer F.Fab))
    (pad MH2 thru_hole circle (at 7.62 -5.08 270) (size 3 3) (drill 2) (layers *.Cu *.Mask))
    (pad MH1 thru_hole circle (at -2.54 5.08 270) (size 3 3) (drill 2) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 2.54 0 270) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 /AOMIN))
    (pad 2 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 GND))
    (model "/Users/joshrogers/OneDrive - The University of Manchester/Electronics/JoshsKiCADLibraries/SamacSys_Parts.3dshapes/031-5539-1010.stp"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Joshs_KiCAD_Footprints:03155391010 (layer F.Cu) (tedit 6179B636)
    (at 137.25 88.25 270)
    (descr 031-5539-1010-2)
    (tags Connector)
    (fp_text reference RF3 (at 1.35 -2.75 180) (layer F.SilkS))
    (fp_text value "AOM OUT2" (at 2.54 0 270) (layer F.SilkS) hide)
    (fp_text user %R (at 2.54 0 270) (layer F.Fab))
    (pad MH2 thru_hole circle (at 7.62 -5.08 270) (size 3 3) (drill 2) (layers *.Cu *.Mask))
    (pad MH1 thru_hole circle (at -2.54 5.08 270) (size 3 3) (drill 2) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 2.54 0 270) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 5 /AOMOUT1))
    (pad 2 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 GND))
    (model "/Users/joshrogers/OneDrive - The University of Manchester/Electronics/JoshsKiCADLibraries/SamacSys_Parts.3dshapes/031-5539-1010.stp"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Joshs_KiCAD_Footprints:03155391010 (layer F.Cu) (tedit 6179B636)
    (at 137.25 113 90)
    (descr 031-5539-1010-2)
    (tags Connector)
    (fp_text reference RF4 (at 1 -2.85) (layer F.SilkS))
    (fp_text value "AOM OUT1" (at 2.54 0 90) (layer F.SilkS) hide)
    (fp_text user %R (at 2.54 0 90) (layer F.Fab))
    (pad MH2 thru_hole circle (at 7.62 -5.08 90) (size 3 3) (drill 2) (layers *.Cu *.Mask))
    (pad MH1 thru_hole circle (at -2.54 5.08 90) (size 3 3) (drill 2) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 2.54 0 90) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 6 /AOMOUT2))
    (pad 2 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 GND))
    (model "/Users/joshrogers/OneDrive - The University of Manchester/Electronics/JoshsKiCADLibraries/SamacSys_Parts.3dshapes/031-5539-1010.stp"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder (layer F.Cu) (tedit 5F68FEEE)
    (at 141.2 100.6)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R3 (at 0 -1.82) (layer F.SilkS))
    (fp_text value 1k (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.55 0) (size 1.3 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.192308)
      (net 2 GND))
    (pad 1 smd roundrect (at -1.55 0) (size 1.3 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.192308)
      (net 6 /AOMOUT2))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder (layer F.Cu) (tedit 5F68FEEE)
    (at 133.75 100.6)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R4 (at 0 -1.82) (layer F.SilkS))
    (fp_text value 1k (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.55 0) (size 1.3 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.192308)
      (net 2 GND))
    (pad 1 smd roundrect (at -1.55 0) (size 1.3 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.192308)
      (net 5 /AOMOUT1))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer B.Cu) (tedit 5A02FF57)
    (at 124.25 95.8 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference U2 (at 0 2.5 90) (layer B.SilkS))
    (fp_text value 522-ZMR250FTA (at 0 -2.5 90) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 3 smd rect (at 1 0 90) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(C4-Pad1)"))
    (pad 2 smd rect (at -1 -0.95 90) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 1 /VDD))
    (pad 1 smd rect (at -1 0.95 90) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_Tantalum_SMD:CP_EIA-3528-12_Kemet-T_Pad1.50x2.35mm_HandSolder (layer F.Cu) (tedit 5EBA9318)
    (at 124.29 89.23)
    (descr "Tantalum Capacitor SMD Kemet-T (3528-12 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
    (tags "capacitor tantalum")
    (attr smd)
    (fp_text reference C1 (at 0 -2.35) (layer F.SilkS))
    (fp_text value 10u (at 0 2.35) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.625 0) (size 1.5 2.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.166667)
      (net 1 /VDD))
    (pad 2 smd roundrect (at 1.625 0) (size 1.5 2.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.166667)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-3528-12_Kemet-T.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_Tantalum_SMD:CP_EIA-6032-15_Kemet-U_Pad2.25x2.35mm_HandSolder (layer F.Cu) (tedit 5EBA9318)
    (at 124.29 93.04)
    (descr "Tantalum Capacitor SMD Kemet-U (6032-15 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
    (tags "capacitor tantalum")
    (attr smd)
    (fp_text reference C2 (at -4.09 -2.55) (layer F.SilkS))
    (fp_text value 1u (at 0 2.55) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -2.55 0) (size 2.25 2.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.111111)
      (net 1 /VDD))
    (pad 2 smd roundrect (at 2.55 0) (size 2.25 2.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.111111)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-6032-15_Kemet-U.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder (layer F.Cu) (tedit 5F68FEEF)
    (at 124.29 96.85)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C3 (at -3.89 -1.05) (layer F.SilkS))
    (fp_text value 0.1u (at 0 1.85) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.5625 0) (size 1.325 1.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.188679)
      (net 1 /VDD))
    (pad 2 smd roundrect (at 1.5625 0) (size 1.325 1.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.188679)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_Tantalum_SMD:CP_EIA-3528-12_Kemet-T_Pad1.50x2.35mm_HandSolder (layer B.Cu) (tedit 5EBA9318)
    (at 124.29 90.2)
    (descr "Tantalum Capacitor SMD Kemet-T (3528-12 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
    (tags "capacitor tantalum")
    (attr smd)
    (fp_text reference C4 (at 0 2.35) (layer B.SilkS))
    (fp_text value 10u (at 0 -2.35) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 1.625 0) (size 1.5 2.35) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.166667)
      (net 2 GND))
    (pad 1 smd roundrect (at -1.625 0) (size 1.5 2.35) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.166667)
      (net 8 "Net-(C4-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-3528-12_Kemet-T.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "2.5V LR" (at 124.4 98.8) (layer B.SilkS))
  (gr_text 10u (at 125.6 88.2) (layer B.SilkS))
  (gr_text . (at 120.75 98.5) (layer F.SilkS))
  (gr_text 2.2k (at 124.4 114) (layer F.SilkS))
  (gr_text 1k (at 126.8 105.6) (layer F.SilkS))
  (gr_line (start 100.4 121) (end 100.4 80) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 148.2 121) (end 100.4 121) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 148.2 80) (end 148.2 121) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 100.4 80) (end 148.2 80) (layer Edge.Cuts) (width 0.05))
  (gr_text 10u (at 128 89.2 -90) (layer F.SilkS))
  (gr_text 1u (at 124.2 93) (layer F.SilkS))
  (gr_text "Gate In" (at 111.2 119.6) (layer F.SilkS))
  (gr_text ______ (at 137.4 81.2 180) (layer F.SilkS))
  (gr_text "RF Out" (at 137.25 81.5) (layer F.SilkS))
  (gr_text "RF Out" (at 137.25 119.6) (layer F.SilkS))
  (gr_text "RF Modulator:\nTTL pulse at Gate In\nconverts to LVTTL and\nswitches RF signal\nat AOM In on/off at the\ntwo complementary \nAOM Out ports" (at 126.6 105.4) (layer B.SilkS))
  (gr_text 0.1u (at 128.6 96.8 -90) (layer F.SilkS))
  (gr_text 1k (at 130 99.8) (layer F.SilkS))
  (gr_text 1k (at 145.2 100.6) (layer F.SilkS))
  (gr_text "+5 V" (at 120.2 83.8 90) (layer B.SilkS))
  (gr_text "RF In" (at 111.25 81.6) (layer F.SilkS))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 148.2 121) (xy 100.4 121) (xy 100.4 80) (xy 148.2 80)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 148.2 121) (xy 100.4 121) (xy 100.4 80) (xy 148.2 80)
      )
    )
  )
)
