(kicad_pcb (version 20171130) (host pcbnew 5.0.0-fee4fd1~66~ubuntu18.04.1)
  (general
    (thickness 1.6)
    (drawings 57)
    (tracks 267)
    (zones 0)
    (modules 23)
    (nets 48)
  )
  (page USLetter)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.397 1.6)
    (pad_drill 0)
    (pad_to_mask_clearance 0.0508)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(U1-Pad16)")
  (net 2 "Net-(U1-Pad35)")
  (net 3 "Net-(J1-Pad7)")
  (net 4 "Net-(J1-Pad6)")
  (net 5 "Net-(J1-Pad5)")
  (net 6 "Net-(J1-Pad4)")
  (net 7 +3V3)
  (net 8 GND)
  (net 9 /Vbat)
  (net 10 "Net-(J4-Pad3)")
  (net 11 "Net-(J4-Pad2)")
  (net 12 "Net-(J4-Pad4)")
  (net 13 /rst)
  (net 14 /Vusb)
  (net 15 "Net-(R1-Pad1)")
  (net 16 "Net-(D1-Pad1)")
  (net 17 "Net-(R2-Pad2)")
  (net 18 /swdio)
  (net 19 /swdclk)
  (net 20 "Net-(J5-Pad9)")
  (net 21 "Net-(J5-Pad8)")
  (net 22 "Net-(J5-Pad7)")
  (net 23 /sda)
  (net 24 /scl)
  (net 25 /en)
  (net 26 /pd13)
  (net 27 /pd14)
  (net 28 /pf3)
  (net 29 /pf2)
  (net 30 /pc10)
  (net 31 /pc11)
  (net 32 /pd15)
  (net 33 /pa0)
  (net 34 /pb13)
  (net 35 /pb12)
  (net 36 /pb11)
  (net 37 "Net-(J2-Pad3)")
  (net 38 /pf2b)
  (net 39 /pf3b)
  (net 40 /pc11b)
  (net 41 /pc10b)
  (net 42 /pa0b)
  (net 43 /pd15b)
  (net 44 "Net-(J2-Pad10)")
  (net 45 "Net-(J2-Pad9)")
  (net 46 "Net-(J2-Pad8)")
  (net 47 "Net-(D2-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net /Vbat)
    (add_net /Vusb)
    (add_net /en)
    (add_net /pa0)
    (add_net /pa0b)
    (add_net /pb11)
    (add_net /pb12)
    (add_net /pb13)
    (add_net /pc10)
    (add_net /pc10b)
    (add_net /pc11)
    (add_net /pc11b)
    (add_net /pd13)
    (add_net /pd14)
    (add_net /pd15)
    (add_net /pd15b)
    (add_net /pf2)
    (add_net /pf2b)
    (add_net /pf3)
    (add_net /pf3b)
    (add_net /rst)
    (add_net /scl)
    (add_net /sda)
    (add_net /swdclk)
    (add_net /swdio)
    (add_net GND)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J2-Pad10)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J2-Pad8)")
    (add_net "Net-(J2-Pad9)")
    (add_net "Net-(J4-Pad2)")
    (add_net "Net-(J4-Pad3)")
    (add_net "Net-(J4-Pad4)")
    (add_net "Net-(J5-Pad7)")
    (add_net "Net-(J5-Pad8)")
    (add_net "Net-(J5-Pad9)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(R2-Pad2)")
    (add_net "Net-(U1-Pad16)")
    (add_net "Net-(U1-Pad35)")
  )
  (module Daniel:SUNTECH_ST-USB-001G (layer F.Cu) (tedit 5BA060F1)
    (at 150.495 109.22 270)
    (attr smd)
    (fp_text reference J4 (at 0 0 270) (layer F.SilkS))
    (fp_text value USB_B_Micro (at -2.2225 5.2705 270) (layer F.SilkS) hide)
    (pad 6 thru_hole oval (at -3.2258 1.27) (size 2.032 1.27) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 GND))
    (pad 6 thru_hole oval (at 3.2258 1.27) (size 2.032 1.27) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 GND))
    (pad 3 smd rect (at 0 -1.655 90) (size 0.381 1.524) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(J4-Pad3)"))
    (pad 2 smd rect (at -0.65 -1.655 90) (size 0.381 1.524) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(J4-Pad2)"))
    (pad 4 smd rect (at 0.65 -1.655 90) (size 0.381 1.524) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(J4-Pad4)"))
    (pad 5 smd rect (at 1.3 -1.655 90) (size 0.381 1.524) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -1.3 -1.655 90) (size 0.381 1.524) (layers F.Cu F.Paste F.Mask)
      (net 14 /Vusb))
    (pad 6 smd rect (at -3.4 -1.478) (size 1.397 1.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 6 smd rect (at 3.4 -1.478) (size 1.397 1.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 6 smd rect (at -1 1.595 270) (size 1.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 6 smd rect (at 1 1.595 270) (size 1.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad Hole np_thru_hole circle (at -2 -1.255 270) (size 0.635 0.635) (drill 0.635) (layers))
    (pad Hole np_thru_hole circle (at 2 -1.255 270) (size 0.635 0.635) (drill 0.635) (layers))
    (model ${KISYS3DMOD}/Connector_USB.3dshapes/USB_Micro-B_Molex_47346-0001.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 5BA0508B)
    (at 151.511 103.505 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D2 (at 0 -1.27) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.35 180) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.8 0) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 7 +3V3))
    (pad 1 smd rect (at -0.8 0) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(D2-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Daniel:E_SWITCH (layer F.Cu) (tedit 5BA03F7F)
    (at 157.48 114.935 180)
    (descr TL3342F160QG)
    (tags E-SWITCH)
    (autoplace_cost180 10)
    (fp_text reference SW1 (at 0 0 180) (layer F.SilkS))
    (fp_text value E_SWITCH (at 0 0 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -3.15 1.9 180) (size 1.7 1) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 2 smd rect (at 3.15 1.9 180) (size 1.7 1) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 3 smd rect (at -3.15 -1.9 180) (size 1.7 1) (layers F.Cu F.Paste F.Mask)
      (net 13 /rst))
    (pad 4 smd rect (at 3.15 -1.9 180) (size 1.7 1) (layers F.Cu F.Paste F.Mask)
      (net 13 /rst))
    (model Discret/SW_PUSH.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/Button_Switch_SMD.3dshapes/SW_SPST_TL3342.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x05_Pitch1.27mm_SMD (layer F.Cu) (tedit 5B9F0F36)
    (at 172.72 109.22)
    (descr "surface-mounted straight pin header, 2x05, 1.27mm pitch, double rows")
    (tags "Surface mounted pin header SMD 2x05 1.27mm double row")
    (attr smd)
    (fp_text reference J5 (at 0 -4.235) (layer F.SilkS))
    (fp_text value Conn_ARM_JTAG_SWD_10 (at 0 4.235) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.95 -2.54) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 7 +3V3))
    (pad 2 smd rect (at 1.95 -2.54) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 18 /swdio))
    (pad 3 smd rect (at -1.95 -1.27) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 4 smd rect (at 1.95 -1.27) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 19 /swdclk))
    (pad 5 smd rect (at -1.95 0) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 6 smd rect (at 1.95 0) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 38 /pf2b))
    (pad 7 smd rect (at -1.95 1.27) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(J5-Pad7)"))
    (pad 8 smd rect (at 1.95 1.27) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(J5-Pad8)"))
    (pad 9 smd rect (at -1.95 2.54) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(J5-Pad9)"))
    (pad 10 smd rect (at 1.95 2.54) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 13 /rst))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x05_Pitch1.27mm_SMD.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_2x05_P1.27mm_Vertical_SMD.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Daniel:JST-S2B-PH (layer F.Cu) (tedit 569ACA8A)
    (at 158.258 104.14)
    (fp_text reference J3 (at 0 -5) (layer B.SilkS))
    (fp_text value BAT (at 0 -10 180) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 1 0) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 9 /Vbat))
    (pad 2 thru_hole circle (at -1 0) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 8 GND))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_PH_S2B-PH-K_1x02_P2.00mm_Horizontal.step
      (offset (xyz 1.015999984741211 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Daniel:BGM113 (layer F.Cu) (tedit 5B9D99B5)
    (at 198.12 104.775 270)
    (attr smd)
    (fp_text reference U1 (at 4.445 10.795) (layer F.SilkS))
    (fp_text value BGM113 (at 3.9 7.175 180) (layer F.Fab))
    (pad 1 smd oval (at 0.9 0.675 270) (size 2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 2 smd oval (at 0.9 1.475 270) (size 2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 3 smd oval (at 0.9 2.275 270) (size 2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 4 smd oval (at 0.9 3.075 270) (size 2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 5 smd oval (at 0.9 3.875 270) (size 2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 6 smd oval (at 0.9 4.675 270) (size 2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 7 smd oval (at 0.9 5.475 270) (size 2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 8 smd oval (at 0.9 6.275 270) (size 2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 7 +3V3))
    (pad 9 smd oval (at 0.9 7.075 270) (size 2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 18 /swdio))
    (pad 10 smd oval (at 0.9 7.875 270) (size 2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 19 /swdclk))
    (pad 11 smd oval (at 0.9 8.675 270) (size 2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 23 /sda))
    (pad 12 smd oval (at 0.9 9.475 270) (size 2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 24 /scl))
    (pad 13 smd oval (at 0.9 10.275 270) (size 2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 34 /pb13))
    (pad 14 smd oval (at 0.9 11.075 270) (size 2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 35 /pb12))
    (pad 15 smd oval (at 0.9 11.875 270) (size 2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 36 /pb11))
    (pad 16 smd oval (at 0.9 12.675 270) (size 2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(U1-Pad16)"))
    (pad 17 smd oval (at 0.9 13.475 270) (size 2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 7 +3V3))
    (pad 18 smd oval (at 0.9 14.275 270) (size 2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 19 smd oval (at 2.575 14.825) (size 2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 38 /pf2b))
    (pad 20 smd oval (at 3.375 14.825) (size 2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 39 /pf3b))
    (pad 21 smd oval (at 4.175 14.825) (size 2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 40 /pc11b))
    (pad 22 smd oval (at 4.975 14.825) (size 2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 41 /pc10b))
    (pad 23 smd oval (at 5.775 14.825) (size 2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 42 /pa0b))
    (pad 24 smd oval (at 6.575 14.825) (size 2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 43 /pd15b))
    (pad 25 smd oval (at 8.25 14.275 270) (size 2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 26 smd oval (at 8.25 13.475 270) (size 2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 32 /pd15))
    (pad 27 smd oval (at 8.25 12.675 270) (size 2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 33 /pa0))
    (pad 28 smd oval (at 8.25 11.875 270) (size 2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 31 /pc11))
    (pad 29 smd oval (at 8.25 11.075 270) (size 2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 30 /pc10))
    (pad 30 smd oval (at 8.25 10.275 270) (size 2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 29 /pf2))
    (pad 31 smd oval (at 8.25 9.475 270) (size 2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 28 /pf3))
    (pad 32 smd oval (at 8.25 8.675 270) (size 2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 27 /pd14))
    (pad 33 smd oval (at 8.25 7.875 270) (size 2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 26 /pd13))
    (pad 34 smd oval (at 8.25 7.075 270) (size 2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 13 /rst))
    (pad 35 smd oval (at 8.25 6.275 270) (size 2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(U1-Pad35)"))
    (pad 36 smd oval (at 8.25 5.475 270) (size 2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
  )
  (module TO_SOT_Packages_SMD:SOT-89-3 (layer F.Cu) (tedit 5BA03EEF)
    (at 162.56 109.22 90)
    (descr SOT-89-3)
    (tags SOT-89-3)
    (attr smd)
    (fp_text reference U2 (at 4.0005 0) (layer F.SilkS))
    (fp_text value MCP1703A (at 12.7 0 180) (layer F.Fab) hide)
    (fp_text user %R (at 0.38 0 180) (layer F.Fab))
    (pad 2 smd trapezoid (at -0.0762 0 180) (size 1.5 1) (rect_delta 0 0.7 ) (layers F.Cu F.Paste F.Mask)
      (net 9 /Vbat))
    (pad 2 smd rect (at 1.3335 0) (size 2.2 1.84) (layers F.Cu F.Paste F.Mask)
      (net 9 /Vbat))
    (pad 3 smd rect (at -1.48 1.5) (size 1 1.5) (layers F.Cu F.Paste F.Mask)
      (net 7 +3V3))
    (pad 2 smd rect (at -1.3335 0) (size 1 1.8) (layers F.Cu F.Paste F.Mask)
      (net 9 /Vbat))
    (pad 1 smd rect (at -1.48 -1.5) (size 1 1.5) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 2 smd trapezoid (at 2.667 0) (size 1.6 0.85) (rect_delta 0 0.6 ) (layers F.Cu F.Paste F.Mask)
      (net 9 /Vbat))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-89-3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-89-3.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_2.5mm (layer F.Cu) (tedit 5B9EC115)
    (at 195.58 118.11)
    (descr "Mounting Hole 2.5mm, no annular")
    (tags "mounting hole 2.5mm no annular")
    (attr virtual)
    (fp_text reference MH2 (at 0 -3.5) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 7.62 3.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.5mm (layer F.Cu) (tedit 5B9EC111)
    (at 195.58 100.33)
    (descr "Mounting Hole 2.5mm, no annular")
    (tags "mounting hole 2.5mm no annular")
    (attr virtual)
    (fp_text reference MH1 (at 0 -3.5) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 8.255 -3.81) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask))
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 5BA05025)
    (at 151.511 114.935 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D1 (at -2.032 0) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.35 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.8 0) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 0.8 0) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 14 /Vusb))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5BA0546B)
    (at 154.94 111.125)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at 0 0 90) (layer F.SilkS))
    (fp_text value 470 (at 3.175 0) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(R2-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5BA050E4)
    (at 154.305 108.585 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at -1.905 0 180) (layer F.SilkS))
    (fp_text value 10k (at 2.54 0 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(R1-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5BA050DB)
    (at 154.305 104.775 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at 1.905 0) (layer F.SilkS))
    (fp_text value 4.7uF (at 0 1.5 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 14 /Vusb))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x12_Pitch2.54mm (layer F.Cu) (tedit 5B9F0D8A)
    (at 163.83 99.06 90)
    (descr "Through hole straight pin header, 1x12, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x12 2.54mm single row")
    (fp_text reference J1 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value TopRow (at 2.54 26.67 180) (layer F.Fab))
    (fp_text user %R (at 0 13.97 180) (layer F.Fab))
    (pad 12 thru_hole oval (at 0 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 /sda))
    (pad 11 thru_hole oval (at 0 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 /scl))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 /pb13))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 /pb12))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 /pb11))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad7)"))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad6)"))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad5)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad4)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /Vusb))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 /en))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /Vbat))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x12_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x16_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 153.67 119.38 90)
    (descr "Through hole straight pin header, 1x16, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x16 2.54mm single row")
    (fp_text reference J2 (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value BottomRow (at -2.54 35.56 180) (layer F.Fab))
    (fp_text user %R (at 0 19.05 180) (layer F.Fab))
    (pad 16 thru_hole oval (at 0 38.1 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 GND))
    (pad 15 thru_hole oval (at 0 35.56 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 /pd13))
    (pad 14 thru_hole oval (at 0 33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 /pd14))
    (pad 13 thru_hole oval (at 0 30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 /pf3))
    (pad 12 thru_hole oval (at 0 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 /pf2))
    (pad 11 thru_hole oval (at 0 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 /pc10))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 "Net-(J2-Pad10)"))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 "Net-(J2-Pad9)"))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 "Net-(J2-Pad8)"))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 /pc11))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 /pa0))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 /pd15))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 GND))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 "Net-(J2-Pad3)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 +3V3))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /rst))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x16_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5BA054AD)
    (at 158.115 111.125 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at 0 0 270) (layer F.SilkS))
    (fp_text value C (at 0 1.5 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 9 /Vbat))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5BA052ED)
    (at 163.576 113.03 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at -2.159 0 180) (layer F.SilkS))
    (fp_text value C (at 0 1.5 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 +3V3))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-5 (layer F.Cu) (tedit 5B9EC687)
    (at 157.48 107.95 180)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U3 (at 0 0 270) (layer F.SilkS))
    (fp_text value MCP73831-2-OT (at 0 2.9 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 5 smd rect (at 1.1 -0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(R1-Pad1)"))
    (pad 4 smd rect (at 1.1 0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 14 /Vusb))
    (pad 3 smd rect (at -1.1 0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 9 /Vbat))
    (pad 2 smd rect (at -1.1 0 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -1.1 -0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(R2-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connect:PINTST (layer F.Cu) (tedit 5BA03D4B)
    (at 148.59 114.3)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference MH3 (at 0 -1.6) (layer F.SilkS) hide)
    (fp_text value Strap (at 0 1.6) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.143 1.143) (drill 0.635) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connectors.3dshapes/PINTST.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connect:PINTST (layer F.Cu) (tedit 5BA03D39)
    (at 148.59 104.14)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference MH4 (at 0 -1.6) (layer F.SilkS) hide)
    (fp_text value Strap (at 0 1.6) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.143 1.143) (drill 0.635) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connectors.3dshapes/PINTST.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5BA0568A)
    (at 193.155 103.505)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C4 (at 1.79 0 90) (layer F.SilkS))
    (fp_text value C (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 +3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5BA0566E)
    (at 182.245 103.505 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C5 (at 1.905 0 270) (layer F.SilkS))
    (fp_text value C (at 0 1.5 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 +3V3))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5BA054D3)
    (at 154.305 100.965 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at 1.905 0) (layer F.SilkS))
    (fp_text value 470 (at 0 1.5 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 36 /pb11))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(D2-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "bgm113\nfeather\nrev0" (at 172.72 109.22) (layer B.SilkS))
  (gr_text scl (at 189.23 104.14 90) (layer B.SilkS))
  (gr_text pb13 (at 186.69 104.14 90) (layer B.SilkS))
  (gr_text sda (at 191.77 104.14 90) (layer B.SilkS))
  (gr_text vusb (at 168.91 104.14 90) (layer B.SilkS))
  (gr_text pb11 (at 181.61 104.14 90) (layer B.SilkS))
  (gr_text pb12 (at 184.15 104.14 90) (layer B.SilkS))
  (gr_text vbat (at 163.83 104.08 90) (layer B.SilkS))
  (gr_text pf2 (at 181.61 114.3 90) (layer B.SilkS))
  (gr_text GND (at 161.29 114.3 90) (layer B.SilkS))
  (gr_text pd13 (at 189.23 114.3 90) (layer B.SilkS))
  (gr_text pd15 (at 163.83 114.3 90) (layer B.SilkS))
  (gr_text GND (at 191.77 114.3 90) (layer B.SilkS))
  (gr_text ~RST (at 153.67 114.3 90) (layer B.SilkS))
  (gr_text pc10 (at 179.07 114.3 90) (layer B.SilkS))
  (gr_text 3V (at 156.21 114.3 90) (layer B.SilkS))
  (gr_text pd14 (at 186.69 114.3 90) (layer B.SilkS))
  (gr_text pa0 (at 166.37 114.3 90) (layer B.SilkS))
  (gr_text pc11 (at 168.91 114.3 90) (layer B.SilkS))
  (gr_text pf3 (at 184.15 114.3 90) (layer B.SilkS))
  (gr_text CHG (at 151.765 116.205) (layer F.SilkS))
  (gr_text GND (at 191.77 118.11 90) (layer F.SilkS))
  (gr_text pd13 (at 189.23 118.11 90) (layer F.SilkS))
  (gr_text pd14 (at 186.69 118.11 90) (layer F.SilkS))
  (gr_text pf3 (at 184.15 118.11 90) (layer F.SilkS))
  (gr_text pf2 (at 181.61 118.11 90) (layer F.SilkS))
  (gr_text pc10 (at 179.07 118.11 90) (layer F.SilkS))
  (gr_text pc11 (at 168.91 118.11 90) (layer F.SilkS))
  (gr_text pa0 (at 166.37 118.11 90) (layer F.SilkS))
  (gr_text pd15 (at 163.83 118.11 90) (layer F.SilkS))
  (gr_text vusb (at 168.91 100.33 90) (layer F.SilkS))
  (gr_text vbat (at 163.83 100.39 90) (layer F.SilkS))
  (gr_text pb11 (at 181.61 100.33 90) (layer F.SilkS))
  (gr_text pb12 (at 184.15 100.33 90) (layer F.SilkS))
  (gr_text pb13 (at 186.69 100.33 90) (layer F.SilkS))
  (gr_text sda (at 191.77 100.33 90) (layer F.SilkS))
  (gr_text scl (at 189.23 100.33 90) (layer F.SilkS))
  (gr_text GND (at 161.29 118.11 90) (layer F.SilkS))
  (gr_text 3V (at 156.21 118.11 90) (layer F.SilkS))
  (gr_text ~RST (at 153.67 118.11 90) (layer F.SilkS))
  (gr_line (start 149.86 120.65) (end 195.58 120.65) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 195.58 97.79) (end 149.86 97.79) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 198.12 118.11) (end 198.12 100.33) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 195.58 118.11) (end 195.58 120.65) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 195.58 100.33) (end 198.12 100.33) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 147.32 100.33) (end 147.32 118.11) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 149.86 118.11) (end 147.32 118.11) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 149.86 100.33) (end 149.86 97.79) (angle -90) (layer Edge.Cuts) (width 0.15))
  (zone (net 0) (net_name "") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 193.04 107.95) (xy 193.04 120.65) (xy 198.12 120.65) (xy 198.12 107.95)
      )
    )
  )
  (zone (net 8) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 147.32 97.79) (xy 198.12 97.79) (xy 198.12 120.65) (xy 147.32 120.65)
      )
    )
  )
  (zone (net 7) (net_name +3V3) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 147.32 97.79) (xy 198.12 97.79) (xy 198.12 120.65) (xy 147.32 120.65)
      )
    )
  )
)
