(kicad_pcb (version 4) (host pcbnew 4.0.1-stable)
  (general
    (links 10)
    (no_connects 0)
    (area 137 92.775 161.713097 111.000001)
    (thickness 1.6)
    (drawings 4)
    (tracks 20)
    (zones 0)
    (modules 4)
    (nets 6)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal hide)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.2)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010f8_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory Gerber/))
  )
  (net 0 "")
  (net 1 GNDPWR)
  (net 2 Vin)
  (net 3 Vout)
  (net 4 On)
  (net 5 "Net-(U1-Pad3)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(U1-Pad3)")
    (add_net On)
  )
  (net_class Power ""
    (clearance 0.2)
    (trace_width 0.5)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GNDPWR)
    (add_net Vin)
    (add_net Vout)
  )
  (module Capacitors_Tantalum_SMD:TantalC_SizeE_EIA-7360_HandSoldering placed (layer F.Cu) (tedit 58765E77)
    (at 144 102 270)
    (descr "Tantal Cap. , Size E, EIA-7360, Hand Soldering,")
    (tags "Tantal Cap. , Size E, EIA-7360, Hand Soldering,")
    (attr smd)
    (fp_text reference CStore (at 0 3.5 270) (layer F.SilkS))
    (fp_text value CP (at 0 4.50088 270) (layer F.Fab) hide)
    (fp_text user + (at -6.35 -3.39852 270) (layer F.SilkS))
    (pad 2 smd rect (at 4.17576 0 270) (size 4.54914 4.39928) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDPWR))
    (pad 1 smd rect (at -4.17576 0 270) (size 4.54914 4.39928) (layers F.Cu F.Paste F.Mask)
      (net 2 Vin))
    (model Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeE_EIA-7360_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering placed (layer F.Cu) (tedit 587661DC)
    (at 150 106 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference "1uF Bypass" (at -1 2 270) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 Vin))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDPWR))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x05 placed (layer F.Cu) (tedit 5876626E)
    (at 155 97)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference "Gnd Vin On Vout Gnd" (at -2 5 90) (layer F.SilkS))
    (fp_text value "Gnd Vin On Vout Gnd" (at 0 -3.1) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GNDPWR))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 Vout))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 On))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 Vin))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GNDPWR))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x05.wrl
      (at (xyz 0 -0.2 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module myFootprints:SOT23-6Handsolderable placed (layer F.Cu) (tedit 587661AA)
    (at 150 99 270)
    (descr "6 pins, \"Small Outline Transistor\"\nbased on Texas Instruments package named: DBV\nTypical part Texas Instruments TPS22860\nDiscrepancy from TI recommendations: rounded pads")
    (fp_text reference TPS22860 (at 0 2 270) (layer F.SilkS))
    (fp_text value TPS22860 (at 0 2.2 270) (layer F.SilkS) hide)
    (pad 1 smd oval (at -1.6 -0.95 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 Vout))
    (pad 2 smd oval (at -1.6 0 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDPWR))
    (pad 3 smd oval (at -1.6 0.95 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(U1-Pad3)"))
    (pad 4 smd oval (at 1.6 0.95 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 Vin))
    (pad 5 smd oval (at 1.6 0 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 Vin))
    (pad 6 smd oval (at 1.6 -0.95 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 On))
  )
  (gr_line (start 140 94.5) (end 157.5 94.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 140 109.5) (end 140 94.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 157.5 109.5) (end 140 109.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 157.5 94.5) (end 157.5 109.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GNDPWR) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 158 110) (xy 138 110) (xy 138 94) (xy 158 94) (xy 158 110)
      )
    )
  )
  (zone (net 1) (net_name GNDPWR) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 137 93) (xy 159 93) (xy 159 111) (xy 137 111)
      )
    )
  )
)
