(kicad_pcb (version 20171130) (host pcbnew "(5.1.5)-3")
  (general
    (thickness 1.6)
    (drawings 17)
    (tracks 145)
    (zones 0)
    (modules 24)
    (nets 29)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user hide)
    (38 B.Mask user hide)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 2)
    (user_trace_width 1.6)
    (user_trace_width 2)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /1)
  (net 2 "Net-(J1-Pad16)")
  (net 3 "Net-(J1-Pad15)")
  (net 4 "Net-(J1-Pad14)")
  (net 5 "Net-(J1-Pad13)")
  (net 6 "Net-(J1-Pad3)")
  (net 7 "Net-(J1-Pad2)")
  (net 8 "Net-(J2-Pad14)")
  (net 9 "Net-(J2-Pad13)")
  (net 10 "Net-(J2-Pad3)")
  (net 11 /L12)
  (net 12 /L11)
  (net 13 /L10)
  (net 14 /L9)
  (net 15 /L8)
  (net 16 /L7)
  (net 17 /L6)
  (net 18 /L5)
  (net 19 /L4)
  (net 20 /R12)
  (net 21 /R11)
  (net 22 /R10)
  (net 23 /R9)
  (net 24 /R8)
  (net 25 /R7)
  (net 26 /R6)
  (net 27 /R5)
  (net 28 /R4)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /1)
    (add_net /L10)
    (add_net /L11)
    (add_net /L12)
    (add_net /L4)
    (add_net /L5)
    (add_net /L6)
    (add_net /L7)
    (add_net /L8)
    (add_net /L9)
    (add_net /R10)
    (add_net /R11)
    (add_net /R12)
    (add_net /R4)
    (add_net /R5)
    (add_net /R6)
    (add_net /R7)
    (add_net /R8)
    (add_net /R9)
    (add_net "Net-(J1-Pad13)")
    (add_net "Net-(J1-Pad14)")
    (add_net "Net-(J1-Pad15)")
    (add_net "Net-(J1-Pad16)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J2-Pad13)")
    (add_net "Net-(J2-Pad14)")
    (add_net "Net-(J2-Pad3)")
  )
  (module ICComponents:logo (layer F.Cu) (tedit 0)
    (at -30.63494 -0.7493)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module ICComponents:WindowFarPads (layer B.Cu) (tedit 5E20DF53)
    (at 34 0 180)
    (fp_text reference J8 (at 1.4318 -10.8712) (layer B.SilkS))
    (fp_text value PadsFarRight (at 1.1524 11.3792) (layer B.Fab))
    (pad 8 smd roundrect (at 1 -8.89 180) (size 2 2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 20 /R12))
    (pad 7 smd roundrect (at 1 -6.35 180) (size 2 2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 21 /R11))
    (pad 6 smd roundrect (at 1 -3.81 180) (size 2 2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 22 /R10))
    (pad 5 smd roundrect (at 1 -1.27 180) (size 2 2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 23 /R9))
    (pad 4 smd roundrect (at 1 1.27 180) (size 2 2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 24 /R8))
    (pad 3 smd roundrect (at 1 3.81 180) (size 2 2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 25 /R7))
    (pad 2 smd roundrect (at 1 6.35 180) (size 2 2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 26 /R6))
    (pad 1 smd roundrect (at 1 8.89 180) (size 2 2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 27 /R5))
  )
  (module ICComponents:WindowFarPads (layer B.Cu) (tedit 5E20DF53)
    (at -32 0 180)
    (fp_text reference J7 (at 1.4318 -10.8712) (layer B.SilkS))
    (fp_text value PadsFarLeft (at 1.1524 11.3792) (layer B.Fab))
    (pad 8 smd roundrect (at 1 -8.89 180) (size 2 2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 11 /L12))
    (pad 7 smd roundrect (at 1 -6.35 180) (size 2 2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 12 /L11))
    (pad 6 smd roundrect (at 1 -3.81 180) (size 2 2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 13 /L10))
    (pad 5 smd roundrect (at 1 -1.27 180) (size 2 2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 14 /L9))
    (pad 4 smd roundrect (at 1 1.27 180) (size 2 2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 15 /L8))
    (pad 3 smd roundrect (at 1 3.81 180) (size 2 2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 16 /L7))
    (pad 2 smd roundrect (at 1 6.35 180) (size 2 2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 17 /L6))
    (pad 1 smd roundrect (at 1 8.89 180) (size 2 2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 18 /L5))
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at -16.15092 18.45818)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R15 (at 0.0397 -1.70434) (layer F.SilkS))
    (fp_text value 10M (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 3 "Net-(J1-Pad15)"))
    (pad 1 smd roundrect (at -1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 2 "Net-(J1-Pad16)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at -16.58968 -18.6055 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R14 (at -0.06698 -1.81102) (layer F.SilkS))
    (fp_text value 10M (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 180) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 1 /1))
    (pad 1 smd roundrect (at -1.4875 0 180) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 7 "Net-(J1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ICComponents:WindowPads (layer B.Cu) (tedit 5E20BDF6)
    (at 26.5 0 180)
    (fp_text reference J2 (at 3.048 -21.3868) (layer Dwgs.User))
    (fp_text value Conn_01x16_Male (at 2.9464 21.0058) (layer B.Fab))
    (pad 16 smd roundrect (at 3.25 -18.84 180) (size 6.5 1.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 "Net-(J1-Pad16)"))
    (pad 15 smd roundrect (at 3.25 -16.5 180) (size 6.5 2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 3 "Net-(J1-Pad15)"))
    (pad 14 smd roundrect (at 3.25 -13.96 180) (size 6.5 2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 8 "Net-(J2-Pad14)"))
    (pad 13 smd roundrect (at 3.25 -11.42 180) (size 6.5 2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 9 "Net-(J2-Pad13)"))
    (pad 12 smd roundrect (at 3.25 -8.88 180) (size 6.5 2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 20 /R12))
    (pad 11 smd roundrect (at 3.25 -6.34 180) (size 6.5 2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 21 /R11))
    (pad 10 smd roundrect (at 3.25 -3.8 180) (size 6.5 2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 22 /R10))
    (pad 9 smd roundrect (at 3.25 -1.26 180) (size 6.5 2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 23 /R9))
    (pad 8 smd roundrect (at 3.25 1.28 180) (size 6.5 2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 24 /R8))
    (pad 7 smd roundrect (at 3.25 3.82 180) (size 6.5 2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 25 /R7))
    (pad 6 smd roundrect (at 3.25 6.36 180) (size 6.5 2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 26 /R6))
    (pad 5 smd roundrect (at 3.25 8.9 180) (size 6.5 2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 27 /R5))
    (pad 4 smd roundrect (at 3.25 11.44 180) (size 6.5 2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 28 /R4))
    (pad 3 smd roundrect (at 3.25 13.98 180) (size 6.5 2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 10 "Net-(J2-Pad3)"))
    (pad 2 smd roundrect (at 3.25 16.52 180) (size 6.5 2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 7 "Net-(J1-Pad2)"))
    (pad 1 smd roundrect (at 3.25 18.86 180) (size 6.5 1.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 /1))
  )
  (module ICComponents:WindowPads (layer B.Cu) (tedit 5E20BDF6)
    (at -20 0 180)
    (fp_text reference J1 (at 3.048 -21.3868) (layer Dwgs.User))
    (fp_text value Conn_01x16_Male (at 2.9464 21.0058) (layer B.Fab))
    (pad 16 smd roundrect (at 3.25 -18.84 180) (size 6.5 1.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 "Net-(J1-Pad16)"))
    (pad 15 smd roundrect (at 3.25 -16.5 180) (size 6.5 2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 3 "Net-(J1-Pad15)"))
    (pad 14 smd roundrect (at 3.25 -13.96 180) (size 6.5 2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(J1-Pad14)"))
    (pad 13 smd roundrect (at 3.25 -11.42 180) (size 6.5 2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(J1-Pad13)"))
    (pad 12 smd roundrect (at 3.25 -8.88 180) (size 6.5 2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 11 /L12))
    (pad 11 smd roundrect (at 3.25 -6.34 180) (size 6.5 2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 12 /L11))
    (pad 10 smd roundrect (at 3.25 -3.8 180) (size 6.5 2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 13 /L10))
    (pad 9 smd roundrect (at 3.25 -1.26 180) (size 6.5 2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 14 /L9))
    (pad 8 smd roundrect (at 3.25 1.28 180) (size 6.5 2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 15 /L8))
    (pad 7 smd roundrect (at 3.25 3.82 180) (size 6.5 2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 16 /L7))
    (pad 6 smd roundrect (at 3.25 6.36 180) (size 6.5 2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 17 /L6))
    (pad 5 smd roundrect (at 3.25 8.9 180) (size 6.5 2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 18 /L5))
    (pad 4 smd roundrect (at 3.25 11.44 180) (size 6.5 2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 /L4))
    (pad 3 smd roundrect (at 3.25 13.98 180) (size 6.5 2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 6 "Net-(J1-Pad3)"))
    (pad 2 smd roundrect (at 3.25 16.52 180) (size 6.5 2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 7 "Net-(J1-Pad2)"))
    (pad 1 smd roundrect (at 3.25 18.86 180) (size 6.5 1.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 /1))
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 17.6 15.24 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R13 (at 0 -1.82 90) (layer F.SilkS))
    (fp_text value 10M (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 8 "Net-(J2-Pad14)"))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 3 "Net-(J1-Pad15)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at -17.6 12.7 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R12 (at 0 -1.82 90) (layer F.SilkS))
    (fp_text value 10M (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 4 "Net-(J1-Pad14)"))
    (pad 1 smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 5 "Net-(J1-Pad13)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 17.6 10.16 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R11 (at 0 -1.82 90) (layer F.SilkS))
    (fp_text value 10M (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 20 /R12))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 9 "Net-(J2-Pad13)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at -17.6 7.62 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R10 (at 0 -1.82 90) (layer F.SilkS))
    (fp_text value 10M (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 11 /L12))
    (pad 1 smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 12 /L11))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 17.6 5.08 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R9 (at 0 -1.82 90) (layer F.SilkS))
    (fp_text value 10M (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 22 /R10))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 21 /R11))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at -17.6 2.54 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R8 (at 0 -1.82 90) (layer F.SilkS))
    (fp_text value 10M (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 13 /L10))
    (pad 1 smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 14 /L9))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 17.6 0 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R7 (at 0 -1.82 90) (layer F.SilkS))
    (fp_text value 10M (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 24 /R8))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 23 /R9))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at -17.6 -2.54 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R6 (at 0 -1.82 90) (layer F.SilkS))
    (fp_text value 10M (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 15 /L8))
    (pad 1 smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 16 /L7))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 17.6 -5.08 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R5 (at 0 -1.82 90) (layer F.SilkS))
    (fp_text value 10M (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 26 /R6))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 25 /R7))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at -17.6 -7.62 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R4 (at 0 -1.82 90) (layer F.SilkS))
    (fp_text value 10M (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 17 /L6))
    (pad 1 smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 18 /L5))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 17.6 -10.16 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R3 (at 0 -1.82 90) (layer F.SilkS))
    (fp_text value 10M (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 28 /R4))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 27 /R5))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at -17.6 -12.7 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R2 (at 0 -1.82 90) (layer F.SilkS))
    (fp_text value 10M (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 19 /L4))
    (pad 1 smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 6 "Net-(J1-Pad3)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 17.6 -15.24 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at 0 -1.82 90) (layer F.SilkS))
    (fp_text value 10M (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 7 "Net-(J1-Pad2)"))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 10 "Net-(J2-Pad3)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ICComponents:4-40MountingHole (layer F.Cu) (tedit 5E20A43E)
    (at 31 15)
    (fp_text reference J6 (at -0.0254 5.1308) (layer Dwgs.User))
    (fp_text value VCath (at 0.0508 -4.7752) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 2.3) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad16)"))
    (pad 1 thru_hole circle (at 2.3 0) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad16)"))
    (pad 1 thru_hole circle (at -2.3 0) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad16)"))
    (pad 1 thru_hole circle (at 0 -2.3) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad16)"))
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.1) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad16)"))
  )
  (module ICComponents:4-40MountingHole (layer F.Cu) (tedit 5E20A43E)
    (at -31 -15)
    (fp_text reference J5 (at -0.0254 5.1308) (layer Dwgs.User))
    (fp_text value VFrish (at 0.0508 -4.7752) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 2.3) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 /1))
    (pad 1 thru_hole circle (at 2.3 0) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 /1))
    (pad 1 thru_hole circle (at -2.3 0) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 /1))
    (pad 1 thru_hole circle (at 0 -2.3) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 /1))
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.1) (layers *.Cu *.Mask)
      (net 1 /1))
  )
  (module ICComponents:4-40MountingHole (layer F.Cu) (tedit 5E20A43E)
    (at -31 15)
    (fp_text reference J4 (at -0.0254 5.1308) (layer Dwgs.User))
    (fp_text value VCath (at 0.0508 -4.7752) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 2.3) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad16)"))
    (pad 1 thru_hole circle (at 2.3 0) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad16)"))
    (pad 1 thru_hole circle (at -2.3 0) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad16)"))
    (pad 1 thru_hole circle (at 0 -2.3) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad16)"))
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.1) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad16)"))
  )
  (module ICComponents:4-40MountingHole (layer F.Cu) (tedit 5E20A43E)
    (at 31 -15)
    (fp_text reference J3 (at 2.30448 2.22888) (layer Dwgs.User))
    (fp_text value VFrish (at 0.0388 -0.14856) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 2.3) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 /1))
    (pad 1 thru_hole circle (at 2.3 0) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 /1))
    (pad 1 thru_hole circle (at -2.3 0) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 /1))
    (pad 1 thru_hole circle (at 0 -2.3) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 /1))
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.1) (layers *.Cu *.Mask)
      (net 1 /1))
  )
  (gr_text "IC Foil Frame v1\nAdam Anthony 1/16/20" (at 30.22092 -0.4064 90) (layer F.SilkS))
  (gr_arc (start -30 15.5) (end -30 20) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 30 15.5) (end 34.5 15.5) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 30 -15.5) (end 30 -20) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start -30 -15.5) (end -34.5 -15.5) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_text FrischGrid (at 0 -19.1516) (layer F.SilkS))
  (gr_text Cathode (at 0 17.73936) (layer F.SilkS))
  (gr_line (start -15 15) (end -15 -15) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 15 15) (end -15 15) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 15 -15) (end 15 15) (layer Edge.Cuts) (width 0.05))
  (gr_line (start -15 -15) (end 15 -15) (layer Edge.Cuts) (width 0.05))
  (gr_line (start -34.5 -15.5) (end -34.5 15.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 30 20) (end -30 20) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 34.5 -15.5) (end 34.5 15.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start -30 -20) (end 30 -20) (layer Edge.Cuts) (width 0.05))
  (zone (net 0) (net_name "") (layer B.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 36.449 22.3393) (xy -36.16706 23.50516) (xy -34.8361 -21.57984) (xy 35.20186 -21.74494)
      )
    )
  )
)
