(kicad_pcb (version 20171130) (host pcbnew "(5.1.10)-1")
  (general
    (thickness 1.6)
    (drawings 36)
    (tracks 126)
    (zones 0)
    (modules 6)
    (nets 16)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.889)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(P1-Pad3)")
  (net 2 "Net-(P1-Pad4)")
  (net 3 "Net-(P1-Pad5)")
  (net 4 "Net-(P1-Pad6)")
  (net 5 "Net-(P1-Pad7)")
  (net 6 "Net-(P2-Pad7)")
  (net 7 "Net-(P2-Pad8)")
  (net 8 "Net-(BZ1-Pad1)")
  (net 9 "Net-(BZ1-Pad2)")
  (net 10 "Net-(J1-Pad1)")
  (net 11 "Net-(J1-Pad4)")
  (net 12 "Net-(JP1-Pad1)")
  (net 13 "Net-(JP1-Pad2)")
  (net 14 "Net-(P2-Pad5)")
  (net 15 "Net-(P2-Pad6)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(BZ1-Pad1)")
    (add_net "Net-(BZ1-Pad2)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(JP1-Pad1)")
    (add_net "Net-(JP1-Pad2)")
    (add_net "Net-(P1-Pad3)")
    (add_net "Net-(P1-Pad4)")
    (add_net "Net-(P1-Pad5)")
    (add_net "Net-(P1-Pad6)")
    (add_net "Net-(P1-Pad7)")
    (add_net "Net-(P2-Pad5)")
    (add_net "Net-(P2-Pad6)")
    (add_net "Net-(P2-Pad7)")
    (add_net "Net-(P2-Pad8)")
  )
  (module XIAM:TomXIAO (layer B.Cu) (tedit 6240C7F5)
    (at 137.16 117.348 180)
    (attr smd)
    (fp_text reference U1 (at 9.3345 21.7805) (layer B.SilkS))
    (fp_text value SeeeduinoXIAO (at 8.89 10.795) (layer B.SilkS))
    (pad 15 smd oval (at 7.7 1.8 90) (size 2.032 1.016) (layers B.Cu B.Paste B.Mask))
    (pad 16 smd oval (at 10.25 1.8 90) (size 2.032 1.016) (layers B.Cu B.Paste B.Mask))
    (pad 17 smd circle (at 7.698803 18.804187 90) (size 1.143 1.143) (layers B.Cu B.Paste B.Mask))
    (pad 18 smd circle (at 10.238803 18.804187 90) (size 1.143 1.143) (layers B.Cu B.Paste B.Mask))
    (pad 19 smd circle (at 7.698803 16.264187 90) (size 1.143 1.143) (layers B.Cu B.Paste B.Mask))
    (pad 20 smd circle (at 10.238803 16.264187 90) (size 1.143 1.143) (layers B.Cu B.Paste B.Mask))
    (pad 1 thru_hole circle (at 1.27 18.034 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 6 "Net-(P2-Pad7)"))
    (pad 14 thru_hole circle (at 16.51 18.034 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 12 "Net-(JP1-Pad1)"))
    (pad 2 thru_hole circle (at 1.27 15.494 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 15 "Net-(P2-Pad6)"))
    (pad 3 thru_hole circle (at 1.27 12.954 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 7 "Net-(P2-Pad8)"))
    (pad 4 thru_hole circle (at 1.27 10.414 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 5 "Net-(P1-Pad7)"))
    (pad 5 thru_hole circle (at 1.27 7.874 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 4 "Net-(P1-Pad6)"))
    (pad 6 thru_hole circle (at 1.27 5.334 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 3 "Net-(P1-Pad5)"))
    (pad 7 thru_hole circle (at 1.27 2.794 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad1)"))
    (pad 13 thru_hole circle (at 16.51 15.494 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad4)"))
    (pad 12 thru_hole circle (at 16.51 12.954 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 8 "Net-(BZ1-Pad1)"))
    (pad 11 thru_hole circle (at 16.51 10.414 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 1 "Net-(P1-Pad3)"))
    (pad 10 thru_hole circle (at 16.51 7.874 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 14 "Net-(P2-Pad5)"))
    (pad 9 thru_hole circle (at 16.51 5.334 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 2 "Net-(P1-Pad4)"))
    (pad 8 thru_hole circle (at 16.51 2.794 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 9 "Net-(BZ1-Pad2)"))
  )
  (module Buzzer_Beeper:Buzzer_15x7.5RM7.6 (layer B.Cu) (tedit 6240AA90)
    (at 142.748 110.236)
    (descr "Generic Buzzer, D15mm height 7.5mm with RM7.6mm")
    (tags buzzer)
    (fp_text reference BZ1 (at 7.62 6.604) (layer B.SilkS))
    (fp_text value Buzzer (at 3.81 -8.89) (layer B.Fab))
    (fp_text user + (at -0.01 2.54) (layer B.Fab))
    (fp_text user + (at -0.01 2.54) (layer B.SilkS))
    (fp_text user %R (at 3.8 4) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(BZ1-Pad1)"))
    (pad 2 thru_hole circle (at 7.6 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(BZ1-Pad2)"))
    (model ${KISYS3DMOD}/Buzzer_Beeper.3dshapes/Buzzer_15x7.5RM7.6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x08_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 111.76 98.044)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (fp_text reference P1 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Display_7735-1 (at -5.08 12.192 90) (layer F.Fab))
    (fp_text user %R (at 0 8.89 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(BZ1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad4)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(P1-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(P1-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(P1-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(P1-Pad6)"))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(P1-Pad7)"))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(JP1-Pad2)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x08_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinSocket_2.54mm:PinSocket_2x04_P2.54mm_Vertical (layer F.Cu) (tedit 5A19A422)
    (at 141.224 98.044 90)
    (descr "Through hole straight socket strip, 2x04, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 2x04 2.54mm double row")
    (fp_text reference P2 (at -0.508 9.652 90) (layer F.SilkS))
    (fp_text value "CC1101 Receiver" (at -6.096 3.048) (layer F.Fab))
    (fp_text user %R (at -1.27 3.81) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad4)"))
    (pad 2 thru_hole oval (at -2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(BZ1-Pad1)"))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(P1-Pad3)"))
    (pad 4 thru_hole oval (at -2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(P1-Pad4)"))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(P2-Pad5)"))
    (pad 6 thru_hole oval (at -2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(P2-Pad6)"))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(P2-Pad7)"))
    (pad 8 thru_hole oval (at -2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(P2-Pad8)"))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_2x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC)
    (at 155.448 98.044 180)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference J1 (at 2.032 1.524) (layer B.SilkS))
    (fp_text value DI/DO (at 0 -9.95) (layer B.Fab))
    (fp_text user %R (at 0 -3.81 -90) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad1)"))
    (pad 2 thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(BZ1-Pad2)"))
    (pad 3 thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(BZ1-Pad1)"))
    (pad 4 thru_hole oval (at 0 -7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad4)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC)
    (at 155.448 114.808)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference JP1 (at -2.54 1.524) (layer B.SilkS))
    (fp_text value "BL Voltage" (at -2.032 -2.032 90) (layer B.Fab))
    (fp_text user %R (at 0 -2.54 -90) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(JP1-Pad1)"))
    (pad 2 thru_hole oval (at 0 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(JP1-Pad2)"))
    (pad 3 thru_hole oval (at 0 -5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(BZ1-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text GND (at 153.416 105.664) (layer B.SilkS))
  (gr_text V4 (at 139.7 116.332) (layer B.SilkS))
  (gr_text Display_7735-1 (at 109.22 106.172 90) (layer B.SilkS))
  (gr_text 3.3V (at 153.924 110.744) (layer B.SilkS))
  (gr_text 5V (at 153.416 113.284) (layer B.SilkS))
  (gr_text 3.3 (at 153.416 103.124) (layer B.SilkS))
  (gr_text D7 (at 153.416 100.584) (layer B.SilkS))
  (gr_text D6 (at 153.416 98.044) (layer B.SilkS))
  (dimension 22.352 (width 0.15) (layer Dwgs.User)
    (gr_text "0.8800 in" (at 99.284 106.68 270) (layer Dwgs.User))
    (feature1 (pts (xy 108.204 117.856) (xy 99.997579 117.856)))
    (feature2 (pts (xy 108.204 95.504) (xy 99.997579 95.504)))
    (crossbar (pts (xy 100.584 95.504) (xy 100.584 117.856)))
    (arrow1a (pts (xy 100.584 117.856) (xy 99.997579 116.729496)))
    (arrow1b (pts (xy 100.584 117.856) (xy 101.170421 116.729496)))
    (arrow2a (pts (xy 100.584 95.504) (xy 99.997579 96.630504)))
    (arrow2b (pts (xy 100.584 95.504) (xy 101.170421 96.630504)))
  )
  (dimension 49.276 (width 0.15) (layer Dwgs.User)
    (gr_text "1.9400 in" (at 132.842 90.648) (layer Dwgs.User))
    (feature1 (pts (xy 157.48 95.504) (xy 157.48 91.361579)))
    (feature2 (pts (xy 108.204 95.504) (xy 108.204 91.361579)))
    (crossbar (pts (xy 108.204 91.948) (xy 157.48 91.948)))
    (arrow1a (pts (xy 157.48 91.948) (xy 156.353496 92.534421)))
    (arrow1b (pts (xy 157.48 91.948) (xy 156.353496 91.361579)))
    (arrow2a (pts (xy 108.204 91.948) (xy 109.330504 92.534421)))
    (arrow2b (pts (xy 108.204 91.948) (xy 109.330504 91.361579)))
  )
  (gr_line (start 108.204 117.856) (end 108.204 95.504) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 157.48 117.856) (end 108.204 117.856) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 157.48 95.504) (end 157.48 117.856) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 108.204 95.504) (end 157.48 95.504) (layer Edge.Cuts) (width 0.05))
  (gr_text D6 (at 139.192 114.3) (layer B.SilkS))
  (gr_text D5 (at 139.192 111.76) (layer B.SilkS))
  (gr_text D4 (at 139.192 109.22) (layer B.SilkS))
  (gr_text D3 (at 139.192 106.68) (layer B.SilkS))
  (gr_text D2 (at 139.192 104.14) (layer B.SilkS))
  (gr_text D1 (at 139.192 101.6) (layer B.SilkS))
  (gr_text D0 (at 139.192 99.06) (layer B.SilkS))
  (gr_text D7 (at 116.84 114.3) (layer B.SilkS))
  (gr_text SCK (at 116.84 111.76) (layer B.SilkS))
  (gr_text MISO (at 116.84 109.22) (layer B.SilkS))
  (gr_text MOSI (at 116.84 106.68) (layer B.SilkS))
  (gr_text 3.3V (at 116.84 104.14) (layer B.SilkS))
  (gr_text Gnd (at 117.348 101.6) (layer B.SilkS))
  (gr_text 5v (at 117.348 99.06) (layer B.SilkS))
  (gr_text BL (at 114.808 115.824) (layer B.SilkS))
  (gr_text RST (at 114.808 113.284) (layer B.SilkS))
  (gr_text DC (at 114.808 110.744) (layer B.SilkS))
  (gr_text CS (at 114.808 108.204) (layer B.SilkS))
  (gr_text CLK (at 114.808 105.664) (layer B.SilkS))
  (gr_text DIN (at 114.808 103.124) (layer B.SilkS))
  (gr_text GND (at 114.808 100.584) (layer B.SilkS))
  (gr_text 3.3V (at 114.808 98.044) (layer B.SilkS))
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 166.116 124.968) (xy 94.996 123.952) (xy 104.016293 87.3697) (xy 165.608 86.36)
      )
    )
    (polygon
      (pts
        (xy 104.016293 87.3697) (xy 103.632 87.376) (xy 104.14 86.868)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 165.1 124.968) (xy 94.488 123.952) (xy 103.124 86.36) (xy 165.608 86.36)
      )
    )
  )
)
