<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.4.2">
<drawing>
<board>
<plain>
<wire x1="31.8516" y1="0" x2="0" y2="0" width="0" layer="20"/>
<wire x1="0" y1="17.78" x2="0" y2="0" width="0" layer="20"/>
<wire x1="0" y1="17.78" x2="31.8516" y2="17.78" width="0" layer="20"/>
<wire x1="31.8516" y1="17.78" x2="31.8516" y2="0" width="0" layer="20"/>
<text>26</text>
<text>3V3</text>
<text>4</text>
<text>27</text>
<text>14</text>
<text>GND</text>
<text>21</text>
<text>RST</text>
<text>33</text>
<text>22</text>
<text>5</text>
<text>18</text>
<text>25</text>
<text>15</text>
<text>BAT</text>
<text>5V</text>
<text>19</text>
<text>23</text>
<text>GND</text>
<text>32</text>
<text>26</text>
<text>3V3</text>
<text>4</text>
<text>27</text>
<text>14</text>
<text>GND</text>
<text>21</text>
<text>RST</text>
<text>33</text>
<text>22</text>
<text>5</text>
<text>18</text>
<text>25</text>
<text>15</text>
<text>BAT</text>
<text>5V</text>
<text>19</text>
<text>23</text>
<text>GND</text>
<text>32</text>
<text>25</text>
<text>33</text>
<text>26</text>
<text>32</text>
<text>27</text>
<text>21</text>
<text>15</text>
<text>22</text>
<text>14</text>
<text>5</text>
<text>4</text>
<text>18</text>
<text>19</text>
<text>23</text>
<text>LEVEL SHIFTER 2.0</text>
<text>https://github.com/swooby/pcb/tree/master/TinyPICO</text>
<text>GPIO to Input Pin #:</text>
</plain>
<libraries>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="2X04/90">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SN74HCT245">
<packages>
<package name="DB20-M">
</package>
</packages>
</library>
<library name="UnexpectedMaker">
<description>Generated from &lt;b&gt;WattsSegment_Display.sch&lt;/b&gt;&lt;p&gt;
by exp-lbrs.ulp</description>
<packages>
<package name="1X10_NO_SILK">
<description>&lt;h3&gt;Plated Through Hole -10 Pin No Silk&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:10&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_10&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Aesthetics&lt;/h3&gt;
This library contiains non-functional items such as logos, build/ordering notes, frame blocks, etc. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="OSHW-LOGO-S">
<description>&lt;h3&gt;Open-Source Hardware (OSHW) Logo - Small - Silkscreen&lt;/h3&gt;
&lt;p&gt;Silkscreen logo for open-source hardware designs.&lt;/p&gt;
&lt;p&gt;Devices using:
&lt;ul&gt;&lt;li&gt;OSHW_LOGO&lt;/li&gt;&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="C0603">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
<library name="pv">
<packages>
<package name="EXB2HV-M">
</package>
</packages>
</library>
<library name="pv_jump-0r-smd">
<description>Soldering jumper and bridges</description>
<packages>
<package name="C0R-JMP_NONE">
<description>&lt;b&gt;0R Jumper Variant D&lt;/b&gt;&lt;p&gt;
Solder type</description>
</package>
</packages>
</library>
<library name="jumper">
<description>&lt;b&gt;Jumpers&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SJ">
<description>&lt;b&gt;Solder jumper&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="JP1" library="pinhead" package="2X04/90" value="">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="8"/>
<attribute name="VALUE"/>
</element>
<element name="LEFT" library="UnexpectedMaker" package="1X10_NO_SILK" value="">
<attribute name="PROD_ID" value="CONN-11563"/>
<attribute name="VALUE"/>
</element>
<element name="RIGHT" library="UnexpectedMaker" package="1X10_NO_SILK" value="">
<attribute name="PROD_ID" value="CONN-11563"/>
<attribute name="VALUE"/>
</element>
<element name="U4" library="SN74HCT245" package="DB20-M" value="SN74HCT245DBRDB20-M">
<attribute name="MANUFACTURER_PART_NUMBER" value="SN74HCT245DBR"/>
<attribute name="NAME"/>
<attribute name="VENDOR" value="Texas Instruments"/>
</element>
<element name="C2" library="adafruit" package="C0603" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="pv" package="EXB2HV-M" value="EXB-2HV331JVEXB2HV-M">
<attribute name="MANUFACTURER_PART_NUMBER" value="EXB2HV331JV"/>
<attribute name="NAME"/>
<attribute name="VENDOR" value="Panasonic"/>
</element>
<element name="6" library="pv_jump-0r-smd" package="C0R-JMP_NONE" value="0R-JUMPD">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="5" library="pv_jump-0r-smd" package="C0R-JMP_NONE" value="0R-JUMPD">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="4" library="pv_jump-0r-smd" package="C0R-JMP_NONE" value="0R-JUMPD">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="3" library="pv_jump-0r-smd" package="C0R-JMP_NONE" value="0R-JUMPD">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="8" library="jumper" package="SJ" value="">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="33"/>
<attribute name="VALUE"/>
</element>
<element name="7" library="jumper" package="SJ" value="">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="33"/>
<attribute name="VALUE"/>
</element>
<element name="2" library="pv_jump-0r-smd" package="C0R-JMP_NONE" value="0R-JUMPD">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="1" library="pv_jump-0r-smd" package="C0R-JMP_NONE" value="0R-JUMPD">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LOGO" library="SparkFun-Aesthetics" package="OSHW-LOGO-S" value="OSHW-LOGOS"/>
</elements>
<signals>
<signal name="GND">
<contactref element="RIGHT" pad="10"/>
<contactref element="LEFT" pad="2"/>
<contactref element="U4" pad="10"/>
<contactref element="C2" pad="2"/>
<contactref element="U4" pad="19"/>
<contactref element="U4" pad="1"/>
</signal>
<signal name="3V3">
<contactref element="LEFT" pad="4"/>
</signal>
<signal name="RESET">
<contactref element="RIGHT" pad="9"/>
</signal>
<signal name="GPIO32">
<contactref element="RIGHT" pad="7"/>
<contactref element="2" pad="1"/>
</signal>
<signal name="GPIO33">
<contactref element="RIGHT" pad="8"/>
<contactref element="1" pad="1"/>
</signal>
<signal name="GPIO25">
<contactref element="LEFT" pad="10"/>
<contactref element="1" pad="3"/>
</signal>
<signal name="GPIO26">
<contactref element="LEFT" pad="9"/>
<contactref element="2" pad="3"/>
</signal>
<signal name="GPIO27">
<contactref element="LEFT" pad="8"/>
<contactref element="3" pad="3"/>
</signal>
<signal name="GPIO14">
<contactref element="LEFT" pad="6"/>
<contactref element="5" pad="3"/>
</signal>
<signal name="GPIO15">
<contactref element="LEFT" pad="7"/>
<contactref element="4" pad="3"/>
</signal>
<signal name="GPIO4">
<contactref element="LEFT" pad="5"/>
<contactref element="6" pad="3"/>
</signal>
<signal name="GPIO5">
<contactref element="RIGHT" pad="4"/>
<contactref element="5" pad="1"/>
</signal>
<signal name="GPIO18">
<contactref element="RIGHT" pad="3"/>
<contactref element="6" pad="1"/>
</signal>
<signal name="GPIO23">
<contactref element="RIGHT" pad="1"/>
<contactref element="8" pad="2"/>
</signal>
<signal name="GPIO22">
<contactref element="RIGHT" pad="5"/>
<contactref element="4" pad="1"/>
</signal>
<signal name="GPIO19">
<contactref element="RIGHT" pad="2"/>
<contactref element="7" pad="2"/>
</signal>
<signal name="GPIO21">
<contactref element="RIGHT" pad="6"/>
<contactref element="3" pad="1"/>
</signal>
<signal name="VBAT">
<contactref element="LEFT" pad="1"/>
</signal>
<signal name="5V">
<contactref element="LEFT" pad="3"/>
<contactref element="U4" pad="20"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="B1">
<contactref element="U4" pad="18"/>
<contactref element="1" pad="2"/>
</signal>
<signal name="B2">
<contactref element="U4" pad="17"/>
<contactref element="2" pad="2"/>
</signal>
<signal name="B3">
<contactref element="U4" pad="16"/>
<contactref element="3" pad="2"/>
</signal>
<signal name="B4">
<contactref element="U4" pad="15"/>
<contactref element="4" pad="2"/>
</signal>
<signal name="B5">
<contactref element="U4" pad="14"/>
<contactref element="5" pad="2"/>
</signal>
<signal name="B6">
<contactref element="U4" pad="13"/>
<contactref element="6" pad="2"/>
</signal>
<signal name="B7">
<contactref element="U4" pad="12"/>
<contactref element="7" pad="1"/>
</signal>
<signal name="B8">
<contactref element="U4" pad="11"/>
<contactref element="8" pad="1"/>
</signal>
<signal name="A1">
<contactref element="U4" pad="2"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="A2">
<contactref element="U4" pad="3"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="A3">
<contactref element="U4" pad="4"/>
<contactref element="R5" pad="3"/>
</signal>
<signal name="A4">
<contactref element="U4" pad="5"/>
<contactref element="R5" pad="4"/>
</signal>
<signal name="A5">
<contactref element="U4" pad="6"/>
<contactref element="R5" pad="5"/>
</signal>
<signal name="A6">
<contactref element="U4" pad="7"/>
<contactref element="R5" pad="6"/>
</signal>
<signal name="A7">
<contactref element="U4" pad="8"/>
<contactref element="R5" pad="7"/>
</signal>
<signal name="A8">
<contactref element="U4" pad="9"/>
<contactref element="R5" pad="8"/>
</signal>
<signal name="N$1">
<contactref element="JP1" pad="1"/>
<contactref element="R5" pad="16"/>
</signal>
<signal name="N$3">
<contactref element="R5" pad="15"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="R5" pad="14"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="N$2">
<contactref element="R5" pad="13"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="N$5">
<contactref element="R5" pad="12"/>
<contactref element="JP1" pad="5"/>
</signal>
<signal name="N$6">
<contactref element="R5" pad="11"/>
<contactref element="JP1" pad="6"/>
</signal>
<signal name="N$7">
<contactref element="R5" pad="10"/>
<contactref element="JP1" pad="7"/>
</signal>
<signal name="N$8">
<contactref element="R5" pad="9"/>
<contactref element="JP1" pad="8"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
