(kicad_pcb (version 20171130) (host pcbnew "(5.1.4-0-10_14)")
  (general
    (thickness 1.6)
    (drawings 26)
    (tracks 55)
    (zones 0)
    (modules 16)
    (nets 15)
  )
  (page A4)
  (layers
    (0 Top signal)
    (31 Bottom signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.000001)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (grid_origin 138.3411 111.3536)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 /SCL)
  (net 3 /SDA)
  (net 4 /VCC)
  (net 5 "Net-(J1-Pad14)")
  (net 6 /T2)
  (net 7 "Net-(J1-Pad12)")
  (net 8 /T1)
  (net 9 /D7)
  (net 10 /D6)
  (net 11 /D5)
  (net 12 /D4)
  (net 13 /D3)
  (net 14 /D2)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /D2)
    (add_net /D3)
    (add_net /D4)
    (add_net /D5)
    (add_net /D6)
    (add_net /D7)
    (add_net /SCL)
    (add_net /SDA)
    (add_net /T1)
    (add_net /T2)
    (add_net /VCC)
    (add_net GND)
    (add_net "Net-(J1-Pad12)")
    (add_net "Net-(J1-Pad14)")
  )
  (module Connector_PinHeader_1.27mm:PinHeader_2x07_P1.27mm_Vertical (layer Top) (tedit 5D92FD1B)
    (at 152.3111 104.3686 270)
    (descr "Through hole straight pin header, 2x07, 1.27mm pitch, double rows")
    (tags "Through hole pin header THT 2x07 1.27mm double row")
    (fp_text reference J1 (at 0.635 -1.695 270) (layer F.SilkS) hide)
    (fp_text value Conn_02x07_Odd_Even (at 0.635 9.315 270) (layer F.Fab))
    (fp_text user %R (at 0.635 3.81) (layer F.Fab))
    (pad 14 thru_hole oval (at 1.27 7.62 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad14)"))
    (pad 13 thru_hole oval (at 0 7.62 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 6 /T2))
    (pad 12 thru_hole oval (at 1.27 6.35 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad12)"))
    (pad 11 thru_hole oval (at 0 6.35 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 8 /T1))
    (pad 10 thru_hole oval (at 1.27 5.08 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 9 thru_hole oval (at 0 5.08 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 8 thru_hole oval (at 1.27 3.81 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 9 /D7))
    (pad 7 thru_hole oval (at 0 3.81 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 10 /D6))
    (pad 6 thru_hole oval (at 1.27 2.54 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 11 /D5))
    (pad 5 thru_hole oval (at 0 2.54 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 12 /D4))
    (pad 4 thru_hole oval (at 1.27 1.27 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 13 /D3))
    (pad 3 thru_hole oval (at 0 1.27 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 14 /D2))
    (pad 2 thru_hole oval (at 1.27 0 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 3 /SDA))
    (pad 1 thru_hole rect (at 0 0 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 2 /SCL))
    (model ${KISYS3DMOD}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_2x07_P1.27mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module chickadee:chickadee_2mm_fcu (layer Top) (tedit 0)
    (at 145.3261 101.1936)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical (layer Bottom) (tedit 5D92F78E)
    (at 143.4211 98.6536 270)
    (descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.54mm single row")
    (fp_text reference J2 (at 0 2.33 270) (layer B.SilkS) hide)
    (fp_text value Conn_01x05_Male (at 0 -12.49 270) (layer B.Fab))
    (fp_text user %R (at 0 -5.08 180) (layer B.Fab))
    (pad 5 thru_hole oval (at 0 -10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /D2))
    (pad 4 thru_hole oval (at 0 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /D4))
    (pad 3 thru_hole oval (at 0 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /D6))
    (pad 2 thru_hole oval (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /T2))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical (layer Bottom) (tedit 5D92F730)
    (at 143.4211 111.3536 270)
    (descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.54mm single row")
    (fp_text reference J3 (at 0 2.33 270) (layer B.SilkS) hide)
    (fp_text value Conn_01x05_Male (at 0 -12.49 270) (layer B.Fab))
    (fp_text user %R (at 0 -5.08 180) (layer B.Fab))
    (pad 5 thru_hole oval (at 0 -10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /D3))
    (pad 4 thru_hole oval (at 0 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /D5))
    (pad 3 thru_hole oval (at 0 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /D7))
    (pad 2 thru_hole oval (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /T1))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module stemmaqt_shift:MOUNTINGHOLE_2.5_PLATED (layer Top) (tedit 0)
    (at 138.3411 98.6536)
    (fp_text reference U$1 (at 0 0) (layer F.SilkS) hide)
    (fp_text value MOUNTINGHOLE2.5 (at 0 0) (layer F.SilkS) hide)
    (pad P$1 thru_hole circle (at 0 0) (size 3.2 3.2) (drill 2.5) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0508))
  )
  (module stemmaqt_shift:MOUNTINGHOLE_2.5_PLATED (layer Top) (tedit 0)
    (at 158.6611 98.6536)
    (fp_text reference U$17 (at 0 0) (layer F.SilkS) hide)
    (fp_text value MOUNTINGHOLE2.5 (at 0 0) (layer F.SilkS) hide)
    (pad P$1 thru_hole circle (at 0 0) (size 3.2 3.2) (drill 2.5) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0508))
  )
  (module stemmaqt_shift:JST_SH4 (layer Top) (tedit 0)
    (at 158.6611 105.0036 90)
    (fp_text reference CONN3 (at -4.6 -3.614 90) (layer F.SilkS) hide)
    (fp_text value STEMMA_I2C_QT (at 0 0 90) (layer F.SilkS) hide)
    (pad MT2 smd rect (at 2.8 1.386 180) (size 1.8 1.2) (layers Top F.Paste F.Mask)
      (solder_mask_margin 0.0508))
    (pad MT1 smd rect (at -2.8 1.386 180) (size 1.8 1.2) (layers Top F.Paste F.Mask)
      (solder_mask_margin 0.0508))
    (pad 4 smd rect (at 1.5 -2.514 180) (size 1.55 0.6) (layers Top F.Paste F.Mask)
      (net 2 /SCL) (solder_mask_margin 0.0508))
    (pad 1 smd rect (at -1.5 -2.514 180) (size 1.55 0.6) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0508))
    (pad 3 smd rect (at 0.5 -2.514 180) (size 1.55 0.6) (layers Top F.Paste F.Mask)
      (net 3 /SDA) (solder_mask_margin 0.0508))
    (pad 2 smd rect (at -0.5 -2.514 180) (size 1.55 0.6) (layers Top F.Paste F.Mask)
      (net 4 /VCC) (solder_mask_margin 0.0508))
  )
  (module stemmaqt_shift:JST_SH4 (layer Top) (tedit 0)
    (at 138.3411 105.0036 270)
    (fp_text reference CONN4 (at -5.715 -2.54 90) (layer F.SilkS) hide)
    (fp_text value STEMMA_I2C_QT (at 0 0 270) (layer F.SilkS) hide)
    (pad MT2 smd rect (at 2.8 1.386) (size 1.8 1.2) (layers Top F.Paste F.Mask)
      (solder_mask_margin 0.0508))
    (pad MT1 smd rect (at -2.8 1.386) (size 1.8 1.2) (layers Top F.Paste F.Mask)
      (solder_mask_margin 0.0508))
    (pad 4 smd rect (at 1.5 -2.514) (size 1.55 0.6) (layers Top F.Paste F.Mask)
      (net 2 /SCL) (solder_mask_margin 0.0508))
    (pad 1 smd rect (at -1.5 -2.514) (size 1.55 0.6) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0508))
    (pad 3 smd rect (at 0.5 -2.514) (size 1.55 0.6) (layers Top F.Paste F.Mask)
      (net 3 /SDA) (solder_mask_margin 0.0508))
    (pad 2 smd rect (at -0.5 -2.514) (size 1.55 0.6) (layers Top F.Paste F.Mask)
      (net 4 /VCC) (solder_mask_margin 0.0508))
  )
  (module stemmaqt_shift:FIDUCIAL_1MM (layer Top) (tedit 0)
    (at 140.7541 109.3851)
    (fp_text reference FID3 (at 0 0) (layer F.SilkS) hide)
    (fp_text value FIDUCIAL_1MM (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd roundrect (at 0 0) (size 1 1) (layers Top F.Mask) (roundrect_rratio 0.5)
      (solder_mask_margin 0.0508))
  )
  (module stemmaqt_shift:FIDUCIAL_1MM (layer Top) (tedit 0)
    (at 155.2321 97.4725)
    (fp_text reference FID4 (at 0 0) (layer F.SilkS) hide)
    (fp_text value FIDUCIAL_1MM (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd roundrect (at 0 0) (size 1 1) (layers Top F.Mask) (roundrect_rratio 0.5)
      (solder_mask_margin 0.0508))
  )
  (module stemmaqt_shift:MOUNTINGHOLE_2.5_PLATED (layer Top) (tedit 0)
    (at 138.3411 111.3536)
    (fp_text reference U$19 (at 0 0) (layer F.SilkS) hide)
    (fp_text value MOUNTINGHOLE2.5 (at 0 0) (layer F.SilkS) hide)
    (pad P$1 thru_hole circle (at 0 0) (size 3.2 3.2) (drill 2.5) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0508))
  )
  (module stemmaqt_shift:MOUNTINGHOLE_2.5_PLATED (layer Top) (tedit 0)
    (at 158.6611 111.3536)
    (fp_text reference U$21 (at 0 0) (layer F.SilkS) hide)
    (fp_text value MOUNTINGHOLE2.5 (at 0 0) (layer F.SilkS) hide)
    (pad P$1 thru_hole circle (at 0 0) (size 3.2 3.2) (drill 2.5) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0508))
  )
  (module stemmaqt_shift:ADAFRUIT_3.5MM (layer Bottom) (tedit 0)
    (at 153.5811 106.9086 90)
    (fp_text reference U$22 (at 0 0 90) (layer B.SilkS) hide)
    (fp_text value "" (at 0 0 90) (layer B.SilkS) hide)
  )
  (module stemmaqt_shift:PCBFEAT-REV-040 (layer Bottom) (tedit 0)
    (at 142.7861 105.0036 90)
    (descr "<b>Revision Level Field</b> - 40 mil<p>\nSet version with global board attribute '>REV'")
    (fp_text reference U$25 (at 0 0 90) (layer B.SilkS) hide)
    (fp_text value "" (at 0 0 90) (layer B.SilkS) hide)
    (fp_text user >REV (at -0.3556 -0.508 90) (layer B.SilkS) hide)
  )
  (module stemmaqt_shift:STEMMAQT (layer Bottom) (tedit 0)
    (at 158.2801 109.4486 90)
    (fp_text reference U$30 (at 0 0 90) (layer B.SilkS) hide)
    (fp_text value "" (at 0 0 90) (layer B.SilkS) hide)
  )
  (module stemmaqt_shift:STEMMAQT (layer Bottom) (tedit 0)
    (at 138.7221 100.5586 270)
    (fp_text reference U$31 (at 0 0 270) (layer B.SilkS) hide)
    (fp_text value "" (at 0 0 270) (layer B.SilkS) hide)
  )
  (gr_text D1-SDA (at 152.9461 108.8136) (layer F.SilkS))
  (gr_text D0-SCL (at 152.9461 101.1936) (layer F.SilkS))
  (gr_text A (at 142.7861 105.0036) (layer B.SilkS))
  (gr_text D2 (at 153.5811 96.8756) (layer F.SilkS))
  (gr_text D4 (at 151.0411 96.8756) (layer F.SilkS))
  (gr_text D6 (at 148.5011 96.8756) (layer F.SilkS))
  (gr_text T2 (at 145.9611 96.8756) (layer F.SilkS))
  (gr_text GND (at 142.7861 96.8756) (layer F.SilkS))
  (gr_text GND (at 142.7861 113.1951) (layer F.SilkS))
  (gr_text D3 (at 153.5811 113.1951) (layer F.SilkS))
  (gr_text D5 (at 151.0411 113.1951) (layer F.SilkS))
  (gr_text D7 (at 148.5011 113.1951) (layer F.SilkS))
  (gr_text T1 (at 145.9611 113.1951) (layer F.SilkS))
  (gr_line (start 135.8011 98.6536) (end 135.8011 111.3536) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 138.3411 111.3536) (end 135.8011 111.3536) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 138.3411 113.8936) (end 158.6611 113.8936) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 158.6611 111.3536) (end 158.6611 113.8936) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 161.2011 111.3536) (end 161.2011 98.6536) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 158.6611 98.6536) (end 161.2011 98.6536) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 158.6611 96.1136) (end 138.3411 96.1136) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 138.3411 98.6536) (end 138.3411 96.1136) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_text "Stemma BitMagic" (at 148.5011 101.8286) (layer B.SilkS))
  (gr_text "Debug Stemma w/BitMagic" (at 148.5011 108.1786) (layer B.SilkS))
  (zone (net 1) (net_name GND) (layer Bottom) (hatch edge 0.508)
    (priority 6)
    (connect_pads (clearance 0.000001))
    (min_thickness 0.127)
    (fill (arc_segments 32) (thermal_gap 0.304) (thermal_bridge_width 0.304))
    (polygon
      (pts
        (xy 161.3281 114.0206) (xy 135.6741 114.0206) (xy 135.6741 95.9866) (xy 161.3281 95.9866)
      )
    )
  )
)
