(kicad_pcb (version 4) (host pcbnew 4.0.4-stable)
  (general
    (links 58)
    (no_connects 6)
    (area 79.650001 53.1 174.85 127.070001)
    (thickness 1.6)
    (drawings 55)
    (tracks 241)
    (zones 0)
    (modules 28)
    (nets 39)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 0.15)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2 2.6)
    (pad_drill 1.2)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 155 65)
    (visible_elements 7FFFF7FF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +3V3)
  (net 2 GND)
  (net 3 +5V)
  (net 4 /GPIO2)
  (net 5 /GPIO3)
  (net 6 /GPIO4)
  (net 7 /GPIO14)
  (net 8 /GPIO15)
  (net 9 /GPIO17)
  (net 10 /GPIO18)
  (net 11 /GPIO27)
  (net 12 /GPIO22)
  (net 13 /GPIO23)
  (net 14 /GPIO24)
  (net 15 /GPIO10)
  (net 16 /GPIO9)
  (net 17 /GPIO25)
  (net 18 /GPIO11)
  (net 19 /GPIO8)
  (net 20 /GPIO7)
  (net 21 /ID_SD)
  (net 22 /ID_SC)
  (net 23 /GPIO5)
  (net 24 /GPIO6)
  (net 25 /GPIO12)
  (net 26 /GPIO13)
  (net 27 /GPIO19)
  (net 28 /GPIO16)
  (net 29 /GPIO26)
  (net 30 /GPIO20)
  (net 31 /GPIO21)
  (net 32 "Net-(ID_EEPROM1-Pad7)")
  (net 33 "Net-(temp1-Pad3)")
  (net 34 "Net-(temp1-Pad5)")
  (net 35 "Net-(temp1-Pad6)")
  (net 36 "Net-(temp1-Pad7)")
  (net 37 "Net-(C2-Pad1)")
  (net 38 "Net-(P4-PadDOUT)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +5V)
    (add_net /GPIO10)
    (add_net /GPIO11)
    (add_net /GPIO12)
    (add_net /GPIO13)
    (add_net /GPIO14)
    (add_net /GPIO15)
    (add_net /GPIO16)
    (add_net /GPIO17)
    (add_net /GPIO18)
    (add_net /GPIO19)
    (add_net /GPIO2)
    (add_net /GPIO20)
    (add_net /GPIO21)
    (add_net /GPIO22)
    (add_net /GPIO23)
    (add_net /GPIO24)
    (add_net /GPIO25)
    (add_net /GPIO26)
    (add_net /GPIO27)
    (add_net /GPIO3)
    (add_net /GPIO4)
    (add_net /GPIO5)
    (add_net /GPIO6)
    (add_net /GPIO7)
    (add_net /GPIO8)
    (add_net /GPIO9)
    (add_net /ID_SC)
    (add_net /ID_SD)
    (add_net GND)
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(ID_EEPROM1-Pad7)")
    (add_net "Net-(P4-PadDOUT)")
    (add_net "Net-(temp1-Pad3)")
    (add_net "Net-(temp1-Pad5)")
    (add_net "Net-(temp1-Pad6)")
    (add_net "Net-(temp1-Pad7)")
  )
  (module .pretty:Schottky_Diode (layer F.Cu) (tedit 58E47028)
    (at 108.6 80.7 90)
    (descr "Diode, Universal, SMA, SMB, Handsoldering,")
    (tags "Diode Universal SMA SMB Handsoldering ")
    (attr smd)
    (fp_text reference DIODE (at 0 -3 90) (layer F.SilkS))
    (fp_text value D_Schottky (at 0 3 90) (layer F.Fab))
    (pad 2 smd rect (at 2 0 90) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 1 smd rect (at -2 0 90) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(C2-Pad1)"))
    (model Diodes_SMD.3dshapes/D_SMA-SMB_Universal_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 180))
    )
  )
  (module .pretty:Neo_RGB_LED (layer F.Cu) (tedit 58E4124E)
    (at 111.82 73.29)
    (descr http://www.cree.com/~/media/Files/Cree/LED-Components-and-Modules/HB/Data-Sheets/CLMVBFKA.pdf)
    (tags "LED Cree PLCC-4")
    (attr smd)
    (fp_text reference NEO (at 0 -3.5) (layer F.SilkS))
    (fp_text value Neo_LED_RGB_IC (at 0 4) (layer F.Fab))
    (pad VDD smd rect (at 2.5 1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(C2-Pad1)"))
    (pad DOUT smd rect (at 2.5 -1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(P4-PadDOUT)"))
    (pad DIN smd rect (at -2.5 1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 10 /GPIO18))
    (pad VSS smd rect (at -2.5 -1.6) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_Cree-PLCC4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 58E4128A)
    (at 99 102.2)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference TEMP (at 0.02 3.45) (layer F.SilkS))
    (fp_text value LM75BD (at 0 3.5) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 /GPIO2))
    (pad 2 smd rect (at -2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 /GPIO3))
    (pad 3 smd rect (at -2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(temp1-Pad3)"))
    (pad 4 smd rect (at -2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at 2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(temp1-Pad5)"))
    (pad 6 smd rect (at 2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(temp1-Pad6)"))
    (pad 7 smd rect (at 2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(temp1-Pad7)"))
    (pad 8 smd rect (at 2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (model Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 58E40BC4)
    (at 135 79.7 90)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference EEPROM (at 0 -3.5 90) (layer F.SilkS))
    (fp_text value CAT24C32 (at 0 3.5 90) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -1.905 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -2.7 -0.635 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -2.7 0.635 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at -2.7 1.905 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at 2.7 1.905 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 21 /ID_SD))
    (pad 6 smd rect (at 2.7 0.635 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 22 /ID_SC))
    (pad 7 smd rect (at 2.7 -0.635 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(ID_EEPROM1-Pad7)"))
    (pad 8 smd rect (at 2.7 -1.905 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (model Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x20_Pitch2.54mm (layer F.Cu) (tedit 58EC6440)
    (at 101.98 66.44 90)
    (descr "Through hole straight pin header, 2x20, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x20 2.54mm double row")
    (fp_text reference PiHEADER (at -2.46 23.64 180) (layer F.SilkS))
    (fp_text value CONN_02X20 (at -2.46 14.21 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /GPIO2))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /GPIO3))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /GPIO4))
    (pad 8 thru_hole oval (at 2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /GPIO14))
    (pad 9 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 10 thru_hole oval (at 2.54 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /GPIO15))
    (pad 11 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /GPIO17))
    (pad 12 thru_hole oval (at 2.54 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /GPIO18))
    (pad 13 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /GPIO27))
    (pad 14 thru_hole oval (at 2.54 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 15 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /GPIO22))
    (pad 16 thru_hole oval (at 2.54 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /GPIO23))
    (pad 17 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (pad 18 thru_hole oval (at 2.54 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /GPIO24))
    (pad 19 thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /GPIO10))
    (pad 20 thru_hole oval (at 2.54 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 21 thru_hole oval (at 0 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /GPIO9))
    (pad 22 thru_hole oval (at 2.54 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /GPIO25))
    (pad 23 thru_hole oval (at 0 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /GPIO11))
    (pad 24 thru_hole oval (at 2.54 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /GPIO8))
    (pad 25 thru_hole oval (at 0 30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 26 thru_hole oval (at 2.54 30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 /GPIO7))
    (pad 27 thru_hole oval (at 0 33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /ID_SD))
    (pad 28 thru_hole oval (at 2.54 33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 /ID_SC))
    (pad 29 thru_hole oval (at 0 35.56 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 /GPIO5))
    (pad 30 thru_hole oval (at 2.54 35.56 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 31 thru_hole oval (at 0 38.1 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 /GPIO6))
    (pad 32 thru_hole oval (at 2.54 38.1 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 /GPIO12))
    (pad 33 thru_hole oval (at 0 40.64 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 /GPIO13))
    (pad 34 thru_hole oval (at 2.54 40.64 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 35 thru_hole oval (at 0 43.18 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 /GPIO19))
    (pad 36 thru_hole oval (at 2.54 43.18 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 /GPIO16))
    (pad 37 thru_hole oval (at 0 45.72 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 /GPIO26))
    (pad 38 thru_hole oval (at 2.54 45.72 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 /GPIO20))
    (pad 39 thru_hole oval (at 0 48.26 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 40 thru_hole oval (at 2.54 48.26 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 /GPIO21))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20_Pitch2.54mm.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58E470D1)
    (at 131.5 72.4 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference 100nF (at -3.05 0.21 540) (layer F.SilkS))
    (fp_text value 100n (at 2.9 -0.1 360) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 58E4136D)
    (at 128 75.6 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference SHUNT (at 2.69 1.19 270) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0 4.93 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 "Net-(ID_EEPROM1-Pad7)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Measurement_Points:Test_Point_2Pads (layer F.Cu) (tedit 58E41366)
    (at 128 81.6 90)
    (descr "Connecteurs 2 pins")
    (tags "CONN DEV")
    (attr virtual)
    (fp_text reference TEST (at 1.27 -2 90) (layer F.SilkS))
    (fp_text value horizTest (at 1.27 2 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.8128) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.4 1.4) (drill 0.8128) (layers *.Cu *.Mask)
      (net 32 "Net-(ID_EEPROM1-Pad7)"))
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E4712F)
    (at 133.6 72.4 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference 1K (at -3.05 -0.04 360) (layer F.SilkS))
    (fp_text value 1K (at 2.89 -0.05 360) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(ID_EEPROM1-Pad7)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E470FE)
    (at 135.7 72.4 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference 3.9K (at -3.05 -0.1 360) (layer F.SilkS))
    (fp_text value 3.9K (at 2.89 0.02 360) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 22 /ID_SC))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E4711D)
    (at 137.8 72.4 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference 3.9K (at -3.05 -0.22 360) (layer F.SilkS))
    (fp_text value 3.9K (at 2.89 -0.1 360) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 21 /ID_SD))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Molex:Molex_KK-6410-02_02x2.54mm_Straight (layer F.Cu) (tedit 58E46F31)
    (at 101 75.2 180)
    (descr "Connector Headers with Friction Lock, 22-27-2021, http://www.molex.com/pdm_docs/sd/022272021_sd.pdf")
    (tags "connector molex kk_6410 22-27-2021")
    (fp_text reference "GPIO14 +" (at 1.2 -4.51 180) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 1.27 4.5 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0.2 180) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 7 /GPIO14))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module Connectors_Molex:Molex_KK-6410-02_02x2.54mm_Straight (layer F.Cu) (tedit 58E46F1F)
    (at 108 112 180)
    (descr "Connector Headers with Friction Lock, 22-27-2021, http://www.molex.com/pdm_docs/sd/022272021_sd.pdf")
    (tags "connector molex kk_6410 22-27-2021")
    (fp_text reference "GPIO4 +" (at 1.24 4.44 180) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 1.27 4.5 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 6 /GPIO4))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module Connectors_Molex:Molex_KK-6410-02_02x2.54mm_Straight (layer F.Cu) (tedit 58E46F10)
    (at 134 112 180)
    (descr "Connector Headers with Friction Lock, 22-27-2021, http://www.molex.com/pdm_docs/sd/022272021_sd.pdf")
    (tags "connector molex kk_6410 22-27-2021")
    (fp_text reference "GPIO20 +" (at 1.26 4.49 180) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 1.27 4.5 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 30 /GPIO20))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module Connectors_Molex:Molex_KK-6410-02_02x2.54mm_Straight (layer F.Cu) (tedit 58E46EEE)
    (at 155 103 180)
    (descr "Connector Headers with Friction Lock, 22-27-2021, http://www.molex.com/pdm_docs/sd/022272021_sd.pdf")
    (tags "connector molex kk_6410 22-27-2021")
    (fp_text reference "GPIO21 +" (at 1.34 -4.52 180) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 1.27 4.5 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 31 /GPIO21))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module Pin_Headers:Pin_Header_Straight_1x08_Pitch2.54mm (layer F.Cu) (tedit 58E41315)
    (at 118 80.7)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (fp_text reference KEY (at -2.69 8.8 90) (layer F.SilkS))
    (fp_text value CONN_01X08 (at 0 20.17) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /GPIO27))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /GPIO23))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /GPIO22))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /GPIO24))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /GPIO10))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /GPIO25))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /GPIO9))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /GPIO8))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x08_Pitch2.54mm.wrl
      (at (xyz 0 -0.35 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module .pretty:PKM13EPYH (layer F.Cu) (tedit 58DBEF8A)
    (at 118.9 109 180)
    (fp_text reference PIEZO (at 0 -2.5 180) (layer F.SilkS))
    (fp_text value Piezo (at 0 3 180) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 2.5 2.5) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at -2.5 0 180) (size 2.5 2.5) (drill 1) (layers *.Cu *.Mask)
      (net 9 /GPIO17))
  )
  (module .pretty:raspiMountingHole (layer F.Cu) (tedit 58890667)
    (at 97 65)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value "Mounting Hole" (at 0 3) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 2.75 2.75) (drill 2.75) (layers *.Cu *.Mask)
      (clearance 3.1))
  )
  (module .pretty:raspiMountingHole (layer F.Cu) (tedit 58890667)
    (at 97 114)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value "Mounting Hole" (at 0 3) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 2.75 2.75) (drill 2.75) (layers *.Cu *.Mask)
      (clearance 3.1))
  )
  (module .pretty:raspiMountingHole (layer F.Cu) (tedit 58890667)
    (at 155 114)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value "Mounting Hole" (at 0 3) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 2.75 2.75) (drill 2.75) (layers *.Cu *.Mask)
      (clearance 3.1))
  )
  (module .pretty:raspiMountingHole (layer F.Cu) (tedit 58890667)
    (at 155 65)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value "Mounting Hole" (at 0 3) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 2.75 2.75) (drill 2.75) (layers *.Cu *.Mask)
      (clearance 3.1))
  )
  (module Connectors_Molex:Molex_KK-6410-02_02x2.54mm_Straight (layer F.Cu) (tedit 58E46EC9)
    (at 154.5 75 180)
    (descr "Connector Headers with Friction Lock, 22-27-2021, http://www.molex.com/pdm_docs/sd/022272021_sd.pdf")
    (tags "connector molex kk_6410 22-27-2021")
    (fp_text reference "GPIO26 +" (at 1.2 -4.49 180) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 1.27 4.5 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 29 /GPIO26))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58DBEFF2)
    (at 113.2 78.3)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference 100nF (at -0.04 2.05) (layer F.SilkS))
    (fp_text value 100n (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module oshw-logo-kicad-copper-10mm:OSHW_COPPER_10MM (layer F.Cu) (tedit 4F4F92AA)
    (at 110.4 94.5 270)
    (fp_text reference OSHW_COPPER_10MM (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value VAL** (at 0 0 270) (layer F.SilkS) hide)
    (pad "" smd trapezoid (at 0 -4.1656 90) (size 1.45796 1.4986) (rect_delta 0 -0.2794 ) (layers F.Cu F.Paste F.Mask))
    (pad "" smd trapezoid (at 2.94386 -2.94386 45) (size 1.45796 1.4986) (rect_delta 0 -0.2794 ) (layers F.Cu F.Paste F.Mask))
    (pad "" smd trapezoid (at 4.1656 0) (size 1.45796 1.4986) (rect_delta 0 -0.2794 ) (layers F.Cu F.Paste F.Mask))
    (pad "" smd trapezoid (at 2.94386 2.94386 315) (size 1.45796 1.4986) (rect_delta 0 -0.2794 ) (layers F.Cu F.Paste F.Mask))
    (pad "" smd trapezoid (at -2.94386 -2.94386 135) (size 1.45796 1.4986) (rect_delta 0 -0.2794 ) (layers F.Cu F.Paste F.Mask))
    (pad "" smd trapezoid (at -4.1656 0 180) (size 1.45796 1.4986) (rect_delta 0 -0.2794 ) (layers F.Cu F.Paste F.Mask))
    (pad "" smd trapezoid (at -2.94386 2.94386 225) (size 1.45796 1.4986) (rect_delta 0 -0.2794 ) (layers F.Cu F.Paste F.Mask))
    (pad "" smd trapezoid (at 0 -2.39522 90) (size 1.08204 2.29108) (rect_delta 0 0.41402 ) (layers F.Cu F.Paste F.Mask))
    (pad "" smd trapezoid (at -0.9144 -2.21234 112.5) (size 1.08204 2.29108) (rect_delta 0 0.41402 ) (layers F.Cu F.Paste F.Mask))
    (pad "" smd trapezoid (at 0.9144 -2.21234 67.5) (size 1.08204 2.29108) (rect_delta 0 0.41402 ) (layers F.Cu F.Paste F.Mask))
    (pad "" smd trapezoid (at 1.69164 -1.69164 45) (size 1.08204 2.29108) (rect_delta 0 0.41402 ) (layers F.Cu F.Paste F.Mask))
    (pad "" smd trapezoid (at -1.69164 -1.69164 135) (size 1.08204 2.29108) (rect_delta 0 0.41402 ) (layers F.Cu F.Paste F.Mask))
    (pad "" smd trapezoid (at 2.21234 -0.9144 22.5) (size 1.08204 2.29108) (rect_delta 0 0.41402 ) (layers F.Cu F.Paste F.Mask))
    (pad "" smd trapezoid (at -2.21234 -0.9144 157.5) (size 1.08204 2.29108) (rect_delta 0 0.41402 ) (layers F.Cu F.Paste F.Mask))
    (pad "" smd trapezoid (at 2.39522 0) (size 1.08204 2.29108) (rect_delta 0 0.41402 ) (layers F.Cu F.Paste F.Mask))
    (pad "" smd trapezoid (at -2.39522 0 180) (size 1.08204 2.29108) (rect_delta 0 0.41402 ) (layers F.Cu F.Paste F.Mask))
    (pad "" smd trapezoid (at -2.21234 0.9144 202.5) (size 1.08204 2.29108) (rect_delta 0 0.41402 ) (layers F.Cu F.Paste F.Mask))
    (pad "" smd trapezoid (at 2.21234 0.9144 337.5) (size 1.08204 2.29108) (rect_delta 0 0.41402 ) (layers F.Cu F.Paste F.Mask))
    (pad "" smd trapezoid (at 1.69164 1.69164 315) (size 1.08204 2.29108) (rect_delta 0 0.41402 ) (layers F.Cu F.Paste F.Mask))
    (pad "" smd trapezoid (at -1.69164 1.69164 225) (size 1.08204 2.29108) (rect_delta 0 0.41402 ) (layers F.Cu F.Paste F.Mask))
    (pad "" smd trapezoid (at -1.32842 1.99136 236.3) (size 0.54102 2.29108) (rect_delta 0 0.20828 ) (layers F.Cu F.Paste F.Mask))
    (pad "" smd trapezoid (at 1.32842 1.99136 303.7) (size 0.54102 2.29108) (rect_delta 0 0.20828 ) (layers F.Cu F.Paste F.Mask))
  )
  (module .pretty:makerspace_4,8mm (layer F.Cu) (tedit 0)
    (at 146.3 107.2 270)
    (fp_text reference G*** (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 270) (layer F.SilkS) hide)
  )
  (module .pretty:ci_wide_6mm (layer B.Cu) (tedit 0)
    (at 145.4 106.4 90)
    (fp_text reference G*** (at 0 0 90) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 90) (layer B.SilkS) hide)
  )
  (module .pretty:tiger_paw_10mm (layer F.Cu) (tedit 0)
    (at 126 89.5 270)
    (fp_text reference G*** (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 270) (layer F.SilkS) hide)
  )
  (module .pretty:tiger_paw_10mm (layer B.Cu) (tedit 0)
    (at 126 89.5 90)
    (fp_text reference G*** (at 0 0 90) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 90) (layer B.SilkS) hide)
  )
  (gr_text "CATS HAT V0.2.1" (at 141.97 107.04 270) (layer F.SilkS))
  (gr_text "Stefan Abare\nGiandre Acosta\nMaurice Barnett\nThor Brockman\nBrice Grooms\nBrad Hord\nJoshua McMillan\nOwen Phillips\nGarrett Ross" (at 144.46 95.83 270) (layer B.SilkS))
  (dimension 18 (width 0.3) (layer Dwgs.User)
    (gr_text "18.000 mm" (at 149 125.71) (layer Dwgs.User))
    (feature1 (pts (xy 158 117) (xy 158 127.06)))
    (feature2 (pts (xy 140 117) (xy 140 127.06)))
    (crossbar (pts (xy 140 124.36) (xy 158 124.36)))
    (arrow1a (pts (xy 158 124.36) (xy 156.873496 124.946421)))
    (arrow1b (pts (xy 158 124.36) (xy 156.873496 123.773579)))
    (arrow2a (pts (xy 140 124.36) (xy 141.126504 124.946421)))
    (arrow2b (pts (xy 140 124.36) (xy 141.126504 123.773579)))
  )
  (dimension 2 (width 0.3) (layer Dwgs.User)
    (gr_text "2.000 mm" (at 139 93.39) (layer Dwgs.User))
    (feature1 (pts (xy 140 97) (xy 140 92.04)))
    (feature2 (pts (xy 138 97) (xy 138 92.04)))
    (crossbar (pts (xy 138 94.74) (xy 140 94.74)))
    (arrow1a (pts (xy 140 94.74) (xy 138.873496 95.326421)))
    (arrow1b (pts (xy 140 94.74) (xy 138.873496 94.153579)))
    (arrow2a (pts (xy 138 94.74) (xy 139.126504 95.326421)))
    (arrow2b (pts (xy 138 94.74) (xy 139.126504 94.153579)))
  )
  (dimension 44 (width 0.3) (layer Dwgs.User)
    (gr_text "44.000 mm" (at 116 125.72) (layer Dwgs.User))
    (feature1 (pts (xy 138 117) (xy 138 127.07)))
    (feature2 (pts (xy 94 117) (xy 94 127.07)))
    (crossbar (pts (xy 94 124.37) (xy 138 124.37)))
    (arrow1a (pts (xy 138 124.37) (xy 136.873496 124.956421)))
    (arrow1b (pts (xy 138 124.37) (xy 136.873496 123.783579)))
    (arrow2a (pts (xy 94 124.37) (xy 95.126504 124.956421)))
    (arrow2b (pts (xy 94 124.37) (xy 95.126504 123.783579)))
  )
  (dimension 24 (width 0.3) (layer Dwgs.User)
    (gr_text "24.000 mm" (at 106 94.95) (layer Dwgs.User))
    (feature1 (pts (xy 118 91.3) (xy 118 96.3)))
    (feature2 (pts (xy 94 91.3) (xy 94 96.3)))
    (crossbar (pts (xy 94 93.6) (xy 118 93.6)))
    (arrow1a (pts (xy 118 93.6) (xy 116.873496 94.186421)))
    (arrow1b (pts (xy 118 93.6) (xy 116.873496 93.013579)))
    (arrow2a (pts (xy 94 93.6) (xy 95.126504 94.186421)))
    (arrow2b (pts (xy 94 93.6) (xy 95.126504 93.013579)))
  )
  (dimension 55 (width 0.3) (layer Dwgs.User)
    (gr_text "55.000 mm" (at 168.35 89.5 270) (layer Dwgs.User))
    (feature1 (pts (xy 157.6 117) (xy 169.7 117)))
    (feature2 (pts (xy 157.6 62) (xy 169.7 62)))
    (crossbar (pts (xy 167 62) (xy 167 117)))
    (arrow1a (pts (xy 167 117) (xy 166.413579 115.873496)))
    (arrow1b (pts (xy 167 117) (xy 167.586421 115.873496)))
    (arrow2a (pts (xy 167 62) (xy 166.413579 63.126504)))
    (arrow2b (pts (xy 167 62) (xy 167.586421 63.126504)))
  )
  (target plus (at 126 89.5) (size 5) (width 0.15) (layer Edge.Cuts))
  (gr_line (start 136.5 117) (end 97 117) (angle 90) (layer Edge.Cuts) (width 0.15))
  (dimension 29 (width 0.3) (layer Dwgs.User)
    (gr_text "29.000 mm" (at 111.5 74.35) (layer Dwgs.User))
    (feature1 (pts (xy 126 65) (xy 126 75.7)))
    (feature2 (pts (xy 97 65) (xy 97 75.7)))
    (crossbar (pts (xy 97 73) (xy 126 73)))
    (arrow1a (pts (xy 126 73) (xy 124.873496 73.586421)))
    (arrow1b (pts (xy 126 73) (xy 124.873496 72.413579)))
    (arrow2a (pts (xy 97 73) (xy 98.126504 73.586421)))
    (arrow2b (pts (xy 97 73) (xy 98.126504 72.413579)))
  )
  (gr_line (start 141.5 117) (end 155 117) (angle 90) (layer Edge.Cuts) (width 0.15))
  (dimension 6.4 (width 0.3) (layer Dwgs.User)
    (gr_text "6.400 mm" (at 155 54.45) (layer Dwgs.User))
    (feature1 (pts (xy 158.2 65) (xy 158.2 53.1)))
    (feature2 (pts (xy 151.8 65) (xy 151.8 53.1)))
    (crossbar (pts (xy 151.8 55.8) (xy 158.2 55.8)))
    (arrow1a (pts (xy 158.2 55.8) (xy 157.073496 56.386421)))
    (arrow1b (pts (xy 158.2 55.8) (xy 157.073496 55.213579)))
    (arrow2a (pts (xy 151.8 55.8) (xy 152.926504 56.386421)))
    (arrow2b (pts (xy 151.8 55.8) (xy 152.926504 55.213579)))
  )
  (dimension 2.74 (width 0.3) (layer Dwgs.User)
    (gr_text "2.740 mm" (at 151.33 65 90) (layer Dwgs.User))
    (feature1 (pts (xy 155 63.63) (xy 149.98 63.63)))
    (feature2 (pts (xy 155 66.37) (xy 149.98 66.37)))
    (crossbar (pts (xy 152.68 66.37) (xy 152.68 63.63)))
    (arrow1a (pts (xy 152.68 63.63) (xy 153.266421 64.756504)))
    (arrow1b (pts (xy 152.68 63.63) (xy 152.093579 64.756504)))
    (arrow2a (pts (xy 152.68 66.37) (xy 153.266421 65.243496)))
    (arrow2b (pts (xy 152.68 66.37) (xy 152.093579 65.243496)))
  )
  (gr_line (start 138 98) (end 138 115.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 140 115.5) (end 140 98) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 140 98) (end 140 115.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 141.5 115.5) (end 141.5 117) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 136.5 115.5) (end 138 115.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 139 98) (end 138 98) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 139 98) (end 139 97) (angle 90) (layer Edge.Cuts) (width 0.15))
  (dimension 17 (width 0.3) (layer Dwgs.User)
    (gr_text "17.000 mm" (at 151.35 105.5 270) (layer Dwgs.User))
    (feature1 (pts (xy 142.5 114) (xy 152.7 114)))
    (feature2 (pts (xy 142.5 97) (xy 152.7 97)))
    (crossbar (pts (xy 150 97) (xy 150 114)))
    (arrow1a (pts (xy 150 114) (xy 149.413579 112.873496)))
    (arrow1b (pts (xy 150 114) (xy 150.586421 112.873496)))
    (arrow2a (pts (xy 150 97) (xy 149.413579 98.126504)))
    (arrow2b (pts (xy 150 97) (xy 150.586421 98.126504)))
  )
  (dimension 11.5 (width 0.3) (layer Dwgs.User)
    (gr_text "11.500 mm" (at 129.15 111.25 90) (layer Dwgs.User))
    (feature1 (pts (xy 135.5 105.5) (xy 127.8 105.5)))
    (feature2 (pts (xy 135.5 117) (xy 127.8 117)))
    (crossbar (pts (xy 130.5 117) (xy 130.5 105.5)))
    (arrow1a (pts (xy 130.5 105.5) (xy 131.086421 106.626504)))
    (arrow1b (pts (xy 130.5 105.5) (xy 129.913579 106.626504)))
    (arrow2a (pts (xy 130.5 117) (xy 131.086421 115.873496)))
    (arrow2b (pts (xy 130.5 117) (xy 129.913579 115.873496)))
  )
  (gr_line (start 98 97.5) (end 95 97.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 99 82.5) (end 99 96.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 98 81.5) (end 95 81.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 98 82.5) (end 98 81.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 98 96.5) (end 99 96.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 94 65) (end 94 80.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 94 98.5) (end 94 114) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 95 98.5) (end 94 98.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 95 80.5) (end 95 81.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (dimension 5 (width 0.3) (layer Dwgs.User)
    (gr_text "5.000 mm" (at 96.5 100.85) (layer Dwgs.User))
    (feature1 (pts (xy 99 97.5) (xy 99 102.2)))
    (feature2 (pts (xy 94 97.5) (xy 94 102.2)))
    (crossbar (pts (xy 94 99.5) (xy 99 99.5)))
    (arrow1a (pts (xy 99 99.5) (xy 97.873496 100.086421)))
    (arrow1b (pts (xy 99 99.5) (xy 97.873496 98.913579)))
    (arrow2a (pts (xy 94 99.5) (xy 95.126504 100.086421)))
    (arrow2b (pts (xy 94 99.5) (xy 95.126504 98.913579)))
  )
  (dimension 5 (width 0.3) (layer Dwgs.User)
    (gr_text "5.000 mm" (at 96.5 77.150001) (layer Dwgs.User))
    (feature1 (pts (xy 99 81.5) (xy 99 75.800001)))
    (feature2 (pts (xy 94 81.5) (xy 94 75.800001)))
    (crossbar (pts (xy 94 78.500001) (xy 99 78.500001)))
    (arrow1a (pts (xy 99 78.500001) (xy 97.873496 79.086422)))
    (arrow1b (pts (xy 99 78.500001) (xy 97.873496 77.91358)))
    (arrow2a (pts (xy 94 78.500001) (xy 95.126504 79.086422)))
    (arrow2b (pts (xy 94 78.500001) (xy 95.126504 77.91358)))
  )
  (dimension 19.5 (width 0.3) (layer Dwgs.User)
    (gr_text "19.500 mm" (at 86.15 71.75 270) (layer Dwgs.User))
    (feature1 (pts (xy 97 81.5) (xy 84.8 81.5)))
    (feature2 (pts (xy 97 62) (xy 84.8 62)))
    (crossbar (pts (xy 87.5 62) (xy 87.5 81.5)))
    (arrow1a (pts (xy 87.5 81.5) (xy 86.913579 80.373496)))
    (arrow1b (pts (xy 87.5 81.5) (xy 88.086421 80.373496)))
    (arrow2a (pts (xy 87.5 62) (xy 86.913579 63.126504)))
    (arrow2b (pts (xy 87.5 62) (xy 88.086421 63.126504)))
  )
  (dimension 19.5 (width 0.3) (layer Dwgs.User)
    (gr_text "19.500 mm" (at 86.15 107.25 90) (layer Dwgs.User))
    (feature1 (pts (xy 97 97.5) (xy 84.8 97.5)))
    (feature2 (pts (xy 97 117) (xy 84.8 117)))
    (crossbar (pts (xy 87.5 117) (xy 87.5 97.5)))
    (arrow1a (pts (xy 87.5 97.5) (xy 88.086421 98.626504)))
    (arrow1b (pts (xy 87.5 97.5) (xy 86.913579 98.626504)))
    (arrow2a (pts (xy 87.5 117) (xy 88.086421 115.873496)))
    (arrow2b (pts (xy 87.5 117) (xy 86.913579 115.873496)))
  )
  (dimension 58 (width 0.3) (layer Dwgs.User)
    (gr_text "58.000 mm" (at 126 122.35) (layer Dwgs.User))
    (feature1 (pts (xy 155 117) (xy 155 123.7)))
    (feature2 (pts (xy 97 117) (xy 97 123.7)))
    (crossbar (pts (xy 97 121) (xy 155 121)))
    (arrow1a (pts (xy 155 121) (xy 153.873496 121.586421)))
    (arrow1b (pts (xy 155 121) (xy 153.873496 120.413579)))
    (arrow2a (pts (xy 97 121) (xy 98.126504 121.586421)))
    (arrow2b (pts (xy 97 121) (xy 98.126504 120.413579)))
  )
  (dimension 49 (width 0.3) (layer Dwgs.User)
    (gr_text "49.000 mm" (at 162.35 89.5 270) (layer Dwgs.User))
    (feature1 (pts (xy 158 114) (xy 163.7 114)))
    (feature2 (pts (xy 158 65) (xy 163.7 65)))
    (crossbar (pts (xy 161 65) (xy 161 114)))
    (arrow1a (pts (xy 161 114) (xy 160.413579 112.873496)))
    (arrow1b (pts (xy 161 114) (xy 161.586421 112.873496)))
    (arrow2a (pts (xy 161 65) (xy 160.413579 66.126504)))
    (arrow2b (pts (xy 161 65) (xy 161.586421 66.126504)))
  )
  (dimension 58 (width 0.3) (layer Dwgs.User)
    (gr_text "58.000 mm" (at 126 58.65) (layer Dwgs.User))
    (feature1 (pts (xy 155 62) (xy 155 57.3)))
    (feature2 (pts (xy 97 62) (xy 97 57.3)))
    (crossbar (pts (xy 97 60) (xy 155 60)))
    (arrow1a (pts (xy 155 60) (xy 153.873496 60.586421)))
    (arrow1b (pts (xy 155 60) (xy 153.873496 59.413579)))
    (arrow2a (pts (xy 97 60) (xy 98.126504 60.586421)))
    (arrow2b (pts (xy 97 60) (xy 98.126504 59.413579)))
  )
  (dimension 49 (width 0.3) (layer Dwgs.User)
    (gr_text "49.000 mm" (at 90.65 89.5 90) (layer Dwgs.User))
    (feature1 (pts (xy 94 65) (xy 89.3 65)))
    (feature2 (pts (xy 94 114) (xy 89.3 114)))
    (crossbar (pts (xy 92 114) (xy 92 65)))
    (arrow1a (pts (xy 92 65) (xy 92.586421 66.126504)))
    (arrow1b (pts (xy 92 65) (xy 91.413579 66.126504)))
    (arrow2a (pts (xy 92 114) (xy 92.586421 112.873496)))
    (arrow2b (pts (xy 92 114) (xy 91.413579 112.873496)))
  )
  (gr_arc (start 97 114) (end 97 117) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 155 114) (end 158 114) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 158 71) (end 158 114) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 158 65) (end 158 71) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 97 65) (end 94 65) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 155 65) (end 155 62) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 97 62) (end 155 62) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing chamfer))
    (polygon
      (pts
        (xy 158 62) (xy 94 62) (xy 94 117) (xy 158 117)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing chamfer))
    (polygon
      (pts
        (xy 158 117) (xy 140 117) (xy 140 97) (xy 138 97) (xy 138 117)
        (xy 94 117) (xy 94 97.5) (xy 99.2 97.5) (xy 99.2 81.6) (xy 94 81.6)
        (xy 94 62) (xy 158 62)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 99.1 81.3) (xy 100.4 81.3) (xy 100.4 98.1) (xy 99.1 98.1)
      )
    )
  )
)
