(kicad_pcb (version 20171130) (host pcbnew "(5.1.2)-2")
  (general
    (thickness 1.6)
    (drawings 69)
    (tracks 385)
    (zones 0)
    (modules 36)
    (nets 71)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 1.27)
    (user_trace_width 2.032)
    (user_trace_width 3.81)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.54 2.54)
    (pad_drill 1.27)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(A1-Pad16)")
  (net 2 "Net-(A1-Pad15)")
  (net 3 "Net-(A1-Pad30)")
  (net 4 "Net-(A1-Pad14)")
  (net 5 GND)
  (net 6 "Net-(A1-Pad13)")
  (net 7 "Net-(A1-Pad28)")
  (net 8 "Net-(A1-Pad12)")
  (net 9 "Net-(A1-Pad11)")
  (net 10 "Net-(A1-Pad10)")
  (net 11 "Net-(A1-Pad9)")
  (net 12 "Net-(A1-Pad24)")
  (net 13 "Net-(A1-Pad8)")
  (net 14 "Net-(A1-Pad23)")
  (net 15 "Net-(A1-Pad7)")
  (net 16 "Net-(A1-Pad22)")
  (net 17 "Net-(A1-Pad6)")
  (net 18 "Net-(A1-Pad21)")
  (net 19 "Net-(A1-Pad5)")
  (net 20 "Net-(A1-Pad20)")
  (net 21 "Net-(A1-Pad19)")
  (net 22 "Net-(A1-Pad3)")
  (net 23 "Net-(A1-Pad18)")
  (net 24 "Net-(A1-Pad2)")
  (net 25 "Net-(A1-Pad17)")
  (net 26 "Net-(A1-Pad1)")
  (net 27 "Net-(IC2-Pad18)")
  (net 28 "Net-(IC2-Pad17)")
  (net 29 "Net-(IC2-Pad16)")
  (net 30 "Net-(IC2-Pad15)")
  (net 31 "Net-(IC2-Pad14)")
  (net 32 "Net-(IC2-Pad13)")
  (net 33 "Net-(IC2-Pad12)")
  (net 34 "Net-(IC2-Pad11)")
  (net 35 "Net-(C2-Pad1)")
  (net 36 "Net-(D1-PadA)")
  (net 37 "Net-(C1-Pad1)")
  (net 38 "Net-(D2-Pad2)")
  (net 39 "Net-(A1-Pad25)")
  (net 40 "Net-(A1-Pad26)")
  (net 41 "Net-(A1-Pad27)")
  (net 42 "Net-(RLY1-Pad3)")
  (net 43 "Net-(RLY2-Pad3)")
  (net 44 "Net-(RLY3-Pad3)")
  (net 45 "Net-(RLY4-Pad3)")
  (net 46 "Net-(RLY5-Pad3)")
  (net 47 "Net-(RLY6-Pad3)")
  (net 48 "Net-(RLY7-Pad3)")
  (net 49 "Net-(RLY8-Pad3)")
  (net 50 "Net-(J7-Pad3)")
  (net 51 "Net-(J7-Pad1)")
  (net 52 "Net-(L1-Pad12)")
  (net 53 "Net-(L1-Pad11)")
  (net 54 "Net-(L1-Pad8)")
  (net 55 "Net-(L1-Pad6)")
  (net 56 "Net-(L1-Pad5)")
  (net 57 "Net-(L1-Pad2)")
  (net 58 "Net-(J4-Pad2)")
  (net 59 "Net-(J8-Pad1)")
  (net 60 "Net-(J10-Pad3)")
  (net 61 "Net-(J10-Pad4)")
  (net 62 "Net-(J10-Pad13)")
  (net 63 "Net-(J10-Pad14)")
  (net 64 "Net-(J10-Pad10)")
  (net 65 "Net-(J10-Pad9)")
  (net 66 "Net-(J10-Pad8)")
  (net 67 "Net-(J10-Pad7)")
  (net 68 "Net-(J10-Pad6)")
  (net 69 "Net-(J10-Pad5)")
  (net 70 "Net-(J10-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 1.27)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(A1-Pad1)")
    (add_net "Net-(A1-Pad10)")
    (add_net "Net-(A1-Pad11)")
    (add_net "Net-(A1-Pad12)")
    (add_net "Net-(A1-Pad13)")
    (add_net "Net-(A1-Pad14)")
    (add_net "Net-(A1-Pad15)")
    (add_net "Net-(A1-Pad16)")
    (add_net "Net-(A1-Pad17)")
    (add_net "Net-(A1-Pad18)")
    (add_net "Net-(A1-Pad19)")
    (add_net "Net-(A1-Pad2)")
    (add_net "Net-(A1-Pad20)")
    (add_net "Net-(A1-Pad21)")
    (add_net "Net-(A1-Pad22)")
    (add_net "Net-(A1-Pad23)")
    (add_net "Net-(A1-Pad24)")
    (add_net "Net-(A1-Pad25)")
    (add_net "Net-(A1-Pad26)")
    (add_net "Net-(A1-Pad27)")
    (add_net "Net-(A1-Pad28)")
    (add_net "Net-(A1-Pad3)")
    (add_net "Net-(A1-Pad30)")
    (add_net "Net-(A1-Pad5)")
    (add_net "Net-(A1-Pad6)")
    (add_net "Net-(A1-Pad7)")
    (add_net "Net-(A1-Pad8)")
    (add_net "Net-(A1-Pad9)")
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(D1-PadA)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(IC2-Pad11)")
    (add_net "Net-(IC2-Pad12)")
    (add_net "Net-(IC2-Pad13)")
    (add_net "Net-(IC2-Pad14)")
    (add_net "Net-(IC2-Pad15)")
    (add_net "Net-(IC2-Pad16)")
    (add_net "Net-(IC2-Pad17)")
    (add_net "Net-(IC2-Pad18)")
    (add_net "Net-(J10-Pad10)")
    (add_net "Net-(J10-Pad13)")
    (add_net "Net-(J10-Pad14)")
    (add_net "Net-(J10-Pad2)")
    (add_net "Net-(J10-Pad3)")
    (add_net "Net-(J10-Pad4)")
    (add_net "Net-(J10-Pad5)")
    (add_net "Net-(J10-Pad6)")
    (add_net "Net-(J10-Pad7)")
    (add_net "Net-(J10-Pad8)")
    (add_net "Net-(J10-Pad9)")
    (add_net "Net-(J4-Pad2)")
    (add_net "Net-(J7-Pad1)")
    (add_net "Net-(J7-Pad3)")
    (add_net "Net-(J8-Pad1)")
    (add_net "Net-(L1-Pad11)")
    (add_net "Net-(L1-Pad12)")
    (add_net "Net-(L1-Pad2)")
    (add_net "Net-(L1-Pad5)")
    (add_net "Net-(L1-Pad6)")
    (add_net "Net-(L1-Pad8)")
    (add_net "Net-(RLY1-Pad3)")
    (add_net "Net-(RLY2-Pad3)")
    (add_net "Net-(RLY3-Pad3)")
    (add_net "Net-(RLY4-Pad3)")
    (add_net "Net-(RLY5-Pad3)")
    (add_net "Net-(RLY6-Pad3)")
    (add_net "Net-(RLY7-Pad3)")
    (add_net "Net-(RLY8-Pad3)")
  )
  (net_class Power ""
    (clearance 0.2)
    (trace_width 3.683)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 130.302 110.236 270)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference J11 (at 0 -2.54 90) (layer F.SilkS))
    (fp_text value "Rate LEDs" (at -2.794 3.81 180) (layer F.SilkS))
    (fp_text user %R (at 0 3.81) (layer F.Fab))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 61 "Net-(J10-Pad4)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 60 "Net-(J10-Pad3)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 101.092 85.09 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 5mm width 2.5mm Capacitor")
    (fp_text reference C3 (at 1.25 -2.5) (layer F.SilkS))
    (fp_text value 0.1uF (at 1.25 2.5) (layer F.SilkS))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 "Net-(C2-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "my library:LLC" (layer F.Cu) (tedit 5DC4DB36)
    (at 99.154999 111.76 180)
    (fp_text reference L1 (at -1.778 -2.794 180) (layer F.SilkS))
    (fp_text value LLC (at -6.604 -2.794 180) (layer F.Fab))
    (fp_text user HV3 (at -5.08 -7.62 180) (layer F.SilkS))
    (fp_text user HV4 (at -5.08 -5.08 180) (layer F.SilkS))
    (fp_text user GND (at -10.16 -10.16 180) (layer F.SilkS))
    (fp_text user HV (at -5.08 -12.7 180) (layer F.SilkS))
    (fp_text user HV2 (at -5.08 -15.24 180) (layer F.SilkS))
    (fp_text user HV1 (at -5.08 -17.78 180) (layer F.SilkS))
    (fp_text user LV4 (at -10.16 -5.08 180) (layer F.SilkS))
    (fp_text user LV3 (at -10.16 -7.62 180) (layer F.SilkS))
    (fp_text user GND (at -5 -10.16 180) (layer F.SilkS))
    (fp_text user LV (at -10.16 -12.7 180) (layer F.SilkS))
    (fp_text user LV2 (at -10.16 -15.24 180) (layer F.SilkS))
    (fp_text user LV1 (at -10.16 -17.78 180) (layer F.SilkS))
    (pad 12 thru_hole circle (at -2.54 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 52 "Net-(L1-Pad12)"))
    (pad 11 thru_hole circle (at -2.54 -7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 53 "Net-(L1-Pad11)"))
    (pad 10 thru_hole circle (at -2.54 -10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 9 thru_hole circle (at -2.54 -12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 "Net-(C1-Pad1)"))
    (pad 8 thru_hole circle (at -2.54 -15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 54 "Net-(L1-Pad8)"))
    (pad 7 thru_hole circle (at -2.54 -17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 59 "Net-(J8-Pad1)"))
    (pad 6 thru_hole circle (at -12.7 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 55 "Net-(L1-Pad6)"))
    (pad 5 thru_hole circle (at -12.7 -7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 56 "Net-(L1-Pad5)"))
    (pad 4 thru_hole circle (at -12.7 -10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 3 thru_hole circle (at -12.7 -12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(A1-Pad17)"))
    (pad 2 thru_hole circle (at -12.7 -15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 57 "Net-(L1-Pad2)"))
    (pad 1 thru_hole circle (at -12.7 -17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 51 "Net-(J7-Pad1)"))
  )
  (module "my library:mEZD71201A" (layer F.Cu) (tedit 5DB4C6B1)
    (at 124.127 139.192 90)
    (fp_text reference RG1 (at -1.016 1.349) (layer F.SilkS))
    (fp_text value mEZD71201A (at 5.1054 -1.4478 90) (layer F.SilkS))
    (fp_text user Vin (at 2.1844 5.8166) (layer F.SilkS))
    (fp_text user GND (at 4.7498 5.6388) (layer F.SilkS))
    (fp_text user Vout (at 7.2644 5.4356) (layer F.SilkS))
    (pad 3 thru_hole circle (at 7.4168 8.5 180) (size 1.59 1.59) (drill 0.89) (layers *.Cu *.Mask)
      (net 37 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 4.8768 8.5 180) (size 1.59 1.59) (drill 0.89) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 1 thru_hole circle (at 2.3368 8.5 180) (size 1.59 1.59) (drill 0.89) (layers *.Cu *.Mask)
      (net 35 "Net-(C2-Pad1)"))
  )
  (module "my library:1N5400" (layer F.Cu) (tedit 5DB5A316)
    (at 129.032 144.526)
    (descr "<B>DIODE</B><p>\ndiameter 5.6 mm, horizontal, grid 15.24 mm")
    (fp_text reference D1 (at 4.826 4.318) (layer F.SilkS))
    (fp_text value 1N5400 (at -3.048 2.1844) (layer F.SilkS))
    (pad C thru_hole circle (at -7.62 0) (size 2.5 2.5) (drill 1.25) (layers *.Cu *.Mask)
      (net 35 "Net-(C2-Pad1)") (solder_mask_margin 0.1016))
    (pad A thru_hole circle (at 7.62 0) (size 2.5 2.5) (drill 1.25) (layers *.Cu *.Mask)
      (net 36 "Net-(D1-PadA)") (solder_mask_margin 0.1016))
  )
  (module "my library:FTR-P3_Relay" (layer F.Cu) (tedit 5DB4CA9E)
    (at 84.328 70.757142 180)
    (descr "12V relay")
    (tags FTR-P3CN012W1)
    (fp_text reference RLY2 (at -3.048 2.685142 270) (layer F.SilkS))
    (fp_text value "Sec2 - FTR-P3CN012W1" (at 7.373428 -2.286) (layer F.SilkS))
    (fp_text user SIG (at 2.032 2.177142) (layer F.Fab))
    (fp_text user PWR (at 3.556 5.479142) (layer F.Fab))
    (fp_text user COM (at 8.636 0.145142) (layer F.Fab))
    (fp_text user NO (at 12.8778 5.733142) (layer F.Fab))
    (fp_text user NC (at 12.446 1.161142) (layer F.Fab))
    (pad 2 thru_hole circle (at 10 5.5 180) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 70 "Net-(J10-Pad2)"))
    (pad 3 thru_hole circle (at 15 0 180) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 43 "Net-(RLY2-Pad3)"))
    (pad 4 thru_hole circle (at 5 0 180) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 35 "Net-(C2-Pad1)"))
    (pad 5 thru_hole circle (at 0 0 180) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 33 "Net-(IC2-Pad12)"))
    (pad 1 thru_hole circle (at 0 5.5 180) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 35 "Net-(C2-Pad1)"))
  )
  (module "my library:FTR-P3_Relay" (layer F.Cu) (tedit 5DB4CA9E)
    (at 84.328 146.304 180)
    (descr "12V relay")
    (tags FTR-P3CN012W1)
    (fp_text reference RLY8 (at -3.048 2.794 270) (layer F.SilkS))
    (fp_text value "Switched Power - FTR-P3CN012W1" (at 3.302 -2.54 180) (layer F.SilkS))
    (fp_text user SIG (at 2.286 2.032) (layer F.Fab))
    (fp_text user PWR (at 3.556 5.588) (layer F.Fab))
    (fp_text user COM (at 8.382 0.254) (layer F.Fab))
    (fp_text user NO (at 12.8778 5.842) (layer F.Fab))
    (fp_text user NC (at 12.7 1.778) (layer F.Fab))
    (pad 2 thru_hole circle (at 10 5.5 180) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 63 "Net-(J10-Pad14)"))
    (pad 3 thru_hole circle (at 15 0 180) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 49 "Net-(RLY8-Pad3)"))
    (pad 4 thru_hole circle (at 5 0 180) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 35 "Net-(C2-Pad1)"))
    (pad 5 thru_hole circle (at 0 0 180) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 27 "Net-(IC2-Pad18)"))
    (pad 1 thru_hole circle (at 0 5.5 180) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 35 "Net-(C2-Pad1)"))
  )
  (module "my library:FTR-P3_Relay" (layer F.Cu) (tedit 5DB4CA9E)
    (at 84.328 133.712852 180)
    (descr "12V relay")
    (tags FTR-P3CN012W1)
    (fp_text reference RLY7 (at -3.048 2.62467 270) (layer F.SilkS))
    (fp_text value "Sec7 - FTR-P3CN012W1" (at 7.373428 -2.45533 180) (layer F.SilkS))
    (fp_text user SIG (at 2.1082 2.140852) (layer F.Fab))
    (fp_text user PWR (at 3.556 5.950852) (layer F.Fab))
    (fp_text user COM (at 8.636 0.362852) (layer F.Fab))
    (fp_text user NO (at 12.954 5.696852) (layer F.Fab))
    (fp_text user NC (at 12.7 1.886852) (layer F.Fab))
    (pad 2 thru_hole circle (at 10 5.5 180) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 64 "Net-(J10-Pad10)"))
    (pad 3 thru_hole circle (at 15 0 180) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 48 "Net-(RLY7-Pad3)"))
    (pad 4 thru_hole circle (at 5 0 180) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 35 "Net-(C2-Pad1)"))
    (pad 5 thru_hole circle (at 0 0 180) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 28 "Net-(IC2-Pad17)"))
    (pad 1 thru_hole circle (at 0 5.5 180) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 35 "Net-(C2-Pad1)"))
  )
  (module "my library:FTR-P3_Relay" (layer F.Cu) (tedit 5DB4CA9E)
    (at 84.328 121.12171 180)
    (descr "12V relay")
    (tags FTR-P3CN012W1)
    (fp_text reference RLY6 (at -3.048 2.50371 270) (layer F.SilkS))
    (fp_text value "Sec6 - FTR-P3CN012W1" (at 7.373428 -2.370664 180) (layer F.SilkS))
    (fp_text user SIG (at 2.1082 2.24971) (layer F.Fab))
    (fp_text user PWR (at 3.556 5.55171) (layer F.Fab))
    (fp_text user COM (at 8.636 0.21771) (layer F.Fab))
    (fp_text user NO (at 12.8778 5.55171) (layer F.Fab))
    (fp_text user NC (at 12.7 1.99571) (layer F.Fab))
    (pad 2 thru_hole circle (at 10 5.5 180) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 65 "Net-(J10-Pad9)"))
    (pad 3 thru_hole circle (at 15 0 180) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 47 "Net-(RLY6-Pad3)"))
    (pad 4 thru_hole circle (at 5 0 180) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 35 "Net-(C2-Pad1)"))
    (pad 5 thru_hole circle (at 0 0 180) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 29 "Net-(IC2-Pad16)"))
    (pad 1 thru_hole circle (at 0 5.5 180) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 35 "Net-(C2-Pad1)"))
  )
  (module "my library:FTR-P3_Relay" (layer F.Cu) (tedit 5DB4CA9E)
    (at 84.328 108.530568 180)
    (descr "12V relay")
    (tags FTR-P3CN012W1)
    (fp_text reference RLY5 (at -3.048 2.866568 270) (layer F.SilkS))
    (fp_text value "Sec5 - FTR-P3CN012W1" (at 7.373428 -2.539998 180) (layer F.SilkS))
    (fp_text user SIG (at 2.032 2.104568) (layer F.Fab))
    (fp_text user PWR (at 3.302 5.406568) (layer F.Fab))
    (fp_text user COM (at 8.382 0.326568) (layer F.Fab))
    (fp_text user NO (at 12.7 5.406568) (layer F.Fab))
    (fp_text user NC (at 12.7 1.596568) (layer F.Fab))
    (pad 2 thru_hole circle (at 10 5.5 180) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 66 "Net-(J10-Pad8)"))
    (pad 3 thru_hole circle (at 15 0 180) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 46 "Net-(RLY5-Pad3)"))
    (pad 4 thru_hole circle (at 5 0 180) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 35 "Net-(C2-Pad1)"))
    (pad 5 thru_hole circle (at 0 0 180) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 30 "Net-(IC2-Pad15)"))
    (pad 1 thru_hole circle (at 0 5.5 180) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 35 "Net-(C2-Pad1)"))
  )
  (module "my library:FTR-P3_Relay" (layer F.Cu) (tedit 5DB4CA9E)
    (at 84.328 95.939426 180)
    (descr "12V relay")
    (tags FTR-P3CN012W1)
    (fp_text reference RLY4 (at -3.048 2.721426 270) (layer F.SilkS))
    (fp_text value "Sec4 - FTR-P3CN012W1" (at 7.373428 -2.455332 180) (layer F.SilkS))
    (fp_text user SIG (at 2.032 1.959426) (layer F.Fab))
    (fp_text user PWR (at 3.302 5.515426) (layer F.Fab))
    (fp_text user COM (at 8.382 -0.072574) (layer F.Fab))
    (fp_text user NO (at 12.7 6.023426) (layer F.Fab))
    (fp_text user NC (at 12.446 1.705426) (layer F.Fab))
    (pad 2 thru_hole circle (at 10 5.5 180) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 67 "Net-(J10-Pad7)"))
    (pad 3 thru_hole circle (at 15 0 180) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 45 "Net-(RLY4-Pad3)"))
    (pad 4 thru_hole circle (at 5 0 180) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 35 "Net-(C2-Pad1)"))
    (pad 5 thru_hole circle (at 0 0 180) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 31 "Net-(IC2-Pad14)"))
    (pad 1 thru_hole circle (at 0 5.5 180) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 35 "Net-(C2-Pad1)"))
  )
  (module "my library:FTR-P3_Relay" (layer F.Cu) (tedit 5DB4CA9E)
    (at 84.328 83.348284 180)
    (descr "12V relay")
    (tags FTR-P3CN012W1)
    (fp_text reference RLY3 (at -3.048 2.576284 90) (layer F.SilkS))
    (fp_text value "Sec3 - FTR-P3CN012W1" (at 7.373428 -2.370666 180) (layer F.SilkS))
    (fp_text user SIG (at 2.1082 2.068284) (layer F.Fab))
    (fp_text user PWR (at 3.302 5.624284) (layer F.Fab))
    (fp_text user COM (at 8.382 0.290284) (layer F.Fab))
    (fp_text user NO (at 12.954 5.878284) (layer F.Fab))
    (fp_text user NC (at 12.446 1.306284) (layer F.Fab))
    (pad 2 thru_hole circle (at 10 5.5 180) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 69 "Net-(J10-Pad5)"))
    (pad 3 thru_hole circle (at 15 0 180) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 44 "Net-(RLY3-Pad3)"))
    (pad 4 thru_hole circle (at 5 0 180) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 35 "Net-(C2-Pad1)"))
    (pad 5 thru_hole circle (at 0 0 180) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 32 "Net-(IC2-Pad13)"))
    (pad 1 thru_hole circle (at 0 5.5 180) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 35 "Net-(C2-Pad1)"))
  )
  (module "my library:FTR-P3_Relay" (layer F.Cu) (tedit 5DB4CA9E)
    (at 84.328 58.166 180)
    (descr "12V relay")
    (tags FTR-P3CN012W1)
    (fp_text reference RLY1 (at -3.048 2.286 90) (layer F.SilkS))
    (fp_text value "Sec1 - FTR-P3CN012W1" (at 7.373428 -3.0988) (layer F.SilkS))
    (fp_text user SIG (at 1.778 2.286) (layer F.Fab))
    (fp_text user PWR (at 3.556 5.588) (layer F.Fab))
    (fp_text user COM (at 8.636 0.254) (layer F.Fab))
    (fp_text user NO (at 12.954 5.588) (layer F.Fab))
    (fp_text user NC (at 12.446 1.27) (layer F.Fab))
    (pad 2 thru_hole circle (at 10 5.5 180) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 68 "Net-(J10-Pad6)"))
    (pad 3 thru_hole circle (at 15 0 180) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 42 "Net-(RLY1-Pad3)"))
    (pad 4 thru_hole circle (at 5 0 180) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 35 "Net-(C2-Pad1)"))
    (pad 5 thru_hole circle (at 0 0 180) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 34 "Net-(IC2-Pad11)"))
    (pad 1 thru_hole circle (at 0 5.5 180) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 35 "Net-(C2-Pad1)"))
  )
  (module "my library:Phoenix_16_pin_5mm_terminal_block" (layer F.Cu) (tedit 5D6B1A83)
    (at 60.198 60.452 270)
    (fp_text reference J10 (at -1.016 1.524) (layer F.SilkS))
    (fp_text value Screw_Terminal_01x16 (at 20 -1 90) (layer F.Fab))
    (pad 16 thru_hole circle (at 77.5 5 270) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 35 "Net-(C2-Pad1)"))
    (pad 15 thru_hole circle (at 72.5 5 270) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 14 thru_hole circle (at 67.5 5 270) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 63 "Net-(J10-Pad14)"))
    (pad 13 thru_hole circle (at 62.5 5 270) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 62 "Net-(J10-Pad13)"))
    (pad 12 thru_hole circle (at 57.5 5 270) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 37 "Net-(C1-Pad1)"))
    (pad 11 thru_hole circle (at 52.5 5 270) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 10 thru_hole circle (at 47.5 5 270) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 64 "Net-(J10-Pad10)"))
    (pad 9 thru_hole circle (at 42.5 5 270) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 65 "Net-(J10-Pad9)"))
    (pad 8 thru_hole circle (at 37.5 5 270) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 66 "Net-(J10-Pad8)"))
    (pad 7 thru_hole circle (at 32.5 5 270) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 67 "Net-(J10-Pad7)"))
    (pad 6 thru_hole circle (at 27.5 5 270) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 68 "Net-(J10-Pad6)"))
    (pad 5 thru_hole circle (at 22.5 5 270) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 69 "Net-(J10-Pad5)"))
    (pad 4 thru_hole circle (at 17.5 5 270) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 61 "Net-(J10-Pad4)"))
    (pad 3 thru_hole circle (at 12.5 5 270) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 60 "Net-(J10-Pad3)"))
    (pad 2 thru_hole circle (at 7.5 5 270) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 70 "Net-(J10-Pad2)"))
    (pad 1 thru_hole circle (at 2.5 5 270) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 5 GND))
  )
  (module "my library:Phoenix_4_pin_5mm_terminal_block" (layer F.Cu) (tedit 5D6B1E0B)
    (at 138.684 101.092 90)
    (fp_text reference J5 (at -1.27 8.128 90) (layer F.SilkS))
    (fp_text value "Motor Power" (at 21.082 4.064 180) (layer F.SilkS))
    (pad 4 thru_hole circle (at 17.5 5 90) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 35 "Net-(C2-Pad1)"))
    (pad 3 thru_hole circle (at 12.5 5 90) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 2 thru_hole circle (at 7.5 5 90) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 61 "Net-(J10-Pad4)"))
    (pad 1 thru_hole circle (at 2.5 5 90) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 60 "Net-(J10-Pad3)"))
  )
  (module "my library:Phoenix_3_pin_5mm_terminal_block" (layer F.Cu) (tedit 5D6B1C8B)
    (at 147.494001 107.656999 270)
    (fp_text reference J2 (at 16.041001 0.936001 90) (layer F.SilkS))
    (fp_text value "Motor Control" (at -1.484999 4.492001 180) (layer F.SilkS))
    (pad 3 thru_hole circle (at 12.5 5 270) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 2 thru_hole circle (at 7.5 5 270) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 8 "Net-(A1-Pad12)"))
    (pad 1 thru_hole circle (at 2.5 5 270) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 6 "Net-(A1-Pad13)"))
  )
  (module "my library:Phoenix_2_pin_5mm_terminal_block" (layer F.Cu) (tedit 5D6B1C47)
    (at 138.684 139.192 90)
    (fp_text reference J1 (at -1.524 8.382 90) (layer F.SilkS))
    (fp_text value "Power In" (at 11.176 4.572 180) (layer F.SilkS))
    (pad 2 thru_hole circle (at 7.5 5 90) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 1 thru_hole circle (at 2.5 5 90) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 36 "Net-(D1-PadA)"))
  )
  (module "my library:DIL18" (layer F.Cu) (tedit 0)
    (at 101.092 100.33 90)
    (descr "<b>Dual In Line Package</b>")
    (fp_text reference IC2 (at -11.684 3.048) (layer F.SilkS))
    (fp_text value ULN2803A (at -9.525 0.635 90) (layer F.SilkS))
    (pad 18 thru_hole oval (at -10.16 -3.81 180) (size 2.6416 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 27 "Net-(IC2-Pad18)") (solder_mask_margin 0.1016))
    (pad 17 thru_hole oval (at -7.62 -3.81 180) (size 2.6416 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 28 "Net-(IC2-Pad17)") (solder_mask_margin 0.1016))
    (pad 16 thru_hole oval (at -5.08 -3.81 180) (size 2.6416 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 29 "Net-(IC2-Pad16)") (solder_mask_margin 0.1016))
    (pad 15 thru_hole oval (at -2.54 -3.81 180) (size 2.6416 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 30 "Net-(IC2-Pad15)") (solder_mask_margin 0.1016))
    (pad 14 thru_hole oval (at 0 -3.81 180) (size 2.6416 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 31 "Net-(IC2-Pad14)") (solder_mask_margin 0.1016))
    (pad 13 thru_hole oval (at 2.54 -3.81 180) (size 2.6416 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 32 "Net-(IC2-Pad13)") (solder_mask_margin 0.1016))
    (pad 12 thru_hole oval (at 5.08 -3.81 180) (size 2.6416 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 33 "Net-(IC2-Pad12)") (solder_mask_margin 0.1016))
    (pad 11 thru_hole oval (at 7.62 -3.81 180) (size 2.6416 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 34 "Net-(IC2-Pad11)") (solder_mask_margin 0.1016))
    (pad 10 thru_hole oval (at 10.16 -3.81 180) (size 2.6416 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 35 "Net-(C2-Pad1)") (solder_mask_margin 0.1016))
    (pad 9 thru_hole oval (at 10.16 3.81 180) (size 2.6416 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 5 GND) (solder_mask_margin 0.1016))
    (pad 5 thru_hole oval (at 0 3.81 180) (size 2.6416 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 11 "Net-(A1-Pad9)") (solder_mask_margin 0.1016))
    (pad 6 thru_hole oval (at 2.54 3.81 180) (size 2.6416 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 13 "Net-(A1-Pad8)") (solder_mask_margin 0.1016))
    (pad 4 thru_hole oval (at -2.54 3.81 180) (size 2.6416 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 10 "Net-(A1-Pad10)") (solder_mask_margin 0.1016))
    (pad 3 thru_hole oval (at -5.08 3.81 180) (size 2.6416 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 9 "Net-(A1-Pad11)") (solder_mask_margin 0.1016))
    (pad 8 thru_hole oval (at 7.62 3.81 180) (size 2.6416 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 17 "Net-(A1-Pad6)") (solder_mask_margin 0.1016))
    (pad 7 thru_hole oval (at 5.08 3.81 180) (size 2.6416 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 15 "Net-(A1-Pad7)") (solder_mask_margin 0.1016))
    (pad 2 thru_hole oval (at -7.62 3.81 180) (size 2.6416 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 4 "Net-(A1-Pad14)") (solder_mask_margin 0.1016))
    (pad 1 thru_hole oval (at -10.16 3.81 180) (size 2.6416 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 2 "Net-(A1-Pad15)") (solder_mask_margin 0.1016))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 145.542 145.796)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference H4 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 53.848 145.796)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference H3 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole (at -0.765 4.318) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 145.796 54.102)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference H2 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 53.848 54.102)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference H1 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 96 56 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J6 (at -0.388 -2.274 90) (layer F.SilkS))
    (fp_text value "Power Source" (at 2.66 2.044) (layer F.SilkS))
    (fp_text user %R (at 0 2.54) (layer F.Fab))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 "Net-(A1-Pad27)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 "Net-(C1-Pad1)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(A1-Pad30)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 111.76 85.598 270)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J9 (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value "VCC Power" (at -2.54 2.54) (layer F.SilkS))
    (fp_text user %R (at 0 2.54) (layer F.Fab))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 "Net-(C1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 58 "Net-(J4-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(A1-Pad17)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 93.726 128.918 180)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J8 (at -0.254 -2.794) (layer F.SilkS))
    (fp_text value "Flow Selection1" (at -2.794 1.016 90) (layer F.Fab))
    (fp_text user %R (at 0 2.54 90) (layer F.Fab))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 50 "Net-(J7-Pad3)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 62 "Net-(J10-Pad13)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 59 "Net-(J8-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 118.364 128.918 180)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J7 (at 2.667 -2.667) (layer F.SilkS))
    (fp_text value "Flow Selection2" (at 2.54 1.016 90) (layer F.Fab))
    (fp_text user %R (at 0 2.54 90) (layer F.Fab))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 50 "Net-(J7-Pad3)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(A1-Pad5)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 51 "Net-(J7-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "my library:Arduino_Nano" (layer F.Cu) (tedit 5D6044E3)
    (at 101.854 76.708 90)
    (descr "Arduino Nano, http://www.mouser.com/pdfdocs/Gravitech_Arduino_Nano3_0.pdf")
    (tags "Arduino Nano")
    (fp_text reference A1 (at -2.54 -2.286 90) (layer F.SilkS))
    (fp_text value Nano33/Nano (at 8.89 20.32) (layer F.SilkS))
    (fp_text user D13 (at 12.1158 35.5854 90) (layer F.SilkS))
    (fp_text user +3V3 (at 11.568181 33.0708 90) (layer F.SilkS))
    (fp_text user AREF (at 11.758657 30.5816 90) (layer F.SilkS))
    (fp_text user A0 (at 12.663419 28.0416 90) (layer F.SilkS))
    (fp_text user A1 (at 12.663419 25.3746 90) (layer F.SilkS))
    (fp_text user A2 (at 12.663419 22.9362 90) (layer F.SilkS))
    (fp_text user A3 (at 12.663419 20.5232 90) (layer F.SilkS))
    (fp_text user A4 (at 12.663419 17.8054 90) (layer F.SilkS))
    (fp_text user A5 (at 12.663419 15.1384 90) (layer F.SilkS))
    (fp_text user A6 (at 12.663419 12.7254 90) (layer F.SilkS))
    (fp_text user A7 (at 12.663419 10.2616 90) (layer F.SilkS))
    (fp_text user +5V (at 12.044371 7.5946 90) (layer F.SilkS))
    (fp_text user RST (at 12.211038 5.1308 90) (layer F.SilkS))
    (fp_text user GND (at 12.044371 2.54 90) (layer F.SilkS))
    (fp_text user VIN (at 12.377705 0.127 90) (layer F.SilkS))
    (fp_text user D12 (at 2.9464 35.6362 90) (layer F.SilkS))
    (fp_text user D11 (at 2.9464 33.02 90) (layer F.SilkS))
    (fp_text user D10 (at 2.9464 30.5816 90) (layer F.SilkS))
    (fp_text user D9 (at 2.470209 28.0162 90) (layer F.SilkS))
    (fp_text user D8 (at 2.470209 25.5016 90) (layer F.SilkS))
    (fp_text user D7 (at 2.470209 22.7838 90) (layer F.SilkS))
    (fp_text user D6 (at 2.470209 20.3962 90) (layer F.SilkS))
    (fp_text user D5 (at 2.470209 17.8308 90) (layer F.SilkS))
    (fp_text user D4 (at 2.470209 15.3416 90) (layer F.SilkS))
    (fp_text user D3 (at 2.470209 12.7254 90) (layer F.SilkS))
    (fp_text user D2 (at 2.470209 10.2108 90) (layer F.SilkS))
    (fp_text user GND (at 3.017828 7.7978 90) (layer F.SilkS))
    (fp_text user RST (at 2.851162 5.2324 90) (layer F.SilkS))
    (fp_text user "D0, RX" (at 4.065447 2.5654 90) (layer F.SilkS))
    (fp_text user "D1, TX" (at 3.9464 0.0508 90) (layer F.SilkS))
    (fp_text user %R (at 5.08 26.162) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.9906) (layers *.Cu *.Mask)
      (net 26 "Net-(A1-Pad1)"))
    (pad 17 thru_hole oval (at 15.24 33.02 90) (size 1.6 1.6) (drill 0.9906) (layers *.Cu *.Mask)
      (net 25 "Net-(A1-Pad17)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.6 1.6) (drill 0.9906) (layers *.Cu *.Mask)
      (net 24 "Net-(A1-Pad2)"))
    (pad 18 thru_hole oval (at 15.24 30.48 90) (size 1.6 1.6) (drill 0.9906) (layers *.Cu *.Mask)
      (net 23 "Net-(A1-Pad18)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.6 1.6) (drill 0.9906) (layers *.Cu *.Mask)
      (net 22 "Net-(A1-Pad3)"))
    (pad 19 thru_hole oval (at 15.24 27.94 90) (size 1.6 1.6) (drill 0.9906) (layers *.Cu *.Mask)
      (net 21 "Net-(A1-Pad19)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.6 1.6) (drill 0.9906) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 20 thru_hole oval (at 15.24 25.4 90) (size 1.6 1.6) (drill 0.9906) (layers *.Cu *.Mask)
      (net 20 "Net-(A1-Pad20)"))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.6 1.6) (drill 0.9906) (layers *.Cu *.Mask)
      (net 19 "Net-(A1-Pad5)"))
    (pad 21 thru_hole oval (at 15.24 22.86 90) (size 1.6 1.6) (drill 0.9906) (layers *.Cu *.Mask)
      (net 18 "Net-(A1-Pad21)"))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.6 1.6) (drill 0.9906) (layers *.Cu *.Mask)
      (net 17 "Net-(A1-Pad6)"))
    (pad 22 thru_hole oval (at 15.24 20.32 90) (size 1.6 1.6) (drill 0.9906) (layers *.Cu *.Mask)
      (net 16 "Net-(A1-Pad22)"))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.6 1.6) (drill 0.9906) (layers *.Cu *.Mask)
      (net 15 "Net-(A1-Pad7)"))
    (pad 23 thru_hole oval (at 15.24 17.78 90) (size 1.6 1.6) (drill 0.9906) (layers *.Cu *.Mask)
      (net 14 "Net-(A1-Pad23)"))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.6 1.6) (drill 0.9906) (layers *.Cu *.Mask)
      (net 13 "Net-(A1-Pad8)"))
    (pad 24 thru_hole oval (at 15.24 15.24 90) (size 1.6 1.6) (drill 0.9906) (layers *.Cu *.Mask)
      (net 12 "Net-(A1-Pad24)"))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 1.6 1.6) (drill 0.9906) (layers *.Cu *.Mask)
      (net 11 "Net-(A1-Pad9)"))
    (pad 25 thru_hole oval (at 15.24 12.7 90) (size 1.6 1.6) (drill 0.9906) (layers *.Cu *.Mask)
      (net 39 "Net-(A1-Pad25)"))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 1.6 1.6) (drill 0.9906) (layers *.Cu *.Mask)
      (net 10 "Net-(A1-Pad10)"))
    (pad 26 thru_hole oval (at 15.24 10.16 90) (size 1.6 1.6) (drill 0.9906) (layers *.Cu *.Mask)
      (net 40 "Net-(A1-Pad26)"))
    (pad 11 thru_hole oval (at 0 25.4 90) (size 1.6 1.6) (drill 0.9906) (layers *.Cu *.Mask)
      (net 9 "Net-(A1-Pad11)"))
    (pad 27 thru_hole oval (at 15.24 7.62 90) (size 1.6 1.6) (drill 0.9906) (layers *.Cu *.Mask)
      (net 41 "Net-(A1-Pad27)"))
    (pad 12 thru_hole oval (at 0 27.94 90) (size 1.6 1.6) (drill 0.9906) (layers *.Cu *.Mask)
      (net 8 "Net-(A1-Pad12)"))
    (pad 28 thru_hole oval (at 15.24 5.08 90) (size 1.6 1.6) (drill 0.9906) (layers *.Cu *.Mask)
      (net 7 "Net-(A1-Pad28)"))
    (pad 13 thru_hole oval (at 0 30.48 90) (size 1.6 1.6) (drill 0.9906) (layers *.Cu *.Mask)
      (net 6 "Net-(A1-Pad13)"))
    (pad 29 thru_hole oval (at 15.24 2.54 90) (size 1.6 1.6) (drill 0.9906) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 14 thru_hole oval (at 0 33.02 90) (size 1.6 1.6) (drill 0.9906) (layers *.Cu *.Mask)
      (net 4 "Net-(A1-Pad14)"))
    (pad 30 thru_hole oval (at 15.24 0 90) (size 1.6 1.6) (drill 0.9906) (layers *.Cu *.Mask)
      (net 3 "Net-(A1-Pad30)"))
    (pad 15 thru_hole oval (at 0 35.56 90) (size 1.6 1.6) (drill 0.9906) (layers *.Cu *.Mask)
      (net 2 "Net-(A1-Pad15)"))
    (pad 16 thru_hole oval (at 15.24 35.56 90) (size 1.6 1.6) (drill 0.9906) (layers *.Cu *.Mask)
      (net 1 "Net-(A1-Pad16)"))
    (model ${KISYS3DMOD}/Module.3dshapes/Arduino_Nano_WithMountingHoles.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 132.842 125.984 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R9 (at 3.81 2.54) (layer F.SilkS))
    (fp_text value 1K (at 4.064 -2.032) (layer F.SilkS))
    (fp_text user %R (at 3.81 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 38 "Net-(D2-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 37 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_THT:LED_D3.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 129.032 120.65 90)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D2 (at 4.064 3.302) (layer F.SilkS))
    (fp_text value LED (at 0.381 -3.81) (layer F.SilkS))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 38 "Net-(D2-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 5 GND))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 91.948 60.96 270)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 5mm width 2.5mm Capacitor")
    (fp_text reference C4 (at -2.794 1.524 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 1.25 2.5 90) (layer F.SilkS))
    (fp_text user %R (at 1.397 0.127 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D10.0mm_P5.00mm (layer F.Cu) (tedit 5AE50EF1)
    (at 95.25 138.176 270)
    (descr "CP, Radial series, Radial, pin pitch=5.00mm, , diameter=10mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 5.00mm  diameter 10mm Electrolytic Capacitor")
    (fp_text reference C2 (at 1.524 -3.556 180) (layer F.SilkS))
    (fp_text value 1000uF (at -3.302 3.556 180) (layer F.SilkS))
    (fp_text user %R (at 2.5 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 1 thru_hole rect (at 0 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 35 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D10.0mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D10.0mm_P5.00mm (layer F.Cu) (tedit 5AE50EF1)
    (at 111.76 138.176 270)
    (descr "CP, Radial series, Radial, pin pitch=5.00mm, , diameter=10mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 5.00mm  diameter 10mm Electrolytic Capacitor")
    (fp_text reference C1 (at 1.524 -3.556 180) (layer F.SilkS))
    (fp_text value 1000uF (at -3.302 4.572 180) (layer F.SilkS))
    (fp_text user %R (at 2.5 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 1 thru_hole rect (at 0 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 37 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D10.0mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x11_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 106.934 56 90)
    (descr "Through hole straight pin header, 1x11, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x11 2.54mm single row")
    (fp_text reference J4 (at 0.12 28.448 90) (layer F.SilkS))
    (fp_text value Switches (at -2.7178 13.0048 180) (layer F.SilkS))
    (fp_text user %R (at 0 12.7) (layer F.Fab))
    (pad 11 thru_hole oval (at 0 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(A1-Pad16)"))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(A1-Pad19)"))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(A1-Pad20)"))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(A1-Pad21)"))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(A1-Pad22)"))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(A1-Pad23)"))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(A1-Pad24)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 "Net-(A1-Pad25)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 "Net-(A1-Pad26)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 58 "Net-(J4-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x11_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x07_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 113.284 92.71 90)
    (descr "Through hole straight pin header, 1x07, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x07 2.54mm single row")
    (fp_text reference J3 (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value "Section LEDs" (at 2.794 7.62) (layer F.SilkS))
    (fp_text user %R (at 0 7.62) (layer F.Fab))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(A1-Pad14)"))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(A1-Pad11)"))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(A1-Pad10)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(A1-Pad9)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(A1-Pad8)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(A1-Pad7)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(A1-Pad6)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x07_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 96.266 61.722 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R11 (at 7.112 1.778 90) (layer F.SilkS))
    (fp_text value 4K7 (at 14.224 1.778 90) (layer F.SilkS))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 40 "Net-(A1-Pad26)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 58 "Net-(J4-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 96.266 80.264 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R10 (at 0.508 -1.778 90) (layer F.SilkS))
    (fp_text value 4K7 (at 15.494 -1.778 90) (layer F.SilkS))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 39 "Net-(A1-Pad25)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 58 "Net-(J4-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text 7 (at 128.524 95.504) (layer F.SilkS))
  (gr_text 6 (at 125.984 95.504) (layer F.SilkS))
  (gr_text 5 (at 123.19 95.504) (layer F.SilkS))
  (gr_text 4 (at 120.904 95.504) (layer F.SilkS))
  (gr_text 3 (at 118.364 95.504) (layer F.SilkS))
  (gr_text 2 (at 115.824 95.504) (layer F.SilkS))
  (gr_text 1 (at 113.284 95.504) (layer F.SilkS))
  (gr_text B (at 125.222 112.76819 90) (layer F.SilkS))
  (gr_text GND (at 122.428 113.792 90) (layer F.SilkS))
  (gr_text GND (at 127.762 113.792 90) (layer F.SilkS))
  (gr_text A (at 130.302 112.696762 90) (layer F.SilkS))
  (gr_text "Nano33   1 & 2\nNano   2 & 3" (at 119.888 102.616) (layer F.SilkS))
  (gr_text "Rate Controller 3.1  14-Nov-2019" (at 120.396 99.568) (layer F.SilkS))
  (gr_text 12V (at 135.620143 83.312) (layer F.SilkS))
  (gr_text GND (at 135.763 88.773) (layer F.SilkS))
  (gr_text "M B" (at 135.691572 93.599) (layer F.SilkS))
  (gr_text "M A" (at 135.620143 98.425) (layer F.SilkS))
  (gr_text 1 (at 121.412 129.032) (layer F.SilkS))
  (gr_text 3 (at 121.403181 123.698) (layer F.SilkS))
  (gr_text 2 (at 121.403181 126.35894) (layer F.SilkS))
  (gr_text 12V (at 62.341143 138.176) (layer F.SilkS))
  (gr_text GND (at 62.484 133.096) (layer F.SilkS))
  (gr_text "SW 12V" (at 63.769715 128.016) (layer F.SilkS))
  (gr_text "FLW Sig" (at 63.912572 123.19) (layer F.SilkS))
  (gr_text "FLW 5V" (at 63.650667 118.11) (layer F.SilkS))
  (gr_text "FLW GND" (at 64.269715 113.03) (layer F.SilkS))
  (gr_text Sec7 (at 62.769715 108.458) (layer F.SilkS))
  (gr_text Sec6 (at 62.769715 103.124) (layer F.SilkS))
  (gr_text Sec5 (at 62.769715 98.044) (layer F.SilkS))
  (gr_text Sec4 (at 62.769715 92.964) (layer F.SilkS))
  (gr_text Sec1 (at 62.769715 88.138) (layer F.SilkS))
  (gr_text Sec3 (at 62.769715 83.058) (layer F.SilkS))
  (gr_text "RT Dec" (at 63.579238 77.978) (layer F.SilkS))
  (gr_text "RT Inc" (at 63.341143 72.898) (layer F.SilkS))
  (gr_text Sec2 (at 62.769715 67.818) (layer F.SilkS))
  (gr_text GND (at 62.484 62.738) (layer F.SilkS))
  (gr_arc (start 146 146) (end 150 146) (angle 90) (layer Edge.Cuts) (width 0.12))
  (gr_arc (start 54 146) (end 54 150) (angle 90) (layer Edge.Cuts) (width 0.12))
  (gr_arc (start 54 54) (end 50 54) (angle 90) (layer Edge.Cuts) (width 0.12))
  (gr_arc (start 146 54) (end 146 50) (angle 90) (layer Edge.Cuts) (width 0.12))
  (gr_text 12V (at 137.668 136.652 90) (layer F.SilkS))
  (gr_text GND (at 137.668 131.572 90) (layer F.SilkS))
  (gr_text 2 (at 98.552 58.674) (layer F.SilkS))
  (gr_text 1 (at 96.012 58.674) (layer F.SilkS))
  (gr_text 3 (at 101.092 58.674) (layer F.SilkS))
  (gr_text 3 (at 106.426 88.138) (layer F.SilkS))
  (gr_text 1 (at 111.76 88.138) (layer F.SilkS))
  (gr_text 2 (at 109.22 88.138) (layer F.SilkS))
  (gr_text 2 (at 90.923181 126.35894) (layer F.SilkS))
  (gr_text 3 (at 90.923181 123.698) (layer F.SilkS))
  (gr_text 1 (at 90.932 129.032) (layer F.SilkS))
  (gr_line (start 54 50) (end 146 50) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 50 54) (end 50 146) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 54 150) (end 146 150) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 150 54) (end 150 146) (layer Edge.Cuts) (width 0.05))
  (gr_text VCC (at 109.5502 51.117476 90) (layer F.SilkS))
  (gr_text On (at 112.1156 52.022238 90) (layer F.SilkS))
  (gr_text "Down\n" (at 132.461 50.117476 90) (layer F.SilkS))
  (gr_text "Up\n" (at 129.8956 52.022238 90) (layer F.SilkS))
  (gr_text Auto (at 127.2032 50.736524 90) (layer F.SilkS))
  (gr_text SW4 (at 124.7902 50.927 90) (layer F.SilkS))
  (gr_text SW3 (at 122.2756 50.927 90) (layer F.SilkS))
  (gr_text SW2 (at 119.8372 50.927 90) (layer F.SilkS))
  (gr_text SW1 (at 117.1702 50.927 90) (layer F.SilkS))
  (gr_text Off (at 114.6556 51.784143 90) (layer F.SilkS))
  (gr_text GND (at 106.934 50.927 90) (layer F.SilkS))
  (gr_text GND (at 137.16 120.142 90) (layer F.SilkS))
  (gr_text PWM (at 137.16 115.062 90) (layer F.SilkS))
  (gr_text DIR (at 137.16 110.236 90) (layer F.SilkS))
  (zone (net 5) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 149.606 54.356) (xy 146.304 50.292) (xy 54.864 50.292) (xy 50.038 54.356) (xy 50.292 145.542)
        (xy 53.848 149.86) (xy 146.304 149.86) (xy 149.606 146.304)
      )
    )
  )
)
