(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 45)
    (no_connects 0)
    (area 143.446499 45.656499 198.183501 99.123501)
    (thickness 1.6)
    (drawings 53)
    (tracks 104)
    (zones 0)
    (modules 17)
    (nets 21)
  )
  (page A4)
  (layers
    (0 Top signal)
    (31 Bottom signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (44 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.1524)
    (user_trace_width 0.1524)
    (user_trace_width 0.2)
    (user_trace_width 0.25)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 0.6)
    (user_trace_width 1.2)
    (trace_clearance 0.3)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.1524)
    (segment_width 0.127)
    (edge_width 0.127)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.762)
    (uvia_drill 0.508)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.127)
    (pcb_text_size 0.6 0.6)
    (mod_edge_width 0.127)
    (mod_text_size 0.6 0.6)
    (mod_text_width 0.127)
    (pad_size 1.524 1.524)
    (pad_drill 0.9)
    (pad_to_mask_clearance 0.05)
    (pad_to_paste_clearance -0.04)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x011fc_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.127000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 4)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory CAM/))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 /ANT1)
  (net 3 /ANT2)
  (net 4 /MEGA-PIN49)
  (net 5 /MEGA-PIN48)
  (net 6 /MEGA-PIN51)
  (net 7 /MEGA-PIN50)
  (net 8 /MEGA-PIN52)
  (net 9 /MEGA-PIN15)
  (net 10 /MEGA-PIN16)
  (net 11 /MEGA-PIN19)
  (net 12 "/MEGA-PIN14(TX)")
  (net 13 /VCC-3.3)
  (net 14 /MEGA_TX0)
  (net 15 /MEGA_RX0)
  (net 16 /LV_TX1)
  (net 17 /LV_VCC)
  (net 18 /LV_RX0)
  (net 19 /MEGA_5V/2)
  (net 20 /HV_VCC)
  (net_class Default "Dit is de standaard class."
    (clearance 0.3)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net /ANT1)
    (add_net /ANT2)
    (add_net /HV_VCC)
    (add_net /LV_RX0)
    (add_net /LV_TX1)
    (add_net /LV_VCC)
    (add_net "/MEGA-PIN14(TX)")
    (add_net /MEGA-PIN15)
    (add_net /MEGA-PIN16)
    (add_net /MEGA-PIN19)
    (add_net /MEGA-PIN48)
    (add_net /MEGA-PIN49)
    (add_net /MEGA-PIN50)
    (add_net /MEGA-PIN51)
    (add_net /MEGA-PIN52)
    (add_net /MEGA_5V/2)
    (add_net /MEGA_RX0)
    (add_net /MEGA_TX0)
    (add_net /VCC-3.3)
    (add_net GND)
  )
  (module BRICE:LEVEL_CONVERTER (layer Top) (tedit 5A086EF3)
    (at 163.83 88.9 270)
    (fp_text reference LS1 (at -3.81 -1.27 270) (layer F.SilkS) hide)
    (fp_text value LEVEL_CONVERTER (at -1.905 -20.32 270) (layer F.Fab))
    (fp_text user CHAN2 (at -2.413 -4.953 270) (layer F.SilkS))
    (fp_text user CHAN1 (at -2.54 -17.78 270) (layer F.SilkS))
    (pad 6 thru_hole circle (at 2.54 -5.08) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 16 /LV_TX1))
    (pad 5 thru_hole circle (at 2.54 -7.62) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at 2.54 -10.16) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 2.54 -12.7) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 2.54 -15.24) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 2.54 -17.78) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 18 /LV_RX0))
    (pad 7 thru_hole circle (at -7.62 -17.78) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 14 /MEGA_TX0))
    (pad 8 thru_hole circle (at -7.62 -15.24) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask))
    (pad 9 thru_hole circle (at -7.62 -12.7) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask))
    (pad 10 thru_hole circle (at -7.62 -10.16) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask))
    (pad 11 thru_hole circle (at -7.62 -7.62) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask))
    (pad 12 thru_hole circle (at -7.62 -5.08) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 15 /MEGA_RX0))
  )
  (module BRICE:ESP8266-SP1_Breakout (layer Top) (tedit 5A083C69)
    (at 159.004 90.17 180)
    (descr "nRF24L01 breakout board")
    (tags "nRF24L01 adapter breakout")
    (fp_text reference ESP1 (at 10.3 -2.5 180) (layer F.SilkS) hide)
    (fp_text value ESP8266-SP01 (at 4.445 10.795 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 16 /LV_TX1))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole circle (at 0 2.54 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 17 /LV_VCC))
    (pad 4 thru_hole circle (at 2.54 2.54 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
    (pad 5 thru_hole circle (at 0 5.08 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
    (pad 6 thru_hole circle (at 2.54 5.08 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
    (pad 7 thru_hole circle (at 0 7.62 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 17 /LV_VCC))
    (pad 8 thru_hole circle (at 2.54 7.62 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 18 /LV_RX0))
  )
  (module BRICE:USBB-PCB (layer Top) (tedit 5A072C49)
    (at 153.035 92.075)
    (fp_text reference USB1 (at -3.81 -8.255) (layer F.SilkS) hide)
    (fp_text value USB_PCB (at -4.445 -6.35) (layer F.Fab))
    (fp_text user 5VCC (at -2.54 -10.16) (layer F.SilkS))
    (fp_text user GND (at -2.54 0 180) (layer F.SilkS))
    (pad 7 thru_hole circle (at -7.62 0.254) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole circle (at -7.62 -10.414) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole circle (at 0 -10.16) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 20 /HV_VCC))
    (pad 4 thru_hole circle (at 0 -7.62) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 0 -5.08) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 0 -2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module BRICE:REGULATEUR (layer Top) (tedit 59E39C05)
    (at 185.42 75.565)
    (fp_text reference U3 (at 3.81 -2.54) (layer F.SilkS) hide)
    (fp_text value REGULATEUR (at 0 2.54) (layer F.Fab))
    (fp_text user 5V (at -2.54 -2.54) (layer F.SilkS))
    (fp_text user 3,3V (at 0 -2.54) (layer F.SilkS))
    (fp_text user GND (at 2.54 -2.54) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.54 0) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 19 /MEGA_5V/2))
    (pad 2 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 13 /VCC-3.3))
    (pad 3 thru_hole circle (at 2.54 0) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module BRICE:Arduino_Mega_RFLINK (layer Top) (tedit 59E3415A)
    (at 99.06 99.06)
    (fp_text reference AR1 (at 10.414 -64.897) (layer F.SilkS) hide)
    (fp_text value ARDUNIO_MEGA_RFLINK_1 (at 10.414 -66.802) (layer F.Fab))
    (fp_text user 5VCC (at 95.25 -52.705) (layer F.SilkS))
    (fp_text user "Arduino Mega Rev 3" (at 72.39 -11.43) (layer B.SilkS) hide)
    (fp_text user 2017 (at 46.99 -50.8) (layer B.SilkS))
    (fp_text user GND (at 95.25 -5.715) (layer F.SilkS))
    (pad A1 thru_hole circle (at 53.34 -2.54) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask))
    (pad A2 thru_hole circle (at 55.88 -2.54) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask))
    (pad A3 thru_hole circle (at 58.42 -2.54) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 58.42 -50.8) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 55.88 -50.8) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at 53.34 -50.8) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask))
    (pad 5V/3 thru_hole circle (at 96.52 -50.8) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask))
    (pad 5V/2 thru_hole circle (at 93.98 -50.8) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 19 /MEGA_5V/2))
    (pad A0 thru_hole circle (at 50.8 -2.54) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask))
    (pad 5 thru_hole circle (at 50.8 -50.8) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 60.96 -50.8) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 14 /MEGA_TX0))
    (pad 0 thru_hole circle (at 63.5 -50.8) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 15 /MEGA_RX0))
    (pad 49 thru_hole circle (at 96.52 -15.24) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 /MEGA-PIN49))
    (pad 48 thru_hole circle (at 93.98 -15.24) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 5 /MEGA-PIN48))
    (pad 51 thru_hole circle (at 96.52 -12.7) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 6 /MEGA-PIN51))
    (pad 50 thru_hole circle (at 93.98 -12.7) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 7 /MEGA-PIN50))
    (pad 53 thru_hole circle (at 96.52 -10.16) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask))
    (pad 52 thru_hole circle (at 93.98 -10.16) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 8 /MEGA-PIN52))
    (pad GND thru_hole circle (at 96.52 -7.62) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad GND thru_hole circle (at 93.98 -7.62) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad A8 thru_hole circle (at 73.66 -2.54) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask))
    (pad A9 thru_hole circle (at 76.2 -2.54) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask))
    (pad A10 thru_hole circle (at 78.74 -2.54) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask))
    (pad A11 thru_hole circle (at 81.28 -2.54) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask))
    (pad A12 thru_hole circle (at 83.82 -2.54) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask))
    (pad A13 thru_hole circle (at 86.36 -2.54) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask))
    (pad A14 thru_hole circle (at 88.9 -2.54) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask))
    (pad A15 thru_hole circle (at 91.44 -2.54) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask))
    (pad 16 thru_hole circle (at 73.66 -50.8) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 10 /MEGA-PIN16))
    (pad 17 thru_hole circle (at 76.2 -50.8) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask))
    (pad 20 thru_hole circle (at 83.82 -50.8) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask))
    (pad 15 thru_hole circle (at 71.12 -50.8) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 9 /MEGA-PIN15))
    (pad 14 thru_hole circle (at 68.58 -50.8) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 12 "/MEGA-PIN14(TX)"))
    (pad 18 thru_hole circle (at 78.74 -50.8) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask))
    (pad 19 thru_hole circle (at 81.28 -50.8) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 11 /MEGA-PIN19))
    (pad 21 thru_hole circle (at 86.36 -50.8) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 96.52 -2.54) (size 3.175 3.175) (drill 3.175) (layers *.Cu *.Mask))
  )
  (module Connectors:SMB_Straight (layer Top) (tedit 59E33AB0)
    (at 184.15 61.595)
    (descr "SMB pcb mounting jack")
    (tags "SMB Jack  Striaght")
    (fp_text reference AE1 (at 0 -4.85) (layer F.SilkS))
    (fp_text value Antenne_Shield (at 0 5.05) (layer F.Fab))
    (pad 2 thru_hole circle (at -2.54 2.54) (size 2.74 2.74) (drill 1.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.54 2.54) (size 2.74 2.74) (drill 1.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.54 -2.54) (size 2.74 2.74) (drill 1.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at -2.54 -2.54) (size 2.74 2.74) (drill 1.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0) (size 2.24 2.24) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 /ANT1))
    (model Connectors.3dshapes/SMB_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:SMB_Straight (layer Top) (tedit 59E34085)
    (at 150.495 61.595)
    (descr "SMB pcb mounting jack")
    (tags "SMB Jack  Striaght")
    (fp_text reference AE2 (at 0 -5.08 180) (layer F.SilkS))
    (fp_text value Antenne_Shield (at 0 5.05) (layer F.Fab))
    (pad 2 thru_hole circle (at -2.54 2.54) (size 2.74 2.74) (drill 1.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.54 2.54) (size 2.74 2.74) (drill 1.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.54 -2.54) (size 2.74 2.74) (drill 1.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at -2.54 -2.54) (size 2.74 2.74) (drill 1.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0) (size 2.24 2.24) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 /ANT2))
    (model Connectors.3dshapes/SMB_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RF_Modules:nRF24L01_Breakout (layer Top) (tedit 5926EB45)
    (at 189.484 91.948 180)
    (descr "nRF24L01 breakout board")
    (tags "nRF24L01 adapter breakout")
    (fp_text reference nR1 (at 8.255 -0.635 180) (layer F.SilkS) hide)
    (fp_text value nRF24L01 (at 13 5 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 13 /VCC-3.3))
    (pad 3 thru_hole circle (at 0 2.54 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 5 /MEGA-PIN48))
    (pad 4 thru_hole circle (at 2.54 2.54 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 4 /MEGA-PIN49))
    (pad 5 thru_hole circle (at 0 5.08 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 8 /MEGA-PIN52))
    (pad 6 thru_hole circle (at 2.54 5.08 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 6 /MEGA-PIN51))
    (pad 7 thru_hole circle (at 0 7.62 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 7 /MEGA-PIN50))
    (pad 8 thru_hole circle (at 2.54 7.62 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module BRICE:RF_RXB6 (layer Top) (tedit 59E3AA38)
    (at 167.64 52.07)
    (fp_text reference RE1 (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value RXB6 (at 0 -5.08) (layer F.Fab))
    (fp_text user Data (at 17.78 1.905 180) (layer F.SilkS))
    (fp_text user Vcc (at 12.7 1.905 180) (layer F.SilkS))
    (fp_text user Gnd (at 20.32 1.905 180) (layer F.SilkS))
    (fp_text user Gnd (at -15.24 1.905 180) (layer F.SilkS))
    (fp_text user Gnd (at -17.78 1.905 180) (layer F.SilkS))
    (fp_text user Ant (at -20.32 1.905 180) (layer F.SilkS))
    (pad 8 thru_hole circle (at -20.32 0) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 /ANT2))
    (pad 7 thru_hole circle (at -17.78 0) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole circle (at -15.24 0) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole circle (at -12.7 0) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask))
    (pad 4 thru_hole rect (at 12.7 0) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 10 /MEGA-PIN16))
    (pad 3 thru_hole circle (at 15.24 0) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 17.78 0) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 11 /MEGA-PIN19))
    (pad 1 thru_hole circle (at 20.32 0) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Capacitors_THT:CP_Radial_D5.0mm_P2.50mm (layer Top) (tedit 59E3AD18)
    (at 158.75 73.66 270)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference C1 (at -1.905 2.54 270) (layer F.SilkS))
    (fp_text value CP (at 1.25 3.81 270) (layer F.Fab))
    (fp_text user %R (at 1.25 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 /LV_VCC))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module BRICE:REGULATEUR (layer Top) (tedit 5A072462)
    (at 149.987 75.565)
    (fp_text reference U4 (at -0.127 -4.445) (layer F.SilkS) hide)
    (fp_text value REGULATEUR (at 0 2.54) (layer F.Fab))
    (fp_text user 5V (at -2.54 -2.54) (layer F.SilkS))
    (fp_text user 3,3V (at 0 -2.54) (layer F.SilkS))
    (fp_text user GND (at 2.54 -2.54) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.54 0) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 20 /HV_VCC))
    (pad 2 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 17 /LV_VCC))
    (pad 3 thru_hole circle (at 2.54 0) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module BRICE:SYN115 (layer Top) (tedit 59E6391E)
    (at 168.402 60.96)
    (fp_text reference U2 (at -5.715 1.27 90) (layer F.SilkS) hide)
    (fp_text value SYN115 (at -3.81 -6.985 180) (layer F.Fab))
    (fp_text user SYN115 (at 5.588 -3.556 90) (layer F.SilkS))
    (fp_text user Ant (at 3.175 -1.905) (layer F.SilkS))
    (fp_text user GND (at 0 -1.905) (layer F.SilkS))
    (fp_text user DAT (at -2.54 -1.905) (layer F.SilkS))
    (fp_text user VCC (at -5.08 -1.905) (layer F.SilkS))
    (pad 4 thru_hole circle (at 3.175 -3.7465 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 /ANT1))
    (pad 3 thru_hole circle (at 0 -3.7465 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at -2.54 -3.7465 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 12 "/MEGA-PIN14(TX)"))
    (pad 1 thru_hole rect (at -5.08 -3.7465 270) (size 1.5 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 9 /MEGA-PIN15))
  )
  (module BRICE:FS1000A (layer Top) (tedit 5A072FC3)
    (at 167.64 66.675)
    (fp_text reference U1 (at -7.874 0.508) (layer F.SilkS) hide)
    (fp_text value FS1000A (at 0 2.54) (layer F.Fab))
    (fp_text user gnd (at 2.54 -2.54) (layer F.SilkS))
    (fp_text user vcc (at 0 -2.54) (layer F.SilkS))
    (fp_text user Dat (at -2.54 -2.54) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.54 0) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 12 "/MEGA-PIN14(TX)"))
    (pad 2 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 9 /MEGA-PIN15))
    (pad 3 thru_hole circle (at 2.54 0) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Symbols:KiCad-Logo2_6mm_SilkScreen (layer Bottom) (tedit 0)
    (at 172.72 61.976 180)
    (descr "KiCad Logo")
    (tags "Logo KiCad")
    (attr virtual)
    (fp_text reference REF*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value KiCad-Logo2_6mm_SilkScreen (at 0.75 0 180) (layer B.Fab) hide)
  )
  (module Symbols:OSHW-Logo2_14.6x12mm_SilkScreen (layer Bottom) (tedit 0)
    (at 175.895 73.533 180)
    (descr "Open Source Hardware Symbol")
    (tags "Logo Symbol OSHW")
    (attr virtual)
    (fp_text reference REF*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value OSHW-Logo2_14.6x12mm_SilkScreen (at 0.75 0 180) (layer B.Fab) hide)
  )
  (module Symbols:WEEE-Logo_8.4x12mm_SilkScreen (layer Bottom) (tedit 0)
    (at 164.846 73.66 180)
    (descr "Waste Electrical and Electronic Equipment Directive")
    (tags "Logo WEEE")
    (attr virtual)
    (fp_text reference REF*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value WEEE-Logo_8.4x12mm_SilkScreen (at 0.75 0 180) (layer B.Fab) hide)
  )
  (module Symbols:ESD-Logo_6.6x6mm_SilkScreen (layer Bottom) (tedit 0)
    (at 160.401 61.976 180)
    (descr "Electrostatic discharge Logo")
    (tags "Logo ESD")
    (attr virtual)
    (fp_text reference REF*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value ESD-Logo_6.6x6mm_SilkScreen (at 0.75 0 180) (layer B.Fab) hide)
  )
  (gr_text "ESP\nRX" (at 181.61 89.408) (layer F.SilkS))
  (gr_text "ESP\nTX" (at 168.91 89.408) (layer F.SilkS))
  (gr_text "MEGA\nTX" (at 181.61 83.312) (layer F.SilkS))
  (gr_text "MEGA\nRX" (at 168.91 83.312) (layer F.SilkS))
  (gr_text ZIONIII (at 165.227 96.647) (layer F.SilkS))
  (gr_line (start 191.77 50.165) (end 191.77 80.772) (angle 90) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 191.77 50.165) (end 198.12 50.165) (angle 90) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 192.532 81.534) (end 197.358 81.534) (angle 90) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 198.12 82.296) (end 198.12 98.298) (angle 90) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 144.272 45.72) (end 191.77 45.72) (angle 90) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 143.51 98.298) (end 143.51 46.482) (angle 90) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 197.358 99.06) (end 144.272 99.06) (angle 90) (layer Edge.Cuts) (width 0.127))
  (gr_arc (start 192.532 80.772) (end 192.532 81.534) (angle 90) (layer Edge.Cuts) (width 0.127))
  (gr_arc (start 197.358 82.296) (end 197.358 81.534) (angle 90) (layer Edge.Cuts) (width 0.127))
  (gr_arc (start 197.358 98.298) (end 198.12 98.298) (angle 90) (layer Edge.Cuts) (width 0.127))
  (gr_arc (start 144.272 98.298) (end 144.272 99.06) (angle 90) (layer Edge.Cuts) (width 0.127))
  (gr_arc (start 144.272 46.482) (end 143.51 46.482) (angle 90) (layer Edge.Cuts) (width 0.127))
  (gr_text "Alimentation\nESP8226-SP01\n5VCC" (at 147.955 86.995) (layer F.SilkS))
  (gr_text "LEVEL\nSHIFTERS\n" (at 175.26 86.106) (layer F.SilkS))
  (gr_text "2017\n" (at 189.23 48.26) (layer F.SilkS))
  (gr_text "REGULATEUR DE\nTENSION ESP8266" (at 149.86 70.485) (layer F.SilkS))
  (gr_text "ESP8226\nSP01" (at 157.607 92.964) (layer F.SilkS))
  (gr_text "REGULATEUR DE\nTENSION NRF24L01" (at 185.42 70.485) (layer F.SilkS))
  (gr_line (start 195.58 45.72) (end 191.77 45.72) (angle 90) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 198.12 48.26) (end 195.58 45.72) (angle 90) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 198.12 50.165) (end 198.12 48.26) (angle 90) (layer Edge.Cuts) (width 0.127))
  (gr_text "NB: \nFS1000A ou SYN115" (at 168.275 61.595) (layer F.SilkS))
  (gr_text RXB6 (at 174.625 52.07) (layer F.SilkS))
  (gr_text NRF24L01 (at 188.214 81.407) (layer F.SilkS))
  (gr_text "DESIGN IN FRENCH\nZIONIII - RFLINK B V1 - WIFI\nhttps://easydomoticz.com/" (at 172.974 86.36) (layer B.SilkS))
  (gr_text FS1000A (at 175.895 65.405 90) (layer F.SilkS))
  (gr_text "RFLINK B V1 - 2017\nWIFI\nRF 433 Mhz et 2,4 Ghz" (at 170.815 74.93) (layer F.SilkS))
  (zone (net 1) (net_name GND) (layer Bottom) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 198.12 50.165) (xy 191.77 50.165) (xy 191.77 59.944) (xy 191.77 81.534) (xy 198.12 81.534)
        (xy 198.12 99.06) (xy 143.51 99.06) (xy 143.51 45.72) (xy 189.23 45.72) (xy 191.77 45.72)
        (xy 195.58 45.72) (xy 198.12 48.26)
      )
    )
    (polygon
      (pts        (xy 146.05 52.705) (xy 148.59 52.705) (xy 148.59 53.975) (xy 151.765 53.975) (xy 151.765 60.325)
        (xy 149.225 60.325) (xy 149.225 56.515) (xy 146.05 56.515)
      )
    )
    (polygon
      (pts        (xy 182.88 60.452) (xy 182.88 62.738) (xy 175.26 62.738) (xy 171.196 58.674) (xy 172.974 56.896)
        (xy 176.53 60.452)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer Top) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 191.77 81.534) (xy 198.12 81.534) (xy 198.12 99.06) (xy 143.51 99.06) (xy 143.51 45.72)
        (xy 191.77 45.72) (xy 195.58 45.72) (xy 198.12 48.26) (xy 198.12 50.165) (xy 191.77 50.165)
      )
    )
  )
)
